ND attack defense probe commands -- display system internal nd raguard policy

Use display system internal nd raguard policy to display information about RA guard policies.

Syntax

Centralized devices:

display system internal nd raguard policy [ policy-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nd raguard policy [ policy-name ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal nd raguard policy [ policy-name ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

policy-name: Specifies an RA guard policy by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a policy name, this command displays information about all RA guard policies.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.