WLAN virtual client probe commands -- display system internal wlan virtual ap (on ACs)

| NOTE: Support for this command depends on the device model.

Use display system internal wlan virtual ap to display virtual AP information.

Syntax

display system internal wlan virtual ap { all | bssid bssid }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all virtual APs.

bssid bssid: Specifies a virtual AP by the BSSID.

WLAN virtual client probe commands -- display system internal wlan virtual client

Use display system internal wlan virtual client to display virtual client information.

Syntax

display system internal wlan virtual client { all | bssid bssid }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all virtual clients.

bssid bssid: Specifies a virtual AP by the BSSID.

WLAN virtual client probe commands -- wlan virtual ap add

Use wlan virtual ap add to create virtual APs.

Syntax

wlan virtual ap add { ipv4 ac-ip-address ap-ip-start | ipv6 ac-ipv6-address ap-ipv6-start } bssid bssid-start [ count count step ap-ip-step bssid-step ] [ port port-start step port-step ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4: Specifies AP IPv4 addresses.

ac-ip-address: Specifies an AC IPv4 address.

ap-ip-start: Specifies the start AP IPv4 address.

ipv6: Specifies AP IPv6 addresses.

ac-ipv6-address: Specifies an AC IPv6 address.

ap-ipv6-start: Specifies the start AP IPv6 address.

bssid bssid-start: Specifies the start BSSID.

count count: Specifies the number of APs to be created. If you do not specify this option, the command creates one virtual AP.

step ap-ip-step bssid-step: Specifies steps by which AP IP addresses and BSSIDs increase.

port port-start: Specifies port numbers used to establish CAPWAP tunnels for virtual APs. The port-start argument specifies the start port number. If you do not specify this option, the command sets the start port number to 1024.

step port-step: Specifies the step by which port numbers increase. If you do not specify this option, the command sets the step to 1.

WLAN virtual client probe commands -- wlan virtual ap delete

Use wlan virtual ap delete to delete virtual APs.

Syntax

wlan virtual ap delete { all | bssid bssid }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all virtual APs.

bssid bssid: Specifies a virtual AP by the BSSID.

WLAN virtual client probe commands -- wlan virtual client add

Use wlan virtual client add to create virtual clients.

Syntax

wlan virtual client add mac client-mac-start { ipv4 client-ip-start | ipv6 client-ipv6-start } [ count count ] [ step client-mac-step client-ip-step ] vlan vlan-id bssid { all | bssid } service-template service-template-name [ non-wmm ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mac client-mac-start: Specifies the start client MAC address.

ipv4: Specifies client IPv4 addresses.

client-ip-start: Specifies the start client IPv4 address.

ipv6: Specifies client IPv6 addresses.

client-ipv6-start: Specifies the start client IPv6 address.

count count: Specifies the number of clients to be created for each virtual AP. If you do not specify this option, the command creates one virtual client for each virtual AP.

step client-mac-step client-ip-step: Specifies steps by which client MAC addresses and IP addresses increase. If you do not specify this option, the command sets both steps to 1.

vlan vlan-id: Specifies a VLAN.

bssid: Specifies virtual APs by BSSIDs for the virtual clients.

all: Specifies all APs. If you specify this keyword, the command creates virtual clients at the specified step for each AP in turn.

bssid: Specifies a virtual AP by the BSSID.

service-template service-template-name: Specifies a service template by its name.

non-wmm: Specifies non-WMM clients. If you do not specify this keyword, the command creates WMM clients.

Usage guidelines

Use the wlan virtual ap add command to create virtual APs before you execute this command.

Related commands

wlan virtual ap add

WLAN virtual client probe commands -- wlan virtual client delete

Use wlan virtual client delete to delete virtual clients.

Syntax

wlan virtual client delete { all | bssid bssid | mac mac-address }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all virtual clients.

mac mac-address: Specifies a virtual client by its MAC address.

bssid bssid: Specifies a virtual AP by the BSSID.