MPLS L3VPN probe commands -- debugging system internal ip vpn-instance

Use debugging system internal ip vpn-instance to enable VPN instance debugging.

Use undo debugging system internal ip vpn-instance to disable VPN instance debugging.

Syntax

Centralized devices:

debugging system internal ip vpn-instance

undo debugging system internal ip vpn-instance

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal ip vpn-instance slot slot-number [ cpu cpu-number ]

undo debugging system internal ip vpn-instance slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal ip vpn-instance chassis chassis-number slot slot-number [ cpu cpu-number ]

undo debugging system internal ip vpn-instance chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

VPN instance debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MPLS L3VPN probe commands -- display system internal ip vpn-binding

Use display system internal ip vpn-binding to display VPN instance binding information for the system kernel.

Syntax

Centralized devices:

display system internal ip vpn-binding

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip vpn-binding slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip vpn-binding chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MPLS L3VPN probe commands -- display system internal ip vpn-instance

Use display system internal ip vpn-instance to display VPN instance information for the system kernel.

Syntax

Centralized devices:

display system internal ip vpn-instance [ instance-name vpn-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip vpn-instance [ instance-name vpn-instance-name ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip vpn-instance [ instance-name vpn-instance-name ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance-name vpn-instance-name: Specifies a VPN instance by its name. The vpn-instance-name argument is a case-sensitive string of 1 to 31 characters.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MPLS L3VPN probe commands -- display system internal ip vpn-instance inactive

Use display system internal ip vpn-instance inactive to display information about VPN instances that are being deleted.

Syntax

display system internal ip vpn-instance inactive

Views

Probe view

Predefined user roles

network-admin

mdc-admin

MPLS L3VPN probe commands -- display system internal ip vpn-instance statistics

Use display system internal ip vpn-instance statistics to display VPN instance statistics for the system kernel.

Syntax

Centralized devices:

display system internal ip vpn-instance statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip vpn-instance statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ip vpn-instance statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MPLS L3VPN probe commands -- display system internal ospf sham-link standby

Use display system internal ospf sham-link standby to display OSPF sham link information for a standby OSPF process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] sham-link [ area area-id ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] sham-link [ area area-id ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Displays sham link information for the OSPF process specified by its ID. The process ID is in the range of 1 to 65535. If you do not specify a process, this command displays sham link information for all OSPF processes.

area area-id: Displays sham link information for the OSPF area specified by its ID, which is an IP address, or an integer. The integer is in the range of 0 to 4294967295. If you do not specify an area, this command displays sham link information for all OSPF areas.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the number of the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

If you do not specify any process or area, this command displays information about all OSPF sham links.

The active OSPF process backs up OSPF peers and routing information to the standby OSPF process only when OSPF NSR is enabled. If OSPF NSR is disabled, this command does not display anything when you execute it by using the standby keyword.