MBUF probe commands -- display system internal mbuf relay statistics

Use display system internal mbuf relay statistics to display MBUF Relay statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mbuf relay statistics slot slot-number [ cpu cpu-number ] [ vcpu vcpu-number ] [ rcv receiver-id ]

Distributed devices in IRF mode:

display system internal mbuf relay statistics chassis chassis-number slot slot-number [ cpu cpu-number ] [ vcpu vcpu-number ] [ rcv receiver-id ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies a member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

vcpu vcpu-number: Specifies a vCPU by its number. If you do not specify a vCPU, this command displays MBUF Relay statistics for all vCPUs on the card.

rcv received-id: Specifies the MBUF Relay receiver by its ID. If you do not specify an MBUF Relay receiver, this command displays MBUF Relay statistics for all the receivers on the VCPU.

MBUF probe commands -- display system internal mbuf socket statistics

Use display system internal mbuf socket statistics to display MBUF socket statistics.

Syntax

Centralized devices:

display system internal mbuf socket statistics

Distributed devices–Centralized IRF devices–In standalone mode:

display system internal mbuf socket statistics slot slot-number [ cpu cpu-number ]

Distributed devices–In IRF mode:

display system internal mbuf socket statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices–In standalone mode.)

slot slot-number: Specifies a member device by its member ID. (Centralized IRF devices, IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number.(Centralized IRF devices, IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices–In IRF mode, IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. (Distributed devices–In IRF mode, IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MBUF probe commands -- reset system internal mbuf relay statistics

Use reset system internal mbuf relay statistics to clear MBUF Relay statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal mbuf relay statistics slot slot-number [ cpu cpu-number ] [ vcpu vcpu-number ] [ rcv receiver-id ]

Distributed devices in IRF mode:

reset system internal mbuf relay statistics chassis chassis-number slot slot-number [ cpu cpu-number ] [ vcpu vcpu-number ] [ rcv receiver-id]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

vcpu vcpu-number: Specifies a vCPU by its number. If you do not specify a vCPU, this command clears MBUF Relay statistics for all vCPUs on the card.

rcv received-id: Specifies the MBUF Relay receiver by its ID. If you do not specify an MBUF Relay receiver, this command clears MBUF Relay statistics for all the receivers on the VCPU.