IP performance optimization probe commands -- display system internal rawip

| NOTE: Support for this command depends on the device model.

Use display system internal rawip to display brief information about RawIP connections.

Syntax

Centralized devices:

display system internal rawip

Distributed devices in standalone mode:Centralized IRF devices:

display system internal rawip slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal rawip chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal tcp

| NOTE: Support for this command depends on the device model.

Use display system internal tcp to display brief information about TCP connections.

Syntax

Centralized devices:

display system internal tcp

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tcp slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal tcp chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal tcp port-info

| NOTE: Support for this command depends on the device model.

Use display system internal tcp port-info to display non-well known TCP port usage.

Syntax

Centralized devices:

display system internal tcp port-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tcp port-info [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal tcp port-info [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays non-well known TCP port usage for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays non-well known TCP port usage for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays non-well known TCP port usage for all member devices if you do not specify a member device. On an IRF 3 system, this command displays usage information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays non-well known TCP port usage for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays non-well known TCP port usage for all cards if you do not specify a card. On an IRF 3 system, this command displays usage information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal tcp-proxy statistics

| NOTE: Support for this command depends on the device model.

Use display system internal tcp-proxy statistics to display TCP proxy statistics about IPv4 and IPv6 TCP connections.

Syntax

Centralized devices:

display system internal tcp-proxy statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tcp-proxy statistics { all | api | error | fsm | packet } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal tcp-proxy statistics { all | api | error | fsm | packet } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Displays all TCP proxy statistics.

api: Displays statistics about API calls.

error: Displays statistics about error packets.

fsm: Displays statistics about finite state machine (FSM) packets.

packet: Displays statistics about input and output TCP packets.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays TCP proxy statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays TCP proxy statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays TCP proxy statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays TCP proxy statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays TCP proxy statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays TCP proxy statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays TCP proxy statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal tcp-proxy verbose

| NOTE: Support for this command depends on the device model.

Use display system internal tcp-proxy verbose to display detailed information about TCP proxy.

Syntax

Centralized devices:

display system internal tcp-proxy verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal tcp-proxy verbose slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal tcp-proxy verbose chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal udp

| NOTE: Support for this command depends on the device model.

Use display system internal udp to display brief information about UDP connections.

Syntax

Centralized devices:

display system internal udp

Distributed devices in standalone mode:Centralized IRF devices:

display system internal udp slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal udp chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- display system internal udp port-info

| NOTE: Support for this command depends on the device model.

Use display system internal udp port-info to display non-well known UDP port usage.

Syntax

Centralized devices:

display system internal udp port-info

Distributed devices in standalone mode:Centralized IRF devices:

display system internal udp port-info [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal udp port-info [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays non-well known UDP port usage for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays non-well known UDP port usage for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays non-well known UDP port usage for all member devices if you do not specify a member device. On an IRF 3 system, this command displays usage information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. If you do not specify a card, this command displays usage information about UDP ports for all cards except for the unassigned ports. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays non-well known UDP port usage for all cards if you do not specify a card. On an IRF 3 system, this command displays usage information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

IP performance optimization probe commands -- reset system internal tcp-proxy statistics

Use reset system internal tcp-proxy statistics to clear TCP proxy statistics for IPv4 and IPv6 TCP connections.

Syntax

reset system internal tcp-proxy statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

IP performance optimization probe commands -- tcp-proxy statistics

| NOTE: Support for this command depends on the device model.

Use tcp-proxy statistics to turn on or off counters for TCP proxy.

Syntax

tcp-proxy statistics { off | on }

Default

Counters are turned off for TCP proxy.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

off: Turns off counters for TCP proxy.

on: Turns on counters for TCP proxy.

Usage guidelines

The TCP proxy counters collect information about the numbers of API calls, input and output TCP packets, error packets, and FSM packets.