OSPFv3 probe commands -- display system internal ospfv3 event-log

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 event-log to display OSPFv3 log information.

Syntax

display system internal ospfv3 event-log { gr | nib | rib }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

gr: Displays GR log information.

nib: Displays NIB log information.

rib: Displays RIB log information.

OSPFv3 probe commands -- display system internal ospfv3 flood-list

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 flood-list to display OSPFv3 flooding information.

Syntax

display system internal ospfv3 [ process-id ] flood-list [ interface-type interface-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays flooding information for all OSPFv3 processes.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays flooding information for all interfaces.

OSPFv3 probe commands -- display system internal ospfv3 interface

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 interface to display OSPFv3 interface information.

Syntax

display system internal ospfv3 interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ipv6-address: Specifies an IPv6 address prefix.

prefix-length: Specifies the prefix length, an integer in the range of 0 to 128.

OSPFv3 probe commands -- display system internal ospfv3 interface standby

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 interface standby to display backup OSPFv3 interface information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospfv3 [ process-id ] interface [ interface-type interface-number | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospfv3 [ process-id ] interface [ interface-type interface-number | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535.

interface-type interface-number: Specifies an interface by its type and number.

verbose: Displays detailed OSPFv3 interface information.

standby slot slot-number: Displays backup OSPFv3 interface information for a card. If you do not specify this option, the command displays OSPFv3 interface information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPFv3 interface information for an IRF member device. If you do not specify this option, the command displays OSPFv3 interface information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPFv3 interface information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPFv3 interface information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Usage guidelines

If you do not specify an OSPFv3 process, this command displays interface information for all OSPFv3 processes.

If you do not specify both the interface-type interface-number argument and the verbose keyword, this command displays brief information for all OSPFv3 interfaces.

OSPFv3 probe commands -- display system internal ospfv3 keychain

Use display system internal ospfv3 keychain to display OSPFv3 keychain information.

Syntax

display system internal ospfv3 keychain [ name keychain-name [ key key-id ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

name keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters. If you do not specify this option, the command displays information about all keychains for an OSPFv3 process.

key key-id: Specifies a key by its ID in the range of 0 to 281474976710655. If you do not specify this option, the command displays information about all keys of the keychain.

OSPFv3 probe commands -- display system internal ospfv3 lsdb

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 lsdb to display OSPFv3 LSA information in the LSDB.

Syntax

display system internal ospfv3 [ process-id ] lsdb { inter-prefix | inter-router | intra-prefix { reference type-1 | reference type-2 } | router }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSA information for all OSPFv3 processes.

inter-prefix: Displays Inter-Area-Prefix LSA information in the LSDB.

inter-router: Displays Inter-Area-Router LSA information in the LSDB.

intra-prefix: Displays Intra-Area-Prefix LSA information in the LSDB.

reference type-1: Displays information about Intra-Area-Prefix LSAs that reference Router LSAs.

reference type-2: Displays information about Intra-Area-Prefix LSAs that reference Network LSAs.

router: Displays Router LSA information in the LSDB.

OSPFv3 probe commands -- display system internal ospfv3 lsdb standby

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 lsdb standby to display backup OSPFv3 LSDB information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospfv3 [ process-id ] lsdb [ { external | grace | inter-prefix | inter-router | intra-prefix | link | network | nssa | router | unknown [ type ] } [ link-state-id ] [ originate-router router-id | self-originate ] | statistics | total | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospfv3 [ process-id ] lsdb [ { external | grace | inter-prefix | inter-router | intra-prefix | link | network | nssa | router | unknown [ type ] } [ link-state-id ] [ originate-router router-id | self-originate ] | statistics | total | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSDB information for all OSPFv3 processes.

external: Displays AS external LSAs (Type-5 LSAs).

grace: Displays Grace-LSAs (Type-11 LSAs).

inter-prefix: Displays Inter-area-prefix LSAs (Type-3 LSAs).

inter-router: Displays Inter-area-router LSAs (Type-4 LSAs).

intra-prefix: Displays Intra-area-prefix LSAs (Type-9 LSAs).

link: Displays Link-LSAs (Type-8 LSAs).

network: Displays Network-LSAs (Type-2 LSAs).

nssa: Displays NSSA LSAs (Type-7 LSAs).

router: Displays Router-LSAs (Type-1 LSAs).

unknown: Displays unknown LSAs.

type: Specifies an LSA type, a hexadecimal string of 0 to ffff. If you do not specify this argument, the command displays all unknown LSAs.

link-state-id: Specifies a link state ID in IPv4 address format.

originate-router router-id: Specifies an advertising router by its ID.

self-originate: Displays locally originated LSAs.

statistics: Displays LSA statistics.

total: Displays the total number of LSAs in the LSDB.

verbose: Displays detailed information. If you do not specify this keyword, the command displays brief information.

standby slot slot-number: Displays backup OSPFv3 LSDB information for a card. If you do not specify this option, the command displays OSPFv3 LSDB information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPFv3 LSDB information for an IRF member device. If you do not specify this option, the command displays OSPFv3 LSDB information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPFv3 LSDB information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPFv3 LSDB information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPFv3 probe commands -- display system internal ospfv3 nib

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 nib to display OSPFv3 next hop information.

Syntax

display system internal ospfv3 nib [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID, a hexadecimal number in the range of 1 to ffffffff.

verbose: Displays detailed OSPFv3 next hop information.

OSPFv3 probe commands -- display system internal ospfv3 peer standby

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 peer standby to display backup OSPFv3 neighbor information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospfv3 [ process-id ] [ area area-id ] peer [ [ interface-type interface-number ] [ verbose ] | peer-router-id | statistics ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospfv3 [ process-id ] [ area area-id ] peer [ [ interface-type interface-number ] [ verbose ] | peer-router-id | statistics ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535.

area area-id: Specifies an area by its ID, an IPv4 address or a decimal integer in the range of 0 to 4294967295 that is translated into the IPv4 address format.

interface-type interface-number: Specifies an interface by its type and number.

verbose: Displays detailed neighbor information.

peer-router-id: Specifies a neighbor router ID.

statistics: Displays OSPFv3 neighbor statistics.

standby slot slot-number: Displays backup OSPFv3 neighbor information for a card. If you do not specify this option, the command displays OSPFv3 neighbor information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPFv3 neighbor information for an IRF member device. If you do not specify this option, the command displays OSPFv3 neighbor information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPFv3 neighbor information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPFv3 neighbor information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

Usage guidelines

If no OSPFv3 process is specified, this command displays neighbor information for all OSPFv3 processes.

If no area is specified, this command displays neighbor information for all OSPFv3 areas.

If both the interface-type interface-number and peer-router-id arguments are not specified, this command displays neighbor information for all interfaces.

OSPFv3 probe commands -- display system internal ospfv3 prefix

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 prefix to display OSPFv3 prefix information.

Syntax

display system internal ospfv3 [ process-id ] prefix { inter | intra } [ ipv6-address prefix-length ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays prefix information for all OSPFv3 processes.

inter: Displays inter-AS prefix information.

intra: Displays intra-AS prefix information.

ipv6-address prefix-length: Specifies an IPv6 address. The ipv6-address argument specifies an IPv6 prefix. The prefix-length argument specifies a prefix length in the range of 0 to 128. If you do not specify this argument, the command displays all OSPFv3 prefix information.

OSPFv3 probe commands -- display system internal ospfv3 router

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 router to display routing information to router nodes.

Syntax

display system internal ospfv3 [ process-id ] router

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays information about all OSPFv3 processes.

OSPFv3 probe commands -- display system internal ospfv3 standby

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 standby to display backup OSPFv3 process information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospfv3 [ process-id ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospfv3 [ process-id ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays information about all OSPFv3 processes.

verbose: Displays detailed OSPFv3 process information. If you do not specify this keyword, the command displays brief OSPFv3 process information.

standby slot slot-number: Displays backup OSPFv3 process information for a card. If you do not specify this option, the command displays OSPFv3 process information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPFv3 process information for an IRF member device. If you do not specify this option, the command displays OSPFv3 process information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPFv3 process information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPFv3 process information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPFv3 probe commands -- display system internal ospfv3 statistics

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 statistics to display OSPFv3 statistics.

Syntax

display system internal ospfv3 [ process-id ] statistics { request-queue | retrans-queue } [ interface-type interface-number ] [ neighbor-id ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays statistics for all OSPFv3 processes.

request-queue: Specifies request queue statistics.

retrans-queue: Specifies retransmission queue statistics.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays statistics for all interfaces.

neighbor-id: Specifies a neighbor by its ID. If you do not specify this argument, the command displays statistics for all neighbors.

OSPFv3 probe commands -- display system internal ospfv3 status

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 status to display OSPFv3 status information.

Syntax

display system internal ospfv3 status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

OSPFv3 probe commands -- display system internal ospfv3 vlink standby

| NOTE: Support for this command depends on the device model.

Use display system internal ospfv3 vlink standby to display backup OSPFv3 virtual link information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospfv3 [ process-id ] vlink standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospfv3 [ process-id ] vlink standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPFv3 process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays virtual link information for all OSPFv3 processes.

standby slot slot-number: Displays backup OSPFv3 virtual link information for a card. If you do not specify this option, the command displays OSPFv3 virtual link information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPFv3 virtual link information for an IRF member device. If you do not specify this option, the command displays OSPFv3 virtual link information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPFv3 virtual link information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPFv3 virtual link information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.