BGP commands -- address-family ipv4

Use address-family ipv4 to create the BGP IPv4 unicast address family, BGP-VPN IPv4 unicast address family, BGP IPv4 RT filter address family, or BGP IPv4 multicast address family, and enter its view, or enter the view of the existing address family.

Use undo address-family ipv4 to remove the BGP IPv4 unicast address family, BGP-VPN IPv4 unicast address family, BGP IPv4 RT filter address family, or BGP IPv4 multicast address family, and all its configurations.

Syntax

In BGP instance view:

address-family ipv4 [ multicast | rtfilter | unicast ]

undo address-family ipv4 [ multicast | rtfilter | unicast ]

In BGP-VPN instance view:

address-family ipv4 [ unicast ]

undo address-family ipv4 [ unicast ]

Default

No BGP IPv4 unicast address family, BGP-VPN IPv4 unicast address family, BGP IPv4 RT filter address family, or BGP IPv4 multicast address family exists.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

multicast: Specifies the IPv4 multicast address family.

rtfilter: Specifies the BGP IPv4 RT filter address family.

unicast: Specifies the IPv4 unicast address family. If this command is executed with the unicast keyword in BGP instance view, it places you into BGP IPv4 unicast address family view. If this command is executed with the unicast keyword in BGP-VPN instance view, it places you into BGP-VPN IPv4 unicast address family view.

Usage guidelines

Configurations made in BGP IPv4 unicast address family view apply only to the BGP IPv4 unicast routes and peers of the public network.

Configurations made in BGP-VPN IPv4 unicast address family view apply only to the BGP IPv4 unicast routes and peers of the specified VPN instance.

Configurations made in BGP IPv4 multicast address family view apply only to the BGP IPv4 multicast routes and peers.

Configurations made in BGP IPv4 RT filter address family view apply only to the BGP IPv4 RT filter routes and peers.

By default, the unicast keyword is used if you do not specify the multicast, rtfilter, or unicast keyword.

Examples

# In BGP instance view, create the BGP IPv4 unicast address family and enter its view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4]

BGP commands -- address-family ipv6

Use address-family ipv6 to create the BGP IPv6 unicast address family, BGP-VPN IPv6 unicast address family, or BGP IPv6 multicast address family, and enter its view, or enter the view of the existing address family.

Use undo address-family ipv6 to remove the BGP IPv6 unicast address family, BGP-VPN IPv6 unicast address family, or BGP IPv6 multicast address family, and all its configurations.

Syntax

In BGP instance view:

address-family ipv6 [ multicast | unicast ]

undo address-family ipv6 [ multicast | unicast ]

In BGP-VPN instance view:

address-family ipv6 [ unicast ]

undo address-family ipv6 [ unicast ]

Default

No BGP IPv6 unicast address family, BGP-VPN IPv6 unicast address family, or BGP IPv6 multicast address family exists.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

unicast: Specifies the IPv6 unicast address family. If this command is executed with the unicast keyword in BGP instance view, it places you into BGP IPv6 unicast address family view. If this command is executed with the unicast keyword in BGP-VPN instance view, it places you into BGP-VPN IPv6 unicast address family view.

multicast: Specifies the IPv6 multicast address family.

Usage guidelines

Configurations made in BGP IPv6 unicast address family view apply only to the BGP IPv6 unicast routes and peers of the public network.

Configurations made in BGP-VPN IPv6 unicast address family view apply only to the BGP IPv6 unicast routes and peers of the specified VPN instance.

Configurations made in BGP IPv6 multicast address family view apply only to the BGP IPv6 multicast routes and peers.

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# In BGP instance view, create the BGP IPv6 unicast address family and enter its view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv6 unicast

[Sysname-bgp-default-ipv6]

BGP commands -- address-family link-state

Use address-family link-state to create the BGP LS address family and enter its view, or enter the view of the existing address family.

Use undo address-family link-state to remove the BGP LS address family and all its configurations.

Syntax

address-family link-state

undo address-family link-state

Default

No BGP LS address family exists.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configurations made in BGP LS address family view apply only to the BGP LS routes and peers of the public network.

Examples

# In BGP instance view, create the BGP LS address family and enter its view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family link-state

[Sysname-bgp-default-ls]

BGP commands -- advertise-rib-active

Use advertise-rib-active to enable BGP to advertise only the optimal BGP routes in the IP routing table.

Use undo advertise-rib-active to restore the default.

Syntax

advertise-rib-active

undo advertise-rib-active

Default

In BGP instance view, BGP advertises optimal routes in the BGP routing table, regardless of whether they are optimal in the IP routing table. In other views, the setting is the same as that in BGP instance view.

Views

BGP instance view

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

The advertise-rib-active command does not apply to the following routes:

· Routes redistributed by the import-route command.

· Routes advertised by the network command.

· Default routes redistributed by the default-route imported command.

· VPNv4 routes.

· VPNv6 routes.

· IPv4 multicast routes.

· IPv6 multicast routes.

This command takes effect only on the routes generated after you execute this command. To apply this command to existing routes, use the reset bgp command to reset BGP sessions.

The setting in BGP unicast address family view applies when it is different from that in BGP instance view.

Examples

# In BGP instance view, enable BGP to advertise optimal routes in the IP routing table.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] advertise-rib-active

BGP commands -- aggregate

Use aggregate to create a summary route in the BGP routing table.

Use undo aggregate to remove a summary route.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP IPv4 multicast address family view:

aggregate ipv4-address { mask-length | mask } [ as-set | attribute-policy route-policy-name | detail-suppressed | origin-policy route-policy-name | suppress-policy route-policy-name ] *

undo aggregate ipv4-address { mask-length | mask }

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

aggregate ipv6-address prefix-length [ as-set | attribute-policy route-policy-name | detail-suppressed | origin-policy route-policy-name | suppress-policy route-policy-name ] *

undo aggregate ipv6-address prefix-length

Default

No summary routes are configured.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies an IPv4 summary address.

mask-length: Specifies a mask length for the IPv4 summary address, in the range of 0 to 32.

mask: Specifies a mask for the IPv4 summary address, in dotted decimal notation.

ipv6-address: Specifies an IPv6 summary address.

prefix-length: Specifies a prefix length for the IPv6 summary address, in the range of 0 to 128.

as-set: Enables the AS_PATH attribute of the summary route to contain the AS path information for all summarized routes. The AS_PATH attribute is of the AS_SET type that requires no sequence when arranging AS numbers. If you do not specify this keyword, the AS_PATH attribute of the summary route contains only the AS number of the local router.

attribute-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to set attributes for the summary route.

detail-suppressed: Advertises only the summary route. If you do not specify this keyword, BGP advertises both the summary route and the more specific routes.

origin-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to select routes to be summarized.

suppress-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter more specific routes to be advertised. Routes permitted by the specified routing policy are not advertised. Routes denied by the specified routing policy are advertised.

Usage guidelines

This command creates a summary route. If the BGP routing table has routes whose destination addresses fall within the specified network, the summary route is added to the BGP routing table. For example, if two routes 10.1.1.0/24 and 10.1.2.0/24 exist in the BGP routing table, configuring the aggregate 10.1.0.0 16 command creates a summary route 10.1.0.0/16.

If the summarized routes have different ORIGIN attributes, the summary route selects the ORIGIN attribute in the sequence of INCOMPLETE, EGP, and IGP. For example, if the ORIGIN attributes of the summarized routes include INCOMPLETE and IGP, the ORIGIN attribute of the summary route is INCOMPLETE.

The COMMUNITY attribute of the summary route includes all the COMMUNITY (or extended community) attribute values if the routes have the following details:

· Summarized routes have different COMMUNITY (or extended community) attribute values.

· The summary route does not have the ATOMIC_AGGREGATE attribute.

Table 1 Functions of the keywords

Keywords | Function
as-set | Enables the summary route to carry the AS path information for all summarized routes. This feature can help avoid routing loops. However, if many routes are summarized and are changed frequently, do not specify this keyword. This configuration causes the summary route to flap with the more specific routes.
attribute-policy | Sets attributes except the AS-PATH attribute for the summary route. The peer route-policy command can achieve the same purpose.
detail-suppressed | Disables advertisement of all more specific routes. To disable advertisement of some more specific routes, use the suppress-policy keyword or the peer filter-policy command.
origin-policy | Summarizes only routes matching a routing policy. If the destination address of a route falls within the summary network but does not match the routing policy, the route is not summarized. It is not controlled by the detail-suppressed and suppress-policy keywords. There is no need to configure apply clauses for the routing policy applied by the origin-policy keyword because they do not take effect.
suppress-policy | Disables advertisement of some more specific routes filtered by a routing policy. The routing policy uses if-match clauses to filter routes. There is no need to configure apply clauses for the routing policy applied by the suppress-policy keyword because they do not take effect.

Examples

# In BGP IPv4 unicast address family view, create summary route 1.1.0.0/16 in the BGP routing table.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] aggregate 1.1.0.0 255.255.0.0

Related commands

display bgp routing-table ipv4 multicast

display bgp routing-table ipv4 unicast

display bgp routing-table ipv6 multicast

display bgp routing-table ipv6 unicast

summary automatic

BGP commands -- balance

Use balance to enable load balancing and set the maximum number of BGP ECMP routes for load balancing.

Use undo balance to disable load balancing.

Syntax

balance [ ebgp | eibgp | ibgp ] number

undo balance [ ebgp | eibgp | ibgp ]

Default

Load balancing is disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ebgp: Enables load balancing over EBGP routes.

eibgp: Enables load balancing between EBGP and IBGP routes.

ibgp: Enables load balancing over IBGP routes.

number: Specifies the maximum number of BGP ECMP routes for load balancing. Its range varies by device model. When it is set to 1, load balancing is disabled.

Usage guidelines

Unlike IGP, BGP has no explicit metric for making load balancing decision. Instead, it implements load balancing by modifying route selection rules.

If multiple BGP routes destined for a network meet the following conditions, the device selects the specified number of routes for load balancing:

· The routes have the same ORIGIN, LOCAL_PREF, and MED attributes. If the balance as-path-neglect command is not configured, the routes must also have the same AS_PATH attribute.

· The routes have the same MPLS label assignment status (labeled or not labeled).

The value range for the number argument depends on the max-ecmp-num command. If you set the maximum number of ECMP routes to m by using the max-ecmp-num command and reboot the device, the number argument in the balance command is in the range of 1 to m.

If you do not specify the ibgp, eibgp, or ebgp keyword, this command enables load balancing over EBGP routes and IBGP routes, but not between EBGP and IBGP routes.

After you execute the balance eibgp number command, the balance [ ebgp | ibgp ] number and undo balance [ ebgp | ibgp ] commands cannot be executed; and vice versa.

Examples

# In BGP IPv4 unicast address family view, enable load balancing and set the maximum number of BGP ECMP routes used for load balancing to 2.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] balance 2

Related commands

balance as-path-neglect

max-ecmp-num

BGP commands -- balance as-path-neglect

Use balance as-path-neglect to enable BGP to ignore the AS_PATH attribute when it implements load balancing.

Use undo balance as-path-neglect to restore the default.

Syntax

balance as-path-neglect

undo balance as-path-neglect

Default

BGP does not ignore the AS_PATH attribute when it implements load balancing.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

For BGP to implement load balancing over routes with different AS_PATH attributes, you must use this command together with the balance command.

After this command is executed, BGP ignores the AS_PATH attributes in the routes for load balancing and changes the attributes of the advertised routes to those of the optimal route. The operations might cause routing loops. In addition, this command might also affect the NetStream data. Therefore, use this command with caution.

Examples

# In BGP IPv4 unicast address family view, enable BGP to ignore the AS_PATH attribute when it implements load balancing.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] balance as-path-neglect

Related commands

balance

BGP commands -- balance as-path-relax

Use balance as-path-relax to enable load balancing for routes that have different AS_PATH attributes of the same length.

Use undo balance as-path-relax to restore the default.

Syntax

balance as-path-relax

undo balance as-path-relax

Default

BGP cannot perform load balancing for routes that have different AS_PATH attributes of the same length.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

For BGP to perform load balancing for routes with different AS_PATH attributes of the same length, you must use this command together with the balance command.

If you configure both the balance as-path-relax and balance as-path-neglect commands, the balance as-path-neglect command takes effect.

After this command is executed, BGP ignores the AS_PATH attributes in the routes for load balancing and changes the attributes of the advertised routes to those of the optimal route. This might cause routing loops and affect NetStream statistics. Therefore, use this command with caution.

Examples

# In BGP IPv4 unicast address family view, enable load balancing for routes that have different AS_PATH attributes of the same length.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] balance as-path-relax

BGP commands -- bestroute as-path-neglect

Use bestroute as-path-neglect to configure BGP to ignore the AS_PATH attribute during optimal route selection.

Use undo bestroute as-path-neglect to restore the default.

Syntax

bestroute as-path-neglect

undo bestroute as-path-neglect

Default

BGP considers the AS_PATH attribute during optimal route selection.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Examples

# In BGP instance view, ignore AS_PATH during optimal route selection.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bestroute as-path-neglect

BGP commands -- bestroute compare-med

Use bestroute compare-med to enable MED comparison for routes on a per-AS basis.

Use undo bestroute compare-med to restore the default.

Syntax

bestroute compare-med

undo bestroute compare-med

Default

MED comparison for routes on a per-AS basis is disabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

By default, BGP does not compare MEDs for routes from the same AS. When a router learns a new route, it compares the route with the optimal route in its BGP routing table. If the new route is more optimal, it becomes the optimal route in the BGP routing table. In this way, route learning sequence might affect optimal route selection.

To solve the selection problem, the router puts routes received from the same AS into a group when the bestroute compare-med command is configured. The router then selects the route with the lowest MED from the same group, and compares routes from different groups.

Examples

# In BGP instance view, enable MED comparison for routes on a per-AS basis.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bestroute compare-med

BGP commands -- bestroute igp-metric-ignore

Use bestroute igp-metric-ignore to configure BGP to ignore IGP metrics during optimal route selection.

Use undo bestroute igp-metric-ignore to restore the default.

Syntax

bestroute igp-metric-ignore

undo bestroute igp-metric-ignore

Default

BGP considers IGP metrics during optimal route selection, and selects the route with the smallest IGP metric as the optimal route.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Examples

# In BGP instance view, ignore IGP metrics during optimal route selection.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bestroute igp-metric-ignore

BGP commands -- bestroute med-confederation

Use bestroute med-confederation to enable MED comparison for routes received from confederation peers.

Use undo bestroute med-confederation to restore the default.

Syntax

bestroute med-confederation

undo bestroute med-confederation

Default

MED comparison is disabled for routes received from confederation peers.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command enables BGP to compare the MEDs of routes received from confederation peers. However, if a route from a confederation peer has an AS number that does not belong to the confederation, BGP does not compare the route with other routes. For example, a confederation has three AS numbers 65006, 65007, and 65009. BGP receives three routes from different confederation peers. The AS_PATH attributes of these routes are 65006 65009, 65007 65009, and 65008 65009, and the MED values of them are 2, 3, and 1. Because the third route's AS_PATH attribute contains AS number 65008, which does not belong to the confederation, BGP does not compare it with other routes. As a result, the first route becomes the optimal route.

Examples

# In BGP instance view, enable MED comparison for routes received from confederation peers.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bestroute med-confederation

BGP commands -- bgp

Use bgp to enable a BGP instance and enter its view.

Use undo bgp to disable a BGP instance.

Syntax

bgp as-number [ instance instance-name ]

undo bgp [ as-number [ instance instance-name ] ]

Default

BGP is disabled and no BGP instances exist.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

as-number: Specifies a local AS by its number in the range of 1 to 4294967295.

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command enables the BGP instance default.

Usage guidelines

A router supports 4-byte AS number.

A BGP router can run multiple BGP processes. Each BGP process corresponds to a BGP instance. BGP maintains an independent routing table for each BGP instance.

You can create multiple public address families for a BGP instance. However, each public address family (except for public IPv4/IPv6 unicast address family and public VPNv4/VPNv6 address family) can belong to only one BGP instance.

You can create multiple VPN instances for a BGP instance, and each VPN instance can have multiple address families. A VPN instance can belong to only one BGP instance.

The IPv4 and IPv6 multicast address families must belong to the same BGP instance.

Different BGP instances can have the same AS number but cannot have the same name.

Examples

# Enable BGP instance default, set the local AS number to 100, and enter BGP instance view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default]

BGP commands -- bgp apply-policy on-startup duration

Use bgp apply-policy on-startup duration to specify the period after reboot within which the startup policy is effective.

Use undo bgp apply-policy on-startup duration to restore the default.

Syntax

bgp apply-policy on-startup duration seconds

undo bgp apply-policy on-startup duration

Default

The startup policy does not take effect.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the period after reboot within which the startup policy is effective, in the range of 0 to 3600 seconds. The number of 0 indicates that the startup policy is effective permanently.

Usage guidelines

This command allows BGP to send route updates with the attribute values specified in the startup policy within the specified period after reboot. Then, BGP can forward traffic through other devices to avoid traffic loss caused by reboot.

Examples

# In BGP instance view, set the period after reboot to 100 seconds within which the startup policy is effective.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bgp apply-policy on-startup duration 100

Related commands

bgp policy on-startup med

BGP commands -- bgp policy on-startup med

Use bgp policy on-startup med to set the MED attribute value in the startup policy.

Use undo bgp policy on-startup med to restore the default.

Syntax

bgp policy on-startup med med-value

undo bgp policy on-startup med

Default

The MED attribute value in the startup policy is 4294967295.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

med-value: Specifies the MED attribute value in the startup policy, in the range of 0 to 4294967295.

Usage guidelines

After you configure this command, BGP uses the specified MED attribute value to send route updates within the specified period after reboot.

Examples

# In BGP instance view, set the MED attribute value in the startup policy to 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bgp policy on-startup med 100

Related commands

bgp apply-policy on-startup

BGP commands -- bgp update-delay on-startup

Use bgp update-delay on-startup to configure BGP to delay sending route updates on reboot.

Use undo bgp update-delay on-startup to restore the default.

Syntax

bgp update-delay on-startup seconds

undo bgp update-delay on-startup

Default

BGP sends route updates immediately on reboot.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the delay time in the range of 0 to 3600 seconds. The value of 0 indicates that BGP does not send route updates after the device reboots.

Usage guidelines

After you execute this command, BGP redistributes all routes from other neighbors on reboot, selects the optimal route, and then advertises it. Using this command can reduce traffic loss caused by reboot.

Examples

# In BGP instance view, configure BGP to delay sending route updates on reboot and set the delay time to 100 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] bgp update-delay on-startup 100

Related commands

bgp update-delay on-startup prefix-list

BGP commands -- bgp update-delay on-startup prefix-list

Use bgp update-delay on-startup prefix-list to configure BGP to immediately send route updates for routes that match a prefix list.

Use undo bgp update-delay on-startup prefix-list to restore the default.

Syntax

bgp update-delay on-startup prefix-list prefix-list-name

undo bgp update-delay on-startup prefix-list

Default

No prefix list is specified to filter routes.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

After the bgp update-delay on-startup command is configured, BGP delays sending updates for all routes on reboot. For BGP to immediately send updates for the specified routes, execute the bgp update-delay on-startup prefix-list command.

This command is available only to IPv4 prefix lists.

Examples

# In BGP instance view, configure BGP to send updates 100 seconds after reboot and immediately send updates for routes that match prefix list aaa.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-100] bgp update-delay on-startup 100

[Sysname-bgp-100] bgp update-delay on-startup prefix-list aaa

Related commands

bgp update-delay on-startup

BGP commands -- bgp-policy accounting

Use bgp-policy accounting to enable BGP policy accounting on an interface.

Use undo bgp-policy accounting to disable BGP policy accounting on an interface.

Syntax

bgp-policy accounting { input | output } * [ source ]

undo bgp-policy accounting { input | output } * [ source ]

Default

BGP policy accounting is disabled on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

input: Enables BGP policy accounting for incoming traffic.

output: Enables BGP policy accounting for outgoing traffic.

source: Classifies IP traffic based on the source IP address. If you do not specify this keyword, the command classifies IP traffic based on the destination IP address.

Usage guidelines

BGP policy accounting provides the following functionalities:

· Classifies IP traffic by BGP path attributes such as NEXT HOP, COMMUNITY, and AS_PATH.

· Assigns an index to each class of traffic.

· Collects statistics based on indexes.

BGP policy accounting supports the following traffic classification policies:

· Source IP address-based policy—BGP searches routes to the source address, obtains the traffic index for the routes, and collects statistics for the traffic identified by the index.

· Destination IP address-based policy—BGP searches routes to the destination address, obtains the traffic index for the routes, and collects statistics for the traffic identified by the index.

Examples

# Enable BGP policy accounting based on source IP address for traffic on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] bgp-policy accounting input output source

# Enable BGP policy accounting based on source IP address for traffic on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] bgp-policy accounting input output source

Related commands

aggregate

apply traffic-index

import-route

network

peer default-route-advertise

peer route-policy

BGP commands -- bmp server

Use bmp server to create a BGP monitoring protocol (BMP) server and enter BMP server view.

Use undo bmp server to remove a BMP server and all its configurations.

Syntax

bmp server server-number

undo bmp server server-number

Default

No BMP servers exist.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

server-number: Specifies a BMP server by its number in the range of 1 to 8.

Examples

# Create BMP server 5 and enter its view.

<Sysname> system-view

[Sysname] bmp server 5

[Sysname-bmpserver-5]

BGP commands -- compare-different-as-med

Use compare-different-as-med to enable MED comparison for routes from peers in different ASs.

Use undo compare-different-as-med to restore the default.

Syntax

compare-different-as-med

undo compare-different-as-med

Default

MED comparison is disabled for routes from peers in different ASs.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

If multiple routes to a destination exist, the route with the smallest MED is selected.

Do not use this command unless relevant ASs adopt the same IGP protocol and routing selection method.

Examples

# In BGP instance view, enable MED comparison for routes from peers in different ASs.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] compare-different-as-med

BGP commands -- confederation id

Use confederation id to configure a confederation ID.

Use undo confederation id to restore the default.

Syntax

confederation id as-number

undo confederation id

Default

No confederation ID is configured.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

as-number: Specifies an AS number that identifies the confederation, in the range of 1 to 4294967295.

Usage guidelines

You can split an AS into several sub-ASs, and each sub-AS remains fully meshed. These sub-ASs form a confederation. Key path attributes of a route, such as the Next_HOP, MED, and LOCAL_PREF, are not discarded when crossing each sub-AS. The sub-ASs still look like one AS from the perspective of other ASs. The AS number is the confederation ID.

Confederation can ensure the integrity of the former AS, and solve the problem of too many IBGP connections in the AS.

Configure the same confederation ID for all routers in one confederation.

For a non-confederation BGP router that establishes a BGP connection to a router in a confederation, the confederation ID is the AS number of the router.

Examples

# Confederation 9 consists of four sub-ASs numbered 38, 39, 40 and 41. Peer 10.1.1.1 is a member of sub-AS 38. Peer 200.1.1.1 is a member outside of confederation 9, which belongs to AS 98. Confederation 9 looks like one AS (with AS number 9) from the perspective of peer 200.1.1.1. This example uses a router in sub-AS 41.

<Sysname> system-view

[Sysname] bgp 41

[Sysname-bgp-default] confederation id 9

[Sysname-bgp-default] confederation peer-as 38 39 40

[Sysname-bgp-default] group Confed38 external

[Sysname-bgp-default] peer Confed38 as-number 38

[Sysname-bgp-default] peer 10.1.1.1 group Confed38

[Sysname-bgp-default] group Remote98 external

[Sysname-bgp-default] peer Remote98 as-number 98

[Sysname-bgp-default] peer 200.1.1.1 group Remote98

Related commands

confederation nonstandard

confederation peer-as

BGP commands -- confederation nonstandard

Use confederation nonstandard to enable compatibility with routers not compliant with RFC 3065 in the confederation.

Use undo confederation nonstandard to restore the default.

Syntax

confederation nonstandard

undo confederation nonstandard

Default

The device is compatible with only routers compliant with RFC 3065 in the confederation.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configure this command on all routers compliant with RFC 3065 to interact with those routers not compliant with RFC 3065 in the confederation.

Examples

# Confederation 100 consists of two sub-ASs, 64000 and 65000, and contains routers not compliant with RFC 3065. Enable compatibility with routers not compliant with RFC 3065 in the confederation.

<Sysname> system-view

[Sysname] bgp 64000

[Sysname-bgp-default] confederation id 100

[Sysname-bgp-default] confederation peer-as 65000

[Sysname-bgp-default] confederation nonstandard

Related commands

confederation id

confederation peer-as

BGP commands -- confederation peer-as

Use confederation peer-as to specify confederation peer sub-ASs.

Use undo confederation peer-as to remove the specified confederation peer sub-ASs.

Syntax

confederation peer-as as-number-list

undo confederation peer-as [ as-number-list ]

Default

No confederation peer sub-ASs are specified.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

as-number-list: Specifies a sub-AS number list. A maximum of 32 sub-ASs can be configured in one command line. The expression is as-number-list = as-number &<1-32>. The as-number argument specifies a sub-AS number in the range of 1 to 4294967295, and &<1-32> indicates that a maximum of 32 numbers can be specified.

Usage guidelines

Before this configuration, use the confederation id command to specify the confederation ID for the sub-ASs.

If the undo confederation peer-as command is executed without the as-number-list argument, all confederation peer sub-ASs are removed.

Examples

# In BGP instance view, specify confederation peer sub-ASs 2000 and 2001.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] confederation id 10

[Sysname-bgp-default] confederation peer-as 2000 2001

Related commands

confederation id

confederation nonstandard

BGP commands -- dampening

Use dampening to enable BGP route dampening.

Use undo dampening to restore the default.

Syntax

dampening [ half-life-reachable half-life-unreachable reuse suppress ceiling | route-policy route-policy-name ] *

undo dampening

Default

Route dampening is disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

half-life-reachable: Specifies a half-life for active routes, in the range of 1 to 45 minutes. By default, the value is 15 minutes.

half-life-unreachable: Specifies a half-life for suppressed routes, in the range of 1 to 45 minutes. By default, the value is 15 minutes.

reuse: Specifies a reuse threshold value for suppressed routes, in the range of 1 to 20000. A suppressed route whose penalty value decreases under the value is reused. By default, the reuse value is 750. The reuse threshold must be less than the suppression threshold.

suppress: Specifies a suppression threshold in the range of 1 to 20000. The route with a penalty value greater than the threshold is suppressed. The default value is 2000.

ceiling: Specifies a ceiling penalty value in the range of 1001 to 20000. The value must be greater than the suppress value. By default, the value is 16000.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

This command dampens only EBGP routes.

If an EBGP peer goes down after you configure this command, routes coming from the peer are dampened but not deleted.

Examples

# In BGP IPv4 unicast address family view, configure BGP route dampening. Set the half-life for both active and suppressed routes to 10 minutes, the reuse threshold to 1000, the suppression threshold to 2000, and the ceiling penalty to 10000.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] dampening 10 10 1000 2000 10000

Related commands

display bgp dampening parameter

BGP commands -- default local-preference

Use default local-preference to configure a default local preference.

Use undo default local-preference to restore the default.

Syntax

default local-preference value

undo default local-preference

Default

The default local preference is 100.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies a default local preference in the range of 0 to 4294967295. A larger value represents a higher preference.

Usage guidelines

You can also use the apply local-preference command in a routing policy to configure the local preference for BGP routes. If no routing policy is configured, all BGP routes use the local preference set by the default local-preference command. If a routing policy is configured, BGP routes matching the routing policy use the local preference set by the apply local-preference command. Other BGP routes use the local preference set by the default local-preference command.

Examples

# In BGP IPv4 unicast address family view, set the default local preference to 180.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] default local-preference 180

Related commands

apply local-preference

route-policy

BGP commands -- default med

Use default med to specify a default MED value.

Use undo default med to restore the default.

Syntax

default med med-value

undo default med

Default

The default MED value is 0.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

med-value: Specifies the default MED value in the range of 0 to 4294967295.

Usage guidelines

BGP selects a MED value in the following order:

1. MED set by the apply cost command.

2. MED set by the med keyword in the import-route command.

3. MED set by the default med command.

4. Original MED of a BGP route, or MED changed from the metric of a redistributed IGP route.

Examples

# In BGP IPv4 unicast address family view, set the default MED to 25.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] default med 25

Related commands

apply cost

import-route

route-policy

BGP commands -- default-route imported

Use default-route imported to enable default route redistribution into the BGP routing table.

Use undo default-route imported to restore the default.

Syntax

default-route imported

undo default-route imported

Default

Default route redistribution into the BGP routing table is disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

By default, BGP does not redistribute default IGP routes. To redistribute default IGP routes into the BGP routing table, you must use the default-route imported command together with the import-route command.

Examples

# In BGP IPv4 unicast address family view, enable default route redistribution from OSPF process 1 into the BGP routing table.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] default-route imported

[Sysname-bgp-default-ipv4] import-route ospf 1

Related commands

import-route

BGP commands -- default-route update-first

Use default-route update-first to enable BGP to first send updates of the default route.

Use undo default-route update-first to restore the default.

Syntax

default-route update-first

undo default-route update-first

Default

BGP does not first send updates of the default route.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Typically a BGP router does not first send update messages of the default route to its peers. If the peer relationship is down, the default route cannot be withdrawn first. Traffic interruption might occur. After you execute this command, BGP first sends withdrawal message of the default route when the peer relationship is down. Traffic can be immediately switched to a valid path to reduce the traffic interruption time.

Examples

# In BGP instance view, enable BGP to first send updates of the default route.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] default-route update-first

BGP commands -- display bgp bmp server

Use display bgp bmp server to display BMP server information.

Syntax

display bgp [ instance instance-name ] bmp server server-number

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BMP server information for the default BGP instance.

server-number: Specifies a BMP server by its number in the range of 1 to 8.

Examples

# Display information about BMP server 1.

<Sysname> display bgp bmp server 1

BMP server number: 1

Server address: 100.1.1.1 Server port: 6895

Client address: 100.1.1.2 Client port: 21452

BMP server state: Connected Up for 00h41m53s

Message statistics:

Total messages sent: 15

INITIATION: 1

TERMINATION: 0

STATS-REPORT: 0

PEER-UP: 4

PEER-DOWN: 3

ROUTE-MON: 7

BMP monitor BGP peers:

10.1.1.1

Table 2 Command output

Field | Description
Server address | IP address of the BMP server used by the TCP connection to the BMP client.
Server port | Port number of the BMP server used by the TCP connection to the BMP client.
Client address | IP address of the BMP client used by the TCP connection to the BMP server.
Client port | Port number of the BMP client used by the TCP connection to the BMP server.
BMP server current state | TCP connection status: · Connected. · Not connected.
Up for | Duration of the TCP connection.
Total messages sent | Number of messages that BGP sends to the BMP server.
INITIATION | Number of initiation messages that BGP sends to the BMP server.
TERMINATION | Number of termination messages that BGP sends to the BMP server.
STATS-REPORT | Number of statistics messages that BGP sends to the BMP server.
PEER-UP | Number of peer-up messages that BGP sends to the BMP server.
PEER-DOWN | Number of peer-down messages that BGP sends to the BMP server.
ROUTE-MON | Number of route monitoring messages that BGP sends to the BMP server.
BMP monitor BGP peers | Peers that are monitored by the BMP server.

Related commands

reset bgp bmp server statistics

BGP commands -- display bgp dampening parameter

Use display bgp dampening parameter to display BGP route dampening parameters.

Syntax

display bgp [ instance instance-name ] dampening parameter { ipv4 | ipv6 } { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] }

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP route dampening parameters for the default BGP instance.

ipv4: Displays BGP IPv4 route dampening parameters.

ipv6: Displays BGP IPv6 route dampening parameters.

multicast: Displays BGP multicast route dampening parameters.

unicast: Displays BGP unicast route dampening parameters.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays BGP route dampening parameters for the public network.

Usage guidelines

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# Display BGP IPv4 unicast route dampening parameters.

<Sysname> display bgp dampening parameter ipv4

Maximum suppression time (in seconds) : 3973

Ceiling value : 16000

Reuse value : 750

Half-life time for reachable routes (in seconds) : 900

Half-life time for unreachable routes (in seconds) : 900

Suppression threshold : 2000

Table 3 Command output

Field | Description
Maximum suppression time | Maximum time (in seconds) for the penalty value to decrease from the ceiling value to the reuse value.
Ceiling value | Penalty ceiling value.
Reuse value | Reuse threshold.

Related commands

dampening

BGP commands -- display bgp group

Use display bgp group to display BGP peer group information.

Syntax

display bgp [ instance instance-name ] group ipv4 { mdt | multicast | rtfilter | [ unicast ] [ vpn-instance vpn-instance-name ] } [ group-name group-name ]

display bgp [ instance instance-name ] group ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ group-name group-name ]

display bgp [ instance instance-name ] group link-state [ group-name group-name ]

display bgp [ instance instance-name ] group vpnv4 [ vpn-instance vpn-instance-name ] [ group-name group-name ]

display bgp [ instance instance-name ] group l2vpn [ evpn ] [ group-name group-name ]

display bgp [ instance instance-name ] group vpnv6 [ group-name group-name ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer group information for the default BGP instance.

ipv4: Displays IPv4 BGP peer group information.

ipv6: Displays IPv6 BGP peer group information.

link-state: Displays BGP LS peer group information.

mdt: Displays BGP MDT peer group information.

multicast: Displays BGP multicast peer group information.

rtfilter: Displays BGP IPv4 RT filter peer group information.

unicast: Displays BGP unicast peer group information.

vpnv4: Displays BGP VPNv4 peer group information.

l2vpn: Displays BGP L2VPN peer group information.

evpn: Displays BGP EVPN peer group information.

vpnv6: Displays BGP VPNv6 peer group information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays BGP peer group information for the public network.

group-name group-name: Specifies a BGP peer group by its name, a case-sensitive string of 1 to 47 characters. If you do not specify a group, this command displays brief information about all BGP peer groups for the specified address family.

Usage guidelines

By default, the unicast keyword is used if the unicast, mdt, and multicast keywords are not specified.

Examples

# Display brief information about all BGP IPv4 unicast peer groups.

BGP peer group: group1

Remote AS: 600

Type: external

Members:

1.1.1.10

BGP peer group: group2

Remote AS number: not specified

Type: external

Members:

2.2.2.2

# Display detailed information about BGP IPv4 unicast peer group group1.

<Sysname> display bgp group ipv4 group-name group1

BGP peer group: group1

Remote AS: 600

Type: external

Maximum number of prefixes allowed: 4294967295

Threshold: 75%

Configured hold time: 180 seconds

Keepalive time: 60 seconds

Minimum time between advertisements: 30 seconds

Peer preferred value: 0

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

Members:

* - Dynamically created peer

Peer AS MsgRcvd MsgSent OutQ PrefRcv Up/Down State

1.1.1.10 600 0 0 0 0 00:00:55 Established

# Display detailed information about BGP IPv6 unicast peer group group2.

<Sysname> display bgp group ipv6 group-name group2

BGP peer group: group2

Remote AS: 600

Type: external

Maximum number of prefixes allowed: 4294967295

Threshold: 75%

Configured hold time: 180 seconds

Keepalive time: 60 seconds

Minimum time between advertisements: 30 seconds

Peer preferred value: 0

IPsec profile name: profile001

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

Members:

* - Dynamically created peer

Peer AS MsgRcvd MsgSent OutQ PrefRcv Up/Down State

2::2 600 0 0 0 0 00:00:45 Established

3::3 600 0 0 0 0 00:00:40 Established

Table 4 Command output

Field | Description
BGP peer group | Name of the BGP peer group.
Remote AS | AS number of the peer group.
Type | Type of the peer groups: · external—EBGP peer group. · internal—IBGP peer group.
Maximum number of prefixes allowed | Maximum number of routes allowed to learn from the peer. This field does not apply to BGP L2VPN.
Threshold | Percentage of received routes from the peer to maximum routes allowed to learn from the peer. If the percentage is reached, the system generates a log message. This field does not apply to BGP L2VPN.
Configured hold time | Configured hold interval in seconds.
Keepalive time | Keepalive interval in seconds.
Minimum time between advertisements | Minimum route advertisement interval in seconds.
Peer preferred value | Preferred value specified for routes from the peer. This field does not apply to BGP L2VPN.
Site-of-Origin | SoO for the peer group.
Routing policy configured | Routing policy configured for the peer group. If you do not specify a routing policy, this field displays No routing policy is configured. This field does not apply to BGP L2VPN.
Members | Information about peers included in the peer group.
* - Dynamically created peer | An asterisk (*) before a peer address indicates that the peer is a dynamic peer.
Peer | IPv4 or IPv6 address of the peer.
AS | AS number of the peer.
MsgRcvd | Number of messages received.
MsgSent | Number of messages sent.
OutQ | Number of messages to be sent.
PrefRcv | For the IPv4, IPv6, VPNv4, and VPNv6 address families, this field displays the number of prefixes received from the peer. For MPLS L2VPN, this field displays the number of label blocks received from the peer. For VPLS, this field displays the total number of label blocks and VPLS PEs discovered by BGP. For the IPv4 MDT address family, this field displays the number of MDT messages received from the peer.
Up/Down | Lasting time of the current BGP session state.
State | Current state of the BGP session between the local router and the peer.
IPsec profile name | IPsec profile applied to the IPv6 BGP peer group.

BGP commands -- display bgp instance-info

Use display bgp instance-info to display information about all BGP instances.

Syntax

display bgp instance-info

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Examples

# Display information about all BGP instances.

<Sysname> display bgp instance-info

Total BGP instances: 3

BGP instance name AS

BGP1 100

BGP2 200

BGP3 300

Table 5 Command output

Field | Description
Total BGP instances | Number of BGP instances.
BGP instance name | BGP instance name.
AS | AS number of the BGP instance.

BGP commands -- display bgp link-state

Use display bgp link-state to display BGP LS information.

Syntax

display bgp [ instance instance-name ] link-state [ ls-prefix | peer { ipv4-address | ipv6-address } { advertised | received } [ statistics ] | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP LS information for the default BGP instance.

ls-prefix: Specifies an LS prefix. If you do not specify this argument, the command displays all BGP LS information.

ipv4-address: Specifies a peer by its IPv4 address.

ipv6-address: Specifies a peer by its IPv6 address.

advertised: Displays advertised LS information.

received: Displays received LS information.

statistics: Displays statistics about LS messages.

Usage guidelines

If you do not specify any parameters, this command displays brief BGP LS information.

Examples

# Display brief BGP LS information for the public network.

<Sysname> display bgp link-state

Total number of routes: 2

BGP local router ID is 1.1.2.1

Status codes: * - valid, > - best, d – dampened, h – history,

s – suppressed, S – stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Prefix codes: E link, V node, T IP reachable route, u/U unknown,

I Identifier, N local node, R remote node, L link, P prefix,

L1/L2 ISIS level-1/level-2, O OSPF, D direct, S static,

a area-ID, , l link-ID, t topology-ID, s ISO-ID,

c confed-ID/ASN, b bgp-identifier, r router-ID,

i if-address, n peer-address, o OSPF Route-type, p IP-prefix

d designated router address

* >e Network : [V][O][I0x0][N[c20][b1.1.1.2][a0.0.0.0][r1.1.1.2]]/376

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 20i

* >e Network : [T][O][I0x0][N[c20][b1.1.1.2][a0.0.0.0][r1.1.1.2]][P[o0x1][p1.1.1.0/24]]/480

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 20i

Table 6 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d - dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Prefix codes | Route status codes: · E – link. · V – node. · T – IP reachable route. · u/U – unknown. · I – Identifier. · N – local node. · R – remote node. · L – link. · P – prefix. · L1/L2 – ISIS level-1/level-2. · O – OSPF. · D – direct. · S – static. · a – area-ID. · l – link-ID. · t – topology-ID. · s – ISO-ID. · c – confed-ID/ASN. · b – bgp-identifier. · r – router-ID. · i – if-address. · n – peer-address. · o – OSPF Route-type. · p – IP-prefix. · d – designated router address.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ? – incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | NLRI for the LS.
NextHop | Next hop IP address.
LocPrf | Local preference.
OutLabel | Outgoing label of the route.
MED | MED attribute.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH—Records the ASs the route has passed, which avoids routing loops. · ORIGIN—Identifies the origin of the route.

# Display detailed BGP LS information with the specified LS prefix.

<Sysname> display bgp link-state [V][O][I0x0][N[c20][b1.1.1.2][a0.0.0.0][r1.1.1.2]]/376

BGP local router ID: 1.1.1.2

Local AS number: 20

Paths: 1 available, 1 best

BGP LS information of [V][O][I0x0][N[c20][b1.1.1.2][a0.0.0.0][r1.1.1.2]]/376:

Imported route.

Original nexthop: 0.0.0.0

OutLabel : NULL

LS : Node flag bits: 30[EA]

AS-path : (null)

Origin : igp

Attribute value : pref-val 32768

State : valid, local, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 7 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
BGP LS information of | NLRI prefix.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
LS | LS attribute: · Node flag bits—Node attribute in hexadecimal format: ?span style='font:7.0pt "Times New Roman"'> 10[A]—OSPF ABR bit. ?span style='font:7.0pt "Times New Roman"'> 30[E]—OSPF External bit. · Metric—Link or prefix cost.
AS-path | AS_PATH attribute of the route, which records the ASs the route has passed and avoids routing loops.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · synchronize. · best.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.

BGP commands -- display bgp network

Use display bgp network to display information about routes advertised by the network command and shortcut routes configured by the network short-cut command.

Syntax

display bgp [ instance instance-name ] network { ipv4 | ipv6 } { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] }

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays information for the default BGP instance.

ipv4: Displays IPv4 address family information.

ipv6: Displays IPv6 address family information.

multicast: Displays BGP multicast address family information.

unicast: Displays BGP unicast address family information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays routing information for the public network.

Usage guidelines

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# Display information about routes advertised by the network command and shortcut routes configured by the network short-cut command in the IPv4 unicast address family.

<Sysname> display bgp network ipv4

BGP local router ID: 192.168.1.135

Local AS number: 100

Network Mask Route-policy Short-cut

20.1.1.0 255.255.255.0 No

40.1.1.0 255.255.255.0 abc No

30.1.1.0 255.255.255.0 Yes

# Display information about routes advertised by the network command and shortcut routes configured by the network short-cut command in the IPv6 unicast address family.

<Sysname> display bgp network ipv6

BGP local router ID: 192.168.1.135

Local AS number: 100

Network PrefixLen Route-policy Short-cut

1:: 24 No

2:: 24 No

3:: 64 policy1 No

2:: 24 Yes

Table 8 Command output

Field | Description
Network | Destination network address of the routes advertised by the network command and the shortcut routes.
Mask | Mask of the destination network address.
PrefixLen | Prefix length of the destination network address.
Route-policy | Routing policy that is applied to the route.
Short-cut | Whether the route is a shortcut route: · Yes. · No.

BGP commands -- display bgp non-stop-routing status

Use display bgp non-stop-routing status to display BGP NSR status information.

Syntax

display bgp [ instance instance-name ] non-stop-routing status

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP NSR status information for the default BGP instance.

Examples

# Display BGP NSR status information.

<Sysname> display bgp non-stop-routing status

BGP NSR status: Not ready

Location of preferred standby process: -

TCP NSR status: Not ready

Table 9 Command output

Field | Description
BGP NSR status | BGP NSR status: · Ready—BGP NSR has backed up BGP neighbor and routing information from the active process to the standby process. In this state, BGP NSR can ensure continuous routing when an active/standby process switchover occurs. · Not ready—BGP NSR is backing up BGP neighbor and routing information from the active process to the standby process. If an active/standby process switchover occurs in this state, traffic is interrupted and the BGP session will be re-established. · Not configured—BGP NSR is disabled.
Location of preferred standby process | (Distributed devices in standalone mode.) ID of the slot where the preferred standby process resides. (Centralized IRF devices.) ID of the IRF member device where the preferred standby process resides. (Distributed devices in IRF mode.) Chassis ID and slot ID where the preferred standby process resides. This field displays - if no standby processes exist.
TCP NSR status | TCP NSR status: · Ready—TCP NSR has backed up TCP connection information from the active process to the standby process. · Not ready—TCP NSR is backing up TCP connection information from the active process to the standby process.

BGP commands -- display bgp paths

Use display bgp paths to display BGP path attribute information.

Syntax

display bgp [ instance instance-name ] paths [ as-regular-expression ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP path attribute information for the default BGP instance.

as-regular-expression: Displays information about BGP path attributes whose AS_PATH attribute matches the specified regular expression. The as-regular-expression argument is a string of 1 to 256 characters. If you do not specify this argument, the command displays information about all BGP path attributes.

Examples

# Display information about all BGP path attributes.

<Sysname> display bgp paths

RefCount MED Path/Origin

3 0 ?

2 0 100i

3 0 100i

1 0 ?

1 0 ?

1 0 ?

Table 10 Command output

Field | Description
RefCount | Number of BGP routes with these path attributes.
MED | MULTI_EXIT_DISC attribute.
Path/Origin | AS_PATH and ORIGIN attributes of the route: · AS_PATH attribute—Records the ASs the route has passed, which avoids routing loops. · ORIGIN attribute—Identifies the origin of the route: ?span style='font:7.0pt "Times New Roman"'> i—Originated in the AS. The origin of routes advertised with the network command is IGP. ?span style='font:7.0pt "Times New Roman"'> e—Learned through EGP. ?span style='font:7.0pt "Times New Roman"'> ?—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.

BGP commands -- display bgp peer

Use display bgp peer to display BGP peer or peer group information.

Syntax

display bgp [ instance instance-name ] peer ipv4 { mdt | multicast | rtfilter | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv4-address mask-length | { ipv4-address | group-name group-name } log-info | [ ipv4-address ] verbose ]

display bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv6-address prefix-length | { ipv6-address | group-name group-name } log-info | [ ipv6-address ] verbose ]

display bgp [ instance instance-name ] peer ipv6 [ unicast ] [ ipv4-address mask-length | ipv4-address log-info | [ ipv4-address ] verbose ]

display bgp [ instance instance-name ] peer link-state [ ipv4-address mask-length | ipv6-address prefix-length | { ipv4-address | ipv6-address | group-name group-name } log-info | [ ipv4-address | ipv6-address ] verbose ]

display bgp [ instance instance-name ] peer vpnv4 [ vpn-instance vpn-instance-name ] [ ipv4-address mask-length | { ipv4-address | group-name group-name } log-info | [ ipv4-address ] verbose ]

display bgp [ instance instance-name ] peer l2vpn [ evpn ] [ ipv4-address mask-length | { ipv4-address | group-name group-name } log-info | [ ipv4-address ] verbose ]

display bgp [ instance instance-name ] peer vpnv6 [ ipv4-address mask-length | { ipv4-address | group-name group-name } log-info | [ ipv4-address ] verbose ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP peer or peer group information for the default BGP instance.

ipv4: Displays IPv4 BGP peer or peer group information.

ipv6: Displays IPv6 BGP peer or peer group information.

link-state: Displays BGP LS peer or peer group information.

vpnv4: Displays BGP VPNv4 peer or peer group information.

l2vpn: Displays BGP L2VPN peer or peer group information.

evpn: Displays BGP EVPN peer or peer group information.

vpnv6: Displays BGP VPNv6 peer or peer group information.

mdt: Displays BGP MDT peer or peer group information.

multicast: Displays BGP multicast peer or peer group information.

rtfilter: Displays BGP IPv4 RT filter peer or peer group information.

unicast: Displays BGP unicast peer or peer group information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays BGP peer or peer group information for the public network.

ipv4-address mask-length: Specifies a subnet. The value range for the mask length is 0 to 32. If you specify a subnet, this command displays information about all dynamic peers in the subnet.

ipv4-address: Specifies a peer by its IPv4 address.

ipv6-address prefix-length: Specifies a subnet. The value range for the prefix length is 0 to 128. If you specify a subnet, this command displays information about all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address.

group-name group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters.

log-info: Displays log information.

verbose: Displays detailed information.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP peers for the specified address family.

By default, the unicast keyword is used if the unicast, mdt, and multicast keywords are not specified.

Examples

# Display brief information about all BGP IPv4 unicast peers.

<Sysname> display bgp peer ipv4

BGP local router ID: 192.168.100.1

Local AS number: 100

Total number of peers: 1 Peers in established state: 1

* - Dynamically created peer

Peer AS MsgRcvd MsgSent OutQ PrefRcv Up/Down State

10.2.1.2 200 13 16 0 0 00:10:34 Established

Table 11 Command output

Field | Description
* - Dynamically created peer | An asterisk (*) before a peer address indicates that the peer is a dynamic peer.
Peer | IPv4 or IPv6 address of the peer.
AS | AS number of the peer.
MsgRcvd | Number of messages received.
MsgSent | Number of messages sent.
OutQ | Number of messages to be sent.
PrefRcv | For the IPv4, IPv6, VPNv4, and VPNv6 address families, this field displays the number of prefixes that have been received from the peer and added into the local BGP routing table. For MPLS L2VPN, this field displays the number of label blocks received from the peer. For VPLS, this field displays the total number of label blocks and VPLS PEs discovered by BGP. For the IPv4 MDT address family, this field displays the number of MDT messages received from the peer.
Up/Down | Lasting time of the current BGP session state.
State | Current state of the BGP session between the local router and the peer.

# Display brief information about all dynamic peers in network 1.1.1.0/24.

<Sysname> display bgp peer ipv4 1.1.1.0 24

Type: EBGP link

Dynamic address range: 1.1.1.0 24

Configured: Active Hold Time: 3 sec Keepalive Time: 1 sec

Address family IPv4 Unicast: Configured

Maximum allowed prefix number: 100

Threshold: 75%

Minimum time between advertisements is 100 seconds

Optional capabilities:

Multi-protocol extended capability has been enabled

Route refresh capability has been enabled

Nexthop self has been configured

Keep-all-routes has been configured

Send community has been configured

Send extend community has been configured

Default route originating has been configured

Multi-hop ebgp has been enabled

Peer preferred value: 100

BFD: Enabled

Site-of-Origin: 1:1

Routing policy configured:

No import as-path-acl list

Export as-path-acl list is: 22

No import prefix list

Export prefix list is: p1

No import route policy

Export route policy is: p1

No import filter-policy

No export filter-policy

Dynamic peers:

1.1.1.3

# Display brief information about all dynamic peers in network 1::/64.

<Sysname> display bgp peer ipv6 1:: 64

Type: IBGP link

Dynamic address range: 1:: 64

Configured: Active Hold Time: 180 sec Keepalive Time: 60 sec

Address family IPv6 Unicast: Configured

Maximum allowed prefix number: 4294967295

Threshold: 75%

Minimum time between advertisements is 15 seconds

Optional capabilities:

Multi-protocol extended capability has been enabled

Route refresh capability has been enabled

Send community has been configured

Peer preferred value: 0

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

Dynamic peers:

1::1

Table 12 Command output

Field | Description
Type | BGP connection type between the local router and the dynamic peer: · IBGP link—IBGP connection. · EBGP link—EBGP connection.
Configured | Timers configured on the local router in seconds, including the hold time (Active Hold Time) and keepalive interval (Keepalive Time).
Address family IPv4 Unicast | IPv4 unicast address family capability.
Address family link-state | LS address family capability.
Address family IPv6 Unicast | IPv6 unicast address family capability.
Address family IPv4 Multicast | IPv4 multicast address family capability.
Address family IPv6 Multicast | IPv6 multicast address family capability.
Address family MDT | IPv4 MDT address family capability.
Address family L2VPN | L2VPN address family capability.
Address family L2VPN VPWS (Draft) | L2VPN VPWS address family capability.
Maximum allowed prefix number | Maximum number of routes allowed to learn from the peer. This field does not apply to BGP L2VPN.
Threshold | Percentage of received routes from the peer to maximum routes allowed to learn from the peer. If the percentage is reached, the system generates alarm messages. This field does not apply to BGP L2VPN.
Minimum time between advertisements | Minimum route advertisement interval in seconds.
Optional capabilities | Optional capabilities supported by the local end.
Peer Preferred Value | Preferred value specified for the routes from the peer. This field does not apply to BGP L2VPN.
BFD | Whether BFD is enabled to detect the link to the BGP peers.
IPsec profile name | IPsec profile applied to the IPv6 BGP peer. This field is available only for the IPv6 unicast and IPv6 multicast address families.
Routing policy configured | Routing policy configured for the peer. If you do not specify a routing policy, this field displays No routing policy is configured. This field does not apply to BGP L2VPN.
Dynamic peers | IP addresses of dynamic peers.

# Display detailed information about BGP IPv4 unicast peer 10.2.1.2.

<Sysname> display bgp peer ipv4 10.2.1.2 verbose

Peer: 10.2.1.2 Local: 192.168.100.1

Type: EBGP link

BGP version 4, remote router ID 192.168.100.2

BGP current state: Established, Up for 00h11m10s

BGP current event: RecvKeepalive

BGP last state: OpenConfirm

Port: Local - 179 Remote - 60672

Configured: Active Hold Time: 180 sec Keepalive Time: 60 sec

Received : Active Hold Time: 180 sec

Negotiated: Active Hold Time: 180 sec Keepalive Time: 60 sec

Peer optional capabilities:

Peer support BGP multi-protocol extended

Peer support BGP route refresh capability

Peer support BGP route AS4 capability

Address family IPv4 Unicast: advertised and received

InQ updates: 0, OutQ updates: 0

NLRI statistics:

Rcvd: UnReach NLRI 0, Reach NLRI 0

Sent: UnReach NLRI 0, Reach NLRI 0

Message statistics:

Msg type Last rcvd time/ Current rcvd count/ History rcvd count/

Last sent time Current sent count History sent count

Open 10:38:50-2013.7.23 1 1

10:38:50-2013.7.23 1 1

Update 10:38:51-2013.7.23 1 1

10:38:51-2013.7.23 1 1

Notification - 0 0

- 0 0

Keepalive 10:38:50-2013.7.23 1 1

10:38:50-2013.7.23 1 1

RouteRefresh - 0 0

- 0 0

Total - 3 3

- 3 3

Maximum allowed prefix number: 4294967295

Threshold: 75%

Minimum time between advertisements is 30 seconds

Optional capabilities:

Multi-protocol extended capability has been enabled

Route refresh capability has been enabled

Peer Preferred Value: 0

GTSM has been enabled, and the maximum number of hops is 10

BFD: Enabled

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

# Display detailed information about BGP IPv6 unicast peer 1::2.

<Sysname> display bgp peer ipv6 1::2 verbose

Peer: 1::2 Local: 192.168.1.136

Type: EBGP link

BGP version 4, remote router ID 192.168.1.135

BGP current state: Established, Up for 00h05m48s

BGP current event: RecvKeepalive

BGP last state: OpenConfirm

Port: Local - 13184 Remote - 179

Configured: Active Hold Time: 180 sec Keepalive Time: 60 sec

Received : Active Hold Time: 180 sec

Negotiated: Active Hold Time: 180 sec Keepalive Time: 60 sec

Peer optional capabilities:

Peer support BGP multi-protocol extended

Peer support BGP route refresh capability

Peer support BGP route AS4 capability

Address family IPv6 Unicast: advertised and received

InQ updates: 0, OutQ updates: 0

NLRI statistics:

Rcvd: UnReach NLRI 0, Reach NLRI 0

Sent: UnReach NLRI 0, Reach NLRI 3

Message statistics:

Msg type Last rcvd time/ Current rcvd count/ History rcvd count/

Last sent time Current sent count History sent count

Open 18:59:15-2013.4.24 1 1

18:59:15-2013.4.24 1 2

Update - 0 0

18:59:16-2013.4.24 1 1

Notification - 0 0

18:59:15-2013.4.24 0 1

Keepalive 18:59:15-2013.4.24 1 1

18:59:15-2013.4.24 1 1

RouteRefresh - 0 0

- 0 0

Total - 2 2

- 3 5

Maximum allowed prefix number: 4294967295

Threshold: 75%

Minimum time between advertisements is 30 seconds

Optional capabilities:

Multi-protocol extended capability has been enabled

Route refresh capability has been enabled

Peer preferred value: 0

GTSM has been enabled, and the maximum number of hops is 10

BFD: Enabled

IPsec profile name: profile001

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

# Display detailed information about BGP L2VPN peer 10.1.1.1.

<Sysname> display bgp peer l2vpn 10.1.1.1 verbose

Peer: 10.1.1.1 Local: 192.168.1.136

Type: EBGP link

BGP version 4, remote router ID 192.168.1.135

BGP current state: Established, Up for 00h01m25s

BGP current event: KATimerExpired

BGP last state: OpenConfirm

Port: Local - 179 Remote - 1049

Configured: Active Hold Time: 180 sec Keepalive Time: 60 sec

Received : Active Hold Time: 180 sec

Negotiated: Active Hold Time: 180 sec Keepalive Time: 60 sec

Peer optional capabilities:

Peer support BGP multi-protocol extended

Peer support BGP route refresh capability

Peer support BGP route AS4 capability

Address family IPv4 Unicast: advertised and received

Address family L2VPN: advertised

Address family L2VPN VPWS (Draft): advertised and received

InQ updates: 0, OutQ updates: 0

NLRI statistics:

Rcvd: UnReach NLRI 0, Reach NLRI 0

Sent: UnReach NLRI 0, Reach NLRI 3

Message statistics:

Msg type Last rcvd time/ Current rcvd count/ History rcvd count/

Last sent time Current sent count History sent count

Open 18:59:15-2013.4.24 1 1

18:59:15-2013.4.24 1 2

Update - 0 0

18:59:16-2013.4.24 1 1

Notification - 0 0

18:59:15-2013.4.24 0 1

Keepalive 18:59:15-2013.4.24 1 1

18:59:15-2013.4.24 1 1

RouteRefresh - 0 0

- 0 0

Total - 2 2

- 3 5

Maximum allowed prefix number: 4294967295

Threshold: 75%

Minimum time between advertisements is 30 seconds

Optional capabilities:

Multi-protocol extended capability has been enabled

Route refresh capability has been enabled

Peer Preferred Value: 0

GTSM has been enabled, and the maximum number of hops is 10

BFD: Enabled

Site-of-Origin: Not specified

Routing policy configured:

No routing policy is configured

Table 13 Command output

Field | Description
Peer | IPv4 or IPv6 address of the peer.
Local | Local router ID.
Type | BGP connection type between the local router and the peer: · IBGP link—IBGP connection. · EBGP link—EBGP connection.
remote router ID | Router ID of the peer.
BGP current state | Current state of the BGP session between the local router and the peer.
Up for | Lasting time of the BGP session.
BGP current event | Current event of the BGP session between the local router and the peer.
BGP last state | Previous state of the BGP session.
Port | TCP port numbers of the local router and its peer.
Configured | Timers configured on the local router in seconds, including the hold time (Active Hold Time) and keepalive interval (Keepalive Time).
Received | Received timer (configured on the peer) in seconds, including the hold time (Active Hold Time).
Negotiated | Negotiated timers in seconds, including the hold time (Active Hold Time) and keepalive interval (Keepalive Time).
Peer optional capabilities | Optional capabilities supported by the peer.
Peer support BGP route AS4 capability | The peer supports 4-byte AS number.
Address family IPv4 Unicast | IPv4 unicast address family capability: routes of the address family can be advertised and received.
Address family LS | LS address family capability: routes of the address family can be advertised and received.
Address family IPv6 Unicast | IPv6 unicast address family capability: routes of the address family can be advertised and received.
Address family IPv4 Multicast | IPv4 multicast address family capability: routes of the address family can be advertised and received.
Address family IPv6 Multicast | IPv6 multicast address family capability: routes of the address family can be advertised and received.
Address family MDT | IPv4 MDT address family capability: routes of the address family can be advertised and received.
Address family L2VPN | L2VPN address family capability: routes of the address family can be advertised and received.
Address family L2VPN VPWS (Draft) | L2VPN VPWS address family capability (draft-kompella-ppvpn-l2vpn-03): routes of the address family can be advertised and received.
InQ updates | Number of received updates to be processed.
OutQ updates | Number of updates to be sent to the peer.
NLRI statistics | Number of the reachable and unreachable routes received from and sent to the peer after the BGP session is established.
Message statistics | BGP message statistics.
Msg type | BGP message type.
Last rcvd time/Last sent time | Time when the most recent BGP message was received from or sent to the peer.
Current rcvd count/Current sent count | Number of BGP messages received from or sent to the peer on the current BGP session.
History rcvd count/History sent count | Number of BGP messages received from or sent to the peer since the BGP peer relationship was established.
Total | Total number of received and sent messages.
Maximum allowed prefix number | Maximum number of routes allowed to learn from the peer. This field does not apply to BGP L2VPN.
Threshold | Percentage of received routes from the peer to maximum routes allowed to learn from the peer. If the percentage is reached, the system generates alarm messages. This field does not apply to BGP L2VPN.
Minimum time between advertisements | Minimum route advertisement interval in seconds.
Optional capabilities | Optional capabilities supported by the local end.
Peer Preferred Value | Preferred value specified for the routes from the peer. This field does not apply to BGP L2VPN.
GTSM has been enabled | GTSM is supported.
the maximum number of hops | Maximum number of hops to the specified peer.
BFD | Whether BFD is enabled to detect the link to the BGP peer.
IPsec profile name | IPsec profile applied to the IPv6 BGP peer. This field is available only for the IPv6 unicast and IPv6 multicast address families.
Routing policy configured | Routing policy configured for the peer. If you do not specify a routing policy, this field displays No routing policy is configured. This field does not apply to BGP L2VPN.

# Display log information for BGP IPv4 unicast peer 1.1.1.1.

<Sysname> display bgp peer ipv4 1.1.1.1 log-info

Peer : 1.1.1.1

Date Time State Notification

Error/SubError

06-Feb-2013 22:54:42 Down Send notification with error 6/4

Cease/Administrative Reset

<administrative reset>

Table 14 Command output

Field | Description
Peer | IPv4 or IPv6 address of the peer.
Date | Date on which the Notification was sent or received.
Time | Time at which the Notification was sent or received.
State | BGP session state: · Up—The BGP session is in Established state. · Down—The BGP session is down.
Notification Error/SubError | Error code of the Notification, indicating the cause of why the BGP session was down. · Error—Refers to the error code, which identifies the type of the Notification. · SubError—Refers to the error subcode of the Notification, which identifies the specific information about the reported error.

BGP commands -- display bgp peer received prefix-list

Use display bgp peer received prefix-list to display the ORF prefix information received by a peer.

Syntax

display bgp [ instance instance-name ] peer ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv4-address received prefix-list

display bgp [ instance instance-name ] peer ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } ipv6-address received prefix-list

display bgp [ instance instance-name ] peer ipv6 [ unicast ] ipv4-address received prefix-list

display bgp [ instance instance-name ] peer { vpnv4 | vpnv6 } ipv4-address received prefix-list

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays ORF prefix information for the default BGP instance.

ipv4: Displays BGP IPv4 peer information.

ipv6: Displays BGP IPv6 peer information.

vpnv4: Displays BGP VPNv4 peer information.

vpnv6: Displays BGP VPNv6 peer information.

multicast: Displays BGP multicast peer information.

unicast: Displays BGP unicast peer information.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify an instance, this command displays information for the public network.

ipv4-address: Specifies a peer by its IPv4 address.

ipv6-address: Specifies a peer by its IPv6 address.

Examples

# Display the ORF prefix information received by peer 10.110.25.20.

<Sysname> display bgp peer ipv4 10.110.25.20 received prefix-list

ORF prefix list entries: 2

index: 10 prefix 1.1.1.0/24 ge 26 le 32

index: 20 prefix 2.1.1.0/24 ge 26 le 32

Table 15 Command output

Field | Description
ORF prefix list entries | Number of ORF prefixes.
index | Prefix index.
prefix | Prefix information.
ge | Greater than or equal to.
le | Less than or equal to.

BGP commands -- display bgp routing-table dampened

Use display bgp routing-table dampened to display dampened BGP routes.

Syntax

display bgp [ instance instance-name ] routing-table dampened { ipv4 | ipv6 } { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] }

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays dampened BGP routes for the default BGP instance.

ipv4: Displays dampened BGP IPv4 routes.

ipv6: Displays dampened BGP IPv6 routes.

multicast: Displays dampened BGP multicast routes.

unicast: Displays dampened BGP unicast routes.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays dampened BGP routes for the public network.

Usage guidelines

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# Display dampened BGP IPv4 unicast routes.

<Sysname> display bgp routing-table dampened ipv4

Total number of routes: 1

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network From Reuse Path/Ogn

de 20.1.1.0/24 10.1.1.2 00:56:27 100i

# Display dampened BGP IPv6 unicast routes.

<Sysname> display bgp routing-table dampened ipv6

Total number of routes: 2

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

de Network : 2:: PrefixLen : 64

From : 10.1.1.1 Reuse : 00:39:49

Path/Ogn: 100i

de Network : 2:: PrefixLen : 64

From : 1::1 Reuse : 00:39:49

Path/Ogn: 100i

Table 16 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
From | IP address from which the route was received.
Reuse | Reuse time of the route.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH attribute—Records the ASs the route has passed, which avoids routing loops. · ORIGIN attribute—Identifies the origin of the route.

Related commands

dampening

reset bgp dampening

BGP commands -- display bgp routing-table flap-info

Use display bgp routing-table flap-info to display BGP route flap statistics.

Syntax

display bgp [ instance instance-name ] routing-table flap-info ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv4-address [ { mask-length | mask } [ longest-match ] ] | as-path-acl as-path-acl-number ]

display bgp [ instance instance-name ] routing-table flap-info ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv6-address prefix-length | as-path-acl as-path-acl-number ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP route flap statistics for the default BGP instance.

ipv4: Displays BGP IPv4 route flap statistics.

ipv6: Displays BGP IPv6 route flap statistics.

multicast: Displays BGP multicast route flap statistics.

unicast: Displays BGP unicast route flap statistics.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays BGP route flap statistics for the public network.

ipv4-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

ipv6-address prefix-length: Displays route flap statistics for BGP IPv6 routes that match the specified network address, and match the prefix length in the range of 0 to 128.

as-path-acl as-path-acl-number: Displays route flap statistics for BGP routes that match the AS path list specified by its number in the range of 1 to 256.

Usage guidelines

If you specify only the ipv4-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, the command displays flap statistics of the route.

If you specify the ipv4-address mask or ipv4-address mask-length argument, and do not specify the longest-match keyword, the command displays flap statistics of the BGP IPv4 unicast or multicast route that matches both the specified destination network address and the mask (or mask length).

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# Display BGP IPv4 unicast route flap statistics.

<Sysname> display bgp routing-table flap-info ipv4

Total number of routes: 1

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network From Flaps Duration Reuse Path/Ogn

de 20.1.1.0/24 10.1.1.2 1 00:02:36 00:53:58 100i

# Display BGP IPv6 unicast route flap statistics.

<Sysname> display bgp routing-table flap-info ipv6

Total number of routes: 2

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

de Network : 2:: PrefixLen : 64

From : 10.1.1.1 Flaps : 5

Duration: 00:03:25 Reuse : 00:39:28

Path/Ogn: 100i

de Network : 2:: PrefixLen : 64

From : 1::1 Flaps : 5

Duration: 00:03:25 Reuse : 00:39:28

Path/Ogn: 100i

Table 17 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
From | Source IP address of the route.
Flaps | Number of routing flaps.
Duration | Duration time of the flap route.
Reuse | Reuse time of the route.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH attribute—Records the ASs the route has passed, which avoids routing loops. · ORIGIN attribute—Identifies the origin of the route.

Related commands

dampening

reset bgp flap-info

BGP commands -- display bgp routing-table ipv4 multicast

Use display bgp routing-table ipv4 multicast to display BGP IPv4 multicast routing information.

Syntax

display bgp [ instance instance-name ] routing-table ipv4 multicast [ ipv4-address [ { mask-length | mask } [ longest-match ] ] | ipv4-address [ mask-length | mask ] advertise-info | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv4-address { advertised-routes | received-routes } [ ipv4-address [ mask-length | mask ] | statistics ] | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv4 multicast routing information for the default BGP instance.

ipv4-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

advertise-info: Displays advertisement information for BGP IPv4 multicast routes.

as-path-acl as-path-acl-number: Displays BGP IPv4 multicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv4 multicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP IPv4 multicast routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP IPv4 multicast routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer ipv4-address: Displays BGP IPv4 multicast routing information advertised to or received from the specified peer.

advertised-routes: Displays BGP IPv4 multicast routing information advertised to the specified peer.

received-routes: Displays BGP IPv4 multicast routing information received from the specified peer.

statistics: Displays routing statistics.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP IPv4 multicast routes.

If you specify only the ipv4-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, the command displays information about the route.

If you specify the ipv4-address mask or ipv4-address mask-length argument and do not specify the longest-match keyword, this command displays information about the BGP IPv4 multicast route that matches both the specified destination network address and the mask (or mask length).

Examples

# Display brief information about all BGP IPv4 multicast routes.

<Sysname> display bgp routing-table ipv4 multicast

Total number of routes: 3

BGP local router ID is 192.168.1.62

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* > 5.5.5.5/32 127.0.0.1 0 32768 ?

* > 192.168.1.0 192.168.1.62 0 32768 ?

* > 192.168.1.62/32 127.0.0.1 0 32768 ?

# Display information about BGP IPv4 multicast routes that match AS path list 20.

<Sysname> display bgp routing-table ipv4 multicast as-path-acl 20

Total number of routes: 3

BGP local router ID is 192.168.1.62

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* > 5.5.5.5/32 127.0.0.1 0 32768 ?

* > 192.168.1.0 192.168.1.62 0 32768 ?

* > 192.168.1.62/32 127.0.0.1 0 32768 ?

# Display information about BGP IPv4 multicast routes that match BGP community list 100.

<Sysname> display bgp routing-table ipv4 multicast community-list 100

Total number of routes: 3

BGP local router ID is 192.168.1.62

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* > 5.5.5.5/32 127.0.0.1 0 32768 ?

* > 192.168.1.0 192.168.1.62 0 32768 ?

* > 192.168.1.62/32 127.0.0.1 0 32768 ?

# Display information about all BGP IPv4 multicast routes advertised to peer 192.168.1.139.

<Sysname> display bgp routing-table ipv4 multicast peer 192.168.1.139 advertised-routes

Total number of routes: 2

BGP local router ID is 192.168.1.62

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf Path/Ogn

* > 5.5.5.5/32 127.0.0.1 0 100 ?

* > 192.168.1.0 192.168.1.62 0 100 ?

# Display information about all BGP IPv4 multicast routes received from peer 192.168.1.139.

<Sysname> display bgp routing-table ipv4 multicast peer 192.168.1.139 received-routes

Total number of routes: 2

BGP local router ID is 192.168.1.62

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* >i 8.8.8.8/32 192.168.1.139 0 100 0 ?

* i 192.168.1.0 192.168.1.139 0 100 0 ?

Table 18 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
NextHop | Next hop IP address.
MED | MULTI_EXIT_DISC attribute.
LocPrf | Local preference value.
PrefVal | Preferred value of the route.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH—Records the ASs the route has passed. · ORIGIN—Identifies the origin of the route.

# Display detailed information about BGP IPv4 multicast routes destined to network 5.5.5.5/32.

<Sysname> display bgp routing-table ipv4 multicast 5.5.5.5 32

BGP local router ID: 192.168.1.139

Local AS number: 100

Paths: 1 available, 1 best

BGP routing table information of 5.5.5.5/32:

From : 192.168.1.62 (192.168.1.62)

Rely nexthop : 192.168.1.62

Original nexthop: 192.168.1.62

OutLabel : NULL

AS-path : (null)

Origin : incomplete

Attribute value : MED 0, localpref 100, pref-val 0

State : valid, internal, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 19 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
From | IP address of BGP peer that advertised the route.
Rely Nexthop | Next hop found by route recursion. If no next hop is found, this field displays not resolved.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
OutLabel | Outgoing label of the route.
AS-path | AS_PATH attribute of the route.
Origin | Origin of the route: · igp—Originated in the AS. The origin of routes advertised with the network command is IGP. · egp—Learned through EGP. · incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · synchronize. · best.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.

# Display statistics for BGP IPv4 multicast routes advertised to peer 192.168.1.62.

<Sysname> display bgp routing-table ipv4 multicast peer 192.168.1.62 advertised-routes statistics

Advertised routes total: 2

# Display statistics for BGP IPv4 multicast routes received from peer 192.168.1.62.

<Sysname> display bgp routing-table ipv4 multicast peer 192.168.1.62 received-routes statistics

Received routes total: 2

Table 20 Command output

Field | Description
Advertised routes total | Total number of advertised routes.
Received routes total | Total number of received routes.

# Display BGP IPv4 multicast route statistics.

<Sysname> display bgp routing-table ipv4 multicast statistics

Total number of routes: 5

Table 21 Command output

Field | Description
Total number of routes | Total number of routes.

# Display advertisement information for the BGP IPv4 multicast route destined to network 8.8.8.8/32.

<Sysname> display bgp routing-table ipv4 multicast 8.8.8.8 32 advertise-info

BGP local router ID: 192.168.1.139

Local AS number: 100

Paths: 1 best

BGP routing table information of 8.8.8.8/32:

Advertised to peers (1 in total):

192.168.1.62

Table 22 Command output

Field | Description
BGP local router ID | Local BGP router ID.
Local AS number | Local AS number.
Paths | Number of optimal routes to the destination.
BGP routing table information of 8.8.8.8/32 | Advertisement information for network 8.8.8.8/32.
Advertised to peers (1 in total) | Peers to which the network has been advertised.

Related commands

ip as-path

ip community-list

BGP commands -- display bgp routing-table ipv4 rtfilter

Use display bgp routing-table ipv4 rtfilter to display BGP IPv4 RT filter routing information.

Syntax

display bgp [ instance instance-name ] routing-table ipv4 rtfilter [ default-rt [ advertise-info ] | [ origin-as as-number ] [ route-target [ advertise-info ] ] | peer ipv4-address { advertised-routes | received-routes } [ default-rt | [ origin-as as-number ] [ route-target ] | statistics ] | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv4 RT filter routing information for the default BGP instance.

default-rt: Displays BGP IPv4 RT filter routing information for an all-zero RT.

origin-as as-number: Specifies an origin AS by its number.

route-target: Specifies an RT, a string of 3 to 21 characters.

An RT has the following formats:

· 16-bit AS number:32-bit user-defined number. For example, 101:3.

· 32-bit IP address:16-bit user-defined number. For example, 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, where the minimum value of the AS number is 65536. For example, 65536:1.

advertise-info: Displays advertisement information for BGP IPv4 RT filter routes.

peer ipv4-address: Displays BGP IPv4 RT filter routing information advertised to or received from the specified peer.

advertised-routes: Displays BGP IPv4 RT filter routing information advertised to the specified peer.

received-routes: Displays BGP IPv4 RT filter routing information received from the specified peer.

statistics: Displays routing statistics.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP IPv4 RT filter routes.

Examples

# Display brief information about all BGP IPv4 RT filter routes.

<Sysname> display bgp routing-table ipv4 rtfilter

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Total number of routes from all PEs: 2

Origin AS: 100

Total number of routes: 2

* >e Network : <100:1> PrefixLen : 96

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0

MED :

Path/Ogn: 100i

* >e Network : <1.1.1.1:1> PrefixLen : 96

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0

MED :

Path/Ogn: 100i

# Display information about BGP IPv4 RT filter routes that match origin AS 100.

<Sysname> display bgp routing-table ipv4 rtfilter origin-as 100

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Origin AS: 100

Total number of routes: 2

* >e Network : <100:1> PrefixLen : 96

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0

MED :

Path/Ogn: 100i

* >e Network : <1.1.1.1:1> PrefixLen : 96

NextHop : 1.1.1.2 LocPrf :

PrefVal : 0

MED :

Path/Ogn: 100i

# Display information about all public BGP IPv4 RT filter routes advertised to peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 rtfilter peer 10.2.1.2 advertised-routes

Total number of routes: 1

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Origin AS: 100

Total number of routes: 1

* > Network : <100:1> PrefixLen : 96

NextHop : 1.1.1.2 LocPrf :

MED : 0

Path/Ogn: i

# Display information about all public BGP IPv4 RT filter routes received from peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 rtfilter peer 10.2.1.2 received-routes

Total number of routes: 1

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Origin AS: 100

Total number of routes: 1

* >e Network : <100:1> PrefixLen : 96

NextHop : 10.1.1.1 LocPrf :

PrefVal : 0

MED : 0

Path/Ogn: 100i

Table 23 Command output

Field | Description
Origin AS | Origin AS of the RT filter routes.
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
NextHop | Next hop IP address.
MED | MULTI_EXIT_DISC attribute.
LocPrf | Local preference value.
PrefVal | Preferred value of the route.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH—Records the ASs the route has passed. · ORIGIN—Identifies the origin of the route.

# Display detailed information about BGP IPv4 RT filter route 100:1.

<Sysname> display bgp routing-table ipv4 rtfilter 100:1

BGP local router ID: 192.168.100.1

Local AS number: 100

Origin AS: 100

Total number of routes: 1

Paths: 1 available, 1 best

BGP routing table information of <100:1>/96:

Imported route.

Original nexthop: 10.2.1.1

OutLabel : NULL

AS-path : (null)

Origin : igp

Attribute value : MED 0, pref-val 32768, pre 0

State : valid, local, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 24 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
Imported route | The BGP RT filter route is locally generated.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
OutLabel | Outgoing label of the route.
AS-path | AS_PATH attribute of the route.
Origin | Origin of the route: · igp—Originated in the AS. The origin of routes advertised with the network command is IGP. · egp—Learned through EGP. · incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · synchronize. · best.
From | IP address of BGP peer that advertised the route.
Rely Nexthop | Next hop found by route recursion. If no next hop is found, this field displays not resolved.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.
Backup route | The route is a backup route.

# Display statistics for BGP IPv4 RT filter routes advertised to peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 rtfilter peer 10.2.1.2 advertised-routes statistics

Advertised routes total: 2

# Display statistics for BGP IPv4 RT filter routes received from peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 rtfilter peer 10.2.1.2 received-routes statistics

Received routes total: 2

Table 25 Command output

Field | Description
Advertised routes total | Total number of advertised routes.
Received routes total | Total number of received routes.

# Display BGP IPv4 RT filter route statistics.

<Sysname> display bgp routing-table ipv4 rtfilter statistics

Total number of routes from all PEs: 6

Origin AS: 100

Total number of routes: 2

Origin AS: 200

Total number of routes: 4

# Display advertisement information for the BGP IPv4 RT filter route 1.1.1.1:1/96.

<Sysname> display bgp routing-table ipv4 rtfilter 1.1.1.1:1 advertise-info

BGP local router ID: 192.168.100.1

Local AS number: 100

Paths: 1 best

Origin AS: 100

Total number of routes: 1

Paths: 1 best

BGP route-target filter information of <1.1.1.1:1>/96:

Advertised to VPN peers (1 in total):

1.1.1.2

Origin AS: 200

Total number of routes: 1

Paths: 1 best

BGP route-target filter information of <1.1.1.1:1>/96:

Advertised to VPN peers (1 in total):

1.1.1.2

Table 26 Command output

Field | Description
Paths | Number of optimal routes to the destination.
BGP route-target filter information of <1.1.1.1:1>/96 | Information about BGP IPv4 RT filter route 1.1.1.1:1/96.
Advertised to VPN peers (1 in total) | Peers to which the network has been advertised.

BGP commands -- display bgp routing-table ipv4 unicast

Use display bgp routing-table ipv4 unicast to display BGP IPv4 unicast routing information.

Syntax

display bgp [ instance instance-name ] routing-table ipv4 [ unicast ] [ vpn-instance vpn-instance-name ] [ ipv4-address [ { mask-length | mask } [ longest-match ] ] | ipv4-address [ mask-length | mask ] advertise-info | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv4-address { advertised-routes | received-routes } [ ipv4-address [ mask-length | mask ] | statistics ] | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv4 unicast routing information for the default BGP instance.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the BGP IPv4 unicast routing information for the public network.

ipv4-address: Specifies a destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

longest-match: Specifies longest match mode, which selects the longest matching route through the following steps:

1. ANDs the specified network address with the mask of each route.

2. Matches a route if the AND result is the same as the network address of the route and the mask of the route is shorter than or equal to the specified mask.

3. Selects the route with the longest mask among the matching routes.

advertise-info: Displays advertisement information for BGP IPv4 unicast routes.

as-path-acl as-path-acl-number: Displays BGP IPv4 unicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv4 unicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays routes exactly matching the specified community list. If you do not specify this keyword, the command displays routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer ipv4-address: Displays BGP IPv4 unicast routing information advertised to or received from the specified peer.

advertised-routes: Displays routing information advertised to the specified peer.

received-routes: Displays routing information received from the specified peer.

statistics: Displays routing statistics.

Usage guidelines

If you do not specify any parameters, this command displays brief information about all BGP IPv4 unicast routes.

If you specify only the ipv4-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, the command displays information about the route.

If you specify the ipv4-address mask or ipv4-address mask-length argument and do not specify the longest-match keyword, this command displays information about the BGP IPv4 unicast route that matches both the specified destination network address and the mask (or mask length).

This command displays BGP IPv4 unicast routing information regardless of whether the unicast keyword is specified.

Examples

# Display brief information about all BGP IPv4 unicast routes.

<Sysname> display bgp routing-table ipv4

Total number of routes: 4

BGP local router ID is 192.168.100.1

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* > 10.2.1.0/24 10.2.1.1 0 0 i

e 10.2.1.2 0 0 200i

* > 192.168.1.0 192.168.1.135 0 0 i

* e 10.2.1.2 0 0 200i

# Display information about BGP IPv4 unicast routes that match AS path list 1.

<Sysname> display bgp routing-table ipv4 as-path-acl 1

Total number of routes: 1

BGP local router ID is 2.2.2.2

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* >e 30.1.1.0/24 20.1.1.1 0 200i

# Display information about all public BGP IPv4 unicast routes advertised to peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 peer 10.2.1.2 advertised-routes

Total number of routes: 2

BGP local router ID is 192.168.100.1

Status codes: * - valid, > - best, d - damped, h - history,

s - suppressed, S - Stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

* > 10.2.1.0/24 10.2.1.1 0 0 i

* > 192.168.1.0 192.168.1.135 0 0 i

# Display information about all public BGP IPv4 unicast routes received from peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 peer 10.2.1.2 received-routes

Total number of routes: 2

BGP local router ID is 192.168.100.1

Status codes: * - valid, > - best, d - damped, h - history,

s - suppressed, S - Stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

Network NextHop MED LocPrf PrefVal Path/Ogn

e 10.2.1.0/24 10.2.1.2 0 0 200i

* e 192.168.1.0 10.2.1.2 0 0 200i

Table 27 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
NextHop | Next hop IP address.
MED | MULTI_EXIT_DISC attribute.
LocPrf | Local preference value.
PrefVal | Preferred value of the route.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH—Records the ASs the route has passed, which avoids routing loops. · ORIGIN—Identifies the origin of the route.

# Display detailed information about BGP IPv4 unicast routes destined to network 10.2.1.0/24.

<Sysname> display bgp routing-table ipv4 10.2.1.0 24

BGP local router ID: 192.168.100.1

Local AS number: 100

Paths: 2 available, 1 best

BGP routing table information of 10.2.1.0/24:

Imported route.

Original nexthop: 10.2.1.1

OutLabel : NULL

AS-path : (null)

Origin : igp

Attribute value : MED 0, pref-val 0, pre 0

State : valid, local, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

From : 10.2.1.2 (192.168.100.2)

Rely nexthop : not resolved

Original nexthop: 10.2.1.2

OutLabel : NULL

AS-path : 200

Origin : igp

Attribute value : MED 0, pref-val 0, pre 255

State : external

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

# Display detailed information about the BGP IPv4 unicast route destined to address 1.1.1.1/32.

<Sysname> display bgp routing-table ipv4 1.1.1.1 32

BGP local router ID: 192.168.100.1

Local AS number: 100

Paths: 2 available, 1 best

BGP routing table information of 1.1.1.1/32:

From : 10.2.1.1 (192.168.100.3)

Rely nexthop : 10.2.1.1

Original nexthop: 10.2.1.1

OutLabel : NULL

AS-path : (null)

Origin : igp

Attribute value : MED 0, pref-val 0, pre 0

State : valid, local, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Backup route.

From : 10.2.1.2 (192.168.100.2)

Rely nexthop : 10.2.1.2

Original nexthop: 10.2.1.2

OutLabel : NULL

AS-path : 200

Origin : igp

Attribute value : MED 0, pref-val 0, pre 255

State : external

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 28 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
OutLabel | Outgoing label of the route.
AS-path | AS_PATH attribute of the route, which records the ASs the route has passed and avoids routing loops.
Origin | Origin of the route: · igp—Originated in the AS. The origin of routes advertised with the network command is IGP. · egp—Learned through EGP. · incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · synchronize. · best.
From | IP address of the BGP peer that advertised the route.
Rely Nexthop | Next hop found by route recursion. If no next hop is found, this field displays not resolved.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.

# Display statistics for public BGP IPv4 unicast routes advertised to peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 peer 10.2.1.2 advertised-routes statistics

Advertised routes total: 2

# Display statistics for public BGP IPv4 unicast routes received from peer 10.2.1.2.

<Sysname> display bgp routing-table ipv4 peer 10.2.1.2 received-routes statistics

Received routes total: 2

Table 29 Command output

Field | Description
Advertised routes total | Total number of advertised routes.
Received routes total | Total number of received routes.

# Display BGP IPv4 unicast route statistics.

<Sysname> display bgp routing-table ipv4 statistics

Total number of routes: 4

Table 30 Command output

Field | Description
Total number of routes | Total number of routes.

# Display advertisement information for the BGP IPv4 unicast route destined to network 10.2.1.0/24.

<Sysname> display bgp routing-table ipv4 10.2.1.0 24 advertise-info

BGP local router ID: 192.168.100.1

Local AS number: 100

Paths: 1 best

BGP routing table information of 10.2.1.0/24:

Advertised to peers (1 in total):

10.2.1.2

Table 31 Command output

Field | Description
BGP local router ID | Local BGP router ID.
Local AS number | Local AS number.
Paths | Number of optimal routes to the destination.
BGP routing table information of 10.2.1.0/24 | Advertisement information for network 10.2.1.0/24.
Advertised to peers (1 in total) | Peers to which the network has been advertised.

Related commands

ip as-path

ip community-list

BGP commands -- display bgp routing-table ipv6 multicast

Use display bgp routing-table ipv6 multicast to display BGP IPv6 multicast routing information.

Syntax

display bgp [ instance instance-name ] routing-table ipv6 multicast [ ipv6-address prefix-length [ advertise-info ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv6 multicast routing information for the default BGP instance.

ipv6-address prefix-length: Specifies the destination network address and prefix length. The value range for the prefix-length argument is 0 to 128. If you do not specify this argument, the command displays brief information about all BGP IPv6 multicast routing information.

advertise-info: Displays advertisement information for BGP IPv6 multicast routes. If you do not specify this keyword, the command displays the BGP IPv6 multicast routing table.

as-path-acl as-path-acl-number: Displays BGP IPv6 multicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv6 multicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays BGP IPv6 multicast routes exactly matching the specified community list. If you do not specify this keyword, the command displays BGP IPv6 multicast routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer: Displays BGP IPv6 multicast routing information advertised to or received from the specified peer.

ipv6-address: Specifies the peer IPv6 address.

advertised-routes: Displays BGP IPv6 multicast routing information advertised to the specified peer.

received-routes: Displays BGP IPv6 multicast routing information received from the specified peer.

statistics: Displays routing statistics.

Examples

# Display brief information about all BGP IPv6 multicast routes.

<Sysname> display bgp routing-table ipv6 multicast

Total number of routes: 5

BGP local router ID is 192.168.1.139

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 1:: PrefixLen : 64

NextHop : :: LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* i Network : 1:: PrefixLen : 64

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 1::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 2::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* >i Network : 5::5 PrefixLen : 128

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

# Display information about BGP IPv6 multicast routes that match AS path list 1.

<Sysname> display bgp routing-table ipv6 multicast as-path-acl 1

Total number of routes: 5

BGP local router ID is 192.168.1.139

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 1:: PrefixLen : 64

NextHop : :: LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* i Network : 1:: PrefixLen : 64

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 1::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 2::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* >i Network : 5::5 PrefixLen : 128

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

# Display information about BGP IPv6 multicast routes that match BGP community list 100.

<Sysname> display bgp routing-table ipv6 multicast community-list 100

Total number of routes: 5

BGP local router ID is 192.168.1.139

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 1:: PrefixLen : 64

NextHop : :: LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* i Network : 1:: PrefixLen : 64

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 1::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* > Network : 2::2 PrefixLen : 128

NextHop : ::1 LocPrf :

PrefVal : 32768 OutLabel : NULL

MED : 0

Path/Ogn: ?

* >i Network : 5::5 PrefixLen : 128

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

# Display information about all BGP IPv6 multicast routes advertised to peer 1::1.

<Sysname> display bgp routing-table ipv6 multicast peer 1::1 advertised-routes

Total number of routes: 2

BGP local router ID is 192.168.1.139

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 1:: PrefixLen : 64

NextHop : :: LocPrf : 100

MED : 0 OutLabel : NULL

Path/Ogn: ?

* > Network : 2::2 PrefixLen : 128

NextHop : ::1 LocPrf : 100

MED : 0 OutLabel : NULL

Path/Ogn: ?

# Display information about all BGP IPv6 multicast routes received from peer 1::1.

<Sysname> display bgp routing-table ipv6 multicast peer 1::1 received-routes

Total number of routes: 2

BGP local router ID is 192.168.1.139

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* i Network : 1:: PrefixLen : 64

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

* >i Network : 5::5 PrefixLen : 128

NextHop : 1::1 LocPrf : 100

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: ?

Table 32 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
PrefixLen | Prefix length of the destination network address.
NextHop | Next hop IP address.
LocPrf | Local preference value.
PrefVal | Preferred value of the route.
OutLabel | Outgoing label of the route.
MED | MULTI_EXIT_DISC attribute.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH—Records the ASs the route has passed, which avoids routing loops. · ORIGIN—Identifies the origin of the route.

# Display detailed information about BGP IPv6 multicast routes destined to network 2::2/128.

<Sysname> display bgp routing-table ipv6 multicast 2::2 128

BGP local router ID: 192.168.1.139

Local AS number: 100

Paths: 1 available, 1 best

BGP routing table information of 2::2/128:

Imported route.

Original nexthop: ::1

OutLabel : NULL

AS-path : (null)

Origin : incomplete

Attribute value : MED 0, pref-val 32768

State : valid, local, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 33 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
OutLabel | Outgoing label of the route.
AS-path | AS_PATH attribute of the route, which records the ASs the route has passed and avoids routing loops.
Origin | Origin of the route: · igp—Originated in the AS. The origin of routes advertised with the network command is IGP. · egp—Learned through EGP. · incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · synchronize. · best.
From | IP address of the BGP peer that advertised the route.
Rely Nexthop | Next hop found by route recursion. If no next hop is found, this field displays not resolved.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.

# Display advertisement information for BGP IPv6 multicast routes destined to network 2::2/128.

<Sysname> display bgp routing-table ipv6 multicast 2::2 128 advertise-info

BGP local router ID: 192.168.1.139

Local AS number: 100

Paths: 1 best

BGP routing table information of 2::2/128:

Advertised to peers (1 in total):

1::1

Table 34 Command output

Field | Description
BGP local router ID | Local BGP router ID.
Local AS number | Local AS number.
Paths | Number of optimal routes to the destination.
BGP routing table information of 2::2/128 | Advertisement information for network 2::2/128.
Advertised to peers (1 in total) | Peers to which the network has been advertised.

# Display statistics for BGP IPv6 multicast routes advertised to peer 1::1.

<Sysname> display bgp routing-table ipv6 multicast peer 1::1 advertised-routes statistics

Advertised routes total: 2

# Display statistics for BGP IPv6 multicast routes received from peer 1::1.

<Sysname> display bgp routing-table ipv6 multicast peer 1::1 received-routes statistics

Received routes total: 2

Table 35 Command output

Field | Description
Advertised routes total | Total number of advertised routes.
Received routes total | Total number of received routes.

# Display BGP IPv6 multicast route statistics.

<Sysname> display bgp routing-table ipv6 multicast statistics

Total number of routes: 5

Table 36 Command output

Field | Description
Total number of routes | Total number of routes.

Related commands

ip as-path

ip community-list

BGP commands -- display bgp routing-table ipv6 unicast

Use display bgp routing-table ipv6 unicast to display BGP IPv6 unicast routing information.

Syntax

display bgp [ instance instance-name ] routing-table ipv6 [ unicast ] [ vpn-instance vpn-instance-name ] [ ipv6-address prefix-length [ advertise-info ] | as-path-acl as-path-acl-number | community-list { { basic-community-list-number | comm-list-name } [ whole-match ] | adv-community-list-number } | peer ipv6-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ] | statistics ]

display bgp [ instance instance-name ] routing-table ipv6 [ unicast ] peer ipv4-address { advertised-routes | received-routes } [ ipv6-address prefix-length | statistics ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP IPv6 unicast routing information for the default BGP instance.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the BGP IPv6 unicast routing information for the public network.

ipv6-address prefix-length: Specifies the destination network address and prefix length. The value range for the prefix-length argument is 0 to 128. If you do not specify this argument, the command displays brief information about all BGP IPv6 unicast routing information.

advertise-info: Displays advertisement information for BGP IPv6 unicast routes. If you do not specify this keyword, the command displays the BGP IPv6 unicast routing table.

as-path-acl as-path-acl-number: Displays BGP IPv6 unicast routes that match the AS path list specified by its number in the range of 1 to 256.

community-list: Displays BGP IPv6 unicast routes that match a community list.

basic-community-list-number: Specifies a basic community list by its number in the range of 1 to 99.

comm-list-name: Specifies a community list by its name, a case-sensitive string of 1 to 63 characters.

whole-match: Displays routes exactly matching the specified community list. If you do not specify this keyword, the command displays routes whose COMMUNITY attributes include the specified community list.

adv-community-list-number: Specifies an advanced community list by its number in the range of 100 to 199.

peer: Displays BGP IPv6 unicast routing information advertised to or received from the specified peer.

ipv4-address: Specifies the peer IPv4 address.

ipv6-address: Specifies the peer IPv6 address.

advertised-routes: Displays routing information advertised to the specified peer.

received-routes: Displays routing information received from the specified peer.

statistics: Displays routing statistics.

Usage guidelines

This command displays BGP IPv6 unicast routing information regardless of whether the unicast keyword is specified.

Examples

# Display brief information about all BGP IPv6 unicast routes.

<Sysname> display bgp routing-table ipv6

Total number of routes: 1

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* >e Network : 3:: PrefixLen : 64

NextHop : 1::2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 100i

# Display information about BGP IPv6 unicast routes that match AS path list 1.

<Sysname> display bgp routing-table ipv6 as-path-acl 1

Total number of routes: 2

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* >e Network : 2:: PrefixLen : 64

NextHop : 1::2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 100i

* >e Network : 3:: PrefixLen : 64

NextHop : 1::2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 100i

# Display information about BGP IPv6 unicast routes that match BGP community list 100.

<Sysname> display bgp routing-table ipv6 community-list 100

Total number of routes: 2

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* >e Network : 2:: PrefixLen : 64

NextHop : 1::2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 100i

* >e Network : 3:: PrefixLen : 64

NextHop : 1::2 LocPrf :

PrefVal : 0 OutLabel : NULL

MED :

Path/Ogn: 100i

# Display information about all BGP IPv6 unicast routes advertised to peer 1::1.

<Sysname> display bgp routing-table ipv6 peer 1::1 advertised-routes

Total number of routes: 1

BGP local router ID is 192.168.1.136

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 2:: PrefixLen : 64

NextHop : :: LocPrf :

MED : 0 OutLabel : NULL

Path/Ogn: i

# Display information about all BGP IPv6 unicast routes received from peer 1::1.

<Sysname> display bgp routing-table ipv6 peer 1::1 received-routes

Total number of routes: 1

BGP local router ID is 192.168.1.135

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* >e Network : 2:: PrefixLen : 64

NextHop : ::FFFF:10.1.1.1 LocPrf :

PrefVal : 0 OutLabel : NULL

MED : 0

Path/Ogn: 100i

Table 37 Command output

Field | Description
Status codes | Status codes: · * – valid—Valid route. · > – best—Optimal route. · d – dampened—Dampened route. · h – history—History route. · s – suppressed—Suppressed route. · S – stale—Stale route. · i – internal—Internal route. · e – external—External route.
Origin | Origin of the route: · i – IGP—Originated in the AS. The origin of routes advertised with the network command is IGP. · e – EGP—Learned through EGP. · ?– incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Network | Destination network address.
PrefixLen | Prefix length of the destination network address.
NextHop | Next hop IPv6 address.
LocPrf | Local preference value.
PrefVal | Preferred value of the route.
OutLabel | Outgoing label of the route.
MED | MULTI_EXIT_DISC attribute.
Path/Ogn | AS_PATH and ORIGIN attributes of the route: · AS_PATH attribute—Records the ASs the route has passed, which avoids routing loops. · ORIGIN attribute—Identifies the origin of the route.

# Display detailed information about BGP IPv6 unicast routes destined to network 2::/64.

<Sysname> display bgp routing-table ipv6 2:: 64

BGP local router ID: 192.168.1.135

Local AS number: 200

Paths: 2 available, 1 best

BGP routing table information of 2::/64:

From : 10.1.1.1 (192.168.1.136)

Relay nexthop : ::FFFF:10.1.1.1

Original nexthop: ::FFFF:10.1.1.1

OutLabel : NULL

AS-path : 100

Origin : igp

Attribute value : MED 0, pref-val 0

State : valid, external, best

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

From : 1::1 (192.168.1.136)

Relay nexthop : 1::1

Original nexthop: 1::1

OutLabel : NULL

AS-path : 100

Origin : igp

Attribute value : MED 0, pref-val 0

State : valid, external

IP precedence : N/A

QoS local ID : N/A

Traffic index : N/A

Table 38 Command output

Field | Description
Paths | Number of routes: · available—Number of valid routes. · best—Number of optimal routes.
Original nexthop | Original next hop of the route. If the route was obtained from a BGP update message, the original next hop is the next hop IP address in the message.
OutLabel | Outgoing label of the route.
AS-path | AS_PATH attribute of the route, which records the ASs the route has passed and avoids routing loops.
Origin | Origin of the route: · igp—Originated in the AS. The origin of routes advertised with the network command is IGP. · egp—Learned through EGP. · incomplete—Unknown origin. The origin of routes redistributed from IGP protocols is INCOMPLETE.
Attribute value | BGP path attributes: · MED—MED value. · localpref—Local preference value. · pref-val—Preferred value. · pre—Route preference.
State | Current state of the route: · valid. · internal. · external. · local. · best.
From | IP address of the BGP peer that advertised the route.
Relay Nexthop | Next hop found by route recursion. If no next hop is found, this field displays not resolved.
IP precedence | IP precedence in the range of 0 to 7. N/A indicates that the route does not support this field.
QoS local ID | QoS local ID in the range of 1 to 4095. N/A indicates that the route does not support this field.
Traffic index | Traffic index in the range of 1 to 64. N/A indicates that the route does not support this field.

# Display advertisement information for BGP IPv6 unicast routes destined to network 2::/64.

<Sysname> display bgp routing-table ipv6 2:: 64 advertise-info

BGP local router ID: 192.168.1.136

Local AS number: 100

Paths: 1 best

BGP routing table information of 2::/64:

Advertised to peers (2 in total):

10.1.1.2

1::2

Table 39 Command output

Field | Description
Paths | Number of optimal routes destined to the specified network.
BGP routing table information of 2::/64 | Advertisement information for BGP routes destined to network 2::/64.
Advertised to peers (2 in total) | Peers to which the route has been advertised, and the number of peers.

# Display statistics for BGP IPv6 unicast routes advertised to peer 1::1.

<Sysname> display bgp routing-table ipv6 peer 1::1 advertised-routes statistics

Advertised routes total: 1

# Display statistics for BGP IPv6 unicast routes received from peer 1::1.

<Sysname> display bgp routing-table ipv6 peer 1::1 received-routes statistics

Received routes total: 1

Table 40 Command output

Field | Description
Advertised routes total | Total number of advertised routes.
Received routes total | Total number of received routes.

# Display BGP IPv6 unicast route statistics.

<Sysname> display bgp routing-table ipv6 statistics

Total number of routes: 4

Table 41 Command output

Field | Description
Total number of routes | Total number of routes.

Related commands

ip as-path

ip community-list

BGP commands -- display bgp routing-table ipv6 unicast inlabel

Use display bgp routing-table ipv6 unicast inlabel to display incoming labels for BGP IPv6 unicast routes.

Syntax

display bgp [ instance instance-name ] routing-table ipv6 [ unicast ] inlabel

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays incoming labels of BGP IPv6 unicast routes in the default BGP instance.

Usage guidelines

This command displays incoming labels for BGP IPv6 unicast routes regardless of whether the unicast keyword is specified.

Examples

# Display incoming labels for all BGP IPv6 unicast routes.

<Sysname> display bgp routing-table ipv6 inlabel

Total number of routes: 2

BGP local router ID is 2.2.2.2

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* > Network : 1::1 PrefixLen : 128

NextHop : 10::1 OutLabel : NULL

InLabel : 1279

* > Network : 10:: PrefixLen : 64

NextHop : :: OutLabel : NULL

InLabel : 1278

Table 42 Command output

Field | Description
Status codes | Status codes. For more information, see Table 37.
Origin | Origin of the route. For more information, see Table 37.
Network | Destination network address.
PrefixLen | Prefix length of the destination network address.
NextHop | Next hop IPv6 address.
OutLabel | Outgoing label of the IPv6 unicast route, which is assigned by the peer 6PE device.
InLabel | Incoming label of the IPv6 unicast route, which is assigned by the local 6PE device.

BGP commands -- display bgp routing-table ipv6 unicast outlabel

Use display bgp routing-table ipv6 unicast outlabel to display outgoing labels for BGP IPv6 unicast routes.

Syntax

display bgp [ instance instance-name ] routing-table ipv6 [ unicast ] outlabel

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command display outgoing labels of BGP IPv6 unicast routes in the default BGP instance.

Usage guidelines

This command displays outgoing labels for BGP IPv6 unicast routes regardless of whether the unicast keyword is specified.

Examples

# Display outgoing labels for all BGP IPv6 unicast routes.

<Sysname> display bgp routing-table ipv6 outlabel

Total number of routes: 2

BGP local router ID is 2.2.2.2

Status codes: * - valid, > - best, d - dampened, h - history,

s - suppressed, S - stale, i - internal, e - external

Origin: i - IGP, e - EGP, ? - incomplete

* >i Network : 4::4 PrefixLen : 128

NextHop : ::FFFF:3.3.3.3 OutLabel : 1279

* >i Network : 20:: PrefixLen : 64

NextHop : ::FFFF:3.3.3.3 OutLabel : 1278

Table 43 Command output

Field | Description
Status codes | Status codes. For more information, see Table 37.
Origin | Origin of the route. For more information, see Table 37.
Network | Destination network address.
PrefixLen | Prefix length of the destination network address.
NextHop | Next hop IPv6 address.
OutLabel | Outgoing label of the IPv6 unicast route, which is assigned by the peer 6PE device.

BGP commands -- display bgp update-group

Use display bgp update-group to display information about BGP update groups.

Syntax

display bgp [ instance instance-name ] update-group ipv4 { mdt | multicast | rtfilter | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv4-address ]

display bgp [ instance instance-name ] update-group ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv6-address ]

display bgp [ instance instance-name ] update-group ipv6 [ unicast ] [ ipv4-address ]

display bgp [ instance instance-name ] update-group link-state [ ipv4-address | ipv6-address ]

display bgp [ instance instance-name ] update-group vpnv4 [ vpn-instance vpn-instance-name ] [ ipv4-address ]

display bgp [ instance instance-name ] update-group l2vpn [ evpn ] [ ipv4-address ]

display bgp [ instance instance-name ] update-group vpnv6 [ ipv4-address ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays BGP update group information for the default BGP instance.

ipv4: Displays BGP update group information for IPv4 address family.

ipv6: Displays BGP update group information for IPv6 address family.

link-state: Displays BGP update group information for LS address family.

vpnv4: Displays BGP update group information for VPNv4 address family.

l2vpn: Displays BGP update group information for L2VPN address family.

evpn: Displays BGP update group information for EVPN address family.

vpnv6: Displays BGP update group information for VPNv6 address family.

mdt: Displays BGP update group information for MDT address family.

multicast: Displays BGP update group information for multicast address family.

rtfilter: Displays BGP update group information for BGP IPv4 RT filter address family.

unicast: Displays BGP update group information for unicast address family.

vpn-instance vpn-instance-name: Displays BGP update group information for the MPLS L3VPN instance specified by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays update group information for the public network.

ipv4-address: Displays BGP update group information for the specified BGP peer.

ipv6-address: Displays BGP update group information for the specified IPv6 BGP peer.

Usage guidelines

The update group feature classifies BGP peers that have the same export policy into an update group. When BGP advertises routes to the peers in the update group, it uses the export policy to filter the routes and generates route updates for all the peers only once.

With this feature, BGP performs one-time policy filtering and encapsulation for a prefix before advertising the prefix to all the peers in the update group. For example, BGP advertises 1000 prefixes to 1000 peers that have the same export policy (in data centers for example). Without the update group feature, BGP matches the export policy 1000 ?1000 times. With the update group feature, BGP matches the export policy only 1000 ? 1 times, improving encapsulation efficiency 1000 times.

If you do not specify any parameters, this command displays all update groups for the specified address family on the public network.

By default, the unicast keyword is used if the unicast, mdt, and multicast keywords are not specified.

Examples

# Display information about all BGP update groups for the IPv4 unicast address family.

<Sysname> display bgp update-group ipv4

Update-group ID: 0

Type: EBGP link

4-byte AS number: Supported

Site-of-Origin: Not specified

Minimum time between advertisements: 30 seconds

OutQ: 0

Members: 1

99.1.1.1

# Display update group information for BGP VPNv4 peer 1.1.1.2 in VPN instance vpn1.

<Sysname> display bgp update-group vpnv4 vpn-instance vpn1 1.1.1.2

Update-group ID: 0

Type: EBGP link

4-byte AS number: Supported

Site-of-Origin: Not specified

Nesting VPN: vpn1

Minimum time between advertisements: 30 seconds

OutQ: 0

Members: 2

1.1.1.2

1.1.1.3

# Display all update group information for the BGP L2VPN address family.

<Sysname> display bgp update-group l2vpn

Update-group ID: 0

Type: IBGP link

4-byte AS number: Supported

Site-of-Origin: Not specified

L2VPN signaling (VPLS): Supported

L2VPN signaling (VPWS): RFC mode

L2VPN auto-discovery: RFC mode

Minimum time between advertisements: 15 seconds

OutQ: 0

Members: 2

2.2.2.9

3.3.3.9

Table 44 Command output

Field | Description
Update-group ID | ID of the update group.
Type | BGP link type: · IBGP link. · EBGP link. · Confed IBGP link—Confederation IBGP link. · Confed EBGP link—Confederation EBGP link.
Label capability: Supported | The peers in the update group support labeled routes.
4-byte AS number: Supported | 4-byte AS number suppression is disabled for the peers in the update group. The peers in the update group support 4-byte AS numbers.
4-byte AS number: Suppressed | 4-byte AS number suppression is enabled for the peers in the update group.
Fake AS | A fake local AS number is configured for the peers in the update group.
Public-AS-Only: Yes | BGP route updates advertised to the peers in the update group only carry the public AS number without the private AS number. · Yes—If a peer uses a private AS number, the AS number is used as an update group classification criterion. If a peer uses a public AS number, the AS number is not used as an update group classification criterion. · No—The AS number is not used as an update group classification criterion.
Substitute-AS: Yes | AS number substitution is enabled.
Minimum time between advertisements: number seconds | Minimum time between advertisements.
Advertising community: Yes | Community advertisement to peers in the update group is enabled.
Route-reflect client: Yes | The peer is a client of the route reflector.
Advertising extended community: Yes | Extended community advertisement to peers in the update group is enabled.
Export AS-path-ACL | AS path ACL used to filter BGP routes advertised to peers in the update group.
Export prefix list | Prefix list used to filter BGP routes advertised to peers in the update group.
Export route policy | Routing policy used to filter BGP routes advertised to peers in the update group.
Export filter-policy | ACL used to filter BGP routes advertised to peers in the update group.
OutQ | Number of prefixes to be advertised to peers in the update group.
Members | Number and IP addresses of peers in the update group.
Nesting VPN | Peers in the update group support nesting VPN.
UPE: Yes | Peers in the update group are UPE devices.
UPE export route policy | An outgoing routing policy is applied to peers in the update group.
L2VPN signaling (VPLS): Supported | Peers in the update group support using NLRI defined in RFC 4761 to advertise VPLS label blocks.
L2VPN signaling (VPWS): RFC mode | Peers in the update group support using NLRI defined in RFC 4761 to advertise MPLS L2VPN label blocks.
L2VPN signaling (VPWS): Draft mode | Peers in the update group support using NLRI defined in the draft draft-kompella-ppvpn-l2vpn-03 to advertise MPLS L2VPN label blocks.
L2VPN auto-discovery: RFC mode | Peers in the update group support using NLRI defined in RFC 6074 to exchange VPLS PE information.
L2VPN auto-discovery: Non-standard mode | Peers in the update group support using non-standard NLRI to exchange VPLS PE information.

BGP commands -- display bgp-policy statistics

Use display bgp-policy statistics to display BGP policy accounting information.

Syntax

display bgp-policy { ip | ipv6 } statistics { input | output } [ interface interface-type interface-number ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ip: Displays BGP policy accounting information for IPv4 traffic.

ipv6: Displays BGP policy accounting information for IPv6 traffic.

input: Displays BGP policy accounting information for incoming traffic.

output: Displays BGP policy accounting information for outgoing traffic.

interface interface-type interface-number: Displays BGP policy accounting information on an interface specified by the interface type and number. If you do not specify an interface, this command displays global BGP policy accounting information.

Examples

# Display global BGP policy accounting information for incoming IPv4 traffic.

<Sysname> display bgp-policy ip statistics input

Statistics for the inbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

# Display global BGP policy accounting information for incoming IPv6 traffic.

<Sysname> display bgp-policy ipv6 statistics input

Statistics for the inbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

# Display BGP policy accounting information for outgoing IPv4 traffic on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> display bgp-policy ip statistics output interface gigabitethernet 1/0/1

Statistics for GigabitEthernet1/0/1 in the outbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

# Display BGP policy accounting information for outgoing IPv6 traffic on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> display bgp-policy ipv6 statistics output interface gigabitethernet 1/0/1

Statistics for GigabitEthernet1/0/1 in the outbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

# Display BGP policy accounting information for outgoing IPv4 traffic on VLAN-interface 10. (Applicable to switches.)

<Sysname> display bgp-policy ip statistics output interface vlan-interface 10

Statistics for Vlan-interface10 in the outbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

# Display BGP policy accounting information for outgoing IPv6 traffic on VLAN-interface 10. (Applicable to switches.)

<Sysname> display bgp-policy ipv6 statistics output interface vlan-interface 10

Statistics for Vlan-interface10 in the outbound direction:

Traffic index Packets Bytes

1 0 0

2 0 0

3 0 0

4 0 0

5 0 0

6 0 0

7 0 0

8 0 0

9 0 0

10 0 0

Table 45 Command output

Field | Description
Packets | Number of packets for traffic with an index.
Bytes | Number of bytes for traffic with an index.

Related commands

bgp-policy accounting

BGP commands -- domain-distinguisher

Use domain-distinguisher to specify an AS number and a router ID for BGP LS messages.

Use undo domain-distinguisher to restore the default.

Syntax

domain-distinguisher as-number:router-id

undo domain-distinguisher

Default

The AS number and router ID of the current BGP process are used.

Views

BGP LS address family view

Predefined user roles

network-admin

mdc-admin

Parameters

as-number:router-id: Specifies the AS number and router ID. The value range for the as-number argument is 1 to 4294967295, and the router ID is in IP address format.

Examples

# Set the AS number and router ID for BGP LS messages to 65009 and 1.1.1.1, respectively.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family link-state

[Sysname-bgp-default-ls] domain-distinguisher 65009:1.1.1.1

BGP commands -- ebgp-interface-sensitive

Use ebgp-interface-sensitive to enable immediate re-establishment of direct EBGP sessions.

Use undo ebgp-interface-sensitive to disable immediate re-establishment of direct EBGP sessions.

Syntax

ebgp-interface-sensitive

undo ebgp-interface-sensitive

Default

Immediate re-establishment of direct EBGP sessions is enabled.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When a direct link to an EBGP peer fails, BGP tears down the session and re-establishes a session to the peer immediately. If the feature is not enabled, the router does not tear down the session until the hold time expires. However, disabling this feature can prevent routing flaps from affecting EBGP session state.

This command applies only to direct EBGP sessions.

Examples

# Enable immediate re-establishment of direct EBGP sessions.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] ebgp-interface-sensitive

BGP commands -- fast-reroute route-policy

Use fast-reroute route-policy to apply a routing policy to fast reroute (FRR) for a BGP address family.

Use undo fast-reroute route-policy to restore the default.

Syntax

fast-reroute route-policy route-policy-name

undo fast-reroute route-policy

Default

No routing policy is applied to FRR.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

You can use the following methods to configure BGP FRR:

· Method 1—Execute the pic command in BGP address family view. BGP calculates a backup next hop for a BGP route in the address family if there are two or more unequal-cost routes to reach the destination.

· Method 2—Execute the fast-reroute route-policy command to use a routing policy in which a backup next hop is specified by using the command apply [ ipv6 ] fast-reroute backup-nexthop. For BGP to generate a backup next hop for the primary route, the backup next hop calculated by BGP must be the same as the specified backup next hop. You can also configure if-match clauses in the routing policy to identify the routes protected by FRR.

If both methods are configured, Method 2 takes precedence over Method 1.

Examples

# Apply routing policy frr-policy to FRR in BGP IPv4 unicast address family view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4

[Sysname-bgp-default-ipv4] fast-reroute route-policy frr-policy

Related commands

apply fast-reroute

apply ipv6 fast-reroute

pic

route-policy

BGP commands -- filter-policy export

Use filter-policy export to filter advertised BGP routes.

Use undo filter-policy export to remove the route filter.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP IPv4 multicast address family view:

filter-policy { ipv4-acl-number | prefix-list prefix-list-name } export [ protocol process-id ]

undo filter-policy export [ protocol process-id ]

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP VPNv6 address family view/BGP IPv6 multicast address family view:

filter-policy { ipv6-acl-number | prefix-list ipv6-prefix-name } export [ protocol process-id ]

undo filter-policy export [ protocol process-id ]

Default

Advertised BGP routes are not filtered.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-acl-number: Specifies an IPv4 ACL by its number in the range of 2000 to 3999, to match routes by destination.

ipv6-acl-number: Specifies an IPv6 ACL by its number in the range of 2000 to 3999, to match routes by destination.

prefix-list prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters, to match routes by destination.

prefix-list ipv6-prefix-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters, to match routes by destination.

protocol: Filters routes redistributed from the routing protocol.

process-id: Specifies a routing protocol by its ID in the range of 1 to 65535. For IPv4 routes, this argument is available only when the protocol is isis, ospf, or rip. For IPv6 routes, this argument is available only when the protocol is isisv6, ospfv3, or ripng.

Usage guidelines

If you specify a protocol (such as direct and isis), this command filters only routes redistributed from the specified protocol. If you do not specify a protocol, this command filters all advertised routes, including the following routes:

· Redistributed from IGP.

· Injected by the network command.

· Learned from BGP peers.

If you use a basic ACL (with a number from 2000 to 2999) configured with the rule [ rule-id ] { deny | permit } source source-address source-wildcard command, the command matches routes whose destination network addresses match the source-address source-wildcard argument. However, it does not match the masks of the destination addresses.

To use an advanced ACL (with a number from 3000 to 3999) in the command, configure the ACL using one of the following steps:

· To deny/permit a route with the specified destination, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard command.

· To deny/permit a route with the specified destination and mask, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard destination dest-addr dest-wildcard command.

The source keyword specifies the destination address of a route and the destination keyword specifies the subnet mask of the destination address. For the mask configuration to take effect, specify a contiguous subnet mask.

Examples

# In BGP IPv4 unicast address family view, use IPv4 basic ACL 2000 to filter advertised BGP IPv4 routes.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] filter-policy 2000 export

Related commands

filter-policy import

peer as-path-acl

peer filter-policy

peer prefix-list

peer route-policy

BGP commands -- filter-policy import

Use filter-policy import to filter received BGP routes.

Use undo filter-policy import to restore the default.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP IPv4 multicast address family view:

filter-policy { ipv4-acl-number | prefix-list prefix-list-name } import

undo filter-policy import

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP VPNv6 address family view/BGP IPv6 multicast address family view:

filter-policy { ipv6-acl-number | prefix-list ipv6-prefix-name } import

undo filter-policy import

Default

Received BGP routes are not filtered.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-acl-number: Specifies an IPv4 ACL by its number in the range of 2000 to 3999, to match routes by destination.

ipv6-acl-number: Specifies an IPv6 ACL by its number in the range of 2000 to 3999, to match routes by destination.

prefix-list prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters, to match routes by destination.

prefix-list ipv6-prefix-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters, to match routes by destination.

Usage guidelines

If you use a basic ACL (with a number from 2000 to 2999) configured with the rule [ rule-id ] { deny | permit } source source-address source-wildcard command, the command matches routes whose destination network addresses match the source-address source-wildcard argument. However, it does not match the masks of the destination addresses.

To use an advanced ACL (with a number from 3000 to 3999) in the command, configure the ACL using one of the following steps:

· To deny/permit a route with the specified destination, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard command.

· To deny/permit a route with the specified destination and mask, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard destination dest-addr dest-wildcard command.

The source keyword specifies the destination address of a route and the destination keyword specifies the subnet mask of the destination address. For the mask configuration to take effect, specify a contiguous subnet mask.

Examples

# In BGP IPv4 unicast address family view, use IPv4 basic ACL 2000 to filter received BGP routes.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] filter-policy 2000 import

Related commands

filter-policy export

peer as-path-acl

peer filter-policy

peer prefix-list

peer route-policy

BGP commands -- flush suboptimal-route

Use flush suboptimal-route to enable BGP to flush the suboptimal BGP route to the RIB.

Use undo flush suboptimal-route to disable BGP from flushing the suboptimal BGP route to the RIB.

Syntax

flush suboptimal-route

undo flush suboptimal-route

Default

BGP is disabled from flushing the suboptimal BGP route to the RIB. Only the optimal route is flushed to the RIB.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command flushes the suboptimal BGP route to the RIB when the following conditions are met:

· The optimal route is generated by the network command or is redistributed by the import-route command.

· The suboptimal route is received from a BGP peer.

After the suboptimal route is flushed to the RIB on a network, BGP immediately switches traffic to the suboptimal route when the optimal route fails.

For example, the device has a static route to the subnet 1.1.1.0/24 that has a higher priority than a BGP route. BGP redistributes the static route and receives a route to 1.1.1.0/24 from a peer. After the flush suboptimal-route command is executed, BGP flushes the received BGP route to the RIB as the suboptimal route. When the static route fails, BGP immediately switches traffic to the suboptimal route if inter-protocol FRR is enabled. For more information about inter-protocol FRR, see Layer 3—IP Routing Configuration Guide.

Examples

# Enable BGP to flush the suboptimal BGP route to the RIB.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] flush suboptimal-route

BGP commands -- graceful-restart

Use graceful-restart to enable BGP Graceful Restart (GR) capability.

Use undo graceful-restart to disable BGP GR capability.

Syntax

graceful-restart

undo graceful-restart

Default

BGP GR capability is disabled.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

GR ensures continuous forwarding when BGP restarts or an active/standby switchover occurs.

BGP peers exchange Open messages containing GR information. If both parties have GR capability, they establish a GR-capable session.

After you execute this command, the device re-establishes BGP sessions.

Examples

# Enable GR capability for BGP process 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] graceful-restart

Related commands

graceful-restart timer purge-time

graceful-restart timer restart

graceful-restart timer wait-for-rib

BGP commands -- graceful-restart timer purge-time

Use graceful-restart timer purge-time to set the Routing Information Base (RIB) purge timer.

Use undo graceful-restart timer purge-time to restore the default.

Syntax

graceful-restart timer purge-time timer

undo graceful-restart timer purge-time

Default

The RIB purge timer is 480 seconds.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

timer: Sets the RIB purge timer in the range of 1 to 6000 seconds.

Usage guidelines

BGP starts the RIB purge timer when an active/standby switchover occurs or BGP restarts. If BGP route exchange is not completed within the RIB purge timer, the GR restarter quits the GR process. It updates the RIB with the BGP routes already learned, and removes the stale routes from RIB.

Enable BGP GR before you execute this command.

Set the RIB purge timer to be long enough to complete GR, especially when large numbers of BGP routes exist.

As a best practice, set the RIB purge timer in the following way:

· Set the timer to be greater than the timer set by the graceful-restart timer wait-for-rib command

· Set the timer to be less than the timer set by the protocol lifetime command.

Examples

# Set the RIB purge timer to 300 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] graceful-restart

[Sysname-bgp-default] graceful-restart timer purge-time 300

Related commands

graceful-restart

graceful-restart timer restart

graceful-restart timer wait-for-rib

protocol lifetime (Layer 3—IP Routing Command Reference)

BGP commands -- graceful-restart timer restart

Use graceful-restart timer restart to configure the GR timer.

Use undo graceful-restart timer restart to restore the default.

Syntax

graceful-restart timer restart timer

undo graceful-restart timer restart

Default

The GR timer is 150 seconds.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

timer: Specifies the GR timer in the range of 3 to 600 seconds.

Usage guidelines

The GR restarter sends the GR timer to the GR helper in an Open message. When the GR helper detects that an active/standby switchover or a BGP restart occurred on the GR restarter, the GR helper performs the following operations:

1. Marks all routes learned from the GR restarter as stale.

2. Starts the GR timer.

3. If no BGP session is established before the GR timer expires, the GR helper removes the stale routes.

Before you configure this command, enable the BGP GR capability.

To apply a new GR timer, you must re-establish BGP sessions.

Examples

# Set the GR timer to 300 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] graceful-restart

[Sysname-bgp-default] graceful-restart timer restart 300

Related commands

graceful-restart

graceful-restart timer purge-time

graceful-restart timer wait-for-rib

BGP commands -- graceful-restart timer wait-for-rib

Use graceful-restart timer wait-for-rib to configure the time to wait for the End-of-RIB marker.

Use undo graceful-restart timer wait-for-rib to restore the default.

Syntax

graceful-restart timer wait-for-rib timer

undo graceful-restart timer wait-for-rib

Default

The time to wait for the End-of-RIB marker is 180 seconds.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

timer: Specifies the time to wait for the End-of-RIB marker, in the range of 3 to 3600 seconds.

Usage guidelines

BGP uses this timer to control the time to receive updates from the peer. The timer is not advertised to the peer.

After the GR restarter and GR helper re-establish a BGP session, they start this timer. If they do not complete route exchange within the time period, the GR restarter does not receive new routes. It updates its routing table and forwarding table with learned BGP routes, and the GR helper removes the stale routes.

This command controls the routing convergence speed. A smaller timer value means faster routing convergence but possibly results in incomplete routing information.

Before configuring this command, you must enable the BGP GR capability.

Examples

# Set the time to wait for the End-of-RIB marker on the local end to 100 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] graceful-restart

[Sysname-bgp-default] graceful-restart timer wait-for-rib 100

Related commands

graceful-restart

graceful-restart timer purge-time

graceful-restart timer restart

BGP commands -- group

Use group to create a peer group.

Use undo group to delete a peer group.

Syntax

group group-name [ external | internal ]

undo group group-name

Default

No peer groups exist.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a name for the peer group, a case-sensitive string of 1 to 47 characters.

external: Creates an EBGP peer group.

internal: Creates an IBGP peer group.

Usage guidelines

In a large-scale network, many peers can use the same route selection policy. You can configure a peer group and add these peers into this group. In this way, peers can share the same policy as the peer group. When the policy of the group is modified, the modification also applies to peers in it.

If you do not specify the internal or external keyword, this command creates an IBGP peer group.

If you perform configurations on a peer group and peers of the peer group, the most recent configuration takes effect.

After you create a peer group, you must use the peer enable command to enable BGP to exchange routing information with the specified peer group.

Examples

# In BGP instance view, create EBGP peer group test with AS number 200, and add EBGP peers 10.1.1.1 and 10.1.2.1 into the group.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] group test external

[Sysname-bgp-default] peer test as-number 200

[Sysname-bgp-default] peer 10.1.1.1 group test

[Sysname-bgp-default] peer 10.1.2.1 group test

Related commands

display bgp group

peer enable

BGP commands -- ignore-first-as

Use ignore-first-as to configure BGP to ignore the first AS number of EBGP route updates.

Use undo ignore-first-as to restore the default.

Syntax

ignore-first-as

undo ignore-first-as

Default

BGP checks the first AS number of a received EBGP route update. If the first AS number is neither that of the BGP peer nor a private AS number, the BGP router disconnects the BGP session to the peer.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Examples

# Configure BGP to ignore the first AS number of EBGP route updates.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] ignore-first-as

BGP commands -- import-route

Use import-route to enable BGP to redistribute routes from an IGP protocol.

Use undo import-route to disable route redistribution from an IGP protocol.

Syntax

import-route protocol [ { process-id | all-processes } [ allow-direct | med med-value | route-policy route-policy-name ] * ]

undo import-route protocol [ process-id | all-processes ]

Default

BGP does not redistribute IGP routes.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

protocol: Redistributes routes from an IGP protocol.

process-id: Specifies a process by its ID in the range of 1 to 65535. The default is 1. For IPv4 routes, it is available only when the protocol is isis, ospf, or rip. For IPv6 routes, it is available only when the protocol is isisv6, ospfv3, or ripng.

all-processes: Redistributes routes from all the processes of the specified IGP protocol. For IPv4 routes, this keyword takes effect only when the protocol is isis, ospf, or rip. For IPv6 routes, this keyword takes effect only when the protocol is isisv6, ospfv3, or ripng.

allow-direct: Redistributes the networks of the local interfaces enabled with the specified routing protocol. By default, the networks of the local interfaces are not redistributed. If you specify both the allow-direct keyword and the route-policy route-policy-name option, make sure the if-match rule defined in the routing policy does not conflict with the allow-direct keyword. For example, if you specify the allow-direct keyword, do not configure the if-match route-type rule for the routing policy. Otherwise, the allow-direct keyword does not take effect.

med med-value: Specifies a MED value for redistributed routes, in the range of 0 to 4294967295. If you do not specify an MED, the metric of a redistributed route is used as its MED.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter redistributed routes or set route attributes for redistributed routes.

Usage guidelines

The import-route command cannot redistribute default IGP routes. To redistribute default IGP routes, use the default-route imported command together with the import-route command.

Only active routes can be redistributed. You can use the display ip routing-table protocol or display ipv6 routing-table protocol command to view route state information.

The ORIGIN attribute of routes redistributed by the import-route command is INCOMPLETE.

Examples

# In BGP IPv4 unicast address family view, redistribute routes from RIP process 1, and set the MED value for redistributed routes to 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] import-route rip 1 med 100

Related commands

display ip routing-table protocol

display ipv6 routing-table protocol

BGP commands -- ip vpn-instance (BGP instance view)

Use ip vpn-instance to create a BGP-VPN instance and enter its view, or enter the view of an existing BGP-VPN instance.

Use undo ip vpn-instance to remove a BGP-VPN instance and all its configurations.

Syntax

ip vpn-instance vpn-instance-name

undo ip vpn-instance vpn-instance-name

Default

No BGP-VPN instances exist.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance-name: Specifies a VPN instance by its name, a case-sensitive string of 1 to 31 characters.

Usage guidelines

After you create a BGP peer in BGP-VPN instance view, the BGP routes learned from the peer are added into the routing table of the specified VPN instance.

This command and all commands in BGP-VPN instance view are typically executed on provider edge (PE) or Multi-VPN-Instance CE (MCE) devices. The commands add routes learned from different sites into different VPN instances.

Before you execute this command, you must perform the following tasks:

· Use the ip vpn-instance command to create the VPN instance in system view.

· Use the route-distinguisher command to configure a route distinguisher (RD) for the VPN instance.

Examples

# Create a BGP-VPN instance and enter its view.

<Sysname> system-view

[Sysname] ip vpn-instance vpn1

[Sysname-vpn-instance-vpn1] route-distinguisher 100:1

[Sysname-vpn-instance-vpn1] quit

[Sysname] bgp 100

[Sysname-bgp-default] ip vpn-instance vpn1

[Sysname-bgp-default-vpn1]

Related commands

ip vpn-instance (system view) (MPLS Command Reference)

route-distinguisher (MPLS Command Reference)

BGP commands -- label-allocation-mode per-prefix

Use label-allocation-mode per-prefix to enable per-prefix label allocation.

Use undo label-allocation-mode per-prefix to restore the default.

Syntax

label-allocation-mode per-prefix

undo label-allocation-mode per-prefix

Default

BGP allocates labels on a per-next-hop basis.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

A change to the label allocation mode enables BGP to re-advertise all routes, which will cause service interruption. Use this command with caution.

Examples

# Enable per-prefix label allocation.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] label-allocation-mode per-prefix

BGP commands -- labeled-route ignore-no-tunnel

Use labeled-route ignore-no-tunnel to disable optimal route selection for labeled routes without tunnel information.

Use undo labeled-route ignore-no-tunnel to restore the default.

Syntax

labeled-route ignore-no-tunnel

undo labeled-route ignore-no-tunnel

Default

Labeled routes without tunnel information can participate in optimal route selection.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Examples

# Disable optimal route selection for labeled routes without tunnel information.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] labeled-route ignore-no-tunnel

BGP commands -- log-peer-change

Use log-peer-change to enable logging for BGP session state changes globally.

Use undo log-peer-change to disable logging for BGP session state changes globally.

Syntax

log-peer-change

undo log-peer-change

Default

Logging for BGP session state changes is enabled globally.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

After you execute both the log-peer-change and peer log-change commands, BGP logs session establishment and disconnection events for the peer or peer group. To display the log information, use the display bgp peer ipv4 unicast log-info command or the display bgp peer ipv6 unicast log-info command. The logs are sent to the information center of the device. The output rules of the logs (whether to output the logs and where to output) are determined by the information center configuration. For more information about information center configuration, see Network Management and Monitoring Configuration Guide.

If you disable logging for BGP session state changes globally or disable logging for a peer or peer group, BGP does not generate logs for session establishments and disconnections.

Examples

# Enable logging for session state changes globally.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] log-peer-change

Related commands

display bgp peer

peer log-change

BGP commands -- log-route-flap

Use log-route-flap to enable logging for BGP route flapping.

Use undo log-route-flap to restore the default.

Syntax

log-route-flap monitor-time monitor-count [ log-count-limit | route-policy route-policy-name ] *

undo log-route-flap

Default

Logging for BGP route flapping is disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP-VPN VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

monitor-time: Specifies the monitoring interval for route flapping, in the range of 1 to 600 minutes.

monitor-count: Specifies the number of route flaps for triggering a log, in the range of 2 to 8.

log-count-limit: Specifies the maximum number of logs allowed to be generated in a minute. The value range for this argument is 1 to 600, and the default value is 200.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

This feature enables BGP to generate logs for BGP route flappings that trigger log generation. The generated logs are sent to the information center. For the logs to be output correctly, you must also configure information center on the device. For more information about the information center, see Network Management and Monitoring Configuration Guide.

This command is applicable only to incoming routes of the specified address family.

Examples

# In BGP IPv4 unicast address family view, enable logging for BGP route flapping. Set the monitoring interval to 10 minutes, the number of route flaps for triggering a log to 5, and the maximum number of allowed logs in a minute to 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] log-route-flap 10 5 100

BGP commands -- network

Use network to inject a network to the BGP routing table and configure BGP to advertise the network.

Use undo network to remove a local network.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP IPv4 multicast address family view:

network ipv4-address [ mask-length | mask ] [ route-policy route-policy-name ]

undo network ipv4-address [ mask-length | mask ]

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

network ipv6-address prefix-length [ route-policy route-policy-name ]

undo network ipv6-address prefix-length

Default

BGP does not advertise local networks.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies an IPv4 network address. If you do not specify the mask or mask-length argument, natural mask is used.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a mask in dotted decimal notation.

ipv6-address: Specifies an IPv6 network address.

prefix-length: Specifies a prefix length in the range of 0 to 128.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter routes or set the route attributes.

Usage guidelines

The network to be injected must be available and active in the local IP routing table.

The ORIGIN attribute of the route injected with the network command is IGP.

When you execute the undo network command, you must specify the same mask or mask length/prefix length that you specified for the network command. Otherwise, the configuration cannot be removed.

Examples

# In BGP IPv4 unicast address family view, inject local network 10.0.0.0/16 to the BGP routing table.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] network 10.0.0.0 255.255.0.0

BGP commands -- network short-cut

Use network short-cut to increase the preference for a received EBGP route. This EBGP route is called a shortcut route.

Use undo network short-cut to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP IPv4 multicast address family view:

network ipv4-address [ mask-length | mask ] short-cut

undo network ipv4-address [ mask-length | mask ] short-cut

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

network ipv6-address prefix-length short-cut

undo network ipv6-address prefix-length short-cut

Default

A received EBGP route has a preference of 255.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies an IPv4 network address. If you do not specify the mask or mask-length argument, natural mask is used.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a mask for the network address, in dotted decimal notation.

ipv6-address: Specifies an IPv6 network address.

prefix-length: Specifies a prefix length in the range of 0 to 128.

Usage guidelines

Different routing protocols might find different routes to the same destination. However, not all of those routes are optimal. For route selection, routing protocols, direct routes, and static routes are assigned different preferences. The route with the highest preference is preferred.

By default, the preference of an EBGP route is lower than a local route. If a device has an EBGP route and a local route to reach the same destination, the device does not select the EBGP route. You can use the network shortcut command to configure the EBGP route to have the same preference as the local route so the EBGP route is more likely to become the optimal route.

You can use the preference command to modify the preferences for external and local BGP routes.

Examples

# In BGP IPv4 unicast address family view, increase the preference of EBGP route 10.0.0.0/16.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] network 10.0.0.0 255.255.0.0 short-cut

Related commands

preference

BGP commands -- non-stop-routing

Use non-stop-routing to enable BGP nonstop routing (NSR).

Use undo non-stop-routing to disable BGP NSR.

Syntax

non-stop-routing

undo non-stop-routing

Default

BGP NSR is disabled.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

BGP NSR ensures continuous routing by synchronizing BGP state and data information from the active BGP process to the standby BGP process. The standby BGP process can seamlessly take over all services when the active process fails.

Examples

# Enable BGP NSR.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] non-stop-routing

Related commands

display bgp non-stop-routing status

BGP commands -- peer advertise-community

Use peer advertise-community to advertise the COMMUNITY attribute to a peer or peer group.

Use undo peer advertise-community to disable the COMMUNITY attribute advertisement to a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP EVPN address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } advertise-community

undo peer { group-name | ipv4-address [ mask-length ] } advertise-community

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } advertise-community

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } advertise-community

In BGP IPv6 multicast address family view/BGP-VPN IPv6 unicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } advertise-community

undo peer { group-name | ipv6-address [ prefix-length ] } advertise-community

Default

No COMMUNITY attribute is advertised to any peers or peer groups.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command advertises the COMMUNITY attribute to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command advertises the COMMUNITY attribute to all dynamic peers in the subnet.

Usage guidelines

The COMMUNITY attribute is a group of specific data carried in update messages. A route can carry one or more COMMUNITY attribute values (each is represented by a 4-byte integer). The receiving router processes the route (for example, determining whether to advertise the route and the scope for advertising the route) based on the COMMUNITY attribute values.

After you execute the peer advertise-community command, routing updates advertised to the peer carry the COMMUNITY attribute.

After you execute the undo peer advertise-community command, BGP, upon receiving a route with the COMMUNITY attribute, removes the COMMUNITY attribute before sending the route to the peer or peer group.

Examples

# In BGP IPv4 unicast address family view, advertise the COMMUNITY attribute to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test advertise-community

Related commands

apply community

if-match community

ip community-list

BGP commands -- peer advertise-ext-community

Use peer advertise-ext-community to advertise the extended community attribute to a peer or peer group.

Use undo peer advertise-ext-community to disable the extended community attribute advertisement to a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } advertise-ext-community

undo peer { group-name | ipv4-address [ mask-length ] } advertise-ext-community

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } advertise-ext-community

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } advertise-ext-community

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } advertise-ext-community

undo peer { group-name | ipv6-address [ prefix-length ] } advertise-ext-community

Default

No extended community attribute is advertised to any peers or peer groups.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command advertises the extended community attribute to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command advertises the extended community attribute to all dynamic peers in the subnet.

Usage guidelines

To meet increasing user demands, BGP defines a new attribute—extended community attribute. The extended community attribute has the following advantages over the COMMUNITY attribute:

· The extended community attribute has an 8-byte length.

· The extended community attribute supports various types. You can select an extended community attribute type as needed to implement route filtering and control. This simplifies configuration and management.

After you execute the peer advertise-ext-community command, route updates sent to the peer or peer group carry the extended community attribute.

After you execute the undo peer advertise-ext-community command, BGP, upon receiving a route with the extended community attribute, removes the extended community attribute before sending the route to the peer or peer group.

Examples

# In BGP IPv4 unicast address family view, advertise the extended community attribute to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test advertise-ext-community

Related commands

apply extcommunity

if-match extcommunity

ip extcommunity-list

BGP commands -- peer allow-as-loop

Use peer allow-as-loop to allow a local AS number to exist in the AS_PATH attribute of routes from a peer or peer group, and to set the number of times the local AS number can appear.

Use undo peer allow-as-loop to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP L2VPN address family view/BGP EVPN address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } allow-as-loop [ number ]

undo peer { group-name | ipv4-address [ mask-length ] } allow-as-loop

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } allow-as-loop [ number ]

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } allow-as-loop

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } allow-as-loop [ number ]

undo peer { group-name | ipv6-address [ prefix-length ] } allow-as-loop

Default

The local AS number is not allowed to exist in the AS_PATH attribute of routes from a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP L2VPN address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP allows a local AS number to exist in the AS_PATH attribute of routes from all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP allows a local AS number to exist in the AS_PATH attribute of routes from all dynamic peers in the subnet.

number: Specifies the number of times for which the local AS number can appear, in the range of 1 to 10. The default number is 1. If the number of times for which the local AS number appears in a route is more than the specified number, BGP considers that a routing loop occurs and discards the route.

Usage guidelines

By default, BGP does not receive routes that contain the local AS number in the AS_PATH attribute to avoid routing loops. However, in some network environments, the AS_PATH attribute of a route from a peer must be allowed to contain the local AS number (for example, a Hub&Spoke network in MPLS L3VPN). Otherwise, the route cannot be advertised correctly.

Examples

# In BGP IPv4 unicast address family view, set the number of times the local AS number can appear in AS_PATH attribute of routes from peer group test to 2.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test allow-as-loop 2

BGP commands -- peer as-number (for a BGP peer group)

Use peer as-number to specify an AS number for a peer group.

Use undo peer as-number to delete the AS number of a peer group.

Syntax

peer group-name as-number as-number

undo peer group-name as-number

Default

No AS number is specified for a peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a name for a peer group, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

as-number: Specifies an AS number for a peer group, in the range of 1 to 4294967295.

Usage guidelines

This command applies only to a peer group with no peers in it.

When you specify an AS number for a peer group and want to add peers to it, make sure the AS number of the peers is the same as the peer group.

If you do not specify an AS number for a peer group, peers added to it can use their own AS numbers.

Examples

# In BGP instance view, set the AS number for peer group test to 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test as-number 100

Related commands

peer group

BGP commands -- peer as-number (for a BGP peer)

Use peer as-number to create a BGP peer and specify its AS number.

Use undo peer to delete a BGP peer.

Syntax

peer { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } as-number as-number

undo peer { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] }

Default

No BGP peers exist.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies the IPv4 address of a peer.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP to establish dynamic peer relationships with all devices in the subnet.

ipv6-address: Specifies the IPv6 address of a peer.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP to establish dynamic peer relationships with all devices in the subnet.

as-number: Specifies an AS number for the peer, in the range of 1 to 4294967295. If the AS numbers of the peer and the local router are the same, the peer is an IBGP peer. If they are different, the peer is an EBGP peer.

Usage guidelines

You can also create a peer and add it to a peer group by using the peer group command.

To modify the AS number of a peer, do not execute the peer as-number command repeatedly. Instead, you must first delete the peer and configure it again.

After you create a peer, you must use the peer enable command to enable BGP to exchange routing information with the specified peer.

For a remote device to establish a peer relationship with the local device, you must specify the IP address of the local device on the remote device.

Examples

# In BGP instance view, create BGP peer 1.1.1.1 and set its AS number to 100.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 100

Related commands

display bgp peer

peer enable

peer group

BGP commands -- peer as-path-acl

Use peer as-path-acl to specify an AS path list to filter routes incoming from or outgoing to a peer or peer group.

Use undo peer as-path-acl to delete the AS path list specified to filter routes incoming from or outgoing to a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } as-path-acl as-path-acl-number { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } as-path-acl { export | import }

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } as-path-acl as-path-acl-number { export | import }

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } as-path-acl { export | import }

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } as-path-acl as-path-acl-number { export | import }

undo peer { group-name | ipv6-address [ prefix-length ] } as-path-acl { export | import }

Default

No AS path list is specified for filtering.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies an AS path list to filter routes incoming from or outgoing to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies an AS path list to filter routes incoming from or outgoing to all dynamic peers in the subnet.

as-path-acl-number: Specifies an AS path list by its number in the range of 1 to 256.

export: Filters outgoing routes.

import: Filters incoming routes.

Usage guidelines

The specified AS path list must have been created with the ip as-path command in system view. If you specify a nonexistent AS path list, all routes can pass the AS path list.

Examples

# In BGP IPv4 unicast address family view, specify AS path list 1 to filter routes outgoing to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test as-path-acl 1 export

Related commands

filter-policy export

filter-policy import

ip as-path

peer filter-policy

peer prefix-list

peer route-policy

BGP commands -- peer bfd

Use peer bfd to enable BFD for the link to a BGP peer or peer group.

Use undo peer bfd to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } bfd [ multi-hop | single-hop ]

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } bfd

Default

BFD is disabled for the link to a BGP peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables BFD for links to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables BFD for links to all dynamic peers in the subnet.

multi-hop: Enables multi-hop BFD.

single-hop: Enables single-hop BFD.

Usage guidelines

When you do not specify the multi-hop keyword or the single-hop keyword:

· If an IBGP peer or peer group is specified, this command enables multi-hop BFD for the IBGP peer or peer group.

· If a directly connected EBGP peer or peer group is specified and the peer ebgp-max-hop command is not configured, this command enables single-hop BFD for the EBGP peer or peer group. If the EBGP peer or peer group is not directly connected or the peer ebgp-max-hop command is configured, this command enables multi-hop BFD for the EBGP peer or peer group.

For more information about multi-hop and single-hop BFD, see High Availability Configuration Guide.

BFD helps speed up BGP routing convergence upon link failures. However, if you have enabled GR, use BFD with caution. BFD might detect a failure before the system performs GR, resulting in GR failure. If you have enabled both BFD and GR for BGP, do not disable BFD during a GR process to avoid GR failure.

To establish a BFD session to a BGP peer, you must configure the same BFD detection mode (multi-hop or single-hop) on the local router and the BGP peer.

Examples

# In BGP instance view, enable BFD for the link to BGP peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test bfd

Related commands

display bfd session (High Availability Command Reference)

display bgp peer

BGP commands -- peer bmp server

Use peer bmp server to specify a peer or peer group to be monitored by the specified BMP servers.

Use undo peer bmp server to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } bmp server server-number-list

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } bmp server

Default

No peer or peer group is specified.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

server-number-list: Specifies a list of up to 8 BMP servers. The value range for the BMP server number is 1 to 8. The BMP servers must have been created.

Usage guidelines

If you execute this command multiple times for a peer or peer group, the most recent configuration takes effect.

Examples

# In BGP instance view, configure BMP server 1 to monitor peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 bmp server 1

Related commands

bmp server

BGP commands -- peer capability-advertise conventional

Use peer capability-advertise conventional to disable the BGP multi-protocol extension, route refresh, and 4-byte AS number features for a peer or peer group.

Use undo peer capability-advertise conventional to enable the BGP multi-protocol extension, route refresh, and 4-byte AS number features for a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise conventional

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise conventional

Default

The BGP multi-protocol extension, route refresh, and 4-byte AS number features are enabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command disables BGP multi-protocol extension and route refresh for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command disables BGP multi-protocol extension and route refresh for all dynamic peers in the subnet.

Usage guidelines

The route refresh feature enables BGP to send and receive Route-refresh messages and implement BGP session soft-reset.

The multi-protocol extension feature enables BGP to advertise and receive routing information for various protocols (for example, IPv6 routing information).

The 4-byte AS number feature enables BGP to use 4-byte AS numbers in the range of 1 to 4294967295.

If both the peer capability-advertise conventional and peer capability-advertise route-refresh commands are executed, the most recent configuration takes effect.

Examples

# In BGP instance view, disable the multi-protocol extension, route refresh, and 4-byte AS number features for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 100

[Sysname-bgp-default] peer 1.1.1.1 capability-advertise conventional

Related commands

display bgp peer

peer capability-advertise route-refresh

BGP commands -- peer capability-advertise orf non-standard

Use peer capability-advertise orf non-standard to enable nonstandard ORF capabilities.

Use undo peer capability-advertise orf non-standard to disable nonstandard ORF capabilities.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise orf non-standard

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise orf non-standard

Default

Nonstandard ORF capabilities are disabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ip-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP to send nonstandard ORF information to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP to send nonstandard ORF information to all dynamic peers in the subnet.

Usage guidelines

To enable BGP peers to exchange nonstandard ORF information, you must configure this command together with the peer capability-advertise orf prefix-list command.

Examples

# Enable nonstandard ORF capabilities for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 capability-advertise orf non-standard

Related commands

peer capability-advertise orf prefix-list

BGP commands -- peer capability-advertise orf prefix-list

Use peer capability-advertise orf prefix-list to enable BGP ORF capabilities.

Use undo peer capability-advertise orf prefix-list to disable BGP ORF capabilities.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } capability-advertise orf prefix-list { both | receive | send }

undo peer { group-name | ipv4-address [ mask-length ] } capability-advertise orf prefix-list { both | receive | send }

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise orf prefix-list { both | receive | send }

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise orf prefix-list { both | receive | send }

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } capability-advertise orf prefix-list { both | receive | send }

undo peer { group-name | ipv6-address [ prefix-length ] } capability-advertise orf prefix-list { both | receive | send }

Default

BGP ORF capabilities are disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

both: Enables BGP to send and receive route fresh messages that carry the ORF information.

receive: Enables BGP to receive route fresh messages that carry the ORF information.

send: Enables BGP to send route fresh messages that carry the ORF information.

Usage guidelines

After you configure this command, the BGP peers negotiate the ORF capabilities through Open messages. After completing the negotiation process, the BGP peers can exchange ORF information through route refresh messages. To enable the peers to exchange nonstandard ORF information, you must also configure the peer capability-advertise orf non-standard command.

Examples

# Enables BGP ORF capabilities for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4

[Sysname-bgp-default-ipv4] peer 1.1.1.1 capability-advertise orf prefix-list both

Related commands

peer capability-advertise orf non-standard

BGP commands -- peer capability-advertise route-refresh

Use peer capability-advertise route-refresh to enable BGP route refresh for a peer or peer group.

Use undo peer capability-advertise route-refresh to disable BGP route refresh for a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise route-refresh

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise route-refresh

Default

BGP route refresh is enabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP route refresh for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables BGP route refresh for all dynamic peers in the subnet.

Usage guidelines

The route refresh feature enables BGP to send and receive Route-refresh messages.

BGP uses the route refresh feature to implement BGP session soft-reset. After a policy is modified, the router advertises a Route-refresh message to the peers. The peers resend their routing information to the router. After receiving the routing information, the router filters the routing information by using the new policy. This method allows you to refresh the BGP routing table and apply the new route selection policy without tearing down BGP sessions.

BGP route refresh requires that both the local router and the peer support route refresh.

If both the peer capability-advertise route-refresh and peer capability-advertise conventional commands are executed, the most recent configuration takes effect.

Examples

# In BGP instance view, enable BGP route refresh for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 100

[Sysname-bgp-default] peer 1.1.1.1 capability-advertise route-refresh

Related commands

display bgp peer

peer capability-advertise conventional

peer keep-all-routes

refresh bgp

BGP commands -- peer capability-advertise suppress-4-byte-as

Use peer capability-advertise suppress-4-byte-as to enable 4-byte AS number suppression.

Use undo peer capability-advertise suppress-4-byte-as to disable 4-byte AS number suppression.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise suppress-4-byte-as

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } capability-advertise suppress-4-byte-as

Default

The 4-byte AS number suppression feature is disabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables 4-byte AS number suppression for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables 4-byte AS number suppression for all dynamic peers in the subnet.

Usage guidelines

BGP supports 4-byte AS numbers. The 4-byte AS number occupies four bytes, in the range of 1 to 4294967295. By default, a device sends an Open message to the peer device for session establishment. The Open message indicates that the device supports 4-byte AS numbers. If the peer device supports 2-byte AS numbers instead of 4-byte AS numbers, the session cannot be established. To resolve this issue, enable the 4-byte AS number suppression feature. The device then sends an Open message to inform the peer that it does not support 4-byte AS numbers, so the BGP session can be established.

If the peer device supports 4-byte AS numbers, do not enable the 4-byte AS number suppression feature. If this feature is enabled, the BGP session cannot be established.

Examples

# In BGP instance view, enable 4-byte AS number suppression for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 100

[Sysname-bgp-default] peer 1.1.1.1 capability-advertise suppress-4-byte-as

Related commands

display bgp peer

BGP commands -- peer connect-interface

Use peer connect-interface to specify a source interface (IPv4 address/IPv6 address) for establishing TCP connections to a peer or peer group.

Use undo peer connect-interface to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } connect-interface interface-type interface-number

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } connect-interface

Default

BGP uses the primary IPv4 or IPv6 address of the output interface in the optimal route destined for the BGP peer or peer group as the source address.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies a source interface for establishing TCP connections to all dynamic peers in the network.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies a source interface for establishing TCP connections to all dynamic peers in the subnet.

interface-type interface-number: Specifies an interface by its type and number.

Usage guidelines

The peer connect-interface command and the peer source-address command can both change the source address for establishing TCP connections. If you execute both commands, the most recent configuration takes effect.

The peer source-address and peer connect-interface commands are applicable to the following scenarios:

· The peer's IPv4/IPv6 address does not belong to the interface directly connected to the local router. To ensure successful TCP connection establishment, use one of the following methods:

?span style='font:7.0pt "Times New Roman"'> Specify the interface to which the IPv4/IPv6 address belongs as the source interface on the peer.

?span style='font:7.0pt "Times New Roman"'> Specify the IPv4/IPv6 address of the interface directly connected to the local router as the source address on the peer.

· A BGP peer at an IPv6 link-local address must be directly connected to the local router. On the local router, you must use the peer connect-interface command to specify the interface directly connected to the BGP peer as the source interface of TCP connections.

· On a BGP router that has multiple links to a peer, the source interface for TCP connection changes because the primary source interface fails. To avoid this problem, specify a loopback interface as the source interface or specify the IP address of a loopback interface as the source address.

· You want to establish multiple BGP sessions to a router. In this case, BGP might fail to determine the source address for each TCP connection based on the optimal route to the peer. To prevent this problem, use one of the following methods:

?span style='font:7.0pt "Times New Roman"'> If the BGP sessions use IP addresses of different interfaces, specify a source interface or source address for each session.

?span style='font:7.0pt "Times New Roman"'> If the BGP sessions use different IP addresses of the same interface, specify a source address for each session.

The source interfaces on the local router and the peer must be reachable to each other.

After you configure this command, BGP immediately tears down the session to a directly connected IBGP peer when the source interface (non-loopback interface) fails and the link state goes down.

To specify an indirectly connected interface on an EBGP peer as the source interface, use the peer ebgp-max-hop command. The command allows the establishment of an EBGP session to the indirectly connected peer.

If an interface has multiple IPv4 addresses, BGP uses the primary IPv4 address to establish TCP connections. If an interface has multiple IPv6 addresses, BGP selects a source IPv6 address. To use an IPv6 address as the source address, specify that IPv6 address by using the peer source-address command.

You cannot specify a virtual template (VT) interface as the source interface for establishing TCP connections because a VT interface cannot process services.

Examples

# In BGP instance view, specify loopback 0 as the source interface for TCP connections to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test connect-interface loopback 0

Related commands

peer ebgp-max-hop

peer source-address

BGP commands -- peer default-route-advertise

Use peer default-route-advertise to advertise a default route to a peer or peer group.

Use undo peer default-route-advertise to disable default route advertisement to a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } default-route-advertise [ route-policy route-policy-name ]

undo peer { group-name | ipv4-address [ mask-length ] } default-route-advertise

In BGP VPNv4 address family view:

peer { group-name | ipv4-address [ mask-length ] } default-route-advertise vpn-instance vpn-instance-name

undo peer { group-name | ipv4-address } default-route-advertise vpn-instance vpn-instance-name

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } default-route-advertise [ route-policy route-policy-name ]

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } default-route-advertise

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } default-route-advertise [ route-policy route-policy-name ]

undo peer { group-name | ipv6-address [ prefix-length ] } default-route-advertise [ route-policy route-policy-name ]

In BGP IPv4 RT filter address family view:

peer { group-name | ipv4-address [ mask-length ] } default-route-advertise [ route-policy route-policy-name ]

undo peer { group-name | ipv4-address [ mask-length ] } default-route-advertise [ route-policy route-policy-name ]

Default

No default route is advertised to any peers or peer groups.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

BGP IPv4 RT filter address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command advertises a default route to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command advertises a default route to all dynamic peers in the subnet.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to modify the route attribute.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters.

Usage guidelines

This command enables the router to send a default route with the next hop being itself to the peer or peer group regardless of whether the default route exists in the routing table.

Examples

# In BGP IPv4 unicast address family view, advertise a default route to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test default-route-advertise

BGP commands -- peer description

Use peer description to configure a description for a peer or peer group.

Use undo peer description to remove the description for a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } description text

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } description

Default

No description information is configured for a peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command configures a description for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command configures a description for all dynamic peers in the subnet.

text: Specifies a description for a peer or peer group, a case-sensitive string of 1 to 79 characters.

Examples

# In BGP instance view, set the description for peer group test to ISP1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test description ISP1

BGP commands -- peer dscp

Use peer dscp to set a DSCP value for outgoing BGP packets.

Use undo peer dscp to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } dscp dscp-value

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } dscp

Default

The DSCP value for outgoing BGP packets is 48.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies a DSCP value for outgoing BGP packets to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies a DSCP value for outgoing BGP packets to all dynamic peers in the subnet.

dscp-value: Specifies a DSCP value in the range of 0 to 63.

Usage guidelines

The DSCP value of an IP packet specifies the priority level of the packet and affects the transmission priority of the packet. A larger DSCP value represents a higher priority.

Examples

# In BGP instance view, set the DSCP value to 10 for outgoing BGP packets to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test dscp 10

BGP commands -- peer ebgp-max-hop

Use peer ebgp-max-hop to enable BGP to establish an EBGP session to an indirectly connected peer or peer group and specify the maximum hop count.

Use undo peer ebgp-max-hop to disable BGP to establish an EBGP session to an indirectly connected peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ebgp-max-hop [ hop-count ]

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ebgp-max-hop

Default

BGP does not establish an EBGP session to an indirectly connected peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP establishes EBGP sessions to all indirectly connected dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP establishes EBGP sessions to all indirectly connected dynamic peers in the subnet.

hop-count: Specifies the maximum number of hop counts, in the range of 1 to 255. The default is 64.

Usage guidelines

To become EBGP peers, two routers must be directly connected and use directly connected interfaces to establish an EBGP session. If they are not directly connected, use the peer ebgp-max-hop command to establish an EBGP session over multiple hops between two peers.

This command takes effect only on routes received after you execute this command. To apply this command to existing routes, use the refresh bgp command to soft-reset BGP sessions.

When the BGP GTSM feature is enabled, two peers can establish an EBGP session after passing GTSM check, regardless of whether the maximum number of hops is reached.

Examples

# In BGP instance view, enable BGP to establish EBGP sessions to indirectly connected EBGP peer group test, and set the maximum hop count to 64 (default).

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test ebgp-max-hop

Related commands

peer ttl-security

BGP commands -- peer enable

Use peer enable to enable BGP to exchange routing information for an address family with a peer or peer group.

Use undo peer enable to disable BGP from exchanging routing information for an address family with a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP-VPN VPNv4 address family view/BGP VPNv6 address family view/BGP L2VPN address family view/BGP EVPN address family view/BGP IPv4 multicast address family view/BGP IPv4 MDT address family view/BGP IPv4 RT filter address family view:

peer { group-name | ipv4-address [ mask-length ] } enable

undo peer { group-name | ipv4-address [ mask-length ] } enable

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } enable

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } enable

In BGP LS address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } enable

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } enable

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } enable

undo peer { group-name | ipv6-address [ prefix-length ] } enable

Default

BGP cannot exchange routing information with a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP-VPN VPNv4 address family view

BGP IPv6 unicast address family view

BGP LS address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP L2VPN address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

BGP IPv4 MDT address family view

BGP IPv4 RT filter address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP exchanges routing information for an address family with all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP exchanges routing information for an address family with all dynamic peers in the subnet.

Usage guidelines

Executing the peer enable command in different views enables BGP to exchange routing information for the corresponding address families with the specified peer.

· In BGP IPv4 unicast address family view, the command enables the capability to exchange IPv4 unicast routing information. It also adds the learned routes to the BGP routing table of the public network.

· In BGP-VPN IPv4 unicast address family view, the command enables the capability to exchange IPv4 unicast routing information. It also adds the learned routes to the BGP routing table of the specified VPN instance.

· In BGP VPNv4 address family view, the command enables the capability to exchange VPNv4 routing information. In an MPLS L3VPN network, execute the command on PE devices in BGP VPNv4 address family view.

· In BGP-VPN VPNv4 address family view, the command enables the capability to exchange VPNv4 routing information. In a nested VPN network, execute this command on ISP PE devices in BGP-VPN VPNv4 address family view to do the following:

?span style='font:7.0pt "Times New Roman"'> Enable the PE devices to exchange BGP VPNv4 routing information with ISP CEs.

?span style='font:7.0pt "Times New Roman"'> Add the VPNv4 routes learned by the PE devices to the routing table of the specified VPN instance.

· In BGP IPv6 unicast address family view, the command enables the capability to exchange IPv6 unicast routing information. It also adds the learned routes to the IPv6 BGP routing table of the public network.

· In BGP-VPN IPv6 unicast address family view, the command enables the capability to exchange IPv6 unicast routing information. It also adds the learned routes to the IPv6 BGP routing table of the specified VPN instance.

· In BGP VPNv6 address family view, the command enables the capability to exchange VPNv6 routing information. In an IPv6 MPLS L3VPN network, execute the command on PE devices in BGP VPNv6 address family view.

· In BGP L2VPN address family view, the command enables the capability to exchange L2VPN information. In an MPLS L2VPN or a VPLS network, execute the command on PE devices in BGP L2VPN address family view.

· In BGP IPv4 multicast address family view, the command enables the capability to exchange IPv4 unicast routes used for RPF check. For information about RPF check, see IP Multicast Configuration Guide.

· In BGP IPv6 multicast address family view, the command enables the capability to exchange IPv6 unicast routes used for RPF check. For information about RPF check, see IP Multicast Configuration Guide.

· In BGP IPv4 MDT address family view, the command enables the capability to exchange MDT information. For multicast VPN, you must configure this command in BGP IPv4 MDT address family view on PEs.

· In BGP IPv4 RT filter address family view, the command enables the capability to exchange IPv4 RT filter routing information. In an MPLS L3VPN network, execute the command on PE devices in BGP IPv4 RT filter address family view.

The undo peer enable command disables BGP to exchange routing information for the corresponding address family with the peer.

Examples

# In BGP IPv4 unicast address family view, enable BGP to exchange IPv4 unicast routing information with peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer 1.1.1.1 enable

Related commands

display bgp peer

BGP commands -- peer fake-as

Use peer fake-as to advertise a fake AS number to a peer or peer group.

Use undo peer fake-as to remove the fake AS number advertised to a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } fake-as as-number

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } fake-as

Default

No fake local AS number is advertised to a peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command advertises a fake AS number to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command advertises a fake AS number to all dynamic peers in the subnet.

as-number: Specifies a fake AS number in the range of 1 to 4294967295.

Usage guidelines

After you move a BGP router from an AS to another AS (from AS 2 to AS 3 for example), you have to modify the AS number of the router on all its EBGP peers. To avoid such modifications, you can configure the router to advertise a fake AS number 2 to its EBGP peers so that the EBGP peers still think that Router A is in AS 2.

The peer fake-as command is applicable only to EBGP peers or peer groups.

If you execute the peer fake-as command on the local router, specify the local router's AS number on the peer as the fake local AS number specified in the command.

Examples

# In BGP instance view, advertise a fake AS number of 200 to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test fake-as 200

BGP commands -- peer filter-policy

Use peer filter-policy to filter routes advertised to or received from a peer or peer group by using an ACL.

Use undo peer filter-policy to remove the ACL specified to filter routes advertised to or received from a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } filter-policy acl-number { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } filter-policy { export | import }

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } filter-policy acl6-number { export | import }

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } filter-policy { export | import }

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } filter-policy acl6-number { export | import }

undo peer { group-name | ipv6-address [ prefix-length ] } filter-policy { export | import }

In BGP VPNv6 address family view:

peer { group-name | ipv4-address [ mask-length ] } filter-policy acl6-number { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } filter-policy { export | import }

Default

No ACL-based filtering is configured.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command filters routes advertised to or received from all dynamic peers in the subnet by using an ACL.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command filters routes advertised to or received from all dynamic peers in the subnet by using an ACL.

acl-number: Specifies an ACL by its number in the range of 2000 to 3999.

acl6-number: Specifies an IPv6 ACL by its number in the range of 2000 to 3999.

export: Filters routes advertised to the peer/peer group.

import: Filters routes received from the peer/peer group.

Usage guidelines

The specified ACL used by the peer filter-policy command must have been created with the acl command in system view. Otherwise, all routes can pass the ACL.

If you use a basic ACL (with a number from 2000 to 2999) configured with the rule [ rule-id ] { deny | permit } source source-address source-wildcard command, the command matches routes whose destination network addresses match the source-address source-wildcard argument without matching the masks of the destination addresses.

To use an advanced ACL (with a number from 3000 to 3999) in the command, configure the ACL using one of the following steps:

· To deny/permit a route with the specified destination, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard command.

· To deny/permit a route with the specified destination and mask, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard destination dest-addr dest-wildcard command.

The source keyword specifies the destination address of a route and the destination keyword specifies the subnet mask of the destination address. For the mask configuration to take effect, specify a contiguous subnet mask.

Examples

# In BGP IPv4 unicast address family view, apply ACL 2000 to filter routes advertised to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test filter-policy 2000 export

Related commands

acl (ACL and QoS Command Reference)

filter-policy export

filter-policy import

peer as-path-acl

peer prefix-list

peer route-policy

BGP commands -- peer group

Use peer group to add a peer to a peer group.

Use undo peer group to delete a peer from a peer group.

Syntax

peer { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } group group-name [ as-number as-number ]

undo peer { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } group group-name

Default

No peers exist in a peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies a peer by its IPv4 address.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command adds all dynamic peers in the subnet to a peer group.

ipv6-address: Specifies a peer by its IPv6 address.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command adds all dynamic peers in the subnet to a peer group.

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

as-number as-number: Specifies an AS for a peer by its number in the range of 1 to 4294967295.

Usage guidelines

You can add a peer to a peer group in the following ways:

· Use the peer as-number command to create a peer and specify its AS number, and then use the peer group command to add the peer to the peer group.

?span style='font:7.0pt "Times New Roman"'> You can specify the as-number keyword for the peer group command. The AS number must be the same as the AS number specified in the peer as-number command.

?span style='font:7.0pt "Times New Roman"'> If you have specified the AS number of the peer group with the peer as-number command, the peer to be added must have the same AS number as the peer group.

?span style='font:7.0pt "Times New Roman"'> To add a peer to an IBGP peer group, the peer must be an IBGP peer.

· Use the peer group command to create a peer and add it to the peer group.

?span style='font:7.0pt "Times New Roman"'> If you have specified the AS number of the peer group with the peer as-number command, you do not need to specify the as-number keyword when you execute the peer group command. This is because the AS number of the peer is the same as the peer group. To specify the as-number keyword for the peer group command, make sure the AS number is the same as the peer group.

?span style='font:7.0pt "Times New Roman"'> If no AS number is specified for an EBGP peer group, specify the as-number keyword when you execute the peer group command.

?span style='font:7.0pt "Times New Roman"'> If no AS number is specified for an IBGP peer group, you do not need to specify the as-number keyword when you execute the peer group command. This is because the AS number of the IBGP peer group is the local AS number. To specify the as-number keyword for the peer group command, make sure the AS number is the same as the local AS number.

If you have specified the AS number of a peer group with the peer as-number command, only the peers with the same AS number can be added to the peer group. All peers in the group share the same AS number. If you have not specified the AS number for a peer group, peers added to it can use their own AS numbers.

After you add a peer to a peer group, you must use the peer enable command to enable BGP to exchange routing information with the peer group.

Examples

# In BGP instance view, add peer 10.1.1.1 to EBGP peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] group test external

[Sysname-bgp-default] peer 10.1.1.1 group test as-number 2004

Related commands

group

peer as-number

peer enable

BGP commands -- peer ignore

Use peer ignore to disable BGP session establishment with a peer or peer group.

Use undo peer ignore to enable BGP session establishment with a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ignore

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ignore

Default

BGP can establish a session to a peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP tears down sessions to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP tears down sessions to all dynamic peers in the subnet.

Usage guidelines

This command enables you to temporarily tear down the BGP session to a peer or peer group. Then you can perform network upgrade and maintenance without needing to delete and reconfigure the peer or peer group. To recover the session, execute the undo peer ignore command.

If a session has been established to a peer, executing the peer ignore command for the peer tears down the session and clears all related routing information.

If sessions have been established to a peer group, executing the peer ignore command for the peer group disables the sessions to all peers in the group and clears all related routing information.

Examples

# In BGP instance view, disable session establishment with peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 ignore

BGP commands -- peer ignore-originatorid

Use peer ignore-originatorid to configure BGP to ignore the ORIGINATOR_ID attribute in BGP route updates.

Use undo peer ignore-originatorid to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ignore-originatorid

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ignore-originatorid

Default

BGP does not ignore the ORIGINATOR_ID attribute in BGP route updates.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP ignores the ORIGINATOR_ID attribute in BGP route updates from all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP ignores the ORIGINATOR_ID attribute in BGP route updates from all dynamic peers in the subnet.

Usage guidelines

Before using this command, make sure it does not cause any routing loops to the network.

Before forwarding a route received from a client, the route reflector adds an ORIGINATOR_ID attribute (the router ID of the client) to the route. By default, BGP drops incoming route updates whose ORIGINATOR_ID attribute is the same as the local router ID.

Some networks such as firewall networks require BGP to accept such route updates. To meet the requirement, you must configure BGP to ignore the ORIGINATOR_ID attribute.

After you execute this command, BGP also ignores the CLUSTER_LIST attribute.

Examples

# In BGP instance view, configure BGP to ignore the ORIGINATOR_ID attribute in BGP route updates from peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 ignore-originatorid

BGP commands -- peer ipsec-profile

Use peer ipsec-profile to apply an IPsec profile to an IPv6 BGP peer or peer group.

Use undo peer ipsec-profile to remove the profile from an IPv6 BGP peer or peer group.

Syntax

peer { group-name | ipv6-address [ prefix-length ] } ipsec-profile profile-name

undo peer { group-name | ipv6-address [ prefix-length ] } ipsec-profile

Default

No IPsec profile is configured for any IPv6 BGP peers or peer groups.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command applies an IPsec profile to all dynamic peers in the subnet.

profile-name: Specifies an IPsec profile by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

IPsec can protect IPv6 BGP packets from data eavesdropping, tampering, and attacks caused by forged IPv6 BGP packets.

When two IPv6 BGP neighbor devices, for example Device A and Device B, are configured with IPsec, Device A encapsulates an IPv6 BGP packet with IPsec before sending it to Device B. If Device B successfully receives and decapsulates the packet, it establishes an IPv6 BGP peer relationship with Device A or learns IPv6 BGP routes to Device A. If Device B receives but fails to decapsulate the packet, or receives a packet not protected by IPsec, it discards the packet.

Configure IPsec to protect IPv6 BGP packets through the following steps:

1. Configure an IPsec transform set.

2. Configure a manual IPsec profile.

3. Execute this command to apply the IPsec profile to an IPv6 BGP peer or peer group.

For more information about IPsec transform sets and IPsec profiles, see Security Configuration Guide.

This command supports only IPsec profiles in manual mode.

If you configure IPsec on a device, you must configure IPsec on its IPv6 BGP peer. Otherwise, IPv6 BGP packets cannot be received.

Examples

# In BGP instance view, apply IPsec profile profile001 to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test ipsec-profile profile001

Related commands

display bgp group

display bgp peer

BGP commands -- peer keep-all-routes

Use peer keep-all-routes to save all route updates from a peer or peer group, regardless of whether the routes have passed the configured routing policy.

Use undo peer keep-all-routes to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } keep-all-routes

undo peer { group-name | ipv4-address [ mask-length ] } keep-all-routes

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } keep-all-routes

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } keep-all-routes

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } keep-all-routes

undo peer { group-name | ipv6-address [ prefix-length ] } keep-all-routes

Default

Route updates from a peer or peer group are not saved.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command saves all route updates from all dynamic peers in the subnet, regardless of whether the routes have passed the configured routing policy.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command saves all route updates from all dynamic peers in the subnet, regardless of whether the routes have passed the configured routing policy.

Usage guidelines

To implement BGP session soft-reset when the local router and a peer or peer group do not support the route refresh feature, use the peer keep-all-routes command. The command saves all route updates received from the peer or peer group. After modifying the route selection policy, filter all saved routes with the new policy to refresh the routing table. This method avoids tearing down BGP sessions.

Examples

# In BGP IPv4 unicast address family view, save all route updates from peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer 1.1.1.1 keep-all-routes

Related commands

peer capability-advertise route-refresh

refresh bgp

BGP commands -- peer keychain

Use peer keychain to enable keychain authentication for a BGP peer or peer group.

Use undo peer keychain to remove keychain authentication for a BGP peer or peer group.

Syntax

peer { group-name | ip-address [ mask-length ] | ipv6-address [ prefix-length ] } keychain keychain-name

undo peer { group-name | ip-address [ mask-length ] | ipv6-address [ prefix-length ] } keychain

Default

Keychain authentication is disabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ip-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ip-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables keychain authentication for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables keychain authentication for all dynamic peers in the subnet.

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters. The keychain must have been created.

Usage guidelines

Keychain authentication enhances the security of TCP connection establishment between BGP peers. It allows BGP peers to establish TCP connections only when the following conditions are met:

· Keychain authentication is enabled on both BGP peers.

· The keys used by the BGP peers have the same authentication algorithm and key string.

BGP supports the HMAC-SHA-256 and MD5 authentication algorithms. To specify an authentication algorithm for a key, use the authentication-algorithm command.

The ID of keys used for authentication can only be in the range of 0 to 63. To create a key, use the key command.

The peer keychain and peer password commands are mutually exclusive.

Examples

# In BGP instance view, configure peer 10.1.1.1 to use keychain abc for authentication.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 10.1.1.1 as-number 100

[Sysname-bgp-default] peer 10.1.1.1 keychain abc

Related commands

authentication-algorithm (Security Command Reference)

key (Security Command Reference)

BGP commands -- peer label-route-capability

Use peer label-route-capability to enable BGP to exchange labeled routes with a peer or peer group.

Use undo peer label-route-capability to disable BGP from exchanging labeled routes with a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] } label-route-capability

undo peer { group-name | ipv4-address [ mask-length ] } label-route-capability

Default

BGP cannot exchange labeled routes with a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP exchanges labeled routes with all dynamic peers in the subnet.

Usage guidelines

On an inter-AS option C network, use this command in BGP IPv4 unicast or BGP-VPN IPv4 unicast address family view to exchange labeled IPv4 unicast routes for inter-AS public LSP establishment.

On a 6PE network, use this command in BGP IPv6 unicast address family view to exchange labeled IPv6 unicast routes for forwarding IPv6 packets over an IPv4 network.

Examples

# In BGP IPv4 unicast address family view, enable BGP to exchange labeled IPv4 routes peer 2.2.2.2.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4

[Sysname-bgp-default-ipv4] peer 2.2.2.2 label-route-capability

BGP commands -- peer log-change

Use peer log-change to enable logging for BGP session state changes for a peer or peer group.

Use undo peer log-change to disable logging for BGP session state changes for a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } log-change

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } log-change

Default

Logging for BGP session state changes is enabled for all peers or peer groups.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must already exist.

ipv4-address: Specifies the IPv4 address of a peer. The peer must already exist.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables the logging of BGP session state changes for all dynamic peers in the subnet.

ipv6-address: Specifies the IPv6 address of a peer. The peer must already exist.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables the logging of BGP session state changes for all dynamic peers in the subnet.

Usage guidelines

After you execute both the log-peer-change and peer log-change commands, BGP logs session establishment and disconnection events for the peer or peer group. To view the log information, use the display bgp peer ipv4 unicast log-info command or the display bgp peer ipv6 unicast log-info command. The logs are sent to the information center of the device. The output rules of the logs (whether to output the logs and where to output) are determined by the information center configuration. For more information about information center configuration, see Network Management and Monitoring Configuration Guide.

If you disable logging for BGP session state changes globally or disable logging for a peer or peer group, BGP does not generate logs for session establishments and disconnections.

Examples

# In BGP instance view, enable logging for BGP session state changes for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 200

[Sysname-bgp-default] peer 1.1.1.1 log-change

Related commands

display bgp peer

log-peer-change

BGP commands -- peer low-memory-exempt

Use peer low-memory-exempt to configure BGP to protect EBGP peers or peer groups when the memory usage reaches level 2 threshold.

Use undo peer low-memory-exempt to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } low-memory-exempt

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } low-memory-exempt

Default

When the memory usage reaches level 2 threshold, BGP tears down an EBGP session to release memory resources periodically.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet in this command, BGP protects all dynamic peers in the subnet when the memory usage reaches level 2 threshold.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet in this command, BGP protects all dynamic peers in the subnet when the memory usage reaches level 2 threshold.

Usage guidelines

When level 2 memory usage threshold is reached, BGP tears down an EBGP session to release memory resources periodically until the memory usage is exempt from level 2 threshold. You can use this command to avoid tearing down the BGP session to an EBGP peer when memory usage reaches level 2 threshold. For more information about thresholds, see Fundamentals Configuration Guide.

Examples

# In BGP instance view, configure BGP to protect EBGP peer 1.1.1.1 when the memory usage reaches level 2 threshold.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 200

[Sysname-bgp-default] peer 1.1.1.1 low-memory-exempt

BGP commands -- peer next-hop-local

Use peer next-hop-local to set the local router as the next hop for routes sent to a peer or peer group.

Use undo peer next-hop-local to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP EVPN address family view/ BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } next-hop-local

undo peer { group-name | ipv4-address [ mask-length ] } next-hop-local

In BGP IPv6 unicast address family view/BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } next-hop-local

undo peer { group-name | ipv6-address [ prefix-length ] } next-hop-local

Default

BGP sets the local router as the next hop for all routes sent to an EBGP peer or peer group.

BGP sets the local router as the next hop for EBGP routes sent to an IBGP peer or peer group for BGP VPNv4 address family. It does not set the local router as the next hop for EBGP routes sent to an IBGP peer or peer group for other address families.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command sets the local router as the next hop for routes sent to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command sets the local router as the next hop for routes sent to all dynamic peers in the subnet.

Usage guidelines

By default, BGP does not set the local router as the next hop for EBGP routes sent to an IBGP peer or peer group. To ensure that an IBGP peer can find the next hop, you can use this command to specify the router as the next hop for routes sent to the IBGP peer.

Examples

# In BGP IPv4 unicast address family view, specify the router as the next hop for routes sent to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test next-hop-local

BGP commands -- peer nexthop-recursive-policy disable

Use peer nexthop-recursive-policy disable to disable route recursion policy control for routes received from the specified peer or peer group.

Use undo peer nexthop-recursive-policy disable to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } nexthop-recursive-policy disable

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } nexthop-recursive-policy disable

Default

The route recursion policy applies to routes received from the specified peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies all dynamic peers in the subnet.

Usage guidelines

If you configure routing policy-based recursive lookup for BGP routes, this route recursion policy applies to BGP routes learned from all peers. This command allows you to disable route recursion policy control for routes learned from certain peers, for example, direct EBGP peers.

Examples

# In BGP instance view, disable route recursion policy control for routes received from peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 as-number 200

[Sysname-bgp-default] peer 1.1.1.1 nexthop-recursive-policy disable

Related commands

protocol nexthop recursive-lookup

BGP commands -- peer password

Use peer password to enable MD5 authentication for a BGP peer or peer group.

Use undo peer password to remove MD5 authentication for a BGP peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } password { cipher | simple } password

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } password

Default

MD5 authentication is disabled.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command enables MD5 authentication for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command enables MD5 authentication for all dynamic peers in the subnet.

cipher: Specifies a password in encrypted form.

simple: Specifies a password in plaintext form. For security purposes, the password specified in plaintext form will be stored in encrypted form.

password: Specifies the password. Its encrypted form is a case-sensitive string of 33 to 137 characters. Its plaintext form is a case-sensitive string of 1 to 80 characters.

Usage guidelines

You can enable MD5 authentication to enhance security using the following methods:

· Perform MD5 authentication when establishing TCP connections. Only the two parties that have the same password configured can establish TCP connections.

· Perform MD5 calculation on TCP segments to avoid modification to the encapsulated BGP packets.

The peer password and peer keychain commands are mutually exclusive.

Examples

# In BGP instance view, perform MD5 authentication on the TCP connection between local router 10.1.100.1 and peer router 10.1.100.2. Set the authentication password to aabbcc in plaintext form.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 10.1.100.2 password simple aabbcc

BGP commands -- peer preferred-value

Use peer preferred-value to set a preferred value for routes received from a peer or peer group.

Use undo peer preferred-value to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } preferred-value value

undo peer { group-name | ipv4-address [ mask-length ] } preferred-value

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } preferred-value value

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } preferred-value

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } preferred-value value

undo peer { group-name | ipv6-address [ prefix-length ] } preferred-value

Default

The preferred value is 0 for routes received from a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies a preferred value for routes received from all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies a preferred value for routes received from all dynamic peers in the subnet.

value: Specifies a preferred value in the range of 0 to 65535.

Usage guidelines

If multiple routes that have the same destination are learned from different peers, you can specify different preferred values for the routes as needed to control BGP path selection. The one with the greatest preferred value is selected as the optimal route to the destination.

The preferred value is used for route selection on the local router and is not advertised to the peer. It has only local significance.

You can also use the apply preferred-value command in a routing policy to configure the preferred value for BGP routes. If both the peer preferred-value and apply preferred-value commands are configured, the apply preferred-value command applies. If the preferred value is not set in the routing policy or no routing policy is configured, the peer preferred-value command applies.

Examples

# In BGP IPv4 unicast address family view, set the preferred value to 50 for routes from peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer 1.1.1.1 preferred-value 50

Related commands

apply preferred-value

route-policy

BGP commands -- peer prefix-list

Use peer prefix-list to specify a prefix list to filter routes received from or advertised to a peer or peer group.

Use undo peer prefix-list to remove the prefix list specified to filter routes received from or advertised to a peer or peer group.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } prefix-list prefix-list-name { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } prefix-list { export | import }

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } prefix-list ipv6-prefix-name { export | import }

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } prefix-list { export | import }

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } prefix-list ipv6-prefix-name { export | import }

undo peer { group-name | ipv6-address [ prefix-length ] } prefix-list { export | import }

In BGP VPNv6 address family view:

peer { group-name | ipv4-address [ mask-length ] } prefix-list ipv6-prefix-name { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } prefix-list { export | import }

Default

No prefix list based filtering is configured.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command uses a prefix list to filter routes received from or advertised to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command uses a prefix list to filter routes received from or advertised to all dynamic peers in the subnet.

prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters.

ipv6-prefix-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters.

export: Applies the filter to routes advertised to the specified peer/peer group.

import: Applies the filter to routes received from the specified peer/peer group.

Usage guidelines

The specified prefix list must have been created with the ip prefix-list or ipv6 prefix-list command in system view. If you specify a nonexistent IPv4/IPv6 prefix list, all routes can pass the prefix list.

Examples

# In BGP IPv4 unicast address family view, use IPv4 prefix list list1 to filter routes advertised to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test prefix-list list1 export

Related commands

filter-policy export

filter-policy import

ip prefix-list

ipv6 prefix-list

peer as-path-acl

peer filter-policy

peer route-policy

BGP commands -- peer public-as-only

Use peer public-as-only to remove private AS numbers in BGP updates sent to an EBGP peer or peer group.

Use undo peer public-as-only to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } public-as-only

undo peer { group-name | ipv4-address [ mask-length ] } public-as-only

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } public-as-only

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } public-as-only

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } public-as-only

undo peer { group-name | ipv6-address [ prefix-length ] } public-as-only

Default

BGP updates sent to an EBGP peer or peer group can carry both public and private AS numbers.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command removes private AS numbers in BGP updates sent to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command removes private AS numbers in BGP updates sent to all dynamic peers in the subnet.

Usage guidelines

Private AS numbers are typically used in test networks, and need not be transmitted in public networks. The range of private AS numbers is from 64512 to 65535.

After you execute the command, you can get the following results:

· If the AS_PATH attribute of a BGP update carries only private AS numbers, the device removes the AS numbers before sending the update to the EBGP peer or peer group.

· If the AS_PATH attribute carries both public and private AS numbers, the command does not take effect. The device sends the BGP update to the EBGP peer or peer group without removing the private AS numbers.

· If the AS_PATH attribute carries AS numbers of the peer or peer group, the command does not take effect. The device sends the BGP update to the peer or peer group without removing the private AS numbers.

This command is applicable only to EBGP peers and peer groups.

Examples

# In BGP IPv4 unicast address family view, remove private AS numbers in BGP updates sent to EBGP peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test public-as-only

BGP commands -- peer reflect-client

Use peer reflect-client to configure the device as a route reflector and specify a peer or peer group as a client.

Use undo peer reflect-client to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP L2VPN address family view/BGP EVPN address family view/BGP IPv4 multicast address family view/BGP IPv4 MDT address family view/BGP IPv4 RT filter address family view:

peer { group-name | ipv4-address [ mask-length ] } reflect-client

undo peer { group-name | ipv4-address [ mask-length ] } reflect-client

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } reflect-client

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } reflect-client

In BGP LS address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } reflect-client

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } reflect-client

In BGP IPv6 multicast address family view/BGP-VPN IPv6 unicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } reflect-client

undo peer { group-name | ipv6-address [ prefix-length ] } reflect-client

Default

Neither the route reflector nor the client is configured.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP LS address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP L2VPN address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

BGP IPv4 MDT address family view

BGP IPv4 RT filter address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command configures the device as a route reflector and specifies all dynamic peers in the subnet as clients.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command configures the device as a route reflector and specifies all dynamic peers in the subnet as clients.

Usage guidelines

Using route reflectors can solve the issue brought by too many IBGP connections. In an AS, a router acts as a route reflector, and other routers act as clients connecting to the route reflector. The route reflector forwards the routing information received from a client to other clients. In this way, all clients can receive routing information from one another without establishing BGP sessions.

Examples

# In BGP IPv4 unicast address family view, configure the local device as a route reflector and specify IBGP peer group test as a client.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test reflect-client

Related commands

reflect between-clients

reflector cluster-id

BGP commands -- peer route-limit

Use peer route-limit to set the maximum number of routes that can be received from a peer or peer group.

Use undo peer route-limit to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } route-limit prefix-number [ { alert-only | discard | reconnect reconnect-time } | percentage-value ] *

undo peer { group-name | ipv4-address [ mask-length ] } route-limit

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-limit prefix-number [ { alert-only | discard | reconnect reconnect-time } | percentage-value ] *

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-limit

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } route-limit prefix-number [ { alert-only | discard | reconnect reconnect-time } | percentage-value ] *

undo peer { group-name | ipv6-address [ prefix-length ] } route-limit

Default

The number of routes that can be received from a peer or peer group is not limited.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP VPNv6 address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies the maximum number of routes that can be received from all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies the maximum number of routes that can be received from all dynamic peers in the subnet.

prefix-number: Specifies the number of routes that can be received from the peer or peer group. Its range varies by device model. The router will tear down the session to the peer or peer group if the following conditions exist:

· The alert-only, discard, and reconnect keywords are not specified.

· The number of routes received from the peer or peer group reaches the prefix-number.

The router will not attempt to re-establish the session to a dynamic BGP peer until the router receives a connection request from the peer. For other peers, you can use the reset bgp command to re-establish the sessions.

alert-only: If the number of routes received from the peer or peer group reaches the prefix-number, the router generates a log message instead of tearing down the session to the peer or peer group. The router can continue to receive routes from the peer or peer group.

discard: If the number of routes received from the peer or peer group reaches the prefix-number, the router retains the session to the peer or peer group. However, it discards excess routes and generates a log message. After the number of routes received from the peer or peer group falls below the prefix-number, the router can continue to receive routes from the peer or peer group. To restore the discarded routes, use the refresh bgp import command to request the peer or peer group to resend the routes.

reconnect reconnect-time: Specifies a reconnect time. After the specified time is reached, the router re-establishes a session to the peer or peer group when the number of routes received from the peer or peer group reaches the prefix-number. The value range for the reconnect-time argument is 1 to 65535 seconds. This option is not available for dynamic BGP peers.

percentage-value: Specifies the threshold value for the router to generate a log message (the router generates a log message when the ratio of the number of received routes to the prefix-number exceeds the percentage value). The value range of this argument is 1 to 100, and the default is 75.

Examples

# In BGP IPv4 unicast address family view, set the maximum number of routes that can be received from peer 1.1.1.1 to 10000. Configure the router to tear down the session to the peer if the number is exceeded.

<Sysname> system-view

[Sysname] bgp 109

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer 1.1.1.1 route-limit 10000

BGP commands -- peer route-policy

Use peer route-policy to apply a routing policy to routes incoming from or outgoing to a peer or peer group.

Use undo peer route-policy to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP VPNv6 address family view/BGP EVPN address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } route-policy route-policy-name { export | import }

undo peer { group-name | ipv4-address [ mask-length ] } route-policy { export | import }

In BGP-VPN VPNv4 address family view:

peer { group-name | ipv4-address [ mask-length ] } route-policy route-policy-name import

undo peer { group-name | ipv4-address [ mask-length ] } route-policy import

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-policy route-policy-name { export | import }

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-policy { export | import }

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } route-policy route-policy-name { export | import }

undo peer { group-name | ipv6-address [ prefix-length ] } route-policy { export | import }

Default

No routing policy is applied to routes incoming from or outgoing to a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP-VPN VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command applies a routing policy to routes incoming from or outgoing to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command applies a routing policy to routes incoming from or outgoing to all dynamic peers in the subnet.

route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

export: Applies the routing policy to routes outgoing to the peer or peer group.

import: Applies the routing policy to routes incoming from the peer or peer group.

Usage guidelines

The specified routing policy must have been configured with the route-policy command in system view. If you specify a nonexistent routing policy, all routes can pass the routing policy.

The if-match interface command, if configured for the applied routing policy, does not take effect on routes.

Examples

# In BGP IPv4 unicast address family view, apply routing policy test-policy to routes outgoing to peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] peer test route-policy test-policy export

Related commands

filter-policy export

filter-policy import

peer as-path-acl

peer filter-policy

peer prefix-list

route-policy

BGP commands -- peer route-update-interval

Use peer route-update-interval to specify an interval for sending the same update to a peer or peer group.

Use undo peer route-update-interval to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-update-interval interval

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } route-update-interval

Default

The interval for sending the same update to an IBGP peer is 15 seconds and the interval for sending the same update to an EBGP peer is 30 seconds.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies an interval for sending the same update to all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies an interval for sending the same update to all dynamic peers in the subnet.

interval: Specifies a minimum interval for sending the same update message, in the range of 0 to 600 seconds.

Usage guidelines

A BGP router sends an update message to its peers when a route is changed. If the route changes frequently, the BGP router sends many updates for the route, resulting in routing flaps. By configuring the interval for sending the same update to a peer or peer group, you can avoid such routing flaps.

Examples

# In BGP instance view, set the interval for sending the same update to peer group test to 10 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test as-number 100

[Sysname-bgp-default] peer test route-update-interval 10

BGP commands -- peer soo

Use peer soo to configure the Site of Origin (SoO) attribute for a BGP peer or peer group.

Use undo peer soo to remove the configuration.

Syntax

In BGP IPv4 unicast address family view/BGP-VPN IPv4 unicast address family view/BGP VPNv4 address family view/BGP-VPN VPNv4 address family view/BGP VPNv6 address family view/BGP IPv4 multicast address family view:

peer { group-name | ipv4-address [ mask-length ] } soo site-of-origin

undo peer { group-name | ipv4-address [ mask-length ] } soo

In BGP IPv6 unicast address family view:

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } soo site-of-origin

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } soo

In BGP-VPN IPv6 unicast address family view/BGP IPv6 multicast address family view:

peer { group-name | ipv6-address [ prefix-length ] } soo site-of-origin

undo peer { group-name | ipv6-address [ prefix-length ] } soo

Default

No SoO attribute is configured for a peer or peer group.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP-VPN VPNv4 address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command configures the SoO attribute for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command configures the SoO attribute for all dynamic peers in the subnet.

site-of-origin: Specifies the SoO attribute, a string of 3 to 21 characters. The SoO attribute has the following formats:

· 16-bit AS number:32-bit user-defined number. For example, 100:3.

· 32-bit IP address:16-bit user-defined number. For example, 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, where the minimum value of the AS number is 65536. For example, 65536:1.

Usage guidelines

The SoO attribute specifies the site where the route was originated. It prevents advertising a route back to the originating site. If the AS-path attribute is lost, the router can use the SoO attribute to avoid routing loops.

After you configure the SoO attribute for a BGP peer or peer group, BGP adds the SoO attribute into the route updates received from the BGP peer or peer group. Before advertising route updates to the peer or peer group, BGP checks the SoO attribute of the route update against the configured SoO attribute. If they are the same, BGP does not advertise the route updates to the BGP peer or peer group to avoid loops.

If a PE configured with AS number substitution connects to multiple CEs in the same VPN site through different interfaces, routing loops will occur. To avoid routing loops, configure the same SoO attribute for the CEs on the PE.

Examples

# In BGP IPv4 unicast address family view, set the SoO attribute to 100:1 for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4

[Sysname-bgp-default-ipv4] peer 1.1.1.1 soo 100:1

Related commands

peer substitute-as

BGP commands -- peer source-address

Use peer source-address to specify a source IPv4 or IPv6 address for establishing TCP connections to a peer or peer group.

Use undo peer source-address to remove the configuration.

Syntax

peer ipv4-address [ mask-length ] source-address source-ipv4-address

peer ipv6-address [ prefix-length ] source-address source-ipv6-address

undo peer { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } source-address

peer group-name source-address { source-ipv4-address | source-ipv6-address } *

undo peer group-name source-address [ source-ipv4-address | source-ipv6-address ]

Default

BGP uses the primary IPv4 or IPv6 address of the output interface in the optimal route destined for the BGP peer or peer group as the source address for TCP connection establishment.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command specifies a source IP address for establishing TCP connections to all dynamic peers in the subnet.

source-ipv4-address: Specifies a source IPv4 address.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command specifies a source IPv6 address for establishing TCP connections to all dynamic peers in the subnet.

source-ipv6-address: Specifies a source IPv6 address.

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

Usage guidelines

The peer connect-interface command and the peer source-address command can both change the source address for establishing TCP connections. If you execute both commands, the most recent configuration takes effect.

The peer source-address and peer connect-interface commands are applicable to the following scenarios:

· The peer's IPv4/IPv6 address does not belong to the interface directly connected to the local router. To ensure successful TCP connection establishment, use one of the following methods:

?span style='font:7.0pt "Times New Roman"'> Specify the interface to which the IPv4/IPv6 address belongs as the source interface on the peer.

?span style='font:7.0pt "Times New Roman"'> Specify the IPv4/IPv6 address of the interface directly connected to the local router as the source address on the peer.

· A BGP peer at an IPv6 link-local address must be directly connected to the local router. On the local router, you must use the peer connect-interface command to specify the interface directly connected to the BGP peer as the source interface of TCP connections.

· On a BGP router that has multiple links to a peer, the source interface for TCP connection changes because the primary source interface fails. To avoid this problem, specify a loopback interface as the source interface or specify the IP address of a loopback interface as the source address.

· You want to establish multiple BGP sessions to a router. In this case, BGP might fail to determine the source address for each TCP connection based on the optimal route to the peer. To prevent this problem, use one of the following methods:

?span style='font:7.0pt "Times New Roman"'> If the BGP sessions use IP addresses of different interfaces, specify a source interface or source address for each session.

?span style='font:7.0pt "Times New Roman"'> If the BGP sessions use different IP addresses of the same interface, specify a source address for each session.

The source addresses on the local router and the peer must be reachable to each other.

To specify the address of an indirectly connected interface as the source address, use the peer ebgp-max-hop command. The command allows the establishment of an EBGP session to the indirectly connected peer.

You can specify both a source IPv4 address and a source IPv6 address for a peer group. BGP uses the source IPv4 address to establish TCP connections to IPv4 peers in the group. It also uses the source IPv6 address to establish TCP connections to IPv6 peers in the group.

Examples

# In BGP instance view, specify source IPv4 address 1.1.1.1 for peer group test.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test source-address 1.1.1.1

Related commands

peer connect-interface

peer ebgp-max-hop

BGP commands -- peer substitute-as

Use peer substitute-as to replace the AS number of a peer or peer group in the AS_PATH attribute with the local AS number.

Use undo peer substitute-as to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } substitute-as

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } substitute-as

Default

The AS number of a peer or peer group in the AS_PATH attribute is not replaced.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command replaces the AS number of all dynamic peers in the subnet in the AS_PATH attribute with the local AS number.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command replaces the AS number of all dynamic peers in the subnet in the AS_PATH attribute with the local AS number.

Usage guidelines

In MPLS L3VPN, if EBGP is used between PE and CE, sites in different geographical areas must have different AS numbers assigned to ensure correct route advertisement.

If different CEs use the same AS number, you must configure the relevant PE to replace the AS number of the CE as its own AS number. This ensures correct advertisement of private network routes.

Examples

# In BGP instance view, substitute the local AS number for the AS number of peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 substitute-as

Related commands

peer soo

BGP commands -- peer timer

Use peer timer to set a keepalive interval and hold time for a peer or peer group.

Use undo peer timer to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } timer keepalive keepalive hold holdtime

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } timer

Default

The keepalive interval is 60 seconds, and the hold time is 180 seconds.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command configures a keepalive interval and hold time for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command configures a keepalive interval and hold time for all dynamic peers in the subnet.

keepalive keepalive: Sets a keepalive interval in the range of 0 to 21845 seconds.

hold holdtime: Sets a hold time in the range of 3 to 65535 seconds. The hold time must be at least three times the keepalive interval.

Usage guidelines

After establishing a BGP session, two routers send keepalive messages at the specified keepalive interval to each other to keep the session.

If a router receives no keepalive or update message from the peer within the hold time, it tears down the session.

The timers configured with this command are preferred to the timers configured with the timer command.

If the hold time settings on the local and peer routers are different, the smaller one is used.

If the hold time is set to 0, no keepalive message will be sent to the peer, and the peer session will never time out. If neither the hold time nor the keepalive interval is set to 0, the actual keepalive interval is the smaller one between one third of the hold time and the keepalive interval.

The timers configured with this command do not take effect until a session is re-established (for example, a session is reset).

Examples

# In BGP instance view, set the keepalive interval and hold time for peer group test to 60 seconds and 180 seconds, respectively.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test timer keepalive 60 hold 180

Related commands

display bgp peer

timer

BGP commands -- peer timer connect-retry

Use peer timer connect-retry to set the session retry timer for a peer or peer group.

Use undo peer timer connect-retry to remove the configuration.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } timer connect-retry retry-time

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } timer connect-retry

Default

The session retry timer is 32 seconds a peer or peer group.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command sets a connection retry timer for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command sets a connection retry timer for all dynamic peers in the subnet.

retry-time: Specifies a session retry timer in the range of 1 to 65535 seconds.

Usage guidelines

To speed up session establishment to a peer or peer group and route convergence, set a small session retry timer. If the BGP session flaps, you can set a large session retry timer to reduce the impact.

The timer set by the peer timer connect-retry command takes precedence over the timer set by the timer connect-retry command.

Examples

# In BGP instance view, set the session retry timer to 30 seconds for peer 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer 1.1.1.1 timer connect-retry 30

Related commands

timer connect-retry

BGP commands -- peer ttl-security

Use peer ttl-security to configure Generalized TTL Security Mechanism (GTSM) for a BGP peer or peer group.

Use undo peer ttl-security to disable BGP GTSM for a peer or peer group.

Syntax

peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ttl-security hops hop-count

undo peer { group-name | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] } ttl-security hops

Default

GTSM is disabled for BGP.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

group-name: Specifies a peer group by its name, a case-sensitive string of 1 to 47 characters. The peer group must have been created.

ipv4-address: Specifies a peer by its IPv4 address. The peer must have been created.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command configures GTSM for all dynamic peers in the subnet.

ipv6-address: Specifies a peer by its IPv6 address. The peer must have been created.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command configures GTSM for all dynamic peers in the subnet.

hops hop-count: Specifies the maximum number of hops to the specified peer, in the range of 1 to 254.

Usage guidelines

GTSM protects a BGP session by comparing the TTL value of an incoming IP packet against the valid TTL range. If the TTL value is within the valid TTL range, the packet is accepted. If not, the packet is discarded.

The valid TTL range is from 255 – the configured hop count + 1 to 255.

When GTSM is configured, the BGP packets sent by the device have a TTL of 255.

When GTSM is configured, the local device can establish an EBGP session to the peer after they pass GTSM check, regardless of whether the maximum number of hops is reached.

To use GTSM, you must configure GTSM on both the local and peer devices. You can specify different hop-count values for them.

Examples

# In BGP instance view, enable GTSM for BGP peer group test and set the maximum number of hops to the specified peer in the peer group to 1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] peer test ttl-security hops 1

Related commands

peer ebgp-max-hop

BGP commands -- pic

Use pic to enable BGP FRR for a BGP address family.

Use undo pic to disable BGP FRR for a BGP address family.

Syntax

pic

undo pic

Default

BGP FRR is disabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

FRR is used in a dual-homing network to protect a primary route with a backup route. It uses ARP (for IPv4), ND (for IPv6), or echo-mode BFD (for IPv4) to detect the connectivity of the primary route. When the primary route fails, BGP directs packets to the backup route.

After you enable FRR, BGP calculates a backup route for each BGP route in the address family if there are two or more unequal-cost routes to reach the destination.

You can also configure BGP FRR by using the fast-reroute route-policy command, which takes precedence over the pic command. For more information about routing policies, see Layer 3—IP Routing Configuration Guide.

Use the pic command with caution because it might cause routing loops in specific scenarios.

Examples

# Enable BGP FRR in BGP IPv4 unicast address family view.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] pic

Related commands

fast-reroute route-policy

BGP commands -- preference

Use preference to configure preferences for BGP routes.

Use undo preference to restore the default.

Syntax

preference { external-preference internal-preference local-preference | route-policy route-policy-name }

undo preference

Default

The preferences of external, internal, and local BGP routes are 255, 255, and 130, respectively.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv6 unicast address family view

BGP-VPN IPv6 unicast address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

external-preference: Specifies a preference for EBGP routes, in the range of 1 to 255.

internal-preference: Specifies a preference for IBGP routes, in the range of 1 to 255.

local-preference: Specifies a preference for local routes, in the range of 1 to 255.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to set the route preference for matching routes. Routes not matching the routing policy use the default preference.

Usage guidelines

Different routing protocols might find different routes to the same destination. However, not all of those routes are optimal. For route selection, routing protocols, direct routes, and static routes are assigned different preferences. The route with the highest preference is preferred.

Configuring the preferences for BGP routes changes the possibility for the routes to become the optimal route.

To use a routing policy to set the preference, you must configure the preference with the apply preference command in the routing policy in advance. Otherwise, all matching routes use the default preference.

Examples

# In BGP IPv4 unicast address family view, set preferences for EBGP, IBGP, and local routes to 20, 20, and 200, respectively.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] preference 20 20 200

BGP commands -- primary-path-detect bfd

Use primary-path-detect bfd to configure BGP FRR to use BFD to detect next hop connectivity for the primary route.

Use undo primary-path-detect bfd to restore the default.

Syntax

primary-path-detect bfd echo

undo primary-path-detect bfd

Default

BGP FRR uses ARP to detect the connectivity to the next hop of the primary route.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

echo: Uses echo-mode BFD to detect the connectivity to the next hop of the primary route.

Examples

# In BGP instance view, configure BGP FRR to use echo-mode BFD to detect next hop connectivity for the primary route.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] primary-path-detect bfd echo

Related commands

fast-reroute route-policy

pic

BGP commands -- reflect between-clients

Use reflect between-clients to enable route reflection between clients.

Use undo reflect between-clients to disable route reflection between clients.

Syntax

reflect between-clients

undo reflect between-clients

Default

Route reflection between clients is enabled.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP LS address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP L2VPN address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

BGP IPv4 MDT address family view

BGP IPv4 RT filter address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When a route reflector is configured, and the clients of a route reflector are fully meshed, route reflection is unnecessary because it consumes more bandwidth resources. You can use the undo reflect between-clients command to disable route reflection instead of modifying network configuration or changing network topology.

After route reflection is disabled between clients, routes can still be reflected between a client and a non-client.

Examples

# In BGP IPv4 unicast address family view, disable route reflection between clients.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] undo reflect between-clients

Related commands

peer reflect-client

reflector cluster-id

BGP commands -- reflector cluster-id

Use reflector cluster-id to configure the cluster ID for a route reflector.

Use undo reflector cluster-id to restore the default.

Syntax

reflector cluster-id { cluster-id | ipv4-address }

undo reflector cluster-id

Default

A route reflector uses its router ID as the cluster ID.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP VPNv4 address family view

BGP IPv6 unicast address family view

BGP LS address family view

BGP-VPN IPv6 unicast address family view

BGP VPNv6 address family view

BGP L2VPN address family view

BGP EVPN address family view

BGP IPv4 multicast address family view

BGP IPv6 multicast address family view

BGP IPv4 MDT address family view

BGP IPv4 RT filter address family view

Predefined user roles

network-admin

mdc-admin

Parameters

cluster-id: Specifies the cluster ID in the format of an integer, in the range of 1 to 4294967295.

ipv4-address: Specifies the cluster ID in the format of an IPv4 address in dotted decimal notation.

Usage guidelines

The route reflector and clients form a cluster. Typically a cluster has one route reflector. The ID of the route reflector is the cluster ID.

You can configure more than one route reflector in a cluster to improve network reliability and prevent a single point of failure. Use this command to configure the same cluster ID for all route reflectors in the cluster to avoid routing loops.

Do not configure the router ID of a client as the cluster ID.

Examples

# In BGP IPv4 unicast address family view, set the cluster ID on the local router (a reflector in the cluster) to 80.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] reflector cluster-id 80

Related commands

peer reflect-client

reflect between-clients

BGP commands -- refresh bgp

Use refresh bgp to manually soft-reset BGP sessions.

Syntax

refresh bgp [ instance instance-name ] { ipv4-address [ mask-length ] | all | external | group group-name | internal } { export | import } ipv4 { multicast | rtfilter | [ unicast ] [ vpn-instance vpn-instance-name ] }

refresh bgp [ instance instance-name ] { ipv6-address [ prefix-length ] | all | external | group group-name | internal } { export | import } ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] }

refresh bgp [ instance instance-name ] ipv4-address [ mask-length ] { export | import } ipv6 [ unicast ]

refresh bgp [ instance instance-name ] { ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] | all | external | group group-name | internal } { export | import } link-state

refresh bgp [ instance instance-name ] { ipv4-address [ mask-length ] | all | external | group group-name | internal } { export | import } vpnv4 [ vpn-instance vpn-instance-name ]

refresh bgp [ instance instance-name ] { ipv4-address [ mask-length ] | all | external | group group-name | internal } { export | import } vpnv6

refresh bgp [ instance instance-name ] { ipv4-address [ mask-length ] | all | external | group group-name | internal } { export | import } l2vpn [ evpn ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command soft-resets BGP sessions for the default BGP instance.

ipv4-address: Soft-resets the BGP session to a peer specified by its IP address.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command soft-resets BGP sessions to all dynamic peers in the subnet.

ipv6-address: Soft-resets the BGP session to a peer specified by its IPv6 address.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command soft-resets BGP sessions to all dynamic peers in the subnet.

all: Soft-resets all BGP sessions.

external: Soft-resets all EBGP sessions.

group group-name: Soft-resets the BGP sessions to the peers of the specified peer group. The group-name argument refers to the name of a peer group, a case-sensitive string of 1 to 47 characters.

internal: Soft-resets all IBGP sessions.

export: Performs outbound soft-reset (filters routes advertised to the specified peer or peer group by using the new configuration).

import: Performs inbound soft-reset (filters routes received from the specified peer or peer group by using the new configuration).

ipv4: Soft-resets BGP sessions for IPv4 address family.

ipv6: Soft-resets BGP sessions for IPv6 address family.

link-state: Soft-resets BGP sessions for LS address family.

multicast: Soft-resets BGP sessions for multicast address family.

rtfilter: Soft-resets BGP sessions for IPv4 RT filter address family

unicast: Soft-resets BGP sessions for unicast address family.

vpnv4: Soft-resets BGP sessions for VPNv4 address family.

vpnv6: Soft-resets BGP sessions for VPNv6 address family.

l2vpn: Soft-resets BGP sessions for L2VPN address family.

evpn: Soft-resets BGP sessions for EVPN address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command soft-resets BGP sessions for the specified address family on the public network.

Usage guidelines

A soft-reset operation enables the router to apply a new route selection policy without tearing down BGP connections.

To apply a new policy to outbound BGP sessions, execute this command with the export keyword. The router uses the new policy to filter routing information and sends the routing information that passes the filtering to the BGP peers.

To apply a new policy to inbound sessions, execute this command with the import keyword. The router advertises a route-refresh message to the peer and the peer resends its routing information to the router. After receiving the routing information, the router uses the new policy to filter the routing information.

This command requires that both the local router and the peer support route refresh.

If the peer keep-all-routes command is configured, the refresh bgp import command does not take effect.

By default, the unicast keyword is used if neither the multicast keyword nor the unicast keyword is specified.

Examples

# Soft-reset all inbound BGP sessions for the IPv4 unicast address family.

<Sysname> refresh bgp all import ipv4

Related commands

peer capability-advertise route-refresh

peer keep-all-routes

BGP commands -- reset bgp

Use reset bgp to reset BGP sessions for the specified address family.

Syntax

reset bgp [ instance instance-name ] { as-number | ipv4-address [ mask-length ] | all | external | group group-name | internal } ipv4 { mdt | multicast | rtfilter | [ unicast ] [ vpn-instance vpn-instance-name ] }

reset bgp [ instance instance-name ] { as-number | ipv6-address [ prefix-length ] | all | external | group group-name | internal } ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] }

reset bgp [ instance instance-name ] ipv4-address [ mask-length ] ipv6 [ unicast ]

reset bgp [ instance instance-name ] { as-number | ipv4-address [ mask-length ] | ipv6-address [ prefix-length ] | all | external | group group-name | internal } { export | import } link-state

reset bgp [ instance instance-name ] { as-number | ipv4-address [ mask-length ] | all | external | group group-name | internal } vpnv4 [ vpn-instance vpn-instance-name ]

reset bgp [ instance instance-name ] { as-number | ipv4-address [ mask-length ] | all | external | group group-name | internal } vpnv6

reset bgp [ instance instance-name ] { as-number | ipv4-address [ mask-length ] | all | external | group group-name | internal } l2vpn [ evpn ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command resets BGP sessions for the default BGP instance.

as-number: Resets BGP sessions to peers in the AS specified by its number in the range of 1 to 4294967295.

ipv4-address: Resets the BGP session to a peer specified by its IPv4 address.

mask-length: Specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command resets BGP sessions to all dynamic peers in the subnet.

ipv6-address: Resets the BGP session to a peer specified by its IPv6 address.

prefix-length: Specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command resets BGP sessions to all dynamic peers in the subnet.

all: Resets all BGP sessions.

external: Resets all EBGP sessions.

group group-name: Resets the BGP sessions to the peers in the peer group specified by its name, a case-sensitive string of 1 to 47 characters.

internal: Resets all IBGP sessions.

ipv4: Resets BGP sessions for IPv4 address family.

ipv6: Resets BGP sessions for IPv6 address family.

link-state: Resets BGP sessions for LS address family.

mdt: Resets BGP sessions for MDT address family.

multicast: Resets BGP sessions for multicast address family.

rtfilter: Resets BGP sessions for IPv4 RT filter address family.

unicast: Resets BGP sessions for unicast address family.

vpnv4: Resets BGP sessions for VPNv4 address family.

vpnv6: Resets BGP sessions for VPNv6 address family.

l2vpn: Resets BGP sessions for L2VPN address family.

evpn: Resets BGP sessions for EVPN address family.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command resets BGP sessions for the specified address family on the public network.

Usage guidelines

A reset operation enables the router to apply a new route selection policy by re-establishing BGP sessions. This operation breaks down BGP sessions for a short period of time.

By default, the unicast keyword is used if the unicast, mdt, and multicast keywords are not specified.

Examples

# Reset all BGP sessions for the IPv4 unicast address family.

<Sysname> reset bgp all ipv4

BGP commands -- reset bgp all

Use reset bgp all to reset all BGP sessions for all address families.

Syntax

reset bgp [ instance instance-name ] all

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command resets all BGP sessions for all address families of the default BGP instance.

Usage guidelines

A reset operation enables the router to apply a new route selection policy by re-establishing BGP sessions. This operation breaks down BGP sessions for a short while.

Examples

# Reset all BGP sessions.

<Sysname> reset bgp all

BGP commands -- reset bgp bmp server statistics

Use reset bgp bmp server statistics to clear BMP server statistics.

Syntax

reset bgp [ instance instance-name ] bmp server server-number statistics

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command clears the BMP server statistics of the default BGP instance.

server-number: Specifies a BMP server by its number in the range of 1 to 8.

Examples

# Clear the statistics of BMP server 1.

<Sysname> reset bgp bmp server 1 statistics

Related commands

display bgp bmp server

BGP commands -- reset bgp dampening

Use reset bgp dampening to clear BGP route dampening information and release suppressed BGP routes.

Syntax

reset bgp [ instance instance-name ] dampening ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv4-address [ mask-length | mask ] ]

reset bgp [ instance instance-name ] dampening ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv6-address prefix-length ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command clears BGP route dampening information and releases suppressed BGP routes for the default BGP instance.

ipv4: Clears BGP IPv4 route dampening information and release suppressed BGP IPv4 routes.

ipv6: Clears BGP IPv6 route dampening information and release suppressed BGP IPv6 routes.

multicast: Clears BGP multicast route dampening information and release suppressed BGP multicast routes.

unicast: Clears BGP unicast route dampening information and release suppressed BGP unicast routes.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command clears BGP route dampening information for the public network, and releases suppressed BGP routes.

ipv4-address: Specifies an IPv4 destination network address. If you do not specify a network address, this command clears all BGP route dampening information, and releases all suppressed BGP routes.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

ipv6-address: Specifies an IPv6 destination network address. If you do not specify a network address, this command clears all BGP route dampening information, and releases all suppressed BGP routes.

prefix-length: Specifies a prefix length in the range of 0 to 128.

Usage guidelines

When you execute the reset bgp dampening ipv4 command:

· If you specify only the ipv4-address argument, the system ANDs the network address with the mask of a route. If the result matches the network address of the route, the command clears dampening information for the route, and releases the suppressed route.

· If you specify the ipv4-address mask or ipv4-address mask-length argument, this command does the following:

?span style='font:7.0pt "Times New Roman"'> Clears dampening information for the route that matches both the specified destination network address and the mask (or mask length).

?span style='font:7.0pt "Times New Roman"'> Releases the suppressed route.

By default, the unicast keyword is used if neither the unicast keyword nor the multicast keyword is specified.

Examples

# Clear dampening information for the BGP IPv4 unicast route to network 20.1.0.0/16 and release the suppressed route.

<Sysname> reset bgp dampening ipv4 20.1.0.0 255.255.0.0

Related commands

dampening

display bgp routing-table dampened

BGP commands -- reset bgp flap-info

Use reset bgp flap-info to clear flap statistics for BGP routes.

Syntax

reset bgp [ instance instance-name ] flap-info ipv4 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv4-address [ mask-length | mask ] | as-path-acl as-path-acl-number | peer ipv4-address [ mask-length ] ]

reset bgp [ instance instance-name ] flap-info ipv6 { multicast | [ unicast ] [ vpn-instance vpn-instance-name ] } [ ipv6-address prefix-length | as-path-acl as-path-acl-number | peer ipv6-address [ prefix-length ] ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command clears flap statistics for the default BGP instance.

ipv4: Clears flap statistics for BGP IPv4 routes.

ipv6: Clears flap statistics for BGP IPv6 routes.

multicast: Clears flap statistics for BGP multicast routes.

unicast: Clears flap statistics for BGP unicast routes.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command clears flap statistics for public BGP routes.

ipv4-address: Specifies an IPv4 destination network address.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a network mask in dotted decimal notation.

ipv6-address: Specifies an IPv6 destination network address.

prefix-length: Specifies a prefix length in the range of 0 to 128.

as-path-acl as-path-acl-number: Specifies an AS path list by its number in the range of 1 to 256, to filter BGP route flap statistics.

peer ipv4-address [ mask-length ]: Clears flap statistics for BGP routes learned from the specified IPv4 BGP peer. The mask-length argument specifies a mask length in the range of 0 to 32. You can use the ipv4-address and mask-length arguments together to specify a subnet. If you specify a subnet, this command clears flap statistics for BGP routes learned from all dynamic peers in the subnet.

peer ipv6-address [ prefix-length ]: Clears flap statistics for BGP routes learned from the specified IPv6 BGP peer. The prefix-length argument specifies a prefix length in the range of 0 to 128. You can use the ipv6-address and prefix-length arguments together to specify a subnet. If you specify a subnet, this command clears flap statistics for BGP routes learned from all dynamic peers in the subnet.

Usage guidelines

When you execute the reset bgp flap-info ipv4 command:

· If you specify only the ipv4-address argument, the system ANDs the IPv4 network address with the mask of a route. If the result matches the IPv4 network address of the route, this command clears the flap statistics of the route.

· If you specify the ipv4-address mask or ipv4-address mask-length argument, this command clears the flap statistics of the route that matches both the specified IPv4 destination network address and the mask (or mask length).

By default, the unicast keyword is used if neither the unicast keyword nor the multicast keyword is specified.

Examples

# Clear flap statistics for the BGP IPv4 unicast route to network 20.1.0.0/16.

<Sysname> reset bgp flap-info ipv4 20.1.0.0 16

Related commands

dampening

display bgp routing-table flap-info

BGP commands -- retain local-label

Use retain local-label to set an update delay for local MPLS labels.

Use undo retain local-label to restore the default.

Syntax

retain local-label retain-time

undo retain local-label

Default

The update delay is 60 seconds.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

retain-time: Specifies the update delay in the range of 1 to 21845 seconds.

Usage guidelines

BGP includes local MPLS labels in advertised VPNv4 routes, VPNv6 routes, labeled IPv4 unicast routes, and labeled IPv6 unicast routes.

When a local label is changed, BGP removes the old label and advertises the new label. Traffic interruption occurs if BGP peers use the old label to forward packets before they learn the new label. To resolve this issue, configure an update delay for local MPLS labels. BGP does not remove the old label before the update delay timer expires.

Examples

# Set the update delay for local MPLS labels to 100 seconds.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] retain local-label 100

BGP commands -- router id

Use router id to configure a global router ID.

Use undo router id to restore the default.

Syntax

router id router-id

undo router id

Default

No global router ID is configured.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

router-id: Specifies a router ID in IP address format.

Usage guidelines

Some routing protocols use a router ID to identify a device. You can configure a global router ID, which is used by routing protocols that have no router ID configured.

If no global router ID is configured, the highest loopback address, if any, is used as the router ID. If no loopback address is available, the highest physical interface IP address is used, regardless of the interface status. If no IP address is configured for any interface, the router ID is 0.0.0.0.

During an active/standby switchover, the standby main processing unit (MPU) checks the validity of the previous router ID backed up before switchover. If it is not valid, it selects a new router ID.

If the interface IP address that is selected as the router ID is removed or modified, a new router ID is selected. The following events will not trigger a router ID re-selection:

· The interface goes down.

· After a physical interface address is selected as the router ID, an IP address is configured for a loopback interface.

· A higher interface IP address is configured.

After a router ID is changed, use the reset command to make it effective.

Examples

# Configure a global router ID as 1.1.1.1.

<Sysname> system-view

[Sysname] router id 1.1.1.1

Related commands

router-id (BGP instance view)

router-id (BGP-VPN instance view)

BGP commands -- router-id (BGP instance view)

Use router-id to configure a router ID for a BGP instance.

Use undo router-id to restore the default.

Syntax

router-id router-id

undo router-id

Default

No router ID is configured for a BGP instance, and the BGP instance uses the global router ID configured by the router id command in system view.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

router-id: Specifies a router ID for BGP, in IP address format.

Usage guidelines

To run BGP, a BGP instance must have a router ID, which is an unsigned 32-bit integer that uniquely identifies the router in the AS.

To modify a non-zero router ID for BGP, execute the router-id command in BGP instance view.

To improve availability, specify the IP address of a loopback interface as the router ID for BGP.

If you execute this command in the same BGP instance view multiple times, the most recent configuration takes effect.

You can configure the same router ID for different BGP instances.

Examples

# In BGP instance view, set the router ID for BGP to 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] router-id 1.1.1.1

Related commands

router id

router-id (BGP-VPN instance view)

BGP commands -- router-id (BGP-VPN instance view)

Use router-id to configure a router ID for a BGP VPN instance.

Use undo router-id to restore the default.

Syntax

router-id { router-id | auto-select }

undo router-id

Default

No router ID is configured for a BGP VPN instance, and the BGP VPN instance uses the router ID configured in BGP instance view. If no router ID is configured in BGP instance view, the BGP VPN instance uses the global router ID configured in system view.

Views

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

router-id: Specifies a router ID in IP address format.

auto-select: Automatically selects a router ID for the BGP VPN instance.

Usage guidelines

To run BGP, a VPN instance of a BGP instance must have a router ID, which is an unsigned 32-bit integer that uniquely identifies the BGP VPN router in the AS.

If the auto-select keyword is specified, the system selects a router ID for the BGP VPN instance in the following order:

1. The highest loopback address in the BGP VPN instance as the router ID.

2. The highest physical interface address in the BGP VPN instance as the router ID, regardless of the interface status.

3. 0.0.0.0 as the router ID.

If a non-zero router ID is selected for the BGP VPN instance, the router ID will not change when a more preferable router ID is available in the BGP VPN instance.

To improve availability, specify the IP address of a loopback interface as the router ID.

You can specify a different router ID for each VPN instance on a device.

If you execute this command in the same BGP-VPN instance view multiple times, the most recent configuration takes effect.

Examples

# In BGP-VPN instance view, set the router ID to 1.1.1.1.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] ip vpn-instance vpn1

[Sysname-bgp-default-vpn1] router-id 1.1.1.1

Related commands

router id

router-id (BGP instance view)

BGP commands -- route-rate-limit

Use route-rate-limit to set the BGP route sending rate.

Use undo route-rate-limit to restore the default.

Syntax

route-rate-limit rate

undo route-rate-limit

Default

The BGP route sending rate is not limited.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

rate: Specifies the maximum number of new routes that BGP can send per second, in the range of 0 to 4294967595. A value of 0 means that BGP does not send newly added routes.

Usage guidelines

For a device with high performance, you can set a high BGP route sending rate as needed. For a device without high performance, set a relatively low BGP route sending rate as a best practice.

This command applies only to IPv4 unicast routes and IPv6 unicast routes.

Examples

# In BGP instance view, set the BGP route sending rate to 1000.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] route-rate-limit 1000

BGP commands -- server

Use server to configure an IP address and port number for a BMP server.

Use undo server to remove the configuration.

Syntax

server address ipv4-address port port-number

undo server

Default

No IP address and port number are configured for the BMP server.

Views

BMP server view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4-address: Specifies an IP address for the BMP server.

port-number: Specifies a port number for the BMP server, in the range of 1 to 65535.

Usage guidelines

After you configure an IP address and port number for a BMP server, the BMP client establishes a TCP connection to the BMP server and sends BMP messages to the BMP server.

Examples

# Configure IP address 100.1.1.1 and port number 8888 for BMP server 5.

<Sysname> system-view

[Sysname] bmp server 5

[Sysname-bmpserver-5] server address 100.1.1.1 port 8888

BGP commands -- snmp context-name

Use snmp context-name to configure an SNMP context for a BGP instance.

Use undo snmp context-name to restore the default.

Syntax

snmp context-name context-name

undo snmp context-name

Default

No SNMP context is configured for a BGP instance.

Views

BGP instance view

Predefined user roles

network-admin

mdc-admin

Parameters

context-name: Specifies an SNMP context by its name, a case-sensitive string of 1 to 32 characters.

Usage guidelines

BGP does not know the BGP instance to which a managed MIB node belongs. To resolve this issue, configure different SNMP contexts for different BGP instances.

The device selects a MIB for an SNMP packet according to the context (for SNMPv3) or community name (for SNMPv1/v2c) in the following ways:

· For an SNMPv3 packet:

?span style='font:7.0pt "Times New Roman"'> The device selects the MIB of the BGP instance default if the packet does not carry a context and no SNMP context was configured for the BGP instance default.

?span style='font:7.0pt "Times New Roman"'> The device selects the MIB of a BGP instance if the packet meets the following conditions:

- Carries a context that was configured with the snmp-agent context command in system view.

- Matches the context of the BGP instance.

?span style='font:7.0pt "Times New Roman"'> The device does not process any MIBs in other situations.

· For an SNMPv1/v2c packet:

?span style='font:7.0pt "Times New Roman"'> The device selects the MIB of the BGP instance default if the following conditions are met:

- No SNMP community to SNMP context mapping was configured with the snmp-agent community-map command in system view.

- No SNMP context was configured for the BGP instance default.

?span style='font:7.0pt "Times New Roman"'> The device selects the MIB of a BGP instance if the SNMP community is mapped to an SNMP context and the context matches the context of the BGP instance.

?span style='font:7.0pt "Times New Roman"'> The device does not process any MIBs in other situations.

For more information about SNMP contexts and community names, see Network Management and Monitoring Configuration Guide.

Do not configure the same SNMP context for different BGP instances.

If you execute this command multiple times, the most recent configuration takes effect.

Examples

# Configure SNMP context bgp-abc for BGP instance abc.

<Sysname> system-view

[Sysname] bgp 100 instance abc

[Sysname-bgp-abc] snmp context-name bgp-abc

Related commands

snmp-agent community-map (Network Management and Monitoring Command Reference)

snmp-agent context (Network Management and Monitoring Command Reference)

BGP commands -- snmp-agent trap enable bgp

Use snmp-agent trap enable bgp to enable SNMP notifications for BGP.

Use undo snmp-agent trap enable bgp to disable SNMP notifications for BGP.

Syntax

snmp-agent trap enable bgp [ instance instance-name ]

undo snmp-agent trap enable bgp [ instance instance-name ]

Default

SNMP notifications for BGP are enabled.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

instance instance-name: Specifies a BGP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command enables SNMP notifications for the default BGP instance.

Usage guidelines

After you enable SNMP notifications for BGP, the device generates a notification when a BGP neighbor state change occurs. The notification includes the neighbor address, the error code and subcode of the most recent error, and the current neighbor state.

For BGP notifications to be sent correctly, you must also configure SNMP on the device. For more information about SNMP configuration, see the network management and monitoring configuration guide for the device.

Examples

# Enable SNMP notifications for BGP.

<Sysname> system-view

[Sysname] snmp-agent trap enable bgp

BGP commands -- statistics-interval

Use statistics-interval to set the interval at which BGP sends statistics information to the BMP server.

Use undo statistics-interval to restore the default.

Syntax

statistics-interval value

undo statistics-interval

Default

BGP does not send statistics information to the BMP server.

Views

BMP server view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies the interval at which BGP sends statistics information to the BMP server, in the range of 1 to 3600 seconds.

Usage guidelines

After establishing a TCP connection to the BMP server, BGP sends statistics information to the BMP server at the specified interval.

Examples

# Set the interval to 5 seconds at which BGP sends statistics information to the BMP server.

<Sysname> system-view

[Sysname] bmp server 5

[Sysname-bmpserver-5] statistics-interval 5

BGP commands -- summary automatic

Use summary automatic to configure automatic route summarization for redistributed IGP subnet routes.

Use undo summary automatic to restore the default.

Syntax

summary automatic

undo summary automatic

Default

Automatic route summarization is not performed for redistributed IGP subnet routes.

Views

BGP IPv4 unicast address family view

BGP-VPN IPv4 unicast address family view

BGP IPv4 multicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

After the summary automatic command is configured, BGP summarizes IGP subnets redistributed by the import-route command.

Automatic summary routes can be manually summarized, but cannot be added to the IP routing table.

Examples

# In BGP IPv4 unicast address family view, configure automatic route summarization for redistributed IGP subnet routes.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] address-family ipv4 unicast

[Sysname-bgp-default-ipv4] summary automatic

Related commands

aggregate

import-route

BGP commands -- timer

Use timer to configure a BGP keepalive interval and hold time.

Use undo timer to restore the default.

Syntax

timer keepalive keepalive hold holdtime

undo timer

Default

The BGP keepalive interval and the hold time are 60 seconds and 180 seconds, respectively.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

keepalive keepalive: Configures a keepalive interval in the range of 0 to 21845 seconds.

hold holdtime: Configures a hold time in seconds, whose value is 0 or in the range of 3 to 65535. The hold time must be at least three times the keepalive interval.

Usage guidelines

After establishing a BGP session, two routers send keepalive messages at the specified keepalive interval to each other to keep the session.

If a router receives no keepalive or update message from the peer within the hold time, it tears down the session.

Use the timer command to configure the keepalive interval and hold time for all BGP peers. Use the peer timer command to configure the keepalive interval and hold time for a peer or peer group. If both commands are configured, the intervals configured by the peer timer command have higher priority.

If the hold time settings on the local and peer routers are different, the smaller one is used.

If the hold time is set to 0, no keepalive message will be sent to the peer, and the peer session will never time out. If neither the hold time nor the keepalive interval is set to 0, the actual keepalive interval is the smaller one between one third of the hold time and the keepalive interval.

The timer command affects only new BGP sessions.

After the timer command is executed, no peer session is closed at once. The configured hold time is used for negotiation in session re-establishment (for example, when you reset the BGP session).

Examples

# In BGP instance view, set the keepalive interval and hold time to 60 seconds and 180 seconds, respectively.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] timer keepalive 60 hold 180

Related commands

display bgp peer

peer timer

BGP commands -- timer connect-retry

Use timer connect-retry to set the session retry timer for all peers and peer groups.

Use undo timer connect-retry to restore the default.

Syntax

timer connect-retry retry-time

undo timer connect-retry

Default

The session retry timer is 32 seconds for all peers and peer groups.

Views

BGP instance view

BGP-VPN instance view

Predefined user roles

network-admin

mdc-admin

Parameters

retry-time: Specifies a session retry timer in the range of 1 to 65535 seconds.

Usage guidelines

To speed up session establishment to a peer or peer group and route convergence, set a small session retry timer. If the BGP session flaps, you can set a large session retry timer to reduce the impact.

The timer set by the peer timer connect-retry command takes precedence over the timer set by the timer connect-retry command.

Examples

# In BGP instance view, set the session retry timer to 30 seconds for all peers.

<Sysname> system-view

[Sysname] bgp 100

[Sysname-bgp-default] timer connect-retry 30

Related commands

peer timer connect-retry