WLAN radio resource measurement commands -- display wlan measure-report

Use display wlan measure-report to display measurement reports for clients.

Syntax

ACs:

display wlan measure-report ap ap-name radio radio-id [ client mac-address mac-address ]

Fat APs:

display wlan measure-report interface interface-type interface-number [ client mac-address mac-address ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ap ap-name: Specifies an AP by its name, a case-insensitive string of 1 to 64 characters. The string can contain letters, digits, underscores (_), left brackets ([), right brackets (]), forward slashes (/), and hyphens (-).

radio radio-id: Specifies a radio by its number. The value range varies by device model.

interface interface-type interface-number: Specifies a radio interface by its type and number.

client mac-address mac-address: Specifies a client by its MAC address. If you do not specify a client, this command displays measurement reports for all clients.

Examples

# (ACs.) Display measurement reports for clients associated with radio 2 of AP ap1.

<Sysname> display wlan measure-report ap ap1 radio 2

Total number of clients: 1

Client MAC address : 0aef-e760-3587

Link measurement:

Link margin : 2 dBm

RCPI : -85 dBm

RSNI : 53 dBm

Noise histogram:

Antenna ID : 3

ANPI : -56 dBm

IPI0 to IPI10 density : 5 12 16 13 8 5 5 15 17 1 3

Spectrum measurement:

Transmit power : 20 dBm

BSS : Detected

OFDM preamble : Detected

Radar : Detected

Unidentified signal : Undetected

CCA busy fraction : 60

RPI0 to RPI7 density : 3 7 11 19 15 23 15 7

Frame report entry:

BSSID : a072-2351-e253

PHY type : fhss

Average RCPI : -10 dBm

Last RSNI : 2 dBm

Last RCPI : -20 dBm

Frames : 1

Dot11BSSAverageAccessDelay group:

Average access delay : 32 ms

BestEffort average access delay : 1 ms

Background average access delay : 1 ms

Video average access delay : 1 ms

Voice average access delay : 1 ms

Clients : 32

Channel utilization rate : 11

Transmit stream:

Traffic ID : 0

Sent MSDUs : 60

Discarded MSDUs : 5

Failed MSDUs : 3

MSDUs resent multiple times : 3

Lost QoS CF-Polls : 2

Average queue delay : 2 ms

Average transmit delay : 1 ms

Bin0 range : 0 to 10 ms

Bin0 to Bin5 : 5 10 10 5 10 10

# (Fat APs.) Display measurement reports for clients associated with the specified radio interface.

<Sysname> display wlan measure-report interface wlan-radio 1/0/1

Total number of clients: 1

Client MAC address : 0aef-e760-3587

Link measurement:

Link margin : 2 dBm

RCPI : -85 dBm

RSNI : 53 dBm

Noise histogram:

Antenna ID : 3

ANPI : -56 dBm

IPI0 to IPI10 density : 5 12 16 13 8 5 5 15 17 1 3

Spectrum measurement:

Transmit power : 20 dBm

BSS : Detected

OFDM preamble : Detected

Radar : Detected

Unidentified signal : Undetected

CCA busy fraction : 60

RPI0 to RPI7 density : 3 7 11 19 15 23 15 7

Frame report entry:

BSSID : a072-2351-e253

PHY type : fhss

Average RCPI : -10 dBm

Last RSNI : 2 dBm

Last RCPI : -20 dBm

Frames : 1

Dot11BSSAverageAccessDelay group:

Average access delay : 32 ms

BestEffort average access delay : 1 ms

Background average access delay : 1 ms

Video average access delay : 1 ms

Voice average access delay : 1 ms

Clients : 32

Channel utilization rate : 11

Transmit stream:

Traffic ID : 0

Sent MSDUs : 60

Discarded MSDUs : 5

Failed MSDUs : 3

MSDUs resent multiple times : 3

Lost QoS CF-Polls : 2

Average queue delay : 2 ms

Average transmit delay : 1 ms

Bin0 range : 0 to 10 ms

Bin0 to Bin5 : 5 10 10 5 10 10

Table 1 Command output

Field | Description
Link margin | Gap between the received RSSI and the lowest available RSSI.
RCPI | Received Channel Power Indicator.
RSNI | Received Signal to Noise Indicator.
ANPI | Average Noise Power Indicator during the measurement.
IPI0 to IPI10 density | Percentage of time for different IPI ranges to the total measurement period. IPIn represents an IPI range. The value for n is in the range of 1 to 10: · 0: IPI  –92 dBm. · 1: –92 dBm < IPI  –89 dBm. · 2: –89 dBm < IPI  –86 dBm. · 3: –86 dBm < IPI  –83 dBm. · 4: –83 dBm < IPI  –80 dBm. · 5: –80 dBm < IPI  –75 dBm · 6: –75 dBm < IPI  –70 dBm. · 7: –70 dBm < IPI  –65 dBm. · 8: –65 dBm < IPI  –60 dBm. · 9: –60 dBm < IPI  –55 dBm. · 10: –55 dBm < IPI.
Transmit power | Transmission power of the client.
BSS | Whether the client has detected wireless packets from other BSSs.
OFDM preamble | Whether the client has detected OFDM preambles.
Radar | Whether the client has detected radar signals.
Unidentified signal | Whether the client has detected unknown signals.
CCA busy fraction | CCA utilization is expressed as a percentage of time that the channel is busy (during the measurement period).
RPI0 to RPI7 density | Percentage of time that each RPI was used during the measurement period. RPIn represents a RPI range. The value for n is in the range of 1 to 7: · 0: RPI  –87 dBm. · 1: –87 dBm < RPI  –82 dBm. · 2: –82 dBm < RPI  –77 dBm. · 3: –77 dBm < RPI  –72 dBm. · 4: –72 dBm < RPI  –67 dBm. · 5: –67 dBm < RPI  –62 dBm. · 6: –62 dBm < RPI  –57 dBm. · 7: –57 dBm < RPI.
PHY type | Physical media type: fhss, dsss, irbaseband, ofdm, hrdsss, or erp.
Frames | Number of frames from the same MAC address and BSSID during the measurement.
Bin0 range | Value range for Bin0.
Bin0 to Bin5 | Number of successfully sent MSDUs for each average delay range. Binx represents an average delay range. The value for x is in the range of 0 to 5: · Bin0: Delay< 10 ms. · Bin1: 10 ms  Delay < 20 ms. · Bin2: 20 ms  Delay < 40 ms. · Bin3: 40 ms  Delay < 80 ms. · Bin4: 80 ms  Delay < 160 ms. · Bin5: 160 ms  Delay.

WLAN radio resource measurement commands -- measure

Use measure enable to enable the specified measurement feature or all measurement features.

Use measure disable to disable the specified measurement feature or all measurement features.

Use undo measure to restore the default.

Syntax

measure { all | link | neighbor | radio | spectrum | tpc } { disable | enable }

undo measure

Default

ACs:

In radio view, the AP uses the configuration in AP group view.

In AP group radio view, measurement is disabled.

Fat APs:

Measurement is disabled.

Views

ACs:

Radio view

AP group radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all measurement features.

link: Specifies link measurement. Link measurement measures RCPI, RSNI, and link redundancy for the requested link.

neighbor: Specifies neighbor measurement. Neighbor measurement measures the channel and BSSID of neighbor APs.

radio: Specifies radio measurement. Radio measurement measures channel load, noise histogram, beacons, frames, station statistics, locations, and transmit streams.

spectrum: Specifies spectrum measurement, which includes basic measurement, Clear Channel Assessment (CCA) measurement, and Receive Power Indication (RPI) measurement.

tpc: Specifies TPC measurement. TPC measurement measures link redundancy and transmission power for clients.

Usage guidelines

You must enable radio resource measurement if you enable link, neighbor, or radio measurement.

You must enable spectrum management if you enable spectrum or TPC measurement. For more information about spectrum management, see WLAN Configuration Guide.

Examples

# (ACs.) Enable spectrum measurement for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] measure spectrum enable

# (ACs.) Enable spectrum measurement for APs with model WA4320i-ACN in AP group apgroup1.

<Sysname> system-view

[Sysname] wlan ap-group apgroup1

[Sysname-wlan-ap-group-apgroup1] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN-radio-1] measure spectrum enable

# (Fat APs.) Enable spectrum measurement.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/1

[Sysname-WLAN-Radio1/0/1] measure spectrum enable

Related commands

measure-duration

measure-interval

resource-measure

spectrum-management

WLAN radio resource measurement commands -- measure-duration

Use measure-duration to set the measurement duration.

Use undo measure-duration to restore the default.

Syntax

measure-duration time

undo measure-duration

Default

ACs:

In radio view, the AP uses the configuration in AP group view.

In AP group radio view, the measurement duration is 500 TUs.

Fat APs:

The measurement duration is 500 TUs.

Views

ACs:

Radio view

AP group radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

time: Specifies the measurement duration in the range of 1 to 10000 TUs. One TU is equal to 1024 microseconds.

Usage guidelines

When measurement is enabled on an AP, the AP adds the measurement duration in the measurement requests sent to clients.

Examples

# (ACs.) Set the measurement duration to 512 TUs for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] measure-duration 512

# (ACs.) Set the measurement duration to 512 TUs for APs with model WA4320i-ACN in AP group apgroup1.

<Sysname> system-view

[Sysname] wlan ap-group apgroup1

[Sysname-wlan-ap-group-apgroup1] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN-radio-1] measure-duration 512

# (Fat APs.) Set the measurement duration to 512 TUs.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] measure-duration 512

Related commands

measure

measure-interval

WLAN radio resource measurement commands -- measure-interval

Use measure-interval to set the measurement interval for an AP to send measurement requests to clients.

Use undo measure-interval to restore the default.

Syntax

measure-interval interval

undo measure-interval

Default

ACs:

In radio view, the AP uses the configuration in AP group view.

In AP group radio view, the measurement interval is 30 seconds.

Fat APs:

The measurement interval is 30 seconds.

Views

ACs:

Radio view

AP group radio view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies the measurement interval in the range of 10 to 60 seconds.

Examples

# (ACs.) Set the measurement interval to 35 seconds for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] measure-interval 35

# (ACs.) Set the measurement interval to 35 seconds for APs with model WA4320i-ACN in AP group apgroup1.

<Sysname> system-view

[Sysname] wlan ap-group apgroup1

[Sysname-wlan-ap-group-apgroup1] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN-radio-1] measure-interval 35

# (Fat APs.) Set the measurement interval to 35 seconds.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] measure-interval 35

Related commands

measure

measure-duration

WLAN radio resource measurement commands -- resource-measure

Use resource-measure enable to enable radio resource measurement.

Use resource-measure disable to disable radio resource measurement.

Use undo resource-measure to restore the default.

Syntax

resource-measure { disable | enable }

undo resource-measure

Default

ACs:

In radio view, the AP uses the configuration in AP group view.

In AP group radio view, radio resource measurement is disabled.

Fat APs:

Radio resource measurement is disabled.

Views

ACs:

Radio view

AP group view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When radio measurement is enabled on an AP, the AP sets the Radio Measurement field to 1 in beacons, probe responses, association responses, or reassociation responses. It notifies the clients that they can send measurement requests. These frames also carry measurement capabilities of the AP to inform clients of measurement types that the AP supports.

The AP periodically sends Measurement Pilot frames to help clients fast discover the AP. Measurement Pilot frames are sent more frequently than beacons and carry less information.

Examples

# (ACs.) Enable radio resource measurement for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 2

[Sysname-wlan-ap-ap1-radio-2] resource-measure enable

# (ACs.) Enable radio resource measurement for APs with model WA4320i-ACN in AP group apgroup1.

<Sysname> system-view

[Sysname] wlan ap-group apgroup1

[Sysname-wlan-ap-group-apgroup1] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN-radio-1] resource-measure enable

# (Fat APs.) Enable radio resource measurement.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] resource-measure enable

WLAN radio resource measurement commands -- rm-capability mode

Use rm-capability mode to set the match mode for client radio resource measurement capabilities.

Use undo rm-capability mode to restore the default.

Syntax

rm-capability mode { all | none | partial }

undo rm-capability mode

Default

ACs:

In radio view, the AP uses the configuration in AP group view.

In AP group radio view, the match mode is none for client radio resource measurement capabilities.

Fat APs:

The match mode is none for client radio resource measurement capabilities.

Views

ACs:

Radio view

AP group view

Fat APs:

Radio interface view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies the all mode. A client is allowed to associate with an AP only when all its radio resource measurement capabilities match the AP's radio resource measurement capabilities.

none: Specifies the none mode. The AP does not check client radio resource measurement capabilities.

partial: Specifies the partial mode. A client is allowed to associate with an AP as long as one of its radio resource measurement capabilities matches any of the AP's radio resource measurement capabilities.

Usage guidelines

The configuration takes effect only when radio resource measurement is enabled.

Examples

# (ACs.) Set the match mode to partial for client radio resource measurement capabilities for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 2

[Sysname-wlan-ap-ap1-radio-2] resource-measure enable

[Sysname-wlan-ap-ap1-radio-2] rm-capability mode partial

# (ACs.) Set the match mode to partial for client radio resource measurement capabilities for APs with model WA4320i-ACN in AP group apgroup1.

<Sysname> system-view

[Sysname] wlan ap-group apgroup1

[Sysname-wlan-ap-group-apgroup1] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-apgroup1-ap-model-WA4320i-ACN-radio-1] rm-capability mode partial

# (Fat APs.) Set the match mode to partial for client radio resource measurement capabilities.

<Sysname> system-view

[Sysname] interface wlan-radio 1/0/2

[Sysname-WLAN-Radio1/0/2] rm-capability mode partial

Related commands

resource-measure