Adjacency table probe commands -- IPv4 adjacency table probe commands -- display system internal adj4 entry

Use display system internal adj4 entry to display detailed information about an IPv4 adjacency entry.

Syntax

Centralized devices:

display system internal adj4 entry ip-address interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal adj4 entry ip-address interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal adj4 entry ip-address interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Displays the IPv4 adjacency entry about the specified IP address.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table probe commands -- IPv4 adjacency table probe commands -- display system internal adj4 statistics

Use display system internal adj4 statistics to display IPv4 adjacency entry statistics.

Syntax

Centralized devices:

display system internal adj4 statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal adj4 statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal adj4 statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table probe commands -- IPv4 adjacency table probe commands -- display system internal adjacent-table

Use display system internal adjacent-table to display IPv4 adjacency entries.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal adjacent-table slot slot-number [ cpu cpu-number ] [ count | verbose ]

Distributed devices in IRF mode:

display system internal adjacent-table chassis chassis-number slot slot-number [ cpu cpu-number ] [ count | verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

count: Displays the number of IPv4 adjacency entries.

verbose: Displays detailed IPv4 adjacency entry information. If you do not specify this keyword, the command displays brief IPv4 adjacency entry information.

Adjacency table probe commands -- IPv4 adjacency table probe commands -- reset system internal adj4 statistics

Use reset system internal adj4 statistics to clear IPv4 adjacency entry statistics.

Syntax

Centralized devices:

reset system internal adj4 statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal adj4 statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal adj4 statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table probe commands -- IPv6 adjacency table probe commands -- display system internal adj6 entry

Use display system internal adj6 entry to display detailed information about an IPv6 adjacency entry.

Syntax

Centralized devices:

display system internal adj6 entry ipv6-address interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal adj6 entry ipv6-address interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal adj6 entry ipv6-address interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Displays the IPv6 adjacency entry about the specified IPv6 address.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table probe commands -- IPv6 adjacency table probe commands -- display system internal adj6 statistics

Use display system internal adj6 statistics to display IPv6 adjacency entry statistics.

Syntax

Centralized devices:

display system internal adj6 statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal adj6 statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal adj6 statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table probe commands -- IPv6 adjacency table probe commands -- display system internal ipv6 adjacent-table

Use display system internal ipv6 adjacent-table to display IPv6 adjacency entries.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 adjacent-table slot slot-number [ cpu cpu-number ] [ count | verbose ]

Distributed devices in IRF mode:

display system internal ipv6 adjacent-table chassis chassis-number slot slot-number [ cpu cpu-number ] [ count | verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

count: Displays the number of IPv6 adjacency entries.

verbose: Displays detailed IPv6 adjacency entry information. If you do not specify this keyword, the command displays brief IPv6 adjacency entry information.

Adjacency table probe commands -- IPv6 adjacency table probe commands -- reset system internal adj6 statistics

Use reset system internal adj6 statistics to clear IPv6 adjacency entry statistics.

Syntax

Centralized devices:

reset system internal adj6 statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal adj6 statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal adj6 statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Adjacency table debugging commands -- debugging system internal adj4

Use debugging system internal adj4 to enable IPv4 adjacency table debugging.

Use undo debugging system internal adj4 to disable IPv4 adjacency table debugging.

Syntax

debugging system internal adj4 { hardware | bind | notify | entry }

undo debugging system internal adj4 { hardware | bind | notify | entry }

Default

IPv4 adjacency table debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

hardware: Specifies hardware debugging for the IPv4 adjacency table.

bind: Specifies VN/NHLFE binding debugging for the IPv4 adjacency table.

notify: Specifies notification debugging for VN/NHLFE binding update in the IPv4 adjacency table.

entry: Specifies entry debugging for the IPv4 adjacency table.

Adjacency table debugging commands -- debugging system internal adj6

Use debugging system internal adj6 to enable IPv6 adjacency table debugging.

Use undo debugging system internal adj6 to disable IPv6 adjacency table debugging.

Syntax

debugging system internal adj6 { hardware | bind | notify | entry }

undo debugging system internal adj6 { hardware | bind | notify | entry }

Default

IPv6 adjacency table debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

hardware: Specifies hardware debugging for the IPv6 adjacency table.

bind: Specifies VN/NHLFE binding debugging for the IPv6 adjacency table.

notify: Specifies notification debugging for VN/NHLFE binding update in the IPv6 adjacency table.

entry: Specifies entry debugging for the IPv6 adjacency table.