Object policy probe commands -- display system internal object-policy

Use display system internal object-policy to display configuration information about an object policy.

Syntax

Centralized devices:

display system internal object-policy { ip | ipv6 } object-policy-name

Distributed devices in standalone mode:Centralized IRF devices:

display system internal object-policy { ip | ipv6 } object-policy-name slot slot-number

Distributed devices in IRF mode:

display system internal object-policy { ip | ipv6 } object-policy-name chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ip: Specifies an IPv4 object policy.

ipv6: Specifies an IPv6 object policy.

object-policy-name: Specifies an object policy by its name, a case-insensitive string of 1 to 63 characters.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)