Packet capture probe commands -- display system internal lps

Use display system internal lps to display Linux Packet Socket (LPS) information.

Syntax

Centralized devices:

display system internal lps

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lps [ slot slot-number ]

Distributed devices in IRF mode:

display system internal lps [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays LPS information for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays LPS information for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays LPS information for all member devices if you do not specify a member device. On an IRF 3 system, this command displays LPS information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays LPS information for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays LPS information for all cards if you do not specify a card. On an IRF 3 system, this command displays LPS information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)