IPoE probe commands -- display system internal ip subscriber session

Use display system internal ip subscriber session to display IPv4 IPoE session information.

Syntax

Centralized devices:

display system internal ip subscriber session interface interface-type interface-number { interface-lease | { ip ip-address mask-length | mac mac-address } [ vlan vlan-id [ second-vlan vlan-id ] ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip subscriber session interface interface-type interface-number { interface-lease | { ip ip-address mask-length | mac mac-address } [ vlan vlan-id [ second-vlan vlan-id ] ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip subscriber session interface interface-type interface-number { interface-lease | { ip ip-address mask-length | mac mac-address } [ vlan vlan-id [ second-vlan vlan-id ] ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

ip ip-address mask-length: Specifies a source IP address with a mask length of 1 to 32.

mac mac-address: Specifies a source MAC address, in the format of H-H-H.

interface-lease: Specifies the IPv4 interface-leased user.

vlan vlan-id: Specifies the outer VLAN ID of the user packet, in the range of 1 to 4094. If you do not specify a VLAN ID, this command displays IPv4 IPoE session information for users that do not have VLAN IDs.

second-vlan vlan-id: Specifies the inner VLAN ID of the user packet, in the range of 1 to 4094. If you do not specify an inner VLAN ID, this command displays IPv4 IPoE session information for users that do not have inner VLAN IDs.

slot slot-number: Specifies a card by its slot number. For an Ethernet interface, this command displays the IPv4 IPoE session information stored on the card that contains the interface if you do not specify a card. For an aggregate interface, this command displays the IPv4 IPoE session information stored on the active MPU if you do not specify a card. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. For an Ethernet interface, this command displays the IPv4 IPoE session information stored on the member device that contains the interface if you do not specify a member device. For an aggregate interface, this command displays the IPv4 IPoE session information stored on the master device if you do not specify a member device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. For an Ethernet interface, this command displays the IPv4 IPoE session information stored on the member device or PEX that contains the interface if you do not specify a member device or PEX. For an aggregate interface, this command displays the IPv4 IPoE session information stored on the master device if you do not specify a member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. For an Ethernet interface, this command displays the IPv4 IPoE session information stored on the card that contains the interface if you do not specify a card. For an aggregate interface, this command displays the IPv4 IPoE session information stored on the global active MPU if you do not specify a card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. For an Ethernet interface, this command displays the IPv4 IPoE session information stored on the card or PEX that contains the interface if you do not specify a card or PEX. For an aggregate interface, this command displays the IPv4 IPoE session information stored on the global active MPU if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPoE probe commands -- display system internal ip subscriber statistics

Use display system internal ip subscriber statistics to display IPv4 IPoE user statistics.

Syntax

Centralized devices:

display system internal ip subscriber statistics [ interface interface-type interface-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip subscriber statistics [ interface interface-type interface-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip subscriber statistics [ interface interface-type interface-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays IPv4 IPoE user statistics for all interfaces.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv4 IPoE user statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv4 IPoE user statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays IPv4 IPoE user statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays IPv4 IPoE user statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv4 IPoE user statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays IPv4 IPoE user statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays IPv4 IPoE user statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

(Distributed devices in standalone mode.) If you do not specify any option, this command displays IPv4 IPoE user statistics for the active MPU.

(Centralized IRF devices.) If you do not specify any option, this command displays IPv4 IPoE user statistics for the master device.

(Distributed devices in IRF mode.) If you do not specify any option, this command displays IPv4 IPoE user statistics for the global active MPU.

IPoE probe commands -- display system internal ipv6 subscriber session

Use display system internal ipv6 subscriber session to display IPv6 IPoE session information.

Syntax

Centralized devices:

display system internal ipv6 subscriber session interface interface-type interface-number { interface-lease | { ipv6 ipv6-address prefix-length | mac mac-address } [ vlan vlan-id [second-vlan vlan-id ] ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 subscriber session interface interface-type interface-number { interface-lease | { ipv6 ipv6-address prefix-length | mac mac-address } [ vlan vlan-id [second-vlan vlan-id ] ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 subscriber session interface interface-type interface-number { interface-lease | { ipv6 ipv6-address prefix-length | mac mac-address } [ vlan vlan-id [second-vlan vlan-id ] ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

ipv6 ipv6-address prefix-length: Specifies a source IPv6 address with a prefix length of 1 to 128.

mac mac-address: Specifies a source MAC address, in the format of H-H-H.

interface-lease: Specifies the IPv6 interface-leased user.

vlan vlan-id: Specifies the outer VLAN ID of the user packet, in the range of 1 to 4094. If you do not specify a VLAN ID, this command displays IPv6 IPoE session information for users that do not have VLAN IDs.

second-vlan vlan-id: Specifies the inner VLAN ID of the user packet, in the range of 1 to 4094. If you do not specify an inner VLAN ID, this command displays IPv6 IPoE session information for users that do not have inner VLAN IDs.

slot slot-number: Specifies a card by its slot number. For an Ethernet interface, this command displays the IPv6 IPoE session information stored on the card that contains the interface if you do not specify a card. For an aggregate interface, this command displays the IPv6 IPoE session information stored on the active MPU if you do not specify a card. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. For an Ethernet interface, this command displays the IPv6 IPoE session information stored on the member device that contains the interface if you do not specify a member device. For an aggregate interface, this command displays the IPv6 IPoE session information stored on the master device if you do not specify a member device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. For an Ethernet interface, this command displays the IPv6 IPoE session information stored on the member device or PEX that contains the interface if you do not specify a member device or PEX. For an aggregate interface, this command displays the IPv6 IPoE session information stored on the master device if you do not specify a member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. For an Ethernet interface, this command displays the IPv6 IPoE session information stored on the card that contains the interface if you do not specify a card. For an aggregate interface, this command displays the IPv6 IPoE session information stored on the global active MPU if you do not specify a card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. For an Ethernet interface, this command displays the IPv6 IPoE session information stored on the card or PEX that contains the interface if you do not specify a card or PEX. For an aggregate interface, this command displays the IPv6 IPoE session information stored on the global active MPU if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPoE probe commands -- display system internal ipv6 subscriber statistics

Use display system internal ipv6 subscriber statistics to display IPv6 IPoE user statistics.

Syntax

Centralized devices:

display system internal ipv6 subscriber statistics [ interface interface-type interface-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 subscriber statistics [ interface interface-type interface-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 subscriber statistics [ interface interface-type interface-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays IPv6 IPoE user statistics for all interfaces.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6 IPoE user statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 IPoE user statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays IPv6 IPoE user statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays IPv6 IPoE user statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 IPoE user statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays IPv6 IPoE user statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays IPv6 IPoE user statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

(Distributed devices in standalone mode.) If you do not specify any option, this command displays IPv6 IPoE user statistics for the active MPU.

(Centralized IRF devices.) If you do not specify any option, this command displays IPv6 IPoE user statistics for the master device.

(Distributed devices in IRF mode.) If you do not specify any option, this command displays IPv6 IPoE user statistics for the global active MPU.