OSPF probe commands -- display system internal ospf event-log

| NOTE: Support for this command depends on the device model.

Use display system internal ospf event-log to display OSPF logs.

Syntax

Centralized devices:

display system internal ospf event-log { gr | ha | igp-ls { control | data } | interface | nib | notify | upgrade }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf event-log { gr | igp-ls { control | data } | interface | nib | notify | { ha | upgrade } [ standby slot slot-number [ cpu cpu-number ] ] }

Distributed devices in IRF mode:

display system internal ospf event-log { gr | igp-ls { control | data } | interface | nib | notify | { ha | upgrade } [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ] }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

gr: Displays GR logs.

ha: Displays HA event processing logs.

igp-ls: Displays link state logs.

control: Displays link state control logs.

data: Displays link state data logs.

interface: Displays interface event logs.

nib: Displays NIB logs.

notify: Displays interface notification logs.

upgrade: Displays smooth upgrade logs.

standby slot slot-number: Displays backup OSPF logs for a card. If you do not specify this option, the command displays OSPF logs. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF logs for an IRF member device. If you do not specify this option, the command displays OSPF logs. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF logs for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF logs. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf event-log spf verbose

Use display system internal ospf event-log spf verbose to display detailed route calculation log information.

Syntax

display system internal ospf [ process-id ] event-log spf verbose [ topology topo-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays detailed route calculation log information for all OSPF processes.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you specify the base topology, this command displays information about the base topology. If you do not specify a topology, this command displays information about all topologies. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf flood-list

| NOTE: Support for this command depends on the device model.

Use display system internal ospf flood-list to display OSPF flooding information.

Syntax

display system internal ospf [ process-id ] flood-list [ interface-type interface-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays flooding information for all OSPF processes.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays flooding information for all interfaces.

OSPF probe commands -- display system internal ospf interface

| NOTE: Support for this command depends on the device model.

Use display system internal ospf interface to display OSPF interface information.

Syntax

display system internal ospf interface [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ip-address { mask | mask-length } ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays information about all interfaces.

ip-address: Specifies an IP address in dotted decimal notation.

mask: Specifies the IP address mask in dotted decimal notation.

mask-length: Specifies the mask length, an integer in the range of 0 to 32.

OSPF probe commands -- display system internal ospf interface standby

Use display system internal ospf interface standby to display backup OSPF interface information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] interface [ interface-type interface-number | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] interface [ interface-type interface-number | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays interface information for all OSPF processes.

interface-type interface-number: Specifies an interface by its type and number.

verbose: Displays detailed OSPF interface information.

standby slot slot-number: Displays backup OSPF interface information for a card. If you do not specify this option, the command displays OSPF interface information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF interface information for an IRF member device. If you do not specify this option, the command displays OSPF interface information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF interface information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF interface information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf keychain

Use display system internal ospf keychain to display OSPF keychain information.

Syntax

display system internal ospf keychain [ name keychain-name [ key key-id ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

name keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters. If you do not specify this option, the command displays information about all keychains for an OSPF process.

key key-id: Specifies a key by its ID in the range of 0 to 281474976710655. If you do not specify this option, the command displays information about all keys of the keychain.

OSPF probe commands -- display system internal ospf link-state

Use display system internal ospf link-state to display OSPF link state information.

Syntax

display system internal ospf link-state [ link | node | prefix | statistics ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

link: Displays link information.

node: Displays node information.

prefix: Displays prefix information.

statistics: Displays link state change statistics.

Usage guidelines

If you do not specify any parameters, this command displays link state information for all OSPF processes.

OSPF probe commands -- display system internal ospf lsdb

| NOTE: Support for this command depends on the device model.

Use display system internal ospf lsdb to display OSPF LSA information in the LSDB.

Syntax

display system internal ospf [ process-id ] lsdb { asbr | ase | nssa | summary }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSA information for all OSPF processes.

asbr: Displays Type-4 LSA (ASBR Summary LSA) information in the LSDB.

ase: Displays Type-5 LSA (AS External LSA) information in the LSDB.

nssa: Displays Type-7 LSA (NSSA External LSA) information in the LSDB.

summary: Displays Type-3 LSA (Network Summary LSA) information in the LSDB.

OSPF probe commands -- display system internal ospf lsdb standby

Use display system internal ospf lsdb standby to display backup OSPF LSDB information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] lsdb [ area area-id | brief | [ { asbr | ase | network | nssa | opaque-area | opaque-as | opaque-link | router | summary } [ link-state-id ] ] [ originate-router advertising-router-id | self-originate ] ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] lsdb [ area area-id | brief | [ { asbr | ase | network | nssa | opaque-area | opaque-as | opaque-link | router | summary } [ link-state-id ] ] [ originate-router advertising-router-id | self-originate ] ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSDB information for all OSPF processes.

area area-id: Specifies an OSPF area by its ID, which is an IP address or a decimal integer in the range of 0 to 4294967295 that is translated into the IP address format. If you do not specify this option, the command displays LSDB information for all OSPF areas.

brief: Displays brief LSDB information.

asbr: Displays Type-4 LSA (ASBR Summary LSA) information in the LSDB.

ase: Displays Type-5 LSA (AS External LSA) information in the LSDB.

network: Displays Type-2 LSA (Network LSA) information in the LSDB.

nssa: Displays Type-7 LSA (NSSA External LSA) information in the LSDB.

opaque-area: Displays Type-10 LSA (Opaque-area LSA) information in the LSDB.

opaque-as: Displays Type-11 LSA (Opaque-AS LSA) information in the LSDB.

opaque-link: Displays Type-9 LSA (Opaque-link LSA) information in the LSDB.

router: Displays Type-1 LSA (Router LSA) information in the LSDB.

summary: Displays Type-3 LSA (Network Summary LSA) information in the LSDB.

link-state-id: Specifies a link state ID in the IP address format.

originate-router advertising-router-id: Specifies an advertising router by its ID.

self-originate: Displays information about self-originated LSAs.

standby slot slot-number: Displays backup OSPF LSDB information for a card. If you do not specify this option, the command displays OSPF LSDB information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF LSDB information for an IRF member device. If you do not specify this option, the command displays OSPF LSDB information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF LSDB information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF LSDB information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf nib

| NOTE: Support for this command depends on the device model.

Use display system internal ospf nib to display OSPF next hop information.

Syntax

display system internal ospf nib [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID, a hexadecimal number in the range of 1 to ffffffff.

verbose: Displays detailed OSPF next hop information.

OSPF probe commands -- display system internal ospf peer standby

Use display system internal ospf peer standby to display backup OSPF neighbor information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] peer [ verbose ] [ interface-type interface-number ] [ neighbor-id ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] peer [ verbose ] [ interface-type interface-number ] [ neighbor-id ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays neighbor information for all OSPF processes.

verbose: Displays detailed neighbor information. If you do not specify this keyword, the command displays brief OSPF neighbor information.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays neighbor information for all interfaces.

neighbor-id: Specifies a neighbor router ID. If you do not specify this argument, the command displays all neighbor information.

standby slot slot-number: Displays backup OSPF neighbor information for a card. If you do not specify this option, the command displays OSPF neighbor information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF neighbor information for an IRF member device. If you do not specify this option, the command displays OSPF neighbor information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF neighbor information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF neighbor information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf peer statistics standby

Use display system internal ospf peer statistics standby to display backup OSPF neighbor statistics.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] peer statistics standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] peer statistics standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays neighbor statistics for all OSPF processes.

standby slot slot-number: Displays backup OSPF neighbor statistics for a card. If you do not specify this option, the command displays OSPF neighbor statistics. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF neighbor statistics for an IRF member device. If you do not specify this option, the command displays OSPF neighbor statistics. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF neighbor statistics for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF neighbor statistics. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf prefix

| NOTE: Support for this command depends on the device model.

Use display system internal ospf prefix to display OSPF prefix information.

Syntax

display system internal ospf [ process-id ] prefix [ ip-address { mask | mask-length } ] [ topology topo-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays prefix information for all OSPF processes.

ip-address: Specifies the destination IP address. If you do not specify this argument, the command displays all prefix information.

mask: Specifies the IP address mask in dotted decimal notation.

mask-length: Specifies the mask length, an integer in the range of 0 to 32.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you specify the base topology, this command displays information about the base topology. If you do not specify a topology, this command displays information about all topologies. Support for this option depends on the device model.

OSPF probe commands -- display system internal ospf router

| NOTE: Support for this command depends on the device model.

Use display system internal ospf router to display routing information to router nodes.

Syntax

display system internal ospf [ process-id ] router [ topology topo-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays information about all OSPF processes.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you specify the base topology, this command displays information about the base topology. If you do not specify a topology, this command displays information about all topologies.

OSPF probe commands -- display system internal ospf statistics

| NOTE: Support for this command depends on the device model.

Use display system internal ospf statistics to display OSPF statistics.

Syntax

display system internal ospf [ process-id ] statistics { confusion-log | { request-queue | retrans-queue } [ interface-type interface-number ] [ neighbor-id ] }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays statistics for all OSPF processes.

confusion-log: Specifies router ID conflict and IP address conflict statistics.

request-queue: Specifies request queue statistics.

retrans-queue: Specifies retransmission queue statistics.

interface-type interface-number: Specifies an interface by its type and number.

neighbor-id: Specifies a neighbor by its ID.

OSPF probe commands -- display system internal ospf status

| NOTE: Support for this command depends on the device model.

Use display system internal ospf status to display OSPF status information.

Syntax

display system internal ospf status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

OSPF probe commands -- display system internal ospf vlink standby

Use display system internal ospf vlink standby to display backup OSPF virtual link information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ospf [ process-id ] vlink standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ospf [ process-id ] vlink standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an OSPF process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays virtual link information for all OSPF processes.

standby slot slot-number: Displays backup OSPF virtual link information for a card. If you do not specify this option, the command displays OSPF virtual link information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup OSPF virtual link information for an IRF member device. If you do not specify this option, the command displays OSPF virtual link information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup OSPF virtual link information for a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays OSPF virtual link information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.

OSPF probe commands -- reset system internal ospf event-log

| NOTE: Support for this command depends on the device model.

Use reset system internal ospf event-log to clear OSPF logs.

Syntax

reset system internal ospf event-log { igp-ls { control | data } | interface | nib | notify }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

igp-ls: Clears link state logs.

control: Clears link state control logs.

data: Clears link state data logs.

interface: Clears interface event logs.

nib: Clears NIB logs.

notify: Clears interface notification logs.

OSPF probe commands -- reset system internal ospf link-state statistics

Use reset system internal ospf link-state statistics to clear OSPF link state statistics.

Syntax

reset system internal ospf link-state statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin