TRILL probe commands -- debugging system internal trill adjacent-table

Use debugging system internal trill adjacent-table to enable TRILL adjacency table debugging.

Use undo debugging system internal trill adjacent-table to disable TRILL adjacency table debugging.

Syntax

debugging system internal trill adjacent-table { all | hardware | message | notify }

undo debugging system internal trill adjacent-table { all | hardware | message | notify }

Default

TRILL adjacency table debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for the TRILL adjacency table.

hardware: Enables hardware debugging for the TRILL adjacency table.

message: Enables message debugging for the TRILL adjacency table.

notify: Enables notification debugging for the TRILL adjacency table.

TRILL probe commands -- debugging system internal trill fib

Use debugging system internal trill fib to enable TRILL unicast FIB debugging.

Use undo debugging system internal trill fib to disable TRILL unicast FIB debugging.

Syntax

debugging system internal trill fib { all | bind | hardware | message }

undo debugging system internal trill fib { all | bind | hardware | message }

Default

TRILL unicast FIB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for the TRILL unicast FIB.

bind: Enables binding debugging for the TRILL unicast FIB.

hardware: Enables hardware debugging for the TRILL unicast FIB.

message: Enables message debugging for the TRILL unicast FIB.

TRILL probe commands -- debugging system internal trill management

Use debugging system internal trill management to enable TRILL management debugging.

Use undo debugging system internal trill management to disable TRILL management debugging.

Syntax

debugging system internal trill management { all | hardware | message }

undo debugging system internal trill management { all | hardware | message }

Default

TRILL management debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for TRILL management.

hardware: Enables hardware debugging for TRILL management.

message: Enables message debugging for TRILL management.

TRILL probe commands -- debugging system internal trill mfib

Use debugging system internal trill mfib to enable TRILL multicast FIB debugging.

Use undo debugging system internal trill mfib to disable TRILL multicast FIB debugging.

Syntax

debugging system internal trill mfib { all | hardware | message }

undo debugging system internal trill mfib { all | hardware | message }

Default

TRILL multicast FIB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for the TRILL multicast FIB.

hardware: Enables hardware debugging for the TRILL multicast FIB.

message: Enables message debugging for the TRILL multicast FIB.

TRILL probe commands -- debugging system internal trill vn

Use debugging system internal trill vn to enable TRILL virtual nexthop (VN) entry debugging.

Use undo debugging system internal trill vn to disable TRILL VN entry debugging.

Syntax

debugging system internal trill vn { all | bind | hardware | message | notify }

undo debugging system internal trill vn { all | bind | hardware | message | notify }

Default

TRILL VN entry debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for TRILL VN entries.

bind: Enables binding debugging for TRILL VN entries.

hardware: Enables hardware debugging for TRILL VN entries.

message: Enables message debugging for TRILL VN entries.

notify: Enables notification debugging for TRILL VN entries.

TRILL probe commands -- debugging system internal trill vr-adjacent-table

Use debugging system internal trill vr-adjacent-table to enable TRILL virtual router (VR) adjacency table debugging.

Use undo debugging system internal trill vr-adjacent-table to disable TRILL VR adjacency table debugging.

Syntax

debugging system internal trill vr-adjacent-table { all | hardware | message | notify }

undo debugging system internal trill vr-adjacent-table { all | hardware | message | notify }

Default

TRILL VR adjacency table debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for the TRILL VR adjacency table.

hardware: Enables hardware debugging for the TRILL VR adjacency table.

message: Enables message debugging for the TRILL VR adjacency table.

notify: Enables notification debugging for the TRILL VR adjacency table.

TRILL probe commands -- debugging system internal trill vr-fib

Use debugging system internal trill vr-fib to enable TRILL VR unicast FIB debugging.

Use undo debugging system internal trill vr-fib to disable TRILL VR unicast FIB debugging.

Syntax

debugging system internal trill vr-fib { all | bind | hardware | message }

undo debugging system internal trill vr-fib { all | bind | hardware | message }

Default

TRILL VR unicast FIB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for the TRILL VR unicast FIB.

hardware: Enables hardware debugging for the TRILL VR unicast FIB.

message: Enables message debugging for the TRILL VR unicast FIB.

notify: Enables notification debugging for the TRILL VR unicast FIB.

TRILL probe commands -- debugging system internal trill vr-vn

Use debugging system internal trill vr-vn to enable TRILL VR VN entry debugging.

Use undo debugging system internal trill vr-vn to disable TRILL VR VN entry debugging.

Syntax

debugging system internal trill vr-vn { all | bind | hardware | message | notify }

undo debugging system internal trill vr-vn { all | bind | hardware | message | notify }

Default

TRILL VR VN entry debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for TRILL VR VN entries.

bind: Enables binding debugging for TRILL VR VN entries.

hardware: Enables hardware debugging for TRILL VR VN entries.

message: Enables message debugging for TRILL VR VN entries.

notify: Enables notification debugging for TRILL VR VN entries.

TRILL probe commands -- display system internal trill adjacent-table

Use display system internal trill adjacent-table to display the TRILL adjacency table.

Syntax

Centralized devices:

display system internal trill adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] | statistics ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] | statistics ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] | statistics ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of adjacency entries.

next-hop nickname interface interface-type interface-number: Specifies an interface of a next-hop RB. The nickname argument specifies the next-hop RB by its nickname, a hexadecimal number in the range of 1 to fffe. The interface-type interface-number argument specifies the interface by its type and number.

reference: Displays information about the references between VNs and adjacency entries.

statistics: Displays statistics.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, this command displays all TRILL adjacency entries.

TRILL probe commands -- display system internal trill fib

Use display system internal trill fib to display the TRILL unicast FIB information.

Syntax

Centralized devices:

display system internal trill fib [ count | nickname nickname | running | statistics ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill fib [ count | nickname nickname | running | statistics ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill fib [ count | nickname nickname | running | statistics ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of unicast FIB entries.

nickname nickname: Specifies an RB by its nickname, a hexadecimal number in the range of 1 to fffe.

running: Displays the running information.

statistics: Displays statistics.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, this command displays all TRILL unicast FIB entries.

TRILL probe commands -- display system internal trill management

Use display system internal trill management to display the TRILL management information.

Syntax

Centralized devices:

display system internal trill management [ interface interface-type interface-number | statistics ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill management [ interface interface-type interface-number | statistics ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill management [ interface interface-type interface-number | statistics ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

statistics: Displays statistics.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, this command displays the global information of TRILL management.

TRILL probe commands -- display system internal trill mfib

Use display system internal trill mfib to display the TRILL multicast FIB (MFIB) information.

Syntax

Centralized devices:

display system internal trill mfib statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill mfib statistics slot slot-number [ cpu cpu-number ]

display system internal trill mfib [ ingress [ vlan vlan-id [ local-entry | remote-entry ] ] | transit [ nickname nickname [ prune-entry | rpf-entry | vlan vlan-id [ mac mac-address ] ] ] ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal trill mfib statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

display system internal trill mfib [ ingress [ vlan vlan-id [ local-entry | remote-entry ] ] | transit [ nickname nickname [ prune-entry | rpf-entry | vlan vlan-id [ mac mac-address ] ] ] ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

statistics: Displays statistics.

ingress: Specifies ingress entries.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

local-entry: Specifies local entries.

remote-entry: Specifies remote entries.

transit: Specifies transit entries.

nickname nickname: Specifies an RB by its nickname, a hexadecimal number in the range of 1 to fffe.

prune-entry: Specifies prune entries.

rpf-entry: Specifies RPF entries.

mac mac-address: Specifies a MAC address.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information for all member devices.. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays information for all member devices if you do not specify a member device. On an IRF 3 system, this command displays information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays information for all cards if you do not specify a card. On an IRF 3 system, this command displays information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, this command displays all TRILL multicast FIB entries.

TRILL probe commands -- display system internal trill port-group

Use display system internal trill port-group to display TRILL port group information.

Syntax

display system internal trill port-group

Views

Probe view

Predefined user roles

network-admin

mdc-admin

TRILL probe commands -- display system internal trill statistics

Use display system internal trill statistics to display the total number of flushed TRILL routing entries.

Syntax

display system internal trill statistics { multicast-route | unicast-route }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

multicast-route: Specifies TRILL multicast routing entries.

unicast-route: Specifies TRILL unicast routing entries.

TRILL probe commands -- display system internal trill status

Use display system internal trill status to display the status of the TRILL protocol processes.

Syntax

display system internal trill status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

TRILL probe commands -- display system internal trill vn

Use display system internal trill vn to display the TRILL VN entry information.

Syntax

Centralized devices:

display system internal trill vn [ count | vnid vn-id [ next-hop nickname | reference ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vn [ count | vnid vn-id [ next-hop nickname | reference ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vn [ count | vnid vn-id [ next-hop nickname | reference ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of VN entries.

vnid vn-id: Specifies a VN entry by its ID, a hexadecimal number in the range of 0 to ffffffff.

next-hop nickname: Specifies a next-hop RB by its nickname, a hexadecimal number in the range of 1 to fffe.

reference: Displays information about TRILL VN entry referencing.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, this command displays all TRILL VN entries.

TRILL probe commands -- display system internal trill vr

Use display system internal trill vr to display TRILL VR information.

Syntax

Centralized devices:

display system internal trill vr [ ipv6 ] [ count | interface interface-type interface-number vrid vr-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vr [ ipv6 ] [ count | interface interface-type interface-number vrid vr-id ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vr [ ipv6 ] [ count | interface interface-type interface-number vrid vr-id ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6: Displays IPv6 TRILL VR information. If you do not specify this keyword, the command displays IPv4 TRILL VR information.

count: Displays the number of entries.

interface interface-type interface-number vrid vr-id: Specifies a VR on an interface. The interface-type interface-number argument specifies the interface by its type and number. The vr-id argument specifies the VR by its ID in the range of 1 to 255.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, the command displays all TRILL VR information.

TRILL probe commands -- display system internal trill vr-adjacent-table

Use display system internal trill vr-adjacent-table to display the TRILL VR adjacency table.

Syntax

Centralized devices:

display system internal trill vr-adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vr-adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vr-adjacent-table [ count | next-hop nickname interface interface-type interface-number [ reference ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of entries.

next-hop nickname interface interface-type interface-number: Specifies an interface of a next-hop RB. The nickname argument specifies the next-hop RB by its nickname, a hexadecimal number in the range of 1 to fffe. The interface-type interface-number argument specifies the interface by its type and number.

reference: Displays information about the references between VR adjacency entries and VR VN entries.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, the command displays information about all TRILL VR adjacency entries.

TRILL probe commands -- display system internal trill vr-fib

Use display system internal trill vr-fib to display the TRILL VR unicast FIB.

Syntax

Centralized devices:

display system internal trill vr-fib [ count | mac mac-address vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vr-fib [ count | mac mac-address vlan vlan-id ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vr-fib [ count | mac mac-address vlan vlan-id ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of entries.

mac mac-address vlan vlan-id: Specifies a MAC address in a VLAN. The mac-address argument specifies the MAC address. The vlan-id argument specifies the VLAN by its ID in the range of 1 to 4094.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, the command displays information about all TRILL VR unicast FIB entries.

TRILL probe commands -- display system internal trill vr-vlan

Use display system internal trill vr-vlan to display information about VLANs enabled with TRILL VRs.

Syntax

Centralized devices:

display system internal trill vr-vlan

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vr-vlan slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vr-vlan chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

TRILL probe commands -- display system internal trill vr-vn

Use display system internal trill vr-vn to display the TRILL VR VN entries.

Syntax

Centralized devices:

display system internal trill vr-vn [ count | vnid vn-id [ next-hop nickname | reference ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal trill vr-vn [ count | vnid vn-id [ next-hop nickname | reference ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal trill vr-vn [ count | vnid vn-id [ next-hop nickname | reference ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays the number of entries.

vnid vn-id: Specifies a VR VN entry by its ID, a hexadecimal number in the range of 0 to ffffffff. If you do not specify this option, the command displays all VR VN entries.

next-hop nickname: Specifies a next-hop RB by its nickname, a hexadecimal number in the range of 1 to fffe. If you do not specify this option, the command displays information about all next-hop RBs.

reference: Displays information about TRILL VR VN entry referencing.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If no parameter is specified, the command displays information about all TRILL VR VN entries.

TRILL probe commands -- reset system internal trill adjacent-table statistics

Use reset system internal trill adjacent-table statistics to clear the TRILL adjacency table statistics.

Syntax

Centralized devices:

reset system internal trill adjacent-table statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal trill adjacent-table statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal trill adjacent-table statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

TRILL probe commands -- reset system internal trill fib statistics

Use reset system internal trill fib statistics to clear the TRILL unicast FIB statistics.

Syntax

Centralized devices:

reset system internal trill fib statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal trill fib statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal trill fib statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

TRILL probe commands -- reset system internal trill management statistics

Use reset system internal trill management statistics to clear the TRILL management statistics.

Syntax

Centralized devices:

reset system internal trill management statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal trill management statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal trill management statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

TRILL probe commands -- reset system internal trill mfib statistics

Use reset system internal trill mfib statistics to clear the TRILL multicast FIB statistics.

Syntax

Centralized devices:

reset system internal trill mfib statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal trill mfib statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal trill mfib statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

TRILL probe commands -- reset system internal trill statistics

Use reset system internal trill statistics to clear statistics about flushed TRILL routing entries.

Syntax

reset system internal trill statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Use this command to clear statistics about flushed TRILL routing entries when the total number of the entries reaches 4294967295.