IPv6 fast forwarding probe commands -- display system internal ipv6 fast-forwarding cache verbose

Use display system internal ipv6 fast-forwarding cache verbose to display detailed information about the IPv6 fast forwarding table.

Syntax

Centralized devices:

display system internal ipv6 fast-forwarding cache [ ipv6-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 fast-forwarding cache [ ipv6-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 fast-forwarding cache [ ipv6-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Displays IPv6 fast forwarding entries for the specified IPv6 address.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about the IPv6 fast forwarding table for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about the IPv6 fast forwarding table for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about the IPv6 fast forwarding table for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about the IPv6 fast forwarding table for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about the IPv6 fast forwarding table for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPv6 fast forwarding probe commands -- display system internal ipv6 fast-forwarding service-information

Use display system internal ipv6 fast-forwarding service-information to display service module IPv6 registration information in the fast forwarding module.

Syntax

display system internal ipv6 fast-forwarding service-information

View

Probe view

Predefined user roles

network-admin

mdc-admin

IPv6 fast forwarding probe commands -- display system internal ipv6 max-ecmp-num

Use display system internal ipv6 max-ecmp-num to display the maximum number of IPv6 ECMP routes.

Syntax

Centralized devices:

display system internal ipv6 max-ecmp-num [ slot slot-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 max-ecmp-num [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 max-ecmp-num [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined use rules

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command display the maximum number of IPv6 ECMP routes for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command display the maximum number of IPv6 ECMP routes for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command display the maximum number of IPv6 ECMP routes for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the maximum number of IPv6 ECMP routes for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays the maximum number of IPv6 ECMP routes for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPv6 fast forwarding probe commands -- display system internal ipv6 fast-forwarding statistics

Use display system internal ipv6 fast-forwarding statistics to display IPv6 fast forwarding statistics.

Syntax

Centralized devices:

display system internal ipv6 fast-forwarding statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 fast-forwarding statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 fast-forwarding statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6 fast forwarding statistics for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 fast forwarding statistics for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPv6 fast forwarding statistics for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 fast forwarding statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPv6 fast forwarding statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPv6 fast forwarding probe commands -- reset system internal ipv6 fast-forwarding statistics

Use reset system internal ipv6 fast-forwarding statistics to clear IPv6 fast forwarding statistics.

Syntax

Centralized devices:

reset system internal ipv6 fast-forwarding statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 fast-forwarding statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ipv6 fast-forwarding statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears IPv6 fast forwarding statistics for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify an IRF member device, this command clears IPv6 fast forwarding statistics for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command clears IPv6 fast forwarding statistics for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears IPv6 fast forwarding statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command clears IPv6 fast forwarding statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.