License management probe commands -- display system internal license buffer-data

Use display system internal license buffer-data to display buffered license data.

Syntax

Centralized devices:

display system internal license buffer-data

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license buffer-data slot slot-number

Distributed devices in IRF mode:

display system internal license buffer-data chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- display system internal license feature-set

Use display system internal license feature-set to display information about supported feature sets.

Syntax

Centralized devices:

display system internal license feature-set

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license feature-set slot slot-number

Distributed devices in IRF mode:

display system internal license feature-set chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- display system internal license fifo

Use display system internal license fifo to display information about FIFO pipes used by licenses.

Syntax

Centralized devices:

display system internal license fifo

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license fifo slot slot-number

Distributed devices in IRF mode:

display system internal license fifo chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- display system internal license lipc

Use display system internal license lipc to display LIPC information for license registration. License LIPC is used for the communication between the license module and the LIPC module.

Syntax

Centralized devices:

display system internal license lipc

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license lipc slot slot-number

Distributed devices in IRF mode:

display system internal license lipc chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- display system internal license lipc hash

Use display system internal license lipc hash to display LIPC information in the hash list for license registration.

Syntax

Centralized devices:

display system internal license lipc hash

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license lipc hash slot slot-number

Distributed devices in IRF mode:

display system internal license lipc hash chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- display system internal license lmi-paa

Use display system internal license lmi-paa to display license manage item (LMI) information and product ability aggregate (PAA) information.

Syntax

Centralized devices:

display system internal license lmi-paa

Distributed devices in standalone mode:Centralized IRF devices:

display system internal license lmi-paa slot slot-number

Distributed devices in IRF mode:

display system internal license lmi-paa chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

License management probe commands -- license check-timer

Use license check-timer to set a check timer for license validity.

Syntax

Centralized devices:

license check-timer interval-value

Distributed devices in standalone mode:Centralized IRF devices:

license check-timer interval-value slot slot-number

Distributed devices in IRF mode:

license check-timer interval-value chassis chassis-number slot slot-number

Default

The check timer for license validity is 86400 seconds (24 hours).

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interval-value: Specifies the check timer for license validity, in seconds. The value range is 10 to 864000. As a best practice, set a value larger than 60 seconds. A timer shorter than 60 seconds might degrade system performance.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

Usage guidelines

A license is valid for a time period in days. The device checks the license for validity at the check interval. If the license does not expire, the device decreases the validity period by 1 day. If the license has expired, the device marks the license as expired.

The setting cannot survive a reboot because it is not saved to the configuration file.

Use this command only for internal tests. By default, the timer is set to the highest value. Changing the setting will cause your license to expire before the expiration date.

License management probe commands -- license file-timer

Use license check-timer to set a check timer for license file availability.

Syntax

Centralized devices:

license file-timer interval-value

Distributed devices in standalone mode:Centralized IRF devices:

license file-timer interval-value slot slot-number

Distributed devices in IRF mode:

license file-timer interval-value chassis chassis-number slot slot-number

Default

The check timer for license file availability is 1800 seconds (30 minutes).

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interval-value: Specifies the check timer for license file availability, in seconds. The value range is 10 to 864000. As a best practice, set a value larger than 60 seconds. A short checker might degrade system performance.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

Usage guidelines

After the device starts up, the system automatically starts the license processes and checks the availability of license files. If a license file is not available, its license file check timer starts. The device periodically checks the file for file recovery. When the license file is recovered, the system deletes the timer.

The setting cannot survive a reboot because it is not saved to the configuration file.