Flow log probe commands -- display system internal userlog mbuf dump

| NOTE: Support for this command depends on the device model.

Use display system internal userlog mbuf dump to display the contents of flow log UDP packets.

Syntax

Centralized devices:

display system internal userlog mbuf dump count number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal userlog mbuf dump count number [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal userlog mbuf dump count number [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count number: Specifies the number of UDP packets to be displayed. The value range for the number argument is 1 to 100.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the contents for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the contents for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the contents for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the contents for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays the contents for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Flow log probe commands -- display system internal userlog statistic

| NOTE: Support for this command depends on the device model.

Use display system internal userlog statistic to display running statistics for the flow log module (USERLOG).

Syntax

Centralized devices:

display system internal userlog statistic

Distributed devices in standalone mode:Centralized IRF devices:

display system internal userlog statistic [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal userlog statistic [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the statistics for the module on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the statistics for the module on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the statistics for the module on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the statistics for the module on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays the statistics for the module on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Flow log probe commands -- display system internal userlog test

| NOTE: Support for this command depends on the device model.

Use display system internal userlog test to test the flow log module and display the test result.

Syntax

Centralized devices:

display system internal userlog test count number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal userlog test count number [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal userlog test count number [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count number: Specifies the number of test packets to be sent. The value range for the number argument is 1 to 3000.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, the test is performed on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, the test is performed on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, the test is performed on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, the test is performed on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, the test is performed on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.