IPv6 policy-based routing probe commands -- display system internal ipv6 pbr fib

Use display system internal ipv6 pbr fib to display next hop information in user mode.

Syntax

Centralized devices:

display system internal ipv6 pbr fib [ vpn-instance vpn-instance-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pbr slot slot-number [ cpu cpu-number ] fib [ vpn-instance vpn-instance-name ]

Distributed devices in IRF mode:

display system internal ipv6 pbr chassis chassis-number slot slot-number [ cpu cpu-number ] fib [ vpn-instance vpn-instance-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. The specified VPN must already exist. If you do not specify a VPN instance, the command displays information about next hops belonging to the public network.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPv6 policy-based routing probe commands -- display system internal ipv6 pbr kernel policy

Use display system internal ipv6 pbr kernel policy to display IPv6 PBR policy information in kernel mode.

Syntax

Centralized devices:

display system internal ipv6 pbr kernel policy [ policy-name [ setup ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pbr slot slot-number [ cpu cpu-number ] kernel policy [ policy-name [ setup ] ]

Distributed devices in IRF mode:

display system internal ipv6 pbr chassis chassis-number slot slot-number [ cpu cpu-number ] kernel policy [ policy-name [ setup ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

policy policy-name: Specifies a policy by its name, a case-sensitive string of 1 to 19 characters.

setup: Displays information about the specified IPv6 PBR policy applied to an interface.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPv6 policy-based routing probe commands -- display system internal ipv6 pbr policy

Use display system internal ipv6 pbr policy to display IPv6 PBR policy information in user mode.

Syntax

Centralized devices:

display system internal ipv6 pbr policy [ policy-name [ setup ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pbr slot slot-number [ cpu cpu-number ] policy [ policy-name [ setup ] ]

Distributed devices in IRF mode:

display system internal ipv6 pbr chassis chassis-number slot slot-number [ cpu cpu-number ] policy [ policy-name [ setup ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

policy policy-name: Specifies a policy by its name, a case-sensitive string of 1 to 19 characters.

setup: Displays information about the specified IPv6 PBR policy applied to an interface.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.