IS-IS commands -- address-family ipv4

Use address-family ipv4 to create the IS-IS IPv4 address family and enter its view.

Use undo address-family ipv4 to delete the IS-IS IPv4 address family and all configurations in the view.

Syntax

address-family ipv4 [ unicast ]

undo address-family ipv4 [ unicast ]

Default

No IS-IS IPv4 address family exists.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

unicast: Specifies the unicast address family (the default).

Examples

# Create the IS-IS IPv4 address family and enter its view.

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv4

[Sysname-isis-100-ipv4]

IS-IS commands -- address-family ipv6

Use address-family ipv6 to create the IS-IS IPv6 address family and enter its view.

Use undo address-family ipv6 to remove the IS-IS IPv6 address family and all configurations in the view.

Syntax

address-family ipv6 [ unicast ]

undo address-family ipv6 [ unicast ]

Default

No IS-IS IPv6 address family exists.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

unicast: Specifies the unicast address family (the default).

Usage guidelines

This command enables IPv6 for an IS-IS process.

Examples

# Create the IS-IS IPv6 address family and enter its view.

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv6

[Sysname-isis-100-ipv6]

IS-IS commands -- area-authentication send-only

Use area-authentication send-only to configure IS-IS not to check the authentication information in the received Level-1 packets, including LSPs, CSNPs, and PSNPs.

Use undo area-authentication send-only to restore the default.

Syntax

area-authentication send-only

undo area-authentication send-only

Default

When area authentication mode and key are configured, a Level-1 or Level-1-2 router checks the authentication information in the received packets.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When area authentication mode and key are configured, a Level-1 or Level-1-2 router adds the key in the specified mode into transmitted Level-1 packets (including LSPs, CSNPs, and PSNPs). It also checks the key in the received Level-1 packets.

To prevent packet exchange failure in case of an authentication key change, configure IS-IS not to check the authentication information in the received packets.

Examples

# Configure IS-IS not to check the authentication information in the received packets.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] area-authentication send-only

Related commands

area-authentication-mode

domain-authentication send-only

isis authentication send-only

IS-IS commands -- area-authentication-mode

Use area-authentication-mode to specify an area authentication mode and a key.

Use undo area-authentication-mode to restore the default.

Syntax

area-authentication-mode { { gca key-id { hmac-sha-1 | hmac-sha-224 | hmac-sha-256 | hmac-sha-384 | hmac-sha-512 } [ nonstandard ] | md5 | simple } { cipher | plain } string | keychain keychain-name } [ ip | osi ]

undo area-authentication-mode

Default

No area authentication mode or key is configured.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

gca: Specifies the Generic Cryptographic Authentication (GCA) mode.

key-id: Uniquely identifies an SA in the range of 1 to 65535. The sender inserts the Key ID into the authentication TLV, and the receiver authenticates the packet by using the SA that is selected based on the Key ID.

hmac-sha-1: Specifies the HMAC-SHA-1 algorithm.

hmac-sha-224: Specifies the HMAC-SHA-224 algorithm.

hmac-sha-256: Specifies the HMAC-SHA-256 algorithm.

hmac-sha-384: Specifies the HMAC-SHA-384 algorithm.

hmac-sha-512: Specifies the HMAC-SHA-512 algorithm.

nonstandard: Specifies the nonstandard GCA mode.

md5: Specifies the MD5 authentication mode.

simple: Specifies the simple authentication mode.

cipher: Specifies a key in encrypted form.

plain: Specifies a key in plaintext form. For security purposes, the key specified in plaintext form will be stored in encrypted form.

string: Specifies the key. Its plaintext form is a case-sensitive string of 1 to 16 characters. Its encrypted form is a case-sensitive string of 33 to 53 characters.

keychain: Specifies the keychain authentication mode.

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters.

ip: Checks IP-related fields in LSPs.

osi: Checks OSI-related fields in LSPs.

Usage guidelines

Area authentication enables IS-IS to discard routes from untrusted routers.

The key in the specified mode is inserted into all outbound Level-1 packets (LSP, CSNP, and PSNP) and is used to authenticate inbound Level-1 packets.

IS-IS keychain authentication can operate correctly only when the keys in the keychain use the HMAC-MD5 authentication algorithm.

· Before IS-IS sends a Level-1 packet, it uses the valid send key obtained from the keychain to authenticate the packet. If no valid send key exists or the valid send key does not use the HMAC-MD5 algorithm, the authentication fails and the packet does not contain authentication information.

· After IS-IS receives a Level-1 packet, it uses a valid accept key obtained from the keychain to authenticate the packet. If no valid accept key exists or all valid accept keys fail to authenticate the packet, the authentication fails and the packet is discarded.

Routers in an area must have the same authentication mode and key.

If neither ip nor osi is specified, OSI-related fields are checked.

When you specify the GCA mode, follow these guidelines:

· If you do not specify the nonstandard keyword, the device can communicate only with devices that use the GCA mode.

· If you specify the nonstandard keyword, the device can communicate only with devices that use the nonstandard GCA mode.

Examples

# Set the area authentication mode to simple, and set the plaintext key to 123456.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] area-authentication-mode simple plain 123456

Related commands

area-authentication send-only

domain-authentication-mode

isis authentication-mode

IS-IS commands -- auto-cost enable

Use auto-cost enable to enable automatic link cost calculation.

Use undo auto-cost enable to disable automatic link cost calculation.

Syntax

auto-cost enable

undo auto-cost enable

Default

Automatic link cost calculation is disabled.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

After automatic link cost calculation is enabled, the link cost is automatically calculated based on the bandwidth reference value of an interface. When the cost-style is wide or wide-compatible, the cost value of an interface is calculated by using the following formula: Cost = (Reference bandwidth value / Link bandwidth) ?10. For other cost styles, Table 1 applies.

Table 1 Automatic cost calculation scheme for cost styles other than wide and wide-compatible

Interface bandwidth | Cost
≤10 Mbps | 60
≤100 Mbps | 50
≤155 Mbps | 40
≤622 Mbps | 30
≤2500 Mbps | 20
>2500 Mbps | 10

Examples

# Enable automatic link cost calculation for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] auto-cost enable

Related commands

bandwidth-reference

cost-style

isis cost

isis ipv6 cost

IS-IS commands -- bandwidth-reference

Use bandwidth-reference to set the bandwidth reference value for automatic link cost calculation.

Use undo bandwidth-reference to restore the default.

Syntax

bandwidth-reference value

undo bandwidth-reference

Default

The bandwidth reference value is 100 Mbps.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies the bandwidth reference value in the range of 1 to 2147483648 Mbps.

Examples

# Set the bandwidth reference of IS-IS process 1 to 200 Mbps.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] bandwidth-reference 200

Related commands

auto-cost enable

isis cost

IS-IS commands -- circuit-cost

Use circuit-cost to set a global IS-IS link cost.

Use undo circuit-cost to remove the configuration.

Syntax

circuit-cost cost-value [ level-1 | level-2 ]

undo circuit-cost [ level-1 | level-2 ]

Default

No global link cost is configured.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

cost-value: Specifies the link cost value. The value range varies by cost style.

· For styles narrow, narrow-compatible, and compatible, the cost value is in the range of 0 to 63.

· For styles wide and wide-compatible, the cost value is in the range of 0 to 16777215.

level-1: Applies the link cost to Level-1.

level-2: Applies the link cost to Level-2.

Usage guidelines

If no level is specified, the specified cost applies to both Level-1 and Level-2.

Examples

# Set the global Level-1 link cost to 11 for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] circuit-cost 11 level-1

Related commands

cost-style

isis cost

IS-IS commands -- cost-style

Use cost-style to set a cost style.

Use undo cost-style to restore the default.

Syntax

cost-style { narrow | wide | wide-compatible | { compatible | narrow-compatible } [ relax-spf-limit ] }

undo cost-style

Default

The IS-IS cost style is narrow.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

narrow: Receives and sends only narrow cost style packets. The narrow cost is in the range of 0 to 63.

wide: Receives and sends only wide cost style packets. The wide cost is in the range of 0 to 16777215.

compatible: Receives and sends both wide and narrow cost style packets.

narrow-compatible: Receives both narrow and wide cost style packets, but sends only narrow cost style packets.

wide-compatible: Receives both narrow and wide cost style packets, but sends only wide cost style packets.

relax-spf-limit: Allows receiving routes with a cost greater than 1023. If you do not specify this keyword, routes with a cost bigger than 1023 will be discarded. This keyword is available only when compatible or narrow-compatible is used.

Examples

# Configure the router to send only narrow cost style packets, but receive both narrow and wide cost style packets.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] cost-style narrow-compatible

Related commands

circuit-cost

isis cost

IS-IS commands -- default-route-advertise

Use default-route-advertise to advertise a default route of 0.0.0.0/0.

Use undo default-route-advertise to restore the default.

Syntax

default-route-advertise [ avoid-learning | [ level-1 | level-1-2 | level-2 ] | route-policy route-policy-name | tag tag ] *

undo default-route-advertise

Default

Default route advertisement is disabled.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

avoid-learning: Avoids learning the default route received in LSPs or generated by using the ATT bit to avoid routing loops.

level-1: Advertises a Level-1 default route.

level-1-2: Advertises both Level-1 and Level-2 default routes.

level-2: Advertises a Level-2 default route.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

tag tag: Specifies the tag value for the default route, in the range of 1 to 4294967295.

Usage guidelines

If no level is specified, a Level-2 default route is advertised.

The Level-1 default route is advertised to other routers in the same area, and the Level-2 default route is advertised to all the Level-2 and Level-1-2 routers.

You can use a routing policy to specify a level for the default route. The apply isis level-1 command in routing policy view can generate a Level-1 default route. The apply isis level-2 command in routing policy view can generate a Level-2 default route. The apply isis level-1-2 command in routing policy view can generate both a Level-1 default route and Level-2 default route.

The tag value specified in the routing policy takes precedence over the tag value specified in this command.

Examples

# Configure IS-IS process 1 to advertise a Level-2 default route.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] default-route-advertise

IS-IS commands -- display isis

Use display isis to display configuration information for an IS-IS process.

Syntax

display isis [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

process-id: Specifies a process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays configuration information for all IS-IS processes.

Examples

# Display IS-IS configuration information.

<Sysname> display isis

IS-IS(1) Protocol Information

Network-entity : 10.0000.0000.0001.00

IS-level : level-1-2

Cost-style : Wide

Fast reroute : Disabled

Preference : 15

LSP-length receive : 1497

LSP-length originate

level-1 : 1497

level-2 : 1497

Maximum imported routes : 1000

Timers

LSP-max-age : 1200

LSP-refresh : 900

SPF intervals : 5 50 200

IPv6 enabled

Multi-topology : Standard

Fast reroute : Disabled

Preference : 15

Maximum imported routes : 1000

SPF intervals : 5 50 200

IPv4-Unicast

Topology red

Topology ID : 6

Preference : 15

Maximum imported routes : 1000000

SPF intervals : 5 50 200

Overload status : Overloaded manually

Table 2 Command output

Field | Description
Network-entity | Network entity name.
IS-level | IS-IS routing level.
Cost-style | Cost style.
Fast-reroute | IS-IS FRR status: · Disabled—IS-IS FRR is disabled. · LFA—IS-IS FRR automatically calculates a backup next hop. · Route-policy—IS-IS FRR specifies a backup next hop by using a routing policy.
Preference | IS-IS route preference.
LSP-length receive | Maximum LSP that can be received.
LSP-length originate | Maximum LSP that can be generated.
Maximum imported routes | Maximum number of redistributed Level-1/Level-2 IPv4/IPv6 routes.
Timers | Timers: · LSP-max-age—Maximum life period of LSPs. · LSP-refresh—Refresh interval of LSPs. · SPF intervals—Interval between SPF calculations.
IPv6 enabled | IPv6 is enabled.
Multi-topology | IPv6 unicast topology mode: · Standard—IPv6 unicast topology standard mode. · Compatible—IPv6 unicast topology compatible mode.
IPv4-Unicast | IPv4 unicast topology is supported.
Topology ID | IPv4 unicast topology ID.
Topology | IPv4 unicast topology name.
Overload status | Overload bit status: · Overloaded manually—The overload bit is set manually. · Overloaded on startup—The overload bit is set on system startup. · Overloaded on startup waiting for nbr system-id up timeout1—The overload bit is set within the timeout1 interval waiting the neighbor system-id to come up. · Overloaded on startup after nbr system-id up timeout1—The overload bit is set within the timeout1 interval after the neighbor system-id comes up. · Overloaded for memory shortage—The overload bit is set for memory shortage. · Overloaded for graceful starting—The overload bit is set during the GR starting period.

IS-IS commands -- display isis event-log graceful-restart

Use display isis event-log graceful-restart to display IS-IS GR log information.

Syntax

Centralized devices:

display isis event-log graceful-restart

Distributed devices in standalone mode:Centralized IRF devices:

display isis event-log graceful-restart slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display isis event-log graceful-restart chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# (Centralized devices.) Display IS-IS GR log information.

<Sysname>display isis event-log graceful-restart

IS-IS loginfo :

Aug 24 14:45:37 2015 Process 1 enter GR restarting phase(Initialization).

Aug 24 14:45:37 2015 Process 1 enter GR phase (LSDB synchronization).

Aug 24 14:45:37 2015 Process 1 enter GR phase (TE tunnel prepare).

Aug 24 14:45:37 2015 Process 1 enter GR phase (First SPF computation).

Aug 24 14:45:37 2015 Process 1 enter GR phase (Redistribution).

Aug 24 14:45:37 2015 Process 1 enter GR phase (Second SPF computation).

Aug 24 14:45:37 2015 Process 1 enter GR phase (LSP stability).

Aug 24 14:45:37 2015 Process 1 enter GR phase (LSP generation).

Aug 24 14:45:37 2015 Process 1 enter GR phase (Finish).

Aug 24 14:45:37 2015 Process 1 GR complete.

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Display IS-IS GR log information for the specified slot.

<Sysname> display isis event-log graceful-restart slot 1

IS-IS loginfo :

Sep 18 08:48:24 2015 slot 1 Process 1 enter GR restarting phase(Initialization).

Sep 18 08:48:24 2015 slot 1 Process 1 enter GR phase (LSDB synchronization).

Sep 18 08:48:24 2015 slot 1 Process 1 enter GR phase (TE tunnel prepare).

Sep 18 08:48:24 2015 slot 1 Process 1 enter GR phase (First SPF computation).

Sep 18 08:48:25 2015 slot 1 Process 1 enter GR phase (Redistribution).

Sep 18 08:48:25 2015 slot 1 Process 1 enter GR phase (Second SPF computation).

Sep 18 08:48:25 2015 slot 1 Process 1 enter GR phase (LSP stability).

Sep 18 08:48:25 2015 slot 1 Process 1 enter GR phase (LSP generation).

Sep 18 08:48:25 2015 slot 1 Process 1 enter GR phase (Finish).

Sep 18 08:48:25 2015 slot 1 Process 1 GR complete.

Table 3 Command output

Field | Description
GR phase | GR phase: · Initialization. · LSDB synchronization. · TE tunnel prepare—Preparing for TE tunnel computation. · First SPF computation. · Redistribution. · Second SPF computation. · LSP stability—Ready to generate LSPs. · LSP generation. · Finish.

IS-IS commands -- display isis event-log lsp

Use display isis event-log lsp to display IS-IS LSP log information.

Syntax

display isis event-log lsp [ level-1 | level-2 ] * [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

level-1: Displays Level-1 LSP log information.

level-2: Displays Level-2 LSP log information.

process-id: Specifies a process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSP log information for all IS-IS processes.

Usage guidelines

If you do not specify a level, the command displays both Level-1 and Level-2 LSP log information.

Examples

# Display IS-IS LSP log information.

<Sysname> display isis event-log lsp

LSP Log for IS-IS(1)

--------------------

Level-1 LSP Log

---------------

Date Time LSPID Seq Num Event

-------------------------------------------------------------------------------

2015-11-06 11:10:45 1111.1111.1111.00-00 0x0000019c LSP received

2015-11-06 09:26:40 1111.1111.1111.01-00 0x00000111 Purged LSP received

2015-11-06 09:26:28 2222.2222.2222.00-00 0x00000181 LSP generated

2015-11-06 09:26:21 2222.2222.2222.00-00 0x00000180 Purged LSP generated

Level-2 SPF Log

---------------

Date Time LSPID Seq Num Event

-------------------------------------------------------------------------------

2015-11-06 11:10:45 1111.1111.1111.00-00 0x0000090d LSP received

2015-11-06 09:26:41 1111.1111.1111.01-00 0x00000101 Purged LSP received

2015-11-06 09:26:27 2222.2222.2222.00-00 0x00000171 LSP generated

2015-11-06 09:26:20 2222.2222.2222.00-00 0x00000170 Purged LSP generated

Table 4 Command output

Field | Description
Date | Date of the LSP change.
Time | Time of the LSP change.
LSPID | LSP ID.
Seq Num | LSP sequence number.
Event | LSP change event: · LSP received. · Purged LSP received. · LSP generated. · Purged LSP generated.

Related commands

reset isis event-log lsp

IS-IS commands -- display isis event-log non-stop-routing

Use display isis event-log non-stop-routing to display IS-IS NSR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display isis event-log non-stop-routing slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display isis event-log non-stop-routing chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Usage guidelines

This command is applicable only to distributed devices or IRF-capable devices.

Examples

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Display IS-IS NSR log information for the specified slot.

<Sysname> display isis event-log non-stop-routing slot 1

IS-IS loginfo :

Sep 18 10:20:44 2015 slot 1 Enter HA Block status

Sep 18 10:20:44 2015 slot 1 Exit HA Block status

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (Initialization).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (Smooth).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (TE tunnel prepare).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (First SPF computation).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (Redistribution).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (Second SPF computation).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (LSP stability).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (LSP generation).

Sep 18 10:24:00 2015 slot 1 Process 100 enter NSR phase (Finish).

Sep 18 10:24:00 2015 slot 1 Process 100 NSR complete.

Table 5 Command output

Field | Description
NSR phase | NSR phase: · Initialization. · Smooth. · TE tunnel prepare—Preparing for TE tunnel computation. · First SPF computation. · Redistribution. · Second SPF computation. · LSP stability—Ready to generate LSPs. · LSP generation. · Finish.

IS-IS commands -- display isis event-log spf

Use display isis event-log spf to display IS-IS route calculation log information.

Syntax

display isis event-log spf [ ipv4 [ topology topo-name ] | ipv6 ] [ [ level-1 | level-2 ] | verbose ] * [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv4: Displays IPv4 IS-IS route calculation log information.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays all IS-IS route calculation log information for the public network. Support for this option depends on the device model.

ipv6: Displays IPv6 IS-IS route calculation log information.

level-1: Displays Level-1 route calculation log information.

level-2: Displays Level-2 route calculation log information.

verbose: Displays detailed route calculation log information. If you do not specify this keyword, the command displays brief route calculation log information.

process-id: Specifies a process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays route calculation log information for all IS-IS processes.

Usage guidelines

If you do not specify the ipv4 or ipv6 keyword, the command displays IPv4 IS-IS route calculation log information for the public network.

If you do not specify a level, the command displays both Level-1 and Level-2 route calculation log information.

Examples

# Display brief IS-IS route calculation log information.

<Sysname> display isis event-log spf

SPF Log for IS-IS(1)

--------------------

Level-1 SPF Log

---------------

Date Time Duration Count Trigger event

-------------------------------------------------------------------------------

2015-09-07 11:10:45 0 4 Interface metric changed

2015-09-07 09:26:40 0 4 LSP updated

2015-09-07 09:26:28 0 2 DIS changed

2015-09-07 09:26:21 0.001 2 LSP updated

2015-09-07 09:26:07 0.001 3 Direct route changed

Level-2 SPF Log

---------------

Date Time Duration Count Trigger event

-------------------------------------------------------------------------------

2015-09-07 11:10:45 0 4 Interface metric changed

2015-09-07 09:26:40 0 4 LSP updated

2015-09-07 09:26:28 0 2 DIS changed

2015-09-07 09:26:21 0 2 LSP updated

2015-09-07 09:26:07 0 3 Direct route changed

# Display detailed IS-IS route calculation log information.

<Sysname> display isis event-log spf verbose

SPF Log for IS-IS(1)

--------------------

Level-1 SPF Log

---------------

Log date : 2015-09-07 11:10:45

Log key : 5

Trigger count : 4

Trigger event : Interface metric changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 1

LFA 0 LFA SPF nodes: 1

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 1 delete: 0

Last 10 routes:

1.1.1.0/24

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:40

Log key : 4

Trigger count : 4

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 1

LFA 0 LFA SPF nodes: 1

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:28

Log key : 3

Trigger count : 2

Trigger event : DIS changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:21

Log key : 2

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0.001 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0.001

Log date : 2015-09-07 09:26:07

Log key : 1

Trigger count : 3

Trigger event : Direct route changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0.001 Add: 1 modify: 0 delete: 0

Last 10 routes:

1.1.1.0/24

Route summary 0 Summary route nodes: 0

Total 0.001

Level-2 SPF Log

---------------

Log date : 2015-09-07 11:10:45

Log key : 5

Trigger count : 4

Trigger event : Interface metric changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 1

LFA 0 LFA SPF nodes: 1

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:40

Log key : 4

Trigger count : 4

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 1

LFA 0 LFA SPF nodes: 1

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:28

Log key : 3

Trigger count : 2

Trigger event : DIS changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:21

Log key : 2

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 09:26:07

Log key : 1

Trigger count : 3

Trigger event : Direct route changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Table 6 Command output

Field | Description
Date | Start date of route calculation.
Time | Start time of route calculation.
Duration | Route calculation duration in seconds. The value is accurate to six decimal places.
Count | Number of events that trigger the current route calculation.
Trigger event | Type of the most recent event that triggers route calculation: · NextHop changed. · DIS changed. · Interface metric changed. · Interface MTR information changed. · SPF link changed. · Default route changed. · Summary route changed. · TE tunnel updated. · TE tunnel metric changed. · IPv6 mode changed. · FRR configuration changed. · Prefix priority configuration changed. · Route preference changed. · ISPF configuration changed. · Import filter policy changed. · ECMP configuration changed. · PIC configuration changed. · Interface LFA exclude changed. · ATT configuration changed. · GR/NSR first SPF. · GR over. · T3 timeout. · Direct route changed. · Logic interface changed. · Route leakage configuration changed. · NSR over. · Entered overload state. · Exited overload state. · Area address changed. · Route policy changed. · Redistributed route updated. · LSP updated. · MT disabled. · MT enabled. · TE tunnel configuration changed. · TE tunnel destination changed. · RIB smooth.
Log date | Generation time of the route calculation logs.
Log key | Route calculation log key.
Trigger count | Number of events that trigger the current route calculation.
SPF details | Detailed information about the route calculation phases.
Phase | Route calculation phase: · TE tunnel ADJ—TE tunnel adjacency calculation. · Topology—Topology calculation. · BSPF—Backup SPF calculation. · LFA—LFA calculation. · Area—Area calculation. · PRC—Prefix calculation. · Route summary—Route summarization calculation.
Description | Route calculation phase description: · TE SPF nodes—Number of SPF nodes for TE tunnel adjacency calculation. · SPF nodes—Number of SPF nodes for topology calculation. · Candidate NBRs—Number of candidate neighbors. · LFA SPF nodes—Number of SPF nodes for LFA calculation. · Area addresses—Number of area addresses. · Add, modify, and delete—Prefix calculation summary. · Last 10 routes—10 routes that are most recently calculated. · Summary route nodes—Number of summarized routes.
Total | Total duration time of all route calculation phases.

# Display brief IPv6 IS-IS route calculation log information.

<Sysname> display isis event-log spf ipv6

SPF Log for IS-IS(1)

--------------------

Level-1 SPF Log

---------------

Date Time Duration Count Trigger event

-------------------------------------------------------------------------------

2015-09-07 11:10:45 0 4 Interface metric changed

2015-09-07 09:26:40 0 4 LSP updated

2015-09-07 09:26:28 0 2 DIS changed

2015-09-07 09:26:21 0.001 2 LSP updated

2015-09-07 09:26:07 0.001 3 Direct route changed

Level-2 SPF Log

---------------

Date Time Duration Count Trigger event

-------------------------------------------------------------------------------

2015-09-07 11:10:45 0 4 Interface metric changed

2015-09-07 09:26:40 0 4 LSP updated

2015-09-07 09:26:28 0 2 DIS changed

2015-09-07 09:26:21 0 2 LSP updated

2015-09-07 09:26:07 0 3 Direct route changed

# Display detailed IPv6 IS-IS route calculation log information.

<Sysname> display isis event-log spf ipv6 verbose

SPF Log for IS-IS(1)

--------------------

Level-1 SPF Log

---------------

Log date : 2015-09-07 02:18:09

Log key : 10

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:18:09

Log key : 9

Trigger count : 2

Trigger event : NextHop changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0.003 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0.003

Log date : 2011-01-01 02:17:40

Log key : 8

Trigger count : 2

Trigger event : Logic interface changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0.005 Add: 1 modify: 0 delete: 0

Last 10 routes:

10::/64

Route summary 0 Summary route nodes: 0

Total 0.005

Log date : 2015-09-07 02:17:38

Log key : 7

Trigger count : 1

Trigger event : Logic interface changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:17:33

Log key : 6

Trigger count : 5

Trigger event : NextHop changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0.003 Add: 0 modify: 0 delete: 1

Last 10 routes:

3::/24

Route summary 0 Summary route nodes: 0

Total 0.003

Log date : 2015-09-07 02:17:21

Log key : 5

Trigger count : 1

Trigger event : Direct route changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0.006 Add: 1 modify: 0 delete: 0

Last 10 routes:

3::/24

Route summary 0 Summary route nodes: 0

Total 0.006

Log date : 2015-09-07 02:17:11

Log key : 4

Trigger count : 1

Trigger event : IPv6 mode changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 01:09:33

Log key : 3

Trigger count : 2

Trigger event : DIS changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0.001 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0.001

Log date : 2015-09-07 01:09:25

Log key : 2

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 01:08:49

Log key : 1

Trigger count : 1

Trigger event : Area address changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Level-2 SPF Log

---------------

Log date : 2015-09-07 02:18:09

Log key : 10

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:18:09

Log key : 9

Trigger count : 2

Trigger event : NextHop changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0.002 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0.001 Summary route nodes: 0

Total 0.003

Log date : 2015-09-07 02:17:40

Log key : 8

Trigger count : 2

Trigger event : Logic interface changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:17:38

Log key : 7

Trigger count : 1

Trigger event : Logic interface changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:17:33

Log key : 6

Trigger count : 5

Trigger event : NextHop changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0.001 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0.001

Log date : 2015-09-07 02:17:21

Log key : 5

Trigger count : 1

Trigger event : Direct route changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 0

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 02:17:11

Log key : 4

Trigger count : 1

Trigger event : IPv6 mode changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0.001 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0.001

Log date : 2015-09-07 01:09:33

Log key : 3

Trigger count : 2

Trigger event : DIS changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 3

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 01:09:25

Log key : 2

Trigger count : 2

Trigger event : LSP updated

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF links changed: 1

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Log date : 2015-09-07 01:08:49

Log key : 1

Trigger count : 1

Trigger event : Area address changed

SPF details :

Phase Duration Description

TE tunnel ADJ 0 TE SPF nodes: 0

Topology 0 SPF nodes: 0

BSPF 0 Candidate NBRs: 0

LFA 0 LFA SPF nodes: 0

Area 0 Area addresses: 1

PRC 0 Add: 0 modify: 0 delete: 0

Route summary 0 Summary route nodes: 0

Total 0

Table 7 Command output

Field | Description
Date | Start date of route calculation.
Time | Start time of route calculation.
Duration | Route calculation duration in seconds. The value is accurate to six decimal places.
Count | Number of events that trigger the current route calculation.
Trigger event | Type of the most recent event that triggers route calculation: · NextHop changed. · DIS changed. · Interface metric changed. · Interface MTR information changed. · SPF link changed. · Default route changed. · Summary route changed. · TE tunnel updated. · TE tunnel metric changed. · IPv6 mode changed. · FRR configuration changed. · Prefix priority configuration changed. · Route preference changed. · ISPF configuration changed. · Import filter policy changed. · ECMP configuration changed. · PIC configuration changed. · Interface LFA exclude changed. · ATT configuration changed. · GR/NSR first SPF. · GR over. · T3 timeout. · Direct route changed. · Logic interface changed. · Route leakage configuration changed. · NSR over. · Entered overload state. · Exited overload state. · Area address changed. · Route policy changed. · Redistributed route updated. · LSP updated. · MT disabled. · MT enabled. · TE tunnel configuration changed. · TE tunnel destination changed. · RIB smooth.
Log date | Generation time of the route calculation logs.
Log key | Route calculation log key.
Trigger count | Number of events that trigger the current route calculation.
SPF details | Detailed information about the route calculation phases.
Phase | Route calculation phase: · TE tunnel ADJ—TE tunnel adjacency calculation. · Topology—Topology calculation. · BSPF—Backup SPF calculation. · LFA—LFA calculation. · Area—Area calculation. · PRC—Prefix calculation. · Route summary—Route summarization calculation.
Description | Route calculation phase description: · TE SPF nodes—Number of SPF nodes for TE tunnel adjacency calculation. · SPF nodes—Number of SPF nodes for topology calculation. · Candidate NBRs—Number of candidate neighbors. · LFA SPF nodes—Number of SPF nodes for LFA calculation. · Area addresses—Number of area addresses. · Add, modify, and delete—Prefix calculation summary. · Last 10 routes—10 routes that are most recently calculated. · Summary route nodes—Number of summarized routes.
Total | Total duration time of all route calculation phases.

Related commands

reset isis event-log spf

IS-IS commands -- display isis graceful-restart status

Use display isis graceful-restart status to display IS-IS GR state.

Syntax

display isis graceful-restart status [ level-1 | level-2 ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

level-1: Displays the IS-IS Level-1 GR state.

level-2: Displays the IS-IS Level-2 GR state.

process-id: Specifies a process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays GR state of all IS-IS processes.

Examples

# Display IS-IS GR state.

<Sysname> display isis graceful-restart status

Restart information for IS-IS(1)

--------------------------------

Restart status: COMPLETE

Restart phase: Finish

Restart t1: 3, count 10; Restart t2: 60; Restart t3: 300

SA Bit: supported

Level-1 restart information

---------------------------

Total number of interfaces: 1

Number of waiting LSPs: 0

Level-2 restart information

---------------------------

Total number of interfaces: 1

Number of waiting LSPs: 0

Table 8 Command output

Field | Description
Restart status | Current GR state: · RESTARTING—In this state, forwarding can be ensured. · STARTING—In this state, forwarding cannot be ensured. · COMPLETE—GR is completed.
Restart phase | Current Restart phase: · Initialization. · LSDB synchronization. · First SPF computation. · Redistribution. · Second SPF computation. · LSP stability—Ready to generate LSPs. · LSP generation. · Finish.
Restart t1 | T1 timer, in seconds.
count | Number of T1 timer expirations.
Restart t2 | T2 timer, in seconds.
Restart t3 | T3 timer, in seconds.
SA Bit | Whether SA is supported.
Total number of interfaces | Total number of IS-IS interfaces.
Number of waiting LSPs | Number of LSPs not obtained by the GR restarter from GR helpers during LSDB synchronization.

IS-IS commands -- display isis interface

Use display isis interface to display IS-IS interface information.

Syntax

display isis interface [ [ interface-type interface-number ] [ verbose ] | statistics ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

interface-type interface-number: Displays information for a specified IS-IS interface. If you do not specify this argument, the command displays information about all interfaces.

verbose: Displays detailed information about an interface. If you do not specify this keyword, the command displays brief information about an interface.

statistics: Displays IS-IS interface statistics.

process-id: Displays IS-IS interface information for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays interface information for all IS-IS processes.

Examples

# Display brief IS-IS interface information. (Applicable to routers.)

<Sysname> display isis interface

Interface information for IS-IS(1)

----------------------------------

Interface: GigabitEthernet1/0/2

Index IPv4 state IPv6 state CircuitID MTU Type DIS

00001 Up Down 1 1497 L1/L2 No/No

# Display detailed IS-IS interface information. (Applicable to routers.)

<Sysname> display isis interface verbose

Interface information for IS-IS(1)

----------------------------------

Interface: GigabitEthernet1/0/2

Index IPv4 state IPv6 state CircuitID MTU Type DIS

00001 Up Down 1 1497 L1/L2 No/No

SNPA address : 000c-29e8-1bd5

IP address : 192.168.220.10

Secondary IP address(es) :

IPv6 link-local address :

Extended circuit ID : 1

CSNP timer value : L1 10 L2 10

Hello timer value : 10

Hello multiplier value : 3

LSP timer value : L12 33

LSP transmit-throttle count : L12 5

Cost : L1 100 L2 100

IPv6 cost : L1 10 L2 10

Priority : L1 64 L2 64

Retransmit timer value : L12 5

LDP state : L1 Init L2 No-LDP

LDP sync state : L1 Init L2 Achieved

MPLS TE status : L1 Disabled L2 Disabled

IPv4 BFD : Disabled

IPv6 BFD : Disabled

IPv4 FRR LFA backup : Enabled

IPv6 FRR LFA backup : Enabled

IPv4 prefix-suppression : Disabled

IPv6 prefix-suppression : Disabled

IPv4 tag : 1

IPv6 tag : 4294967295

IPv4 primary path detection mode: BFD ctrl

IPv6 primary path detection mode: BFD ctrl

IPv4-Unicast :

Topology ipv4_unicast_multopo

Topology ID : 6

Cost : L1 444 L2 444

FRR LFA backup : Disabled

Prefix-suppression : Enabled

Tag : 44444444

# Display brief IS-IS interface information. (Applicable to switches.)

<Sysname> display isis interface

Interface information for IS-IS(1)

----------------------------------

Interface: Vlan-interface100

Index IPv4 state IPv6 state CircuitID MTU Type DIS

00001 Up Down 1 1497 L1/L2 No/No

# Display detailed IS-IS interface information. (Applicable to switches.)

<Sysname> display isis interface verbose

Interface information for IS-IS(1)

----------------------------------

Interface: Vlan-interface100

Index IPv4 state IPv6 state CircuitID MTU Type DIS

00001 Up Down 1 1497 L1/L2 No/No

SNPA address : 000c-29e8-1bd5

IP address : 192.168.220.10

Secondary IP address(es) :

IPv6 link-local address :

Extended circuit ID : 1

CSNP timer value : L1 10 L2 10

Hello timer value : 10

Hello multiplier value : 3

LSP timer value : L12 33

LSP transmit-throttle count : L12 5

Cost : L1 100 L2 100

IPv6 cost : L1 10 L2 10

Priority : L1 64 L2 64

Retransmit timer value : L12 5

LDP state : L1 Init L2 No-LDP

LDP sync state : L1 Init L2 Achieved

MPLS TE status : L1 Disabled L2 Disabled

IPv4 BFD : Disabled

IPv6 BFD : Disabled

IPv4 FRR LFA backup : Enabled

IPv6 FRR LFA backup : Enabled

IPv4 prefix-suppression : Disabled

IPv6 prefix-suppression : Disabled

IPv4 tag : 1

IPv6 tag : 4294967295

IPv4 primary path detection mode: BFD ctrl

IPv6 primary path detection mode: BFD ctrl

IPv4-Unicast :

Topology ipv4_unicast_multopo

Topology ID : 6

Cost : L1 444 L2 444

FRR LFA backup : Disabled

Prefix-suppression : Enabled

Tag : 44444444

Table 9 Command output

Field | Description
Interface | Interface type and number.
Index | Interface index.
IPv4 state | IPv4 state.
IPv6 state | IPv6 state.
CircuitID | Circuit ID.
MTU | Interface MTU.
Type | Interface link adjacency type.
DIS | Indicates whether the interface is elected as the Level-1/Level-2 DIS. In a P2P network, this field displays a hyphen (-) because DIS election is not performed.
SNPA address | Subnet access point address.
IP address | Primary IP address.
Secondary IP address(es) | Secondary IP addresses.
IPv6 link-local address | IPv6 link local address.
Extended circuit ID | Extended circuit ID for a P2P link.
CSNP timer value | Interval for sending CSNP packets.
Hello timer value | Interval for sending Hello packets.
Hello multiplier value | Number of invalid Hello packets.
LSP timer value | Minimum interval for sending LSP packets.
LSP transmit-throttle count | Number of LSP packets sent each time.
Cost | Cost of the interface.
IPv6 cost | IPv6 link cost of the interface.
Priority | DIS priority.
Retransmit timer value | Retransmission interval for LSPs on a P2P link.
MPLS TE status | MPLS TE status: Enabled or Disabled.
LDP state | LDP state: · Init—LDP is not reported. · No-LDP—LDP is not configured. · Not ready—LDP session is not established. · Ready—LDP session is established.
LDP sync state | LDP synchronization state: · Init—Initialized. · Achieved—Synchronized. · Max cost—Maintain the maximum cost.
IPv4 BFD | Whether BFD for IS-IS is enabled: · Disabled. · Enabled.
IPv6 BFD | Whether BFD for IPv6 IS-IS is enabled: · Disabled. · Enabled.
IPv4 FRR LFA backup | Whether LFA calculation is enabled for IPv4 FRR: · Disabled. · Enabled.
IPv6 FRR LFA backup | Whether LFA calculation is enabled for IPv6 FRR: · Disabled. · Enabled.
IPv4 prefix-suppression | Whether IPv4 IS-IS prefix suppression is enabled: · Disabled. · Enabled.
IPv6 prefix-suppression | Whether IPv6 IS-IS prefix suppression is enabled: · Disabled. · Enabled.
IPv4 tag | IPv4 tag value of the interface.
IPv6 tag | IPv6 tag value of the interface.
IPv4 primary path detection mode | IPv4 primary path detection mode: · BFD ctrl—BFD control packet mode. · BFD echo—BFD echo packet mode.
IPv6 primary path detection mode | IPv6 primary path detection mode: · BFD ctrl—BFD control packet mode. · BFD echo—BFD echo packet mode.
IPv4-Unicast | IPv4 unicast topology supported by the interface.
Topology | IPv4 unicast topology name.
Topology ID | IPv4 unicast topology ID.

# Display IS-IS interface statistics.

<Sysname> display isis interface statistics

Interface statistics information for IS-IS(1)

--------------------------------------------

Type IPv4 up/down IPv6 up/down

LAN 1/0 0/0

P2P 0/0 0/0

Table 10 Command output

Field | Description
Type | Network type of the interface: · LAN—Broadcast network. · P2P—Point-to-point network.
IPv4 up | Number of IS-IS interfaces in up state.
IPv4 down | Number of IS-IS interfaces in down state.
IPv6 up | Number of IS-ISv6 interfaces in up state.
IPv6 down | Number of IS-ISv6 interfaces in down state.

IS-IS commands -- display isis lsdb

Use display isis lsdb to display IS-IS LSDB information.

Syntax

display isis lsdb [ [ level-1 | level-2 ] | local | [ lsp-id lspid | lsp-name lspname ] | verbose ] * [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

level-1: Displays the level-1 LSDB.

level-2: Displays the level-2 LSDB.

local: Displays LSP information generated locally.

lsp-id lspid: Specifies an LSP ID, in the form of sysID. Pseudo ID-fragment num, where sysID represents the originating node or pseudo node. Pseudo ID is separated by a dot from sysID and by a hyphen from fragment num.

lsp-name lspname: Specifies the LSP name, in the form of Symbolic name.Pseudo ID-fragment num, where Pseudo ID is separated by a dot from Symbolic name and by a hyphen from fragment num. If the Pseudo ID is 0, specify the LSP name in the form Symbolic name-fragment num.

verbose: Displays LSDB detailed information. If you do not specify this keyword, the command displays brief information about LSDB.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSDBs for all IS-IS processes.

Usage guidelines

If no level is specified, the command displays both Level-1 and Level-2 LSDB information.

Examples

# Display brief Level-1 LSDB information.

<Sysname> display isis lsdb level-1

Database information for IS-IS(1)

--------------------------------

Level-1 Link State Database

---------------------------

LSPID Seq Num Checksum Holdtime Length ATT/P/OL

-------------------------------------------------------------------------------

0000.0000.0001.00-00* 0x00000087 0xf846 1152 183 0/0/0

0000.0000.0003.00-00 0x00000005 0x4bee 520 177 0/0/0

0000.0000.0003.00-01 0x00000004 0x7245 520 45 0/0/0

0000.0000.0011.00-00 0x0000000b 0xcdf6 815 183 0/0/0

*-Self LSP, +-Self LSP(Extended), ATT-Attached, P-Partition, OL-Overload

# Display detailed Level-1 LSDB information.

<Sysname> display isis lsdb level-1 verbose

Database information for IS-IS(1)

--------------------------------

Level-1 Link State Database

---------------------------

LSPID Seq Num Checksum Holdtime Length ATT/P/OL

-------------------------------------------------------------------------------

0000.0000.0001.00-00* 0x00000080 0x73f 1185 183 0/0/0

Source 0000.0000.0001.00

NLPID IPv4

Area address 10

IPv4 address 192.168.220.10

MT ID 0000 (-/-)

MT ID 0002 (-/-)

MT ID 0006 (-/-)

+NBR ID

0000.0000.0011.00 Cost: 100

Admin group: 0x00000000

Physical bandwidth: 12500000 bytes/sec

Reservable bandwidth: 0 bytes/sec

Unreserved bandwidth for each TE class:

TE class 0: 0 bytes/sec TE class 1: 0 bytes/sec

TE class 2: 0 bytes/sec TE class 3: 0 bytes/sec

TE class 4: 0 bytes/sec TE class 5: 0 bytes/sec

TE class 6: 0 bytes/sec TE class 7: 0 bytes/sec

TE class 8: 0 bytes/sec TE class 9: 0 bytes/sec

TE class 10: 0 bytes/sec TE class 11: 0 bytes/sec

TE class 12: 0 bytes/sec TE class 13: 0 bytes/sec

TE class 14: 0 bytes/sec TE class 15: 0 bytes/sec

TE cost: 10

Bandwidth constraint model: Prestandard DS-TE RDM

Bandwidth constraints:

BC[0] : 0 bytes/sec BC[1] : 0 bytes/sec

Neighbor IP address: 192.168.220.30

Interface IP address: 192.168.220.10

IPv6 unicast NBR ID

6464.6464.6464.01 Cost: 10 MT ID: 2

MT NBR ID

6464.6464.6464.01 Cost: 10 MT ID: 6

+IP-Extended

192.168.220.0 255.255.255.0 Cost: 100

IPv4 unicast

1.1.1.1 255.255.255.255 Cost: 0 MT ID: 6

IPv4 unicast

10.10.10.0 255.255.255.0 Cost: 10 MT ID: 6

IPv6 unicast

1:1:1::1/128 Cost: 0 MT ID: 2

IPv6 unicast

10:10:10::/64 Cost: 10 MT ID: 2

Router ID 1.1.1.1

0000.0000.0003.00-00 0x00000005 0x4bee 887 177 0/0/0

Source 0000.0000.0003.00

NLPID IPv4

Area address 10

IPv4 address 10.10.10.10

IPv4 address 192.168.220.20

+NBR ID

0000.0000.0001.00 Cost: 10

Admin group: 0x00000000

Physical bandwidth: 12500000 bytes/sec

Reservable bandwidth: 0 bytes/sec

Unreserved bandwidth for each TE class:

TE class 0: 0 bytes/sec TE class 1: 0 bytes/sec

TE class 2: 0 bytes/sec TE class 3: 0 bytes/sec

TE class 4: 0 bytes/sec TE class 5: 0 bytes/sec

TE class 6: 0 bytes/sec TE class 7: 0 bytes/sec

TE class 8: 0 bytes/sec TE class 9: 0 bytes/sec

TE class 10: 0 bytes/sec TE class 11: 0 bytes/sec

TE class 12: 0 bytes/sec TE class 13: 0 bytes/sec

TE class 14: 0 bytes/sec TE class 15: 0 bytes/sec

TE cost: 10

Bandwidth constraint model: Prestandard DS-TE RDM

Bandwidth constraints:

BC[0]: 0 bytes/sec BC[1]: 0 bytes/sec

Interface IP address: 192.168.220.20

Neighbor IP address: 192.168.220.10

Router ID 3.3.3.3

0000.0000.0003.00-01 0x00000004 0x7245 887 45 0/0/0

Source 0000.0000.0003.00

+IP-Extended

10.10.10.0 255.255.255.0 Cost: 10

+IP-Extended

192.168.220.0 255.255.255.0 Cost: 10

*-Self LSP, +-Self LSP(Extended), ATT-Attached, P-Partition, OL-Overload

Table 11 Command output

Field | Description
LSPID | LSP ID.
Seq Num | LSP sequence number.
Checksum | LSP checksum.
Holdtime | LSP lifetime, which decreases as time elapses.
Length | LSP length.
ATT/P/OL | · ATT—Attach bit. · P—Partition bit. · OL—Overload bit. 1 means the LSP bit is set and 0 means the LSP bit is not set.
Source | System ID of the originating router.
HOST NAME | Dynamic host name of the originating router.
ORG ID | Original system ID of the virtual system of the originating router.
NLPID | Network layer protocol the originating router runs.
Area address | Area address of the originating router.
IPv4 address | IP address of the originating router's IS-IS interface.
IPv6 address | IPv6 address of the originating router's IS-ISv6 interface.
MT ID 0000 (-/-) MT ID 0002 (-/-) MT ID 0006 (-/-) | Topology supported by the originating router (0/0/0 indicates ATT/P/OL): · 0000—Base topology. · 0002—IPv6 unicast topology. · 0006—IPv4 unicast topology. · (-/-)—Attach bit/overload bit.
NBR ID | Neighbor ID of the originating router.
MT NBR ID | IPv4 unicast topology neighbor information about the originating router.
IPv6 unicast NBR ID | IPv6 unicast neighbor information about the originating router.
Admin group | Link management group attribute.
Interface IP address | IP address of the interface connected to the remote end.
Neighbor IP address | Neighbor interface IP address.
Physical bandwidth | Physical bandwidth.
Reservable bandwidth | Reserved bandwidth.
Unreserved bandwidth for each TE class | Available bandwidth reserved for each TE class.
TE class | Available bandwidth for each of the 8 or 16 TE classes.
TE cost | TE cost.
Bandwidth constraint model | Bandwidth constraint model: · Prestandard DS-TE RDM. · IETF DS-TE RDM. · IETF DS-TE MAM.
BC | Bandwidth constraint value. The Prestandard model supports 2 BCs, and the IETF modes support a maximum of 8 BCs.
Router ID | Router ID.
IP-Internal | Internal IP address and mask of the originating router.
IP-External | External IP address and mask of the originating router.
IP-Extended | Extended IP address and mask of the originating router.
Cost | Cost.
Auth | Authentication information of the originating router.
IPV6 | Internal IPv6 address and prefix of the originating router.
IPV6-Ext | External IPv6 address and prefix of the originating router.
IPv4 unicast | IPv4 unicast reachability information about the originating router.
IPv6 unicast | Internal IPv6 unicast reachability information about the originating router.
IPv6 unicast-ext | External IPv6 unicast reachability information about the originating router.

IS-IS commands -- display isis lsdb statistics

Use display isis lsdb statistics to display IS-IS LSDB statistics.

Syntax

display isis lsdb statistics [ level-1 | level-2 ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

level-1: Displays Level-1 LSDB statistics.

level-2: Displays Level-2 LSDB statistics.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSDB statistics for all IS-IS processes.

Usage guidelines

If you do not specify a level, the command displays both Level-1 and Level-2 LSDB statistics.

Examples

# Display IS-IS LSDB statistics.

<Sysname> display isis lsdb statistics

Database Statistics information for IS-IS(1)

-----------------------------------------

Level-1 LSDB Statistics

-----------------------

LSP source ID LSP count

--------------------------------------------------------------------------------

Total 333

1111.1111.1111.00 1

2222.2222.2222.00 256

2222.2222.2222.01 1

bbbb.bbbb.0001.00 75

Level-2 LSDB Statistics

-----------------------

LSP source ID LSP count

--------------------------------------------------------------------------------

Total 663

1111.1111.1111.00 256

2222.2222.2222.00 256

2222.2222.2222.01 1

aaaa.aaaa.0001.00 75

bbbb.bbbb.0001.00 75

Table 12 Command output

Field | Description
LSP count | Number of LSPs generated by a source.
Total | Number of LSPs generated by all sources.

Related commands

display isis lsdb

IS-IS commands -- display isis mesh-group

Use display isis mesh-group to display IS-IS mesh group configuration information.

Syntax

display isis mesh-group [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

process-id: Displays IS-IS mesh-group configuration for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays IS-IS mesh group configuration information for all IS-IS processes.

Examples

# Add Serial 2/1/0 and Serial 2/1/1 to mesh group 100.

<Sysname> system-view

[Sysname] interface serial 2/1/0

[Sysname-Serial2/1/0] isis mesh-group 100

[Sysname-Serial2/1/0] quit

[Sysname] interface serial 2/1/1

[Sysname-Serial2/1/1] isis mesh-group 100

# Display IS-IS mesh-group configuration information.

[Sysname-Serial2/1/1] display isis mesh-group

Mesh Group information for IS-IS(1)

----------------------------------------------------------------------

Interface Status

Serial2/1/0 Blocked

Serial2/1/1 100

Table 13 Command output

Field | Description
Interface | Interface name.
Status | Mesh group the interface belongs to/whether a blocked interface is configured.

IS-IS commands -- display isis name-table

Use display isis name-table to display the host name-to-system ID mapping table.

Syntax

display isis name-table [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

process-id: Displays the host name to system ID mapping table for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays the host name to system ID mapping table for all IS-IS processes.

Examples

# Display the IS-IS host name to system ID mapping table.

<Sysname> display isis name-table

Name table information for IS-IS(1)

-----------------------------------

System ID Hostname Type Level

6789.0000.0001 RUTA DYNAMIC Level-1

6789.0000.0001 RUTA DYNAMIC Level-2

0000.0000.0041 RUTB STATIC Level-1

0000.0000.0041 RUTB STATIC Level-2

6789.0000.0001.01 DIS-A DYNAMIC Level-1

0000.0000.0041.01 DIS-B DYNAMIC Level-2

Table 14 Command output

Field | Description
System ID | System ID.
Hostname | Host name.
Type | Mapping type: · STATIC. · DYNAMIC.
Level | Level on which the system ID-to-host name mapping takes effect: Level-1 or Level-2.

IS-IS commands -- display isis non-stop-routing status

Use display isis non-stop-routing status to display IS-IS NSR status.

Syntax

display isis non-stop-routing status

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Examples

# Display IS-IS NSR status.

<Sysname> display isis non-stop-routing status

Nonstop Routing information for IS-IS(1)

----------------------------------------

NSR phase: Finish

Table 15 Command output

Field | Description
NSR phase | NSR phase: · Initialization. · Smooth. · First SPF computation. · Redistribution. · Second SPF computation. · LSP stability—Ready to generate LSPs. · LSP generation. · Finish.

IS-IS commands -- display isis packet

Use display isis packet to display IS-IS packet statistics.

Syntax

display isis packet { csnp | hello | lsp | psnp } by-interface [ verbose ] [ interface-type interface-number ] [ process-id ]

display isis packet { csnp | hello | lsp | psnp } [ verbose ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

csnp: Displays CSNP packet statistics.

hello: Displays hello packet statistics.

lsp: Displays LSP packet statistics.

psnp: Displays PSNP packet statistics.

by-interface: Displays packet statistics on a per-interface basis.

verbose: Displays detailed packet statistics.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this option, the command displays IS-IS packet statistics for all interfaces.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays packet statistics for all IS-IS processes.

Examples

# Display detailed hello packet statistics on a per-interface basis. (Applicable to routers.)

<Sysname> display isis packet hello by-interface verbose

Hello packet information for IS-IS(1)

-------------------------------------

Interface: GigabitEthernet1/0/1

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

Bad system ID length : 0 Bad circuit type : 0

Bad auth TLV: 0 Bad area address TLV : 0

Auth failure : 0 Excessive area addresses : 0

Bad NBR TLV : 0 Excessive auth TLVs : 0

Excessive IF Addr TLVs: 0 Excessive IF addresses : 0

Bad IF address TLV : 0 Duplicate system ID : 0

Bad TLV length : 0 Bad IP address : 0

Duplicate IP address : 0 Mismatched area address : 0

Mismatched protocol : 0 Mismatched network type : 0

Bad IPv6 address TLV : 0 Bad IPv6 address : 0

Duplicate IPv6 address: 0 Bad MT ID TLV : 0

SNPA conflict (LAN) : 0 Excessive NBR SNPAs (LAN) : 0

Mismatched level (LAN): 0 Bad 3-Way option TLV (P2P) : 0

No common MT ID (P2P) : 0 Bad circuit ID (P2P) : 0

# Display detailed hello packet statistics on a per-interface basis. (Applicable to switches.)

<Sysname> display isis packet hello by-interface verbose

Hello packet information for IS-IS(1)

-------------------------------------

Interface: Vlan-interface10

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

Bad system ID length : 0 Bad circuit type : 0

Bad auth TLV: 0 Bad area address TLV : 0

Auth failure : 0 Excessive area addresses : 0

Bad NBR TLV : 0 Excessive auth TLVs : 0

Excessive IF Addr TLVs: 0 Excessive IF addresses : 0

Bad IF address TLV : 0 Duplicate system ID : 0

Bad TLV length : 0 Bad IP address : 0

Duplicate IP address : 0 Mismatched area address : 0

Mismatched protocol : 0 Mismatched network type : 0

Bad IPv6 address TLV : 0 Bad IPv6 address : 0

Duplicate IPv6 address: 0 Bad MT ID TLV : 0

SNPA conflict (LAN) : 0 Excessive NBR SNPAs (LAN) : 0

Mismatched level (LAN): 0 Bad 3-Way option TLV (P2P) : 0

No common MT ID (P2P) : 0 Bad circuit ID (P2P) : 0

# Display detailed hello packet statistics.

<Sysname> display isis packet hello verbose

Hello packet information for IS-IS(1)

-------------------------------------

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

Bad system ID length : 0 Bad circuit type : 0

Bad auth TLV : 0 Bad area address TLV : 0

Auth failure : 0 Excessive area addresses : 0

Bad NBR TLV : 0 Excessive auth TLVs : 0

Excessive IF Addr TLVs : 0 Excessive IF addresses : 0

Bad IF address TLV : 0 Duplicate system ID : 0

Bad TLV length : 0 Bad IP address : 0

Duplicate IP address : 0 Mismatched area address : 0

Mismatched protocol : 0 Mismatched network type : 0

Bad IPv6 address TLV : 0 Bad IPv6 address : 0

Duplicate IPv6 address : 0 Bad MT ID TLV : 0

SNPA conflict (LAN) : 0 Excessive NBR SNPAs (LAN) : 0

Mismatched level (LAN) : 0 Bad 3-Way option TLV (P2P) : 0

No common MT ID (P2P) : 0 Bad circuit ID (P2P) : 0

Table 16 Command output

Field | Description
Input packets with errors | Statistics for packets with the following errors: · Bad packet length—Invalid packet length. · Bad header length—Invalid header length. · Jumbo packet—The packet length exceeds the buffer size or the interface MTU. · Bad protocol description—Invalid protocol description. · Bad protocol ID—Invalid protocol identifier. · Bad protocol version—Invalid protocol version. · Unknown packet type—Unknown packet type. · Bad max area count—Invalid maximum number of area addresses. · Bad system ID length—Invalid system ID length. · Bad circuit type—Invalid interface type. · Bad auth TLV—Invalid authentication TLV. · Bad area address TLV—Invalid area address TLV. · Auth failure—Authentication failure. · Excessive area addresses—Excessive area addresses. · Bad NBR TLV—Invalid neighbor TLV. · Excessive auth TLVs—Excessive authentication TLVs. · Excessive IF Addr TLVs—Excessive interface address TLVs. · Excessive IF addresses—Excessive interface addresses. · Bad IF address TLV—Invalid interface address TLV. · Duplicate system ID—Duplicate system IDs. · Bad TLV length—Invalid TLV length. · Bad IP address—The IP address does not belong to the same network as the local interface address. · Duplicate IP address—Duplicate IP addresses. · Mismatched area address—Mismatched area addresses. · Mismatched protocol—Mismatched protocols. · Mismatched network type—Mismatched network types. · Bad IPv6 address TLV—Invalid IPv6 address TLV. · Bad IPv6 address—Invalid IPv6 address. · Duplicate IPv6 address—Duplicate IPv6 addresses. · Bad MT ID TLV—Invalid topology ID TLV. · SNPA conflict (LAN)—SNPA conflict. · Excessive NBR SNPAs (LAN)—Excessive neighbor SNPAs. · Mismatched level (LAN)—Mismatched levels. · Bad 3-Way option TLV (P2P)—Invalid three-way handshake information. · No common MT ID (P2P)—No common topology ID. · Bad circuit ID (P2P)—Invalid circuit ID.

# Display detailed LSP packet statistics on a per-interface basis. (Applicable to routers.)

<Sysname> display isis packet lsp by-interface verbose

LSP packet information for IS-IS(1)

-----------------------------------

Interface: GigabitEthernet1/0/1

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Illegal IS type : 0

Sequence number is 0: 0 Checksum is 0 : 0

Incorrect checksum : 0 Bad TLV length : 0

Mismatched protocol : 0 Bad auth TLV : 0

Auth failure : 0 Excessive auth TLVs : 0

Bad NBR TLV : 0 Bad extended IS TLV : 0

Bad IF address TLV : 0 Bad IPv6 IF address TLV : 0

Bad alias TLV : 0 Bad IP reachability TLV : 0

Bad MT IS TLV : 0 Bad area address TLV : 0

Bad MT ID TLV : 0 Bad MT IP TLV : 0

Bad MT IPv6 TLV : 0 Bad IPv6 reachability TLV: 0

Bad router ID TLV : 0

# Display detailed LSP packet statistics on a per-interface basis. (Applicable to switches.)

<Sysname> display isis packet lsp by-interface verbose

LSP packet information for IS-IS(1)

-----------------------------------

Interface: Vlan-interface10

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Illegal IS type : 0

Sequence number is 0: 0 Checksum is 0 : 0

Incorrect checksum : 0 Bad TLV length : 0

Mismatched protocol : 0 Bad auth TLV : 0

Auth failure : 0 Excessive auth TLVs : 0

Bad NBR TLV : 0 Bad extended IS TLV : 0

Bad IF address TLV : 0 Bad IPv6 IF address TLV : 0

Bad alias TLV : 0 Bad IP reachability TLV : 0

Bad MT IS TLV : 0 Bad area address TLV : 0

Bad MT ID TLV : 0 Bad MT IP TLV : 0

Bad MT IPv6 TLV : 0 Bad IPv6 reachability TLV: 0

Bad router ID TLV : 0

# Display detailed LSP packet statistics.

<Sysname> display isis packet lsp verbose

LSP packet information for IS-IS(1)

-----------------------------------

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Illegal IS type : 0

Sequence number is 0 : 0 Checksum is 0 : 0

Incorrect checksum : 0 Bad TLV length : 0

Mismatched protocol : 0 Bad auth TLV : 0

Auth failure : 0 Excessive auth TLVs : 0

Bad NBR TLV : 0 Bad extended IS TLV : 0

Bad IF address TLV : 0 Bad IPv6 IF address TLV : 0

Bad alias TLV : 0 Bad IP reachability TLV : 0

Bad MT IS TLV : 0 Bad area address TLV : 0

Bad MT ID TLV : 0 Bad MT IP TLV : 0

Bad MT IPv6 TLV : 0 Bad IPv6 reachability TLV : 0

Bad router ID TLV : 0

Table 17 Command output

Field | Description
Input packets with errors | Statistics for packets with the following errors: · Bad packet length—Invalid packet length. · Bad header length—Invalid header length. · Jumbo packet—The packet length exceeds the maximum length of packets that can be received. · SNPA conflict (LAN)—SNPA conflict. · Smaller than header—The packet length is smaller than the fixed header length. · Bad protocol description—Invalid protocol description. · Bad protocol ID—Invalid protocol identifier. · Bad protocol version—Invalid protocol version. · Unknown packet type—Unknown packet type. · Bad max area count—Invalid maximum number of area addresses. · No active NBR—The packet is from an unknown neighbor. · Bad system ID length—Invalid system ID length. · Mismatched level—Mismatched levels. · Illegal IS type—Invalid IS type. · Sequence number is 0—The sequence number is 0. · Checksum is 0—The checksum is 0. · Incorrect checksum—Incorrect checksum. · Bad TLV length—Invalid TLV length. · Mismatched protocol—Mismatched protocols. · Bad auth TLV—Invalid authentication TLV. · Auth failure—Authentication failure. · Excessive auth TLVs—Excessive authentication TLVs. · Bad NBR TLV—Invalid neighbor TLV. · Bad extended IS TLV—Invalid extended IS TLV. · Bad IF address TLV—Invalid interface address TLV. · Bad IPv6 IF address TLV—Invalid IPv6 interface address TLV. · Bad alias TLV—Invalid alias TLV. · Bad IP reachability TLV—Invalid IP reachability TLV. · Bad MT IS TLV—Invalid topology IS TLV. · Bad area address TLV—Invalid area address TLV. · Bad MT ID TLV—Invalid topology ID TLV. · Bad MT IP TLV—Invalid IPv4 topology TLV. · Bad MT IPv6 TLV—Invalid IPv6 topology TLV. · Bad IPv6 reachability TLV—Invalid IPv6 reachability TLV. · Bad router ID TLV—Invalid router ID TLV.

# Display detailed CSNP packet statistics on a per-interface basis. (Applicable to routers.)

<Sysname> display isis packet csnp by-interface verbose

CSNP packet information for IS-IS(1)

------------------------------------

Interface: GigabitEthernet1/0/1

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header: 0 Bad protocol description: 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type: 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

# Display detailed CSNP packet statistics on a per-interface basis. (Applicable to switches.)

<Sysname> display isis packet csnp by-interface verbose

CSNP packet information for IS-IS(1)

------------------------------------

Interface: Vlan-interface10

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header: 0 Bad protocol description: 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type: 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

# Display detailed CSNP packet statistics.

<Sysname> display isis packet csnp verbose

CSNP packet information for IS-IS(1)

------------------------------------

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

Table 18 Command output

Field | Description
Input packets with errors | Statistics for packets with the following errors: · Bad packet length—Invalid packet length. · Bad header length—Invalid header length. · Jumbo packet—The packet length exceeds the maximum length of packets that can be received. · SNPA conflict (LAN)—SNPA conflict. · Smaller than header—The packet length is smaller than the fixed header length. · Bad protocol description—Invalid protocol description. · Bad protocol ID—Invalid protocol identifier. · Bad protocol version—Invalid protocol version. · Unknown packet type—Unknown packet type. · Bad max area count—Invalid maximum number of area addresses. · No active NBR—The packet is from an unknown neighbor. · Bad system ID length—Invalid system ID length. · Mismatched level—Mismatched levels. · Bad TLV length—Invalid TLV length. · Auth failure—Authentication failure. · Bad auth TLV—Invalid authentication TLV. · Bad LSP TLV length—Invalid LSP TLV length. · Excessive auth TLVs—Excessive authentication TLVs. · Excessive LSPs—Excessive LSPs. · Bad LSP ID—Invalid LSP ID.

# Display detailed PSNP packet statistics on a per-interface basis. (Applicable to routers.)

<Sysname> display isis packet psnp by-interface verbose

PSNP packet information for IS-IS(1)

------------------------------------

Interface: GigabitEthernet1/0/1

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header: 0 Bad protocol description: 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type: 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

# Display detailed PSNP packet statistics on a per-interface basis. (Applicable to switches.)

<Sysname> display isis packet psnp by-interface verbose

PSNP packet information for IS-IS(1)

------------------------------------

Interface: Vlan-interface10

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header: 0 Bad protocol description: 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type: 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

# Display detailed PSNP packet statistics.

<Sysname> display isis packet psnp verbose

PSNP packet information for IS-IS(1)

------------------------------------

Total output packets : 0 Total output error packets : 0

Total input packets : 0 Total input error packets : 0

Input packets with errors

Bad packet length : 0 Bad header length : 0

Jumbo packet : 0 SNPA conflict (LAN) : 0

Smaller than header : 0 Bad protocol description : 0

Bad protocol ID : 0 Bad protocol version : 0

Unknown packet type : 0 Bad max area count : 0

No active NBR : 0 Bad system ID length : 0

Mismatched level : 0 Bad TLV length : 0

Auth failure : 0 Bad auth TLV : 0

Bad LSP TLV length : 0 Excessive auth TLVs : 0

Excessive LSPs : 0 Bad LSP ID : 0

Table 19 Command output

Field | Description
Input packets with errors | Statistics for packets with the following errors: · Bad packet length—Invalid packet length. · Bad header length—Invalid header length. · Jumbo packet—The packet length exceeds the maximum length of packets that can be received. · SNPA conflict (LAN)—SNPA conflict. · Smaller than header—The packet length is smaller than the fixed header length. · Bad protocol description—Invalid protocol description. · Bad protocol ID—Invalid protocol identifier. · Bad protocol version—Invalid protocol version. · Unknown packet type—Unknown packet type. · Bad max area count—Invalid maximum number of area addresses. · No active NBR—The packet is from an unknown neighbor. · Bad system ID length—Invalid system ID length. · Mismatched level—Mismatched levels. · Bad TLV length—Invalid TLV length. · Auth failure—Authentication failure. · Bad auth TLV—Invalid authentication TLV. · Bad LSP TLV length—Invalid LSP TLV length. · Excessive auth TLVs—Excessive authentication TLVs. · Excessive LSPs—Excessive LSPs. · Bad LSP ID—Invalid LSP ID.

Related commands

reset isis packet

IS-IS commands -- display isis peer

Use display isis peer to display IS-IS neighbor information.

Syntax

display isis peer [ statistics | verbose ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

statistics: Displays IS-IS neighbor statistics.

verbose: Displays detailed IS-IS neighbor information. If you do not specify this keyword, the command displays brief IS-IS neighbor information.

process-id: Displays IS-IS neighbor information for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays neighbor information for all IS-IS processes.

Examples

# Display brief IS-IS neighbor information. (Applicable to routers.)

<Sysname> display isis peer

Peer information for IS-IS(1)

-----------------------------

System Id: 0000.0000.0001

Interface: GE1/0/2 Circuit Id: 0000.0000.0001.01

State: Up HoldTime: 27s Type: L1(L1L2) PRI: 64

System Id: 0000.0000.0001

Interface: GE1/0/2 Circuit Id: 0000.0000.0001.01

State: Up HoldTime: 27s Type: L2(L1L2) PRI: 64

# Display detailed IS-IS neighbor information. (Applicable to routers.)

<Sysname> display isis peer verbose

Peer information for IS-IS(1)

----------------------------

System ID: 0000.1111.2222

Interface: GE1/0/2 Circuit Id: 0000.1111.2222.01

State: Up Holdtime: 6s Type: L1(L1L2) PRI: 64

Area address(es): 49

Peer IP address(es): 12.0.0.2

Peer local circuit ID: 1

Peer circuit SNPA address: 000c-293b-c4be

Uptime: 00:05:07

Adj protocol: IPv4

Adj P2P three-way handshake: No

Graceful Restart capable

Restarting signal: No

Suppress adjacency advertisement: No

Local topology:

0

Remote topology:

0 2

System ID: 0000.0000.0002

Interface: GE1/0/3 Circuit Id: 001

State: Up HoldTime: 27s Type: L1L2 PRI: --

Area address(es): 49

Peer IP address(es): 192.168.220.30

Peer local circuit ID: 1

Peer circuit SNPA address: 000c-29fd-ed69

Uptime: 00:05:07

Adj protocol: IPv4

Adj P2P three-way handshake: Yes

Peer extended circuit ID: 2

Graceful Restart capable

Restarting signal: No

Suppress adjacency advertisement: No

# Display brief IS-IS neighbor information. (Applicable to switches.)

<Sysname> display isis peer

Peer information for IS-IS(1)

-----------------------------

System Id: 0000.0000.0001

Interface: Vlan100 Circuit Id: 0000.0000.0001.01

State: Up HoldTime: 27s Type: L1(L1L2) PRI: 64

System Id: 0000.0000.0001

Interface: Vlan100 Circuit Id: 0000.0000.0001.01

State: Up HoldTime: 27s Type: L2(L1L2) PRI: 64

# Display detailed IS-IS neighbor information. (Applicable to switches.)

<Sysname> display isis peer verbose

Peer information for IS-IS(1)

----------------------------

System ID: 0000.1111.2222

Interface: Vlan100 Circuit Id: 0000.1111.2222.01

State: Up Holdtime: 6s Type: L1(L1L2) PRI: 64

Area address(es): 49

Peer IP address(es): 12.0.0.2

Peer local circuit ID: 1

Peer circuit SNPA address: 000c-293b-c4be

Uptime: 00:05:07

Adj protocol: IPv4

Adj P2P three-way handshake: No

Graceful Restart capable

Restarting signal: No

Suppress adjacency advertisement: No

Local topology:

0

Remote topology:

0 2

System ID: 0000.0000.0002

Interface: Vlan101 Circuit Id: 001

State: Up HoldTime: 27s Type: L1L2 PRI: --

Area address(es): 49

Peer IP address(es): 192.168.220.30

Peer local circuit ID: 1

Peer circuit SNPA address: 000c-29fd-ed69

Uptime: 00:05:07

Adj protocol: IPv4

Adj P2P three-way handshake: Yes

Peer extended circuit ID: 2

Graceful Restart capable

Restarting signal: No

Suppress adjacency advertisement: No

Table 20 Command output

Field | Description
System Id | System ID of the neighbor.
Interface | Interface connecting to the neighbor.
Circuit Id | Circuit ID.
State | Circuit state.
HoldTime | Within the holdtime, if no hellos are received from the neighbor, the neighbor is considered down. If a hello is received, the holdtime is reset to the initial value.
Type | Circuit type: · L1—Means the circuit type is Level-1 and the neighbor is a Level-1 router. · L2—Means the circuit type is Level-2 and the neighbor is a Level-2 router. · L1(L1L2)—Means the circuit type is Level-1 and the neighbor is a Level-1-2 router. · L2(L1L2)—Means the circuit type is Level-2 and the neighbor is a Level-1-2 router.
PRI | DIS priority of the neighbor.
Area address(es) | Area address of the neighbor.
Peer IP address(es) | IP address of the neighbor.
Peer IPv6 address(es) | IPv6 address of the neighbor.
Uptime | Time elapsed since the neighbor relationship was formed.
Adj Protocol | Adjacency protocol: IPv4 or IPv6.
Peer local circuit ID | Circuit ID of the neighbor.
Peer circuit SNPA address | SNPA address of the neighbor.
Adj P2P three-way handshake | Indicates whether the neighbor supports P2P three-way handshake.
Peer extended circuit ID | Extended circuit ID of the neighbor interface. This field is available when the neighbor supports three-way handshake.
Graceful Restart capable | The neighbor has the GR helper capability.
Restarting signal | RR flag.
Suppress adjacency advertisement | SA flag.
Local topology | List of topologies supported by the local interface.
Remote topology | List of topologies supported by the neighbor interface.

‌

# Display IS-IS neighbor statistics.

<Sysname> display isis peer statistics

Peer Statistics information for IS-IS(1)

---------------------------------------

Type IPv4 Up/Init IPv6 Up/Init

LAN Level-1 1/0 0/0

LAN Level-2 1/0 0/0

P2P 0/0 0/0

Table 21 Command output

Field | Description
Type | Neighbor type: · LAN Level-1—Number of Level-1 neighbors whose network type is broadcast. · LAN Level-2—Number of Level-2 neighbors whose network type is broadcast. · P2P—Number of neighbors whose network type is P2P.
IPv4 Up | Number of IPv4 neighbors in up state.
IPv4 Init | Number of IPv4 neighbors in init state.
IPv6 Up | Number of IPv6 neighbors in up state.
IPv6 Init | Number of IPv6 neighbors in init state.

‌

IS-IS commands -- display isis redistribute

Use display isis redistribute to display the redistributed IS-IS routing information.

Syntax

display isis redistribute [ ipv4 [ topology topo-name ] [ ip-address mask-length ] | ipv6 [ ipv6-address prefix-length ] ] [ level-1 | level-2 ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv4: Displays the redistributed IPv4 routing information.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays redistributed IS-IS routing information for the public network.

ipv6: Displays the redistributed IPv6 routing information.

ipv6-address prefix-length: Displays redistributed routes for the specified IPv6 address and mask length. The value range for the prefix-length argument is 1 to 128.

ip-address mask-length: Specifies the destination IP address and mask length.

process-id: Specifies the IS-IS process by its ID in the range of 1 to 65535.

level-1: Displays the IS-IS Level-1 routing information.

level-2: Displays the IS-IS Level-2 routing information.

Usage guidelines

If you do not specify the ipv4 or ipv6 keyword, the command displays redistributed IPv4 routing information.

If you do not specify an IS-IS level, this command displays both Level-1 and Level-2 routing information.

Examples

# Display redistributed IPv4 IS-IS routing information.

<Sysname> display isis redistribute 1

Route information for IS-IS(1)

------------------------------

Level-1 IPv4 Redistribute Table

--------------------------------

Type IPv4 Destination IntCost ExtCost Tag State

--------------------------------------------------------------------------------

D 192.168.30.0/24 0 0 Active

D 11.11.11.11/32 0 0

D 10.10.10.0/24 0 0

Table 22 Command output

Field | Description
Route information for IS-IS(1) | IS-IS process of the redistributed routing information.
Level-1 IPv4 Redistribute Table | Redistributed IPv4 routing information of IS-IS Level-1.
Level-2 IPv4 Redistribute Table | Redistributed IPv4 routing information of IS-IS Level-2.
Type | Redistributed route type.
IPV4 Destination | IPv4 destination address.
IntCost | Internal cost of the route.
ExtCost | External cost of the route.
Tag | Tag value.
State | Indicates whether the route is valid.

‌

# Display redistributed IPv6 IS-IS routing information.

<Sysname> display isis redistribute ipv6 1

Route information for IS-IS(1)

------------------------------

Level-1 IPv6 Redistribute Table

--------------------------------

Type : direct Destination: 12:1::/64

IntCost : 0 Tag :

State : Active

Level-2 IPv6 Redistribute Table

--------------------------------

Type : direct Destination: 12:1::/64

IntCost : 0 Tag :

State : Active

Table 23 Command output

Field | Description
Route information for IS-IS(1) | Redistributed routing information for IPv6 IS-IS process 1.
Level-1 IPv6 Redistribute Table | Redistributed IPv6 IS-IS Level-1 routing information.
Level-2 IPv6 Redistribute Table | Redistributed IPv6 IS-IS Level-2 routing information.
Type | Redistributed route types: · Direct. · IS-ISv6. · Static. · OSPFv3. · BGP4+. · RIPng.
Destination | IPv6 destination address.
IntCost | Internal route cost.
Tag | Tag value.
State | Indicates whether the redistributed route is valid.

IS-IS commands -- display isis route

Use display isis route to display IS-IS routing information.

Syntax

display isis route [ ipv4 [ topology topo-name ] [ ip-address mask-length ] | ipv6 [ ipv6-address prefix-length ] ] [ [ level-1 | level-2 ] | verbose ] * [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv4: Displays IPv4 IS-IS routing information.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays IPv4 IS-IS routing information for the public network.

ip-address mask-length: Displays IPv4 IS-IS routing information for the specified IP address. The mask-length argument is in the range of 0 to 32.

ipv6: Displays IPv6 IS-IS routing information.

ipv6-address prefix-length: Displays IPv6 IS-IS routing information for the specified IPv6 address. The prefix-length argument is in the range of 0 to 128.

verbose: Displays detailed IS-IS routing information. If you do not specify this keyword, the command displays brief IS-IS routing information

process-id: Displays IS-IS routing information for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify an IS-IS process, this command displays routing information for all IS-IS processes.

level-1: Displays Level-1 IS-IS routes.

level-2: Displays Level-2 IS-IS routes.

Usage guidelines

If you do not specify the ipv4 or ipv6 keyword, the command displays IPv4 IS-IS routing information.

If you do not specify a level, this command displays both Level-1 and Level-2 routing information.

Examples

# Display brief IPv4 IS-IS routing information. (Applicable to routers.)

<Sysname> display isis route

Route information for IS-IS(1)

-----------------------------

Level-1 IPv4 Forwarding Table

-----------------------------

IPv4 Destination IntCost ExtCost ExitInterface NextHop Flags

-------------------------------------------------------------------------------

8.8.8.0/24 10 NULL GE1/0/2 Direct D/L/-

9.9.9.0/24 20 NULL GE1/0/2 8.8.8.5 R/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Level-2 IPv4 Forwarding Table

-----------------------------

IPv4 Destination IntCost ExtCost ExitInterface NextHop Flags

-------------------------------------------------------------------------------

8.8.8.0/24 10 NULL D/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

# Display brief IPv4 IS-IS routing information. (Applicable to switches.)

<Sysname> display isis route

Route information for IS-IS(1)

-----------------------------

Level-1 IPv4 Forwarding Table

-----------------------------

IPv4 Destination IntCost ExtCost ExitInterface NextHop Flags

-------------------------------------------------------------------------------

8.8.8.0/24 10 NULL Vlan100 Direct D/L/-

9.9.9.0/24 20 NULL Vlan100 8.8.8.5 R/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Level-2 IPv4 Forwarding Table

-----------------------------

IPv4 Destination IntCost ExtCost ExitInterface NextHop Flags

-------------------------------------------------------------------------------

8.8.8.0/24 10 NULL D/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Table 24 Command output

Field | Description
Route information for IS-IS(1) | Route information for IS-IS process 1.
Level-1 IPv4 Forwarding Table | IPv4 IS-IS routing information for Level-1.
Level-2 IPv4 Forwarding Table | IPv4 IS-IS routing information for Level-2.
IPv4 Destination | IPv4 destination address.
IntCost | Internal cost.
ExtCost | External cost.
ExitInterface | Output interface.
NextHop | Next hop.
Flags | Routing state flag: · D—Direct route. · R—The route has been added into the routing table. · L—The route has been advertised in an LSP. · U—Penetration flag. Setting it to UP can prevent an LSP sent from L2 to L1 from being sent back to L2.

# Display detailed IPv4 IS-IS routing information. (Applicable to routers.)

<Sysname> display isis route verbose

Route information for IS-IS(1)

-----------------------------

Level-1 IPv4 Forwarding Table

-----------------------------

IPV4 Dest : 8.8.8.0/24 Int. Cost : 10 Ext. Cost : NULL

Admin Tag : - Src Count : 2 Flag : D/L/-

NextHop : Interface : ExitIndex :

Direct GE1/0/2 0x00000000

Nib ID : 0x0

IPV4 Dest : 9.9.9.0/24 Int. Cost : 20 Ext. Cost : NULL

Admin Tag : - Src Count : 1 Flag : R/L/-

NextHop : Interface : ExitIndex :

8.8.8.5 GE1/0/2 0x00000003

Nib ID : 0x0

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Level-2 IPv4 Forwarding Table

-----------------------------

IPV4 Dest : 8.8.8.0/24 Int. Cost : 10 Ext. Cost : NULL

Admin Tag : - Src Count : 2 Flag : D/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

# Display detailed IPv4 IS-IS routing information. (Applicable to switches.)

<Sysname> display isis route verbose

Route information for IS-IS(1)

-----------------------------

Level-1 IPv4 Forwarding Table

-----------------------------

IPV4 Dest : 8.8.8.0/24 Int. Cost : 10 Ext. Cost : NULL

Admin Tag : - Src Count : 2 Flag : D/L/-

NextHop : Interface : ExitIndex :

Direct Vlan100 0x00000000

Nib ID : 0x0

IPV4 Dest : 9.9.9.0/24 Int. Cost : 20 Ext. Cost : NULL

Admin Tag : - Src Count : 1 Flag : R/L/-

NextHop : Interface : ExitIndex :

8.8.8.5 Vlan100 0x00000003

Nib ID : 0x0

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Level-2 IPv4 Forwarding Table

-----------------------------

IPV4 Dest : 8.8.8.0/24 Int. Cost : 10 Ext. Cost : NULL

Admin Tag : - Src Count : 2 Flag : D/L/-

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Table 25 Command output

Field | Description
Route information for IS-IS(1) | Route information for IS-IS process 1.
Level-1 IPv4 Forwarding Table | IPv4 IS-IS routing information for Level-1.
Level-2 IPv4 Forwarding Table | IPv4 IS-IS routing information for Level-2.
IPV4 Dest | IPv4 destination.
Int. Cost | Internal cost.
Ext. Cost | External cost.
Admin Tag | Tag.
Src Count | Count of advertising sources.
Flag | Route state flag: · R—The route has been installed into the routing table. · L—The route has been flooded in an LSP. · U—Route leaking flag. Setting it to UP can prevent an LSP sent from L2 to L1 from being sent back to L2.
Next Hop | Next hop.
Interface | Output interface.
ExitIndex | Index of the output interface.
Nib ID | ID assigned by the routing management module (next hop index).

# Display IPv6 IS-IS routing information. (Applicable to routers.)

<Sysname> display isis route ipv6

Route information for IS-IS(1)

------------------------------

Level-1 IPv6 forwarding table

-----------------------------

Destination: 2001:1:: PrefixLen: 64

Flag : R/L/- Cost : 20

Next hop : FE80::200:5EFF:FE64:8905 Interface: GE1/0/1

Destination: 2001:2:: PrefixLen: 64

Flag : D/L/- Cost : 10

Next hop : Direct Interface: GE1/0/1

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

Level-2 IPv6 forwarding table

-----------------------------

Destination: 2001:1:: PrefixLen: 64

Flag : -/-/- Cost : 20

Destination: 2001:2:: PrefixLen: 64

Flag : D/L/- Cost : 10

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

# Display IPv6 IS-IS routing information. (Applicable to switches.)

<Sysname> display isis route ipv6

Route information for IS-IS(1)

------------------------------

Level-1 IPv6 forwarding table

-----------------------------

Destination: 2001:1:: PrefixLen: 64

Flag : R/L/- Cost : 20

Next hop : FE80::200:5EFF:FE64:8905 Interface: Vlan100

Destination: 2001:2:: PrefixLen: 64

Flag : D/L/- Cost : 10

Next hop : Direct Interface: Vlan100

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

Level-2 IPv6 forwarding table

-----------------------------

Destination: 2001:1:: PrefixLen: 64

Flag : -/-/- Cost : 20

Destination: 2001:2:: PrefixLen: 64

Flag : D/L/- Cost : 10

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

Table 26 Command output

Field | Description
Destination | IPv6 destination prefix.
PrefixLen | Length of the prefix.
Flag/Flags | Route flag: · D—This is a direct route. · R—The route has been added into the routing table. · L—The route has been advertised in an LSP. · U—Route leaking flag, indicating that the Level-1 route is from Level-2. U means the route will not be returned to Level-2.
Cost | Route cost.
Next hop | Next hop.
Interface | Output interface.

‌

# Display detailed IPv6 IS-IS routing information. (Applicable to routers.)

<Sysname> display isis route ipv6 verbose

Route information for IS-IS(1)

------------------------------

Level-1 IPv6 forwarding table

-----------------------------

IPv6 dest : 2001:1::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : Direct

Interface : GE1/0/1

Nib ID : 0x0

IPv6 dest : 2001:2::/64

Flag : R/-/- Cost : 20

Admin tag : - Src count : 2

Nexthop : FE80::200:5EFF:FE64:8905

Interface : GE1/0/1

BkNexthop : FE80::200:5EFF:FE64:8905

BkInterface : GE1/0/1

Nib ID : 0x24000002

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

Level-2 IPv6 Forwarding Table

-----------------------------

IPv6 dest : 2001:1::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : -

Interface : -

Nib ID : -

IPv6 dest : 2001:2::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : -

Interface : -

Nib ID : -

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

# Display detailed IPv6 IS-IS routing information. (Applicable to switches.)

<Sysname> display isis route ipv6 verbose

Route information for IS-IS(1)

------------------------------

Level-1 IPv6 forwarding table

-----------------------------

IPv6 dest : 2001:1::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : Direct

Interface : Vlan101

Nib ID : 0x0

IPv6 dest : 2001:2::/64

Flag : R/-/- Cost : 20

Admin tag : - Src count : 2

Nexthop : FE80::200:5EFF:FE64:8905

Interface : Vlan101

BkNexthop : FE80::200:5EFF:FE64:8905

BkInterface : Vlan101

Nib ID : 0x24000002

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down bit set

Level-2 IPv6 Forwarding Table

-----------------------------

IPv6 dest : 2001:1::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : -

Interface : -

Nib ID : -

IPv6 dest : 2001:2::/64

Flag : D/L/- Cost : 10

Admin tag : - Src count : 2

Nexthop : -

Interface : -

Nib ID : -

Flags: D-Direct, R-Added to Rib, L-Advertised in LSPs, U-Up/Down Bit Set

Table 27 Command output

Field | Description
IPv6 dest | IPv6 destination address and prefix.
Flag/Flags | Route flag: · D—This is a direct route. · R—The route has been added into the routing table. · L—The route has been advertised in an LSP. · U—Route leaking flag, indicating the Level-1 route is from Level-2. U means the route will not be returned to Level-2.
Cost | Route cost.
Admin tag | Administrative tag.
Src count | Number of advertisement sources.
Nexthop | Next hop.
Interface | Output interface.
BkNexthop | Backup next hop.
BkInterface | Backup output interface.
Nib ID | Next hop index assigned by the routing management module.

‌

IS-IS commands -- display isis spf-tree

Use display isis spf-tree to display IS-IS SPF tree information.

Syntax

display isis spf-tree [ ipv4 [ topology topo-name ] | ipv6 ] [ [ level-1 | level-2 ] | verbose ] * [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv4: Displays IPv4 IS-IS SPF tree information.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays IPv4 IS-IS SPF tree information for the public network.

ipv6: Displays IPv6 IS-IS SPF tree information.

level-1: Displays Level-1 IS-IS SPF tree information. If you do not specify a level, the command displays both Level-1 and Level-2 SPF tree information.

level-2: Displays Level-2 SPF tree information. If you do not specify a level, the command displays both Level-1 and Level-2 SPF tree information.

verbose: Displays detailed IS-IS SPF tree information. If you do not specify this keyword, the command displays brief IS-IS SPF tree information.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays SPF tree information for all IS-IS processes.

Usage guidelines

If you do not specify the ipv4 or ipv6 keyword, the command displays IPv4 IS-IS SPF tree information.

Examples

# Display brief IPv4 IS-IS SPF tree information.

<Sysname> display isis spf-tree

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

--------------------------

SpfNode NodeFlag SpfLink LinkCost LinkFlag

-------------------------------------------------------------------------------

0000.0000.0032.00 S/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/C/-/-/-/-/-/-

-->0000.0000.0064.00 10 -/-/C/-/-/-/-/-/-

0000.0000.0032.01 S/-/-/R/-/-

-->0000.0000.0064.00 0 -/-/C/-/-/-/-/-/-

-->0000.0000.0032.00 0 -/-/-/P/-/-/-/-/-

0000.0000.0064.00 S/-/-/R/-/-

-->0000.0000.0032.00 10 -/-/-/P/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/-/P/-/-/-/-/-

Level-2 Shortest Path Tree

--------------------------

SpfNode NodeFlag SpfLink LinkCost LinkFlag

-------------------------------------------------------------------------------

0000.0000.0032.00 S/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/C/-/-/-/-/-/-

-->0000.0000.0064.00 10 -/-/C/-/-/-/-/-/-

0000.0000.0032.01 S/-/-/R/-/-

-->0000.0000.0064.00 0 -/-/C/-/-/-/-/-/-

-->0000.0000.0032.00 0 -/-/-/P/-/-/-/-/-

0000.0000.0064.00 S/-/-/R/-/-

-->0000.0000.0032.00 10 -/-/-/P/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/-/P/-/-/-/-/-

# Display detailed IPv4 IS-IS SPF tree information. (Applicable to routers.)

<Sysname> display isis spf-tree verbose

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0001.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Adjacent Interface: N/A

Cost: 10 Nexthop : N/A

SpfNode : 0000.0000.0004.00

Distance : 10

Te Distance : 10

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x14000000

TE tunnel count: 1

Destination: 4.4.4.4 Interface : Tun0

TE cost : 10 Final cost : 10

Add nexthop: YES Add TLV : YES

Nexthop count : 2

Neighbor : 0000.0000.0004.00 Interface : Tun0

Nexthop : 4.4.4.4

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

Neighbor : 0000.0000.0004.00 Interface : GE1/0/1

Nexthop : 1.1.1.3

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 10 Nexthop : N/A

AdvMtID: 0

SpfNode : 0000.0000.0004.04

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x14000001

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0001.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 0 Nexthop : N/A

-->0000.0000.0004.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: GE1/0/1

Cost: 0 Nexthop : 1.1.1.3

Level-2 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0001.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Adjacent Interface: N/A

Cost: 10 Nexthop : N/A

SpfNode : 0000.0000.0004.00

Distance : 10

TE distance : 10

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 1

Destination: 4.4.4.4 Interface : Tun0

TE cost : 10 Final cost : 10

Add nexthop: YES Add TLV : YES

Nexthop count : 2

Neighbor : 0000.0000.0004.00 Interface : Tun0

Nexthop : 4.4.4.4

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

Neighbor : 0000.0000.0004.00 Interface : GE1/0/1

Nexthop : 1.1.1.3

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 10 Nexthop : N/A

AdvMtID: 0

SpfNode : 0000.0000.0004.04

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0001.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 0 Nexthop : N/A

-->0000.0000.0004.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: GE1/0/1

Cost: 0 Nexthop : 1.1.1.3

# Display detailed IPv4 IS-IS SPF tree information. (Applicable to switches.)

<Sysname> display isis spf-tree verbose

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0001.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Adjacent Interface: N/A

Cost: 10 Nexthop : N/A

SpfNode : 0000.0000.0004.00

Distance : 10

Te Distance : 10

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x14000000

TE tunnel count: 1

Destination: 4.4.4.4 Interface : Tun0

TE cost : 10 Final cost : 10

Add nexthop: YES Add TLV : YES

Nexthop count : 2

Neighbor : 0000.0000.0004.00 Interface : Tun0

Nexthop : 4.4.4.4

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

Neighbor : 0000.0000.0004.00 Interface : Vlan50

Nexthop : 1.1.1.3

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 10 Nexthop : N/A

AdvMtID: 0

SpfNode : 0000.0000.0004.04

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x14000001

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0001.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 0 Nexthop : N/A

-->0000.0000.0004.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: Vlan50

Cost: 0 Nexthop : 1.1.1.3

Level-2 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0001.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Adjacent Interface: N/A

Cost: 10 Nexthop : N/A

SpfNode : 0000.0000.0004.00

Distance : 10

TE distance : 10

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 1

Destination: 4.4.4.4 Interface : Tun0

TE cost : 10 Final cost : 10

Add nexthop: YES Add TLV : YES

Nexthop count : 2

Neighbor : 0000.0000.0004.00 Interface : Tun0

Nexthop : 4.4.4.4

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

Neighbor : 0000.0000.0004.00 Interface : Vlan50

Nexthop : 1.1.1.3

BkNeighbor : N/A BkInterface: N/A

BkNexthop : N/A

SpfLink count : 1

-->0000.0000.0004.04

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 10 Nexthop : N/A

AdvMtID: 0

SpfNode : 0000.0000.0004.04

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0001.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: N/A

Cost: 0 Nexthop : N/A

-->0000.0000.0004.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type: Remote Interface: Vlan50

Cost: 0 Nexthop : 1.1.1.3

Table 28 Command output

Field | Description
SpfNode | ID of the topology node.
Distance | Shortest distance from the root node to the local node.
TE distance | Shortest distance from the root node to the local node (including tunnel links). If tunnel is not configured, TE distance equals to Distance.
NodeFlag | Node flag: · S—The node is on the SPF tree. · T—The node is on the tent list. · O—The node is overloaded. · R—The node is directly connected. · I—The node is isolated. · D—The node is to be deleted.
RelayNibID | Next hop ID of the node after route recursion.
TE tunnel count | Number of tunnels destined to this node.
Destination | Destination router.
TE cost | IGP cost of the TE tunnel.
Final cost | Final cost of the TE tunnel.
Nexthop count | Next hop count.
Nexthop | Primary next hop of the node or the link advertising source.
AdvMtID | Topology from which the routing information is learned: · 0—Base topology. · 6-4094—Other topologies.
Interface | Primary output interface of the node or the link advertising source.
BkNexthop | Backup next hop.
BkInterface | Backup output interface.
Neighbor | ID of the primary next hop neighbor.
BkNeighbor | ID of the backup next hop neighbor.
SpfLink | Topology link.
SpfLink count | Number of topology links.
LinkCost | Link cost.
LinkNewCost | New link cost.
LinkFlag | Link flag: · I—The link is isolated. · D—The link is to be deleted. · C—The neighbor is a child node. · P—The neighbor is the parent node. · V—The link is involved. · N—The link is a new path. · L—The link is on the change list. · U—The protocol usage of the link is changed. · H—The next hop of the link is changed.
LinkSrcCnt | Number of link advertising sources.
Type | Type of the link advertising source: · Adjacent—The link advertising source is a local neighbor. · Remote—The link advertising source is advertised by a remote node in an LSP.
Cost | Cost of the link advertising source.

# Display brief IPv6 IS-IS SPF tree information.

<Sysname> display isis spf-tree ipv6

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

----------------------------------

SpfNode NodeFlag SpfLink LinkCost LinkFlag

-------------------------------------------------------------------------------

0000.0000.0032.00 S/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/C/-/-/-/-/-/-

-->0000.0000.0064.00 10 -/-/C/-/-/-/-/-/-

0000.0000.0032.01 S/-/-/R/-/-

-->0000.0000.0064.00 0 -/-/C/-/-/-/-/-/-

-->0000.0000.0032.00 0 -/-/-/P/-/-/-/-/-

0000.0000.0064.00 S/-/-/R/-/-

-->0000.0000.0032.00 10 -/-/-/P/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/-/P/-/-/-/-/-

Level-2 Shortest Path Tree

----------------------------------

SpfNode NodeFlag SpfLink LinkCost LinkFlag

-------------------------------------------------------------------------------

0000.0000.0032.00 S/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/C/-/-/-/-/-/-

-->0000.0000.0064.00 10 -/-/C/-/-/-/-/-/-

0000.0000.0032.01 S/-/-/R/-/-

-->0000.0000.0064.00 0 -/-/C/-/-/-/-/-/-

-->0000.0000.0032.00 0 -/-/-/P/-/-/-/-/-

0000.0000.0064.00 S/-/-/R/-/-

-->0000.0000.0032.00 10 -/-/-/P/-/-/-/-/-

-->0000.0000.0032.01 10 -/-/-/P/-/-/-/-/-

# Display detailed Level-1 IPv6 IS-IS SPF tree information. (Applicable to routers.)

<Sysname> display isis spf-tree ipv6 level-1 verbose

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0032.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0032.01

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: N/A

Cost : 10 Nexthop : N/A

-->0000.0000.0064.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: Tun1

Cost : 10 Nexthop : FE80::A0A:A40

SpfNode : 0000.0000.0032.01

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0064.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: GE1/0/2

Cost : 10 Nexthop : FE80::200:12FF:FE34:1

-->0000.0000.0032.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: N/A

Cost : 0 Nexthop : N/A

SpfNode : 0000.0000.0064.00

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 2

Neighbor : 0000.0000.0064.00 Interface : GE1/0/2

NextHop : FE80::200:12FF:FE34:1

BkNeighbor: N/A BkInterface: N/A

BkNextHop : N/A

Neighbor : 0000.0000.0064.00 Interface : Tun1

NextHop : FE80::A0A:A40

BkNeighbor: N/A BkInterface: N/A

BkNextHop : N/A

SpfLink count : 2

-->0000.0000.0032.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type : Remote Interface: N/A

Cost : 10 Nexthop : N/A

AdvMtID : 0

-->0000.0000.0064.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Remote Interface: Tun1

Cost : 10 Nexthop : FE80::A0A:A40

AdvMtID : 0

# Display detailed Level-1 IPv6 IS-IS SPF tree information. (Applicable to switches.)

<Sysname> display isis spf-tree ipv6 level-1 verbose

Shortest Path Tree for IS-IS(1)

-------------------------------

Flags: S-Node is on SPF tree T-Node is on tent list

O-Node is overload R-Node is directly reachable

I-Node or Link is isolated D-Node or Link is to be deleted

C-Neighbor is child P-Neighbor is parent

V-Link is involved N-Link is a new path

L-Link is on change list U-Protocol usage is changed

H-Nexthop is changed

Level-1 Shortest Path Tree

--------------------------

SpfNode : 0000.0000.0032.00

Distance : 0

TE distance : 0

NodeFlag : S/-/-/-/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0032.01

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: N/A

Cost : 10 Nexthop : N/A

-->0000.0000.0064.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: Tun1

Cost : 10 Nexthop : FE80::A0A:A40

SpfNode : 0000.0000.0032.01

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 0

SpfLink count : 2

-->0000.0000.0064.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: Vlan2

Cost : 10 Nexthop : FE80::200:12FF:FE34:1

-->0000.0000.0032.00

LinkCost : 0

LinkNewCost : 0

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type : Adjacent Interface: N/A

Cost : 0 Nexthop : N/A

SpfNode : 0000.0000.0064.00

Distance : 10

TE distance : 10

NodeFlag : S/-/-/R/-/-

RelayNibID : 0x0

TE tunnel count: 0

Nexthop count : 2

Neighbor : 0000.0000.0064.00 Interface : Vlan2

NextHop : FE80::200:12FF:FE34:1

BkNeighbor: N/A BkInterface: N/A

BkNextHop : N/A

Neighbor : 0000.0000.0064.00 Interface : Tun1

NextHop : FE80::A0A:A40

BkNeighbor: N/A BkInterface: N/A

BkNextHop : N/A

SpfLink count : 2

-->0000.0000.0032.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/-/P/-/-/-/-/-

LinkSrcCnt : 1

Type : Remote Interface: N/A

Cost : 10 Nexthop : N/A

AdvMtID : 0

-->0000.0000.0064.00

LinkCost : 10

LinkNewCost : 10

LinkFlag : -/-/C/-/-/-/-/-/-

LinkSrcCnt : 1

Type : Remote Interface: Tun1

Cost : 10 Nexthop : FE80::A0A:A40

AdvMtID : 0

Table 29 Command output

Field | Description
SpfNode | ID of the topology node.
Distance | Shortest distance from the root node to the current node.
TE distance | Shortest distance from the root node to the current node (including tunnel links). If no tunnels are configured, TE distance equals Distance.
NodeFlag | Node flag: · S—The node is on the SPF tree. · T—The node is on the tent list. · O—The node is overloaded. · R—The node is directly connected. · I—The node is isolated. · D—The node is to be deleted.
TE tunnel count | Number of tunnels destined for this node.
Nexthop count | Number of next hops.
NextHop | Primary next hop of the node or the link advertising source.
AdvMtID | Topology from which the routing information is learned: · 0—Base topology. · 6-4094—Other topologies.
Interface | Primary output interface of the node or the link advertising source.
BkNextHop | Backup next hop.
BkInterface | Backup output interface.
Neighbor | ID of the primary next hop neighbor.
BkNeighbor | ID of the backup next hop neighbor.
SpfLink | Topology link.
SpfLink count | Number of topology links.
LinkCost | Link cost.
LinkNewCost | New link cost.
LinkFlag | Link flag: · I—The link is isolated. · D—The link is to be deleted. · C—The neighbor is a child node. · P—The neighbor is the parent node. · V—The link is involved. · N—The link is a new path. · L—The link is on the change list. · U—The protocol of the link is changed. · H—The next hop of the link is changed.
LinkSrcCnt | Number of link advertising sources.
Type | Type of the link advertising source: · Adjacent—The link advertising source is a local neighbor. · Remote—The link advertising source is advertised by a remote node in an LSP.
Cost | Cost of the link advertising source.

‌

IS-IS commands -- display isis statistics

Use display isis statistics to display IS-IS statistics.

Syntax

display isis statistics [ ipv4 [ topology topo-name ] | ipv6 ] [ level-1 | level-1-2 | level-2 ] [ process-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv4: Displays IPv4 IS-IS statistics. If you do not specify this option, the command displays both IPv4 and IPv6 statistics.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays IS-IS statistics for the public network.

ipv6: Displays IPv6 IS-IS statistics.

level-1: Displays IS-IS Level-1 statistics.

level-1-2: Displays IS-IS Level-1-2 statistics.

level-2: Displays IS-IS Level-2 statistics.

process-id: Displays statistics for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify an IS-IS process, this command displays the statistics for all IS-IS processes.

Usage guidelines

If you do not specify a level, this command displays both Level-1 and Level-2 routing information.

Examples

# Display IS-IS statistics.

<Sysname> display isis statistics

Statistics information for IS-IS(1)

----------------------------------

Level-1 Statistics

------------------

MTR(base)

Learnt routes information:

Total IPv4 Learnt Routes in IPv4 Routing Table: 1

Imported routes information:

IPv4 Imported Routes:

Static: 0 Direct: 0

ISIS: 0 BGP: 0

RIP: 0 OSPF: 0

Total Number: 0

MTR(base)

Learnt routes information:

Total IPv6 Learnt Routes in IPv6 Routing Table: 0

Imported routes information:

IPv6 Imported Routes:

Static: 0 Direct: 0

ISISv6: 0 BGP4+: 0

RIPng: 0 OSPFv3: 0

Total Number: 0

Lsp information:

LSP Source ID: No. of used LSPs

7777.8888.1111 001

Level-2 Statistics

------------------

MTR(base)

Learnt routes information:

Total IPv4 Learnt Routes in IPv4 Routing Table: 0

Imported routes information:

IPv4 Imported Routes:

Static: 0 Direct: 0

ISIS: 0 BGP: 0

RIP: 0 OSPF: 0

Total Number: 0

MTR(base)

Learnt routes information:

Total IPv6 Learnt Routes in IPv6 Routing Table: 0

Imported routes information:

IPv6 Imported Routes:

Static: 0 Direct: 0

ISISv6: 0 BGP4+: 0

RIPng: 0 OSPFv3: 0

Total Number: 0

Lsp information:

LSP Source ID: No. of used LSPs

7777.8888.1111 001

Table 30 Command output

Field | Description
Statistics information for IS-IS(processid) | Statistics for the IS-IS process.
Level-1 Statistics | Level-1 statistics.
Level-2 Statistics | Level-2 statistics.
MTR(topo-name) | MTR topology. base represents the base topology.
Learnt routes information | · Total IPv4 Learnt Routes in IPv4 Routing Table—Number of learned IPv4 routes. · Total IPv6 Learnt Routes in IPv6 Routing Table—Number of learned IPv6 routes.
IPv4 Imported Routes | Numbers of different types of redistributed IPv4 routes, including static, direct, IS-IS, BGP, RIP, and OSPF routes.
IPv6 Imported Routes | Numbers of different types of redistributed IPv6 routes, including static, direct, IS-ISv6, BGP4+, RIPng, and OSPFv3 routes.
Lsp information | LSP information: · LSP Source ID—ID of the source system. · No. of used LSPs—Number of used LSPs.

IS-IS commands -- display osi

Use display osi to display OSI connection information.

Syntax

Centralized devices:

display osi

Distributed devices in standalone mode:Centralized IRF devices:

display osi [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display osi [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays OSI connection information for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays OSI connection information for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays OSI connection information for all member devices if you do not specify a member device. On an IRF 3 system, this command displays information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays OSI connection information for all cards on all IRF member devices. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays OSI connection information for all cards if you do not specify a card. On an IRF 3 system, this command displays OSI connection information for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# (Centralized devices.) Display OSI connection information. (Applicable to routers.)

<Sysname> display osi

Total OSI socket number: 2

Location:

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

GigabitEthernet1/0/1

MAC address: 0180-c200-0014

Location:

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

GigabitEthernet1/0/1

MAC address: 0180-c200-0014

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Display OSI connection information. (Applicable to routers.)

<Sysname> display osi

Total OSI socket number: 2

Location: slot 0 cpu 0

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

GigabitEthernet1/0/1

MAC address: 0180-c200-0014

Location: slot 0 cpu 0

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

GigabitEthernet1/0/1

MAC address: 0180-c200-0014

# (Centralized devices.) Display OSI connection information. (Applicable to switches.)

<Sysname> display osi

Total OSI socket number: 2

Location:

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

Vlan-interface100

MAC address: 0180-c200-0014

Location:

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

Vlan-interface100

MAC address: 0180-c200-0014

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Display OSI connection information. (Applicable to switches.)

<Sysname> display osi

Total OSI socket number: 2

Location: slot 0 cpu 0

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

Vlan-interface100

MAC address: 0180-c200-0014

Location: slot 0 cpu 0

Creator: isisd[1539]

State: N/A

Options: SO_FILTER

Error: 0

Receiving buffer(cc/hiwat/lowat/drop/state): 0 / 1048576 / 1 / 0 / N/A

Sending buffer(cc/hiwat/lowat/state): 0 / 262144 / 512 / N/A

Type: 2

Enabled interfaces:

Vlan-interface100

MAC address: 0180-c200-0014

Table 31 Command output

Field | Description
Total OSI socket number | Total number of OSI sockets.
Cpu | CPU number.
Creator | Name of the socket creator. The process ID of the creator is displayed in the square brackets.
State | This field always displays N/A.
Options | Socket options: · SO_FILTER—Filter option is configured. · N/A—No option is configured.
Error | Number of errors that affect the socket session.
Receiving buffer(cc/hiwat/lowat/drop/state) | Receiving buffer information, including the current used space, maximum space, minimum space, number of dropped packets, and status.
Sending buffer(cc/hiwat/lowat/state) | Sending buffer information, including the current used space, maximum space, minimum space, and status.
Type | Type 2 socket, corresponding to unreliable connectionless-oriented transport layer protocols.
Enabled interfaces | Input interfaces and matched multicast MAC addresses. Only packets received from Ethernet link-layer interfaces need to match the multicast MAC addresses.

IS-IS commands -- display osi statistics

Use display osi statistics to display OSI packet statistics.

Syntax

Centralized devices:

display osi statistics

Distributed devices in standalone mode:Centralized IRF devices:

display osi statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display osi statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays OSI packet statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays OSI packet statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays OSI packet statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays information for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays OSI packet statistics for all cards on all IRF member devices. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays OSI packet statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays OSI packet statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display OSI packet statistics.

<Sysname> display osi statistics

Received packets:

Total: 35

Relay received: 35

Relay forwarded: 35

Invalid service slot: 0

No matched socket: 0

Not delivered, input socket full: 0

Sent packets:

Total: 19

Relay forwarded: 19

Relay received: 19

Failed: 0

Table 32 Command output

Field | Description
Received packets | Statistics of received packets: · Total—Total number of received link layer packets. · Relay received—Number of inbound packets on LPUs relayed from other cards. This count is not included in the total count of received packets. · Relay forwarded—Number of inbound packets relayed to LPUs. · Invalid service slot—Number of discarded packets due to unavailable LPUs. · No matched socket—Number of discarded packets due to mismatches in input interfaces, MAC addresses, or connection filter criteria. · Not delivered, input socket full—Number of undelivered packets due to a socket receiving buffer overflow.
Sent packets | Statistics of sent packets: · Total—Total number of packets that IS-IS sent over OSI connections. · Relay forwarded—Number of outbound packets relayed to the cards that hosts the output interfaces. This count is not included in the total count of sent packets. · Relay received—Number of outbound packets on the cards that hosts the output interfaces. These packets are relayed from other cards. · Failed—Number of packets failed to be sent.

Related commands

reset osi statistics

IS-IS commands -- distribute bgp-ls

Use distribute bgp-ls to advertise IS-IS link state information to BGP.

Use undo distribute bgp-ls to restore the default.

Syntax

distribute bgp-ls [ instance-id id ] [ level-1 | level-2 ]

undo distribute bgp-ls [ level-1 | level-2 ]

Default

The device does not advertise IS-IS link state information to BGP.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

instance-id id: Specifies an instance by its ID in the range of 0 to 65535. If you do not specify this option, the command advertises IS-IS link state information of instance 0 to BGP.

level-1: Advertises the Level-1 IS-IS link state information to BGP.

level-2: Advertises the Level-2 IS-IS link state information to BGP.

Usage guidelines

After the device advertises IS-IS link state information to BGP, BGP can advertise the information for intended applications.

If multiple IS-IS processes have the same instance ID and link state information, only the link state information of the IS-IS process with the smallest process ID is advertised.

To advertise the same link state information of different IS-IS processes to BGP, specify different instance IDs for the IS-IS processes.

If you do not specify a level for the distribute bgp-ls command, both Level-1 and Level-2 IS-IS link state information are advertised to BGP.

If you do not specify a level for the undo distribute bgp-ls command, neither Level-1 nor Level-2 IS-IS link state information can be advertised to BGP.

Examples

# Advertise link state information of IS-IS process 1 to BGP.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] distribute bgp-ls

IS-IS commands -- domain-authentication send-only

Use domain-authentication send-only to configure IS-IS not to check the authentication information in the received Level-2 packets, including LSPs, CSNPs, and PSNPs.

Use undo domain-authentication send-only to restore the default.

Syntax

domain-authentication send-only

undo domain-authentication send-only

Default

When domain authentication mode and key are configured, a Level-2 or Level-1-2 router checks the authentication information in the received packets.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When domain authentication mode and key are configured, a Level-2 or Level-1-2 router adds the key in the specified mode into transmitted Level-2 packets (including LSPs, CSNPs, and PSNPs). It also checks the key in the received Level-2 packets.

To prevent packet exchange failure in case of an authentication key change, configure IS-IS not to check the authentication information in the received packets.

Examples

# Configure IS-IS not to check the authentication information in the received packets.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] domain-authentication send-only

Related commands

area-authentication send-only

domain-authentication-mode

isis authentication send-only

IS-IS commands -- domain-authentication-mode

Use domain-authentication-mode to specify the routing domain authentication mode and a key.

Use undo domain-authentication-mode to restore the default.

Syntax

domain-authentication-mode { { gca key-id { hmac-sha-1 | hmac-sha-224 | hmac-sha-256 | hmac-sha-384 | hmac-sha-512 } [ nonstandard ] | md5 | simple } { cipher | plain } string | keychain keychain-name } [ ip | osi ]

undo domain-authentication-mode

Default

No routing domain authentication mode or key is configured.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

gca: Specifies the GCA mode.

key-id: Uniquely identifies an SA in the range of 1 to 65535. The sender inserts the Key ID into the authentication TLV, and the receiver authenticates the packet by using the SA that is selected based on the Key ID.

hmac-sha-1: Specifies the HMAC-SHA-1 algorithm.

hmac-sha-224: Specifies the HMAC-SHA-224 algorithm.

hmac-sha-256: Specifies the HMAC-SHA-256 algorithm.

hmac-sha-384: Specifies the HMAC-SHA-384 algorithm.

hmac-sha-512: Specifies the HMAC-SHA-512 algorithm.

nonstandard: Specifies the nonstandard GCA authentication mode.

md5: Specifies the MD5 authentication mode.

simple: Specifies the simple authentication mode.

cipher: Specifies a key in encrypted form.

plain: Specifies a key in plaintext form. For security purposes, the key specified in plaintext form will be stored in encrypted form.

string: Specifies the key. Its plaintext form is a case-sensitive string of 1 to 16 characters. Its encrypted form is a case-sensitive string of 33 to 53 characters.

keychain: Specifies the keychain authentication mode.

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters.

ip: Checks IP-related fields in LSPs.

osi: Checks OSI-related fields in LSPs.

Usage guidelines

The configured key in the specified mode is inserted into all outgoing Level-2 packets (LSP, CSNP, and PSNP) and is used for authenticating the incoming Level-2 packets.

IS-IS keychain authentication can operate correctly only when the keys in the keychain use the HMAC-MD5 authentication algorithm.

· Before IS-IS sends a Level-2 packet, it uses the valid send key obtained from the keychain to authenticate the packet. If no valid send key exists or the valid send key does not use the HMAC-MD5 algorithm, the authentication fails and the packet does not contain the authentication information.

· After IS-IS receives a Level-2 packet, it uses a valid accept key obtained from the keychain to authenticate the packet. If no valid accept key exists or all valid accept keys fail to authenticate the packet, the authentication fails and the packet is discarded.

All the backbone routers must have the same authentication mode and key.

If neither ip nor osi is specified, the OSI-related fields in LSPs are checked.

When you specify the GCA mode, follow these guidelines:

· If you do not specify the nonstandard keyword, the device can communicate only with devices that use the GCA mode.

· If you specify the nonstandard keyword, the device can communicate only with devices that use the nonstandard GCA mode.

Examples

# Set the routing domain authentication mode to simple, and set the plaintext key to 123456.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] domain-authentication-mode plain 123456

Related commands

area-authentication-mode

domain-authentication send-only

isis authentication-mode

IS-IS commands -- fast-reroute

Use fast-reroute to configure IS-IS FRR.

Use undo fast-reroute to disable IS-IS FRR.

Syntax

fast-reroute { lfa | route-policy route-policy-name }

undo fast-reroute

Default

IS-IS FRR is disabled.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

lfa: Calculates a backup next hop through Loop Free Alternate (LFA) calculation for all routes.

route-policy route-policy-name: Uses the specified routing policy to designate a backup next hop. The route-policy-name argument is a case-sensitive string of 1 to 63 characters.

Usage guidelines

ECMP routes do not support FRR.

The LFA calculation of FRR and IS-IS TE are mutually exclusive.

Example

# Enable FRR for IS-IS process 1 and configure IS-IS FRR to calculate a backup next hop through LFA calculation for all routes.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] fast-reroute lfa

IS-IS commands -- filter-policy export

Use filter-policy export to configure IS-IS to filter redistributed routes.

Use undo filter-policy export to remove the configuration.

Syntax

filter-policy { acl-number | prefix-list prefix-list-name | route-policy route-policy-name } export [ protocol [ process-id ] ]

undo filter-policy export [ protocol [ process-id ] ]

Default

IS-IS does not filter redistributed routes.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

acl-number: Specifies an ACL by its number in the range of 2000 to 3999 to filter redistributed routes.

prefix-list prefix-list-name: Specifies a prefix list by its name, a case-sensitive string of 1 to 63 characters, to filter redistributed routes by destination address.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter redistributed routes.

protocol: Filters routes redistributed from the specified routing protocol. If no protocol is specified, the command filters all redistributed routes.

process-id: Specifies a process by its ID in the range of 1 to 65535. This argument is available only when the protocol is isis, ospf, rip, isisv6, ospfv3, or ripng. The default process ID is 1.

Usage guidelines

This command filters routes redistributed by the import-route command. Only routes that have not been filtered can be advertised.

To use an advanced ACL (with a number from 3000 to 3999) in the command, configure the ACL using one of the following methods:

· To deny/permit a route with the specified destination, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard command.

· To deny/permit a route with the specified destination and mask, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard destination dest-addr dest-wildcard command.

The source keyword specifies the destination address of a route and the destination keyword specifies the subnet mask of the route. For the configuration to take effect, specify a contiguous subnet mask.

Examples

# Use basic ACL 2000 to filter redistributed routes.

<Sysname> system-view

[Sysname] acl basic 2000

[Sysname-acl-ipv4-basic-2000] rule deny source 192.168.10.0 0.0.0.255

[Sysname-acl-ipv4-basic-2000] quit

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] filter-policy 2000 export

# Configure advanced ACL 3000 to permit only route 113.0.0.0/16 to pass. Use advanced ACL 3000 to filter redistributed routes.

<Sysname> system-view

[Sysname] acl advanced 3000

[Sysname-acl-ipv4-adv-3000] rule 10 permit ip source 113.0.0.0 0 destination 255.255.0.0 0

[Sysname-acl-ipv4-adv-3000] rule 100 deny ip

[Sysname-acl-ipv4-adv-3000] quit

[Sysname] isis 1

[Sysname-isis 1] address-family ipv4

[Sysname-isis-1-ipv4] filter-policy 3000 export

Related commands

display isis route

IS-IS commands -- filter-policy import

Use filter-policy import to configure IS-IS to filter routes calculated using received LSPs.

Use undo filter-policy import to restore the default.

Syntax

filter-policy { acl-number | prefix-list prefix-list-name | route-policy route-policy-name } import

undo filter-policy import

Default

IS-IS does not filter routes calculated using received LSPs.

Views

IS-IS IPv4 unicast address family vie w

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

acl-number: Specifies an ACL by its number in the range of 2000 to 3999 to filter routes calculated using received LSPs.

prefix-list prefix-list-name: Specifies a prefix list by its name, a case-sensitive string of 1 to 63 characters, to filter routes calculated using received LSPs by destination address.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter received routes.

Usage guidelines

This command filters received routes. Only routes that have not been filtered can be added into the routing table.

To use an advanced ACL (with a number from 3000 to 3999) in the command, configure the ACL using one of the following methods:

· To deny/permit a route with the specified destination, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard command.

· To deny/permit a route with the specified destination and mask, use the rule [ rule-id ] { deny | permit } ip source sour-addr sour-wildcard destination dest-addr dest-wildcard command.

The source keyword specifies the destination address of a route and the destination keyword specifies the subnet mask of the route. For the configuration to take effect, specify a contiguous subnet mask.

Examples

# Use basic ACL 2000 to filter routes calculated using received LSPs.

<Sysname> system-view

[Sysname] acl basic 2000

[Sysname-acl-ipv4-basic-2000] rule deny source 192.168.10.0 0.0.0.255

[Sysname-acl-ipv4-basic-2000] quit

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] filter-policy 2000 import

# Use advanced ACL 3000 to filter routes calculated using received LSPs and install only route 113.0.0.0/16 to the IP routing table.

<Sysname> system-view

[Sysname] acl advanced 3000

[Sysname-acl-ipv4-adv-3000] rule 10 permit ip source 113.0.0.0 0 destination 255.255.0.0 0

[Sysname-acl-ipv4-adv-3000] rule 100 deny ip

[Sysname-acl-ipv4-adv-3000] quit

[Sysname] isis 1

[Sysname-isis 1] address-family ipv4

[Sysname-isis-1-ipv4] filter-policy 3000 import

Related commands

display ip routing-table

IS-IS commands -- flash-flood

Use flash-flood to enable IS-IS LSP flash flooding.

Use undo flash-flood to disable IS-IS LSP flash flooding.

Syntax

flash-flood [ flood-count flooding-count | max-timer-interval flooding-interval | [ level-1 | level-2 ] ] *

undo flash-flood [ level-1 | level-2 ]

Default

IS-IS LSP flash flooding is disabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

flood-count flooding-count: Specifies the maximum number of LSPs to be flooded before the next SPF calculation, in the range of 1 to 15. The default is 5.

max-timer-interval flooding-interval: Specifies the delay of the flash flooding, in the range of 10 to 50000 milliseconds. The default is 10.

level-1: Enables flash flooding for Level-1.

level-2: Enables flash flooding for Level-2.

Usage guidelines

If no level is specified, the command enables IS-IS LSP flash flooding for both Level-1 and Level-2.

Examples

# Enable fast flooding, and set the maximum LSPs to be sent to 10 and the delay time to 100 milliseconds.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] flash-flood flood-count 10 max-timer-interval 100

IS-IS commands -- graceful-restart

Use graceful-restart to enable IS-IS GR.

Use undo graceful-restart to disable IS-IS GR.

Syntax

graceful-restart

undo graceful-restart

Default

IS-IS GR is disabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

IS-IS GR and IS-IS NSR are mutually exclusive. Therefore, do not configure the graceful-restart command and the non-stop-routing command at the same time.

Examples

# Enable GR for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] graceful-restart

Related commands

graceful-restart suppress-sa

IS-IS commands -- graceful-restart suppress-sa

Use graceful-restart suppress-sa to suppress the Suppress-Advertisement (SA) bit during restart.

Use undo graceful-restart suppress-sa to restore the default.

Syntax

graceful-restart suppress-sa

undo graceful-restart suppress-sa

Default

The SA bit is set during restart.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Suppressing the SA bit is mainly for avoiding black hole route. If a router starts or reboots without keeping the local forwarding table, sending packets to the router might result in severe packet loss. To avoid this, you can set the SA bit of the hello packet sent by the GR restarter to 1. Upon receiving such hello packets, the GR helpers will not advertise the GR restarter through LSP.

Examples

# Suppress the SA bit during graceful restart.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] graceful-restart suppress-sa

Related commands

graceful-restart

IS-IS commands -- graceful-restart t1

Use graceful-restart t1 to set the T1 timer.

Use undo graceful-restart t1 to restore the default.

Syntax

graceful-restart t1 seconds count count

undo graceful-restart t1

Default

The T1 timer is 3 seconds and can expire 10 times.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the T1 timer in the range of 3 to 10 seconds.

count: Specifies the number of times that the T1 timer can expire, in the range of 1 to 20.

Usage guidelines

The T1 timer specifies the number of times that GR restarter can send a Restart TLV with the RR bit set. After restart, the GR restarter sends a Restart TLV with the RR bit set to its neighbor. If the restarting router receives a Restart TLV with the RA set from its neighbor before the T1 timer expires, the GR process starts. Otherwise, the GR process fails.

Examples

# Set the T1 timer of IS-IS process 1 to 5 seconds, and the expiration times to 5.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] graceful-restart t1 5 count 5

Related commands

graceful-restart

graceful-restart t2

graceful-restart t3

IS-IS commands -- graceful-restart t2

Use graceful-restart t2 to set the T2 timer.

Use undo graceful-restart t2 to restore the default.

Syntax

graceful-restart t2 seconds

undo graceful-restart t2

Default

The T2 timer is 60 seconds.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the T2 timer in the range of 30 to 65535 seconds.

Usage guidelines

The T2 timer specifies the LSDB synchronization interval. Each LSDB has a T2 timer. The Level-1-2 router has two T2 timers: a Level-1 timer and a Level-2 timer. If the LSDBs have not achieved synchronization before the two timers expire, the GR process fails.

Examples

# Set the T2 timer of IS-IS process 1 to 50 seconds.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] graceful-restart t2 50

Related commands

graceful-restart

graceful-restart t1

graceful-restart t3

IS-IS commands -- graceful-restart t3

Use graceful-restart t3 to set the T3 timer.

Use undo graceful-restart t3 to restore the default.

Syntax

graceful-restart t3 seconds

undo graceful-restart t3

Default

The T3 timer is 300 seconds.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the T3 timer in the range of 300 to 65535 seconds.

Usage guidelines

The T3 timer specifies the GR interval. The GR interval is set as the holdtime in hello PDUs. Within the interval, the neighbors maintain their adjacency with the GR restarter. If the GR process has not completed within the holdtime, the neighbors tear down the neighbor relationship and the GR process fails.

Examples

# Set the T3 timer of IS-IS process 1 to 500 seconds.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] graceful-restart t3 500

Related commands

graceful-restart

graceful-restart t1

graceful-restart t2

IS-IS commands -- ignore-att

Use ignore-att to configure IS-IS not to calculate the default route through the ATT bit.

Use undo ignore-att to restore the default.

Syntax

ignore-att

undo ignore-att

Default

IS-IS calculates the default route through the ATT bit.

Views

IS-IS view

IS-IS IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Examples

# Configure IS-IS not to calculate the default route through the ATT bit.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] ignore-att

IS-IS commands -- import-route

Use import-route to redistribute routes from another routing protocol or another IS-IS process.

Use undo import-route to remove the redistribution.

Syntax

In IS-IS IPv4 unicast address family view/IS-IS IPv4 unicast topology view:

import-route protocol [ as-number ] [ process-id | all-processes | allow-ibgp ] [ allow-direct | cost cost-value | cost-type { external | internal } | [ level-1 | level-1-2 | level-2 ] | route-policy route-policy-name | tag tag ] *

undo import-route protocol [ process-id | all-processes ]

In IS-IS IPv6 unicast address family view:

import-route protocol [ as-number | process-id ] [ allow-ibgp ] [ allow-direct | cost cost-value | [ level-1 | level-1-2 | level-2 ] | route-policy route-policy-name | tag tag ] *

undo import-route protocol [ process-id ]

Default

IS-IS does not redistribute routes from other routing protocols or processes.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

protocol: Redistributes routes from a routing protocol.

as-number: Specifies an AS by its number in the range of 1 to 4294967295. This argument applies only to the BGP or BGP4+ protocol. If you do not specify this argument, the command redistributes all IPv4 or IPv6 EBGP routes. As a best practice, specify an AS to prevent the system from redistributing excessive routes.

process-id: Specifies a process by its ID in the range of 1 to 65535. It is available only when the protocol is isis, ospf, rip, ripng, isisv6, or ospfv3.

all-processes: Redistributes routes from all the processes of the specified routing protocol. This keyword takes effect only when the protocol is rip, ospf, or isis.

allow-ibgp: Allows redistribution of IBGP routes. It is available when the protocol is BGP or BGP4+.

allow-direct: Redistributes the networks of the local interfaces enabled with the specified routing protocol. By default, the networks of the local interfaces are not redistributed. If you specify both the allow-direct keyword and the route-policy route-policy-name option, make sure the if-match rule defined in the routing policy does not conflict with the allow-direct keyword. For example, if you specify the allow-direct keyword, do not configure the if-match route-type rule for the routing policy. Otherwise, the allow-direct keyword does not take effect.

cost cost-value: Specifies a cost for redistributed routes, which is in the range of 0 to 4261412864.

· For the styles of narrow, narrow-compatible, and compatible, the cost is in the range of 0 to 63.

· For the styles of wide and wide-compatible, the cost is in the range of 0 to 4261412864.

cost-type { external | internal }: Specifies the cost type. The internal type indicates internal routes, and the external type indicates external routes. If external is specified, the cost of a redistributed route is added by 64 to make internal routes take priority over external routes. The type is external by default. The keywords are available only when the cost type is narrow, narrow-compatible, or compatible.

level-1: Redistributes routes into the Level-1 routing table.

level-1-2: Redistributes routes into both Level-1 and Level-2 routing tables.

level-2: Redistributes routes into the Level-2 routing table. If no level is specified, the routes are redistributed into the Level-2 routing table by default.

route-policy route-policy-name: Redistributes only routes matching the specified routing policy. The route-policy-name argument is a case-sensitive string of 1 to 63 characters.

tag tag: Specifies a tag value for marking redistributed routes, in the range of 1 to 4294967295.

Usage guidelines

IS-IS takes all the redistributed routes as external routes to destinations outside the IS-IS routing domain.

The effective cost varies by cost style. For the styles of narrow, narrow-compatible, and compatible, the cost is in the range of 0 to 63. If the cost is more than 63, 63 is used. For the style of wide or wide-compatible, the configured value is the effective value.

This import-route command cannot redistribute default routes. The command redistributes only active routes. To display route state information, use the display ip routing-table protocol command.

The import-route bgp or import-route bgp4+ command redistributes only EBGP routes.

The import-route bgp allow-ibgp or import-route bgp4+ allow-ibgp command redistributes both EBGP and IBGP routes. Because this command might cause routing loops, use it with caution.

The undo import-route protocol all-processes command removes only the configuration made by the import-route protocol all-processes command, instead of the configuration made by the import-route protocol process-id command.

Examples

# Redistribute static routes into IS-IS, and set the cost for redistributed routes to 15.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] import-route static cost 15

Related commands

import-route limit

IS-IS commands -- import-route isis level-1 into level-2

Use import-route isis level-1 into level-2 to enable route advertisement from Level-1 to Level-2.

Use undo import-route isis level-1 into level-2 to disable route advertisement from Level-1 to Level-2.

Syntax

import-route isis level-1 into level-2 [ filter-policy { ipv4-acl-number | prefix-list prefix-list-name | route-policy route-policy-name } | tag tag ] *

undo import-route isis level-1 into level-2

Default

Route advertisement from Level-1 to Level-2 is enabled.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Parameters

filter-policy: Specifies a filtering policy.

ipv4-acl-number: Specifies an ACL by its number in the range of 2000 to 3999 to filter routes from Level-1 to Level-2.

prefix-list prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters, to filter routes from Level-1 to Level-2 by destination address.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to filter routes from Level-1 to Level-2.

tag tag: Specifies a tag for marking redistributed routes, in the range of 1 to 4294967295.

Usage guidelines

If a routing policy is used, the routing policy must be specified in the import-route isis level-1 into level-2 command to filter routes from Level-1 to Level-2. Other routing policies specified for route reception and redistribution do not affect the route leaking.

If a filtering policy is configured, only Level-1 routes not filtered out can be advertised into the Level-2 area.

Examples

# Enable route advertisement from Level-1 to Level-2.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] import-route isis level-1 into level-2

Related commands

import-route

import-route isis level-1 into level-2

IS-IS commands -- import-route isis level-2 into level-1

Use import-route isis level-2 into level-1 to enable route advertisement from Level-2 to Level-1.

Use undo import-route isis level-2 into level-1 to restore the default.

Syntax

import-route isis level-2 into level-1 [ filter-policy { ipv4-acl-number | prefix-list prefix-list-name | route-policy route-policy-name } | tag tag ] *

undo import-route isis level-2 into level-1

Default

Route advertisement from Level-2 to Level-1 is disabled.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Parameters

filter-policy: Specifies a filtering policy.

ipv4-acl-number: Specifies an ACL by its number in the range of 2000 to 3999 to filter routes from Level-2 to Level-1.

prefix-list prefix-list-name: Specifies an IPv4 prefix list by its name, a case-sensitive string of 1 to 63 characters, to filter routes from Level-2 to Level-1 by destination address.

route-policy route-policy-name: Uses the specified routing policy to filter routes from Level-2 to Level-1. The route-policy-name argument is a case-sensitive string of 1 to 63 characters.

tag tag: Specifies a tag for marking redistributed routes, in the range of 1 to 4294967295.

Usage guidelines

If a routing policy is used, the routing policy must be specified in the import-route isis level-2 into level-1 command to filter routes from Level-2 to Level-1. Other routing policies specified for route reception and redistribution does not affect the route leaking.

If a filtering policy is configured, only Level-2 routes not filtered out can be advertised into the Level-1 area.

Examples

# Enable route advertisement from Level-2 to Level-1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] import-route isis level-2 into level-1

Related commands

import-route

import-route isis level-1 into level-2

IS-IS commands -- import-route isisv6 level-1 into level-2

Use import-route isisv6 level-1 into level-2 to enable route advertisement from Level-1 to Level-2.

Use undo import-route isisv6 level-1 into level-2 to disable route advertisement from Level-1 to Level-2.

Syntax

import-route isisv6 level-1 into level-2 [ filter-policy { ipv6-acl-number | prefix-list prefix-list-name | route-policy route-policy-name } | tag tag ] *

undo import-route isisv6 level-1 into level-2

Default

Route advertisement from Level-1 to Level-2 is enabled.

Views

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

filter-policy: Specifies a filtering policy.

ipv6-acl-number: Specifies an IPv6 ACL by its number in the range of 2000 to 3999.

prefix-list prefix-list-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

tag tag: Specifies an administrative tag for marking redistributed routes, in the range of 1 to 4294967295.

Usage guidelines

This command enables a Level-1-2 router to redistribute Level-1 routes to Level-2 routers and Level-1-2 routers in the local area.

Examples

# Enable route advertisement from Level-1 to Level-2.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv6

[Sysname-isis-1-ipv6] import-route isisv6 level-1 into level-2

IS-IS commands -- import-route isisv6 level-2 into level-1

Use import-route isisv6 level-2 into level-1 to enable IPv6 IS-IS route advertisement from Level-2 to Level-1.

Use undo import-route isisv6 level-2 into level-1 to restore the default.

Syntax

import-route isisv6 level-2 into level-1 [ filter-policy { ipv6-acl-number | prefix-list prefix-list-name | route-policy route-policy-name } | tag tag ] *

undo import-route isisv6 level-2 into level-1

Default

Route advertisement from Level-2 to Level-1 is disabled.

Views

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

filter-policy: Specifies a filtering policy.

ipv6-acl-number: Specifies an IPv6 ACL by its number in the range of 2000 to 3999.

prefix-list prefix-list-name: Specifies an IPv6 prefix list by its name, a case-sensitive string of 1 to 63 characters.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

tag: Specifies an administrative tag for marking redistributed routes, in the range of 1 to 4294967295.

Usage guidelines

This command enables a Level-1-2 router to redistribute Level-2 routes to the Level-1 and Level-1-2 routers in the local area.

Examples

# Enable IPv6 IS-IS route advertisement from Level-2 to Level-1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv6

[Sysname-isis-1-ipv6] import-route isisv6 level-2 into level-1

IS-IS commands -- import-route limit

Use import-route limit to configure the maximum number of redistributed Level 1/Level 2 routes.

Use undo import-route limit to restore the default.

Syntax

import-route limit number

undo import-route limit

Default

The maximum number of redistributed Level 1/Level 2 routes varies by device model.

Views

IS-IS IPv4 unicast address family vie w

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

number: Specifies the maximum number of redistributed Level 1/Level 2 routes. The value range for this argument varies by device model.

Examples

# Configure IS-IS process 1 to redistribute up to 1000 Level 1/Level 2 routes.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] import-route limit 1000

Related commands

import-route

switch-routing-mode ipv6-128

IS-IS commands -- isis

Use isis to enable IS-IS and enter IS-IS view.

Use undo isis to disable IS-IS.

Syntax

isis [ process-id ] [ vpn-instance vpn-instance-name ]

undo isis [ process-id ]

Default

IS-IS is disabled.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. The default is 1.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If no VPN instance is specified, the IS-IS process runs on the public network.

Examples

# Enable IS-IS process 1 and set the system ID to 0000.0000.0002 and area ID to 01.0001.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 01.0001.0000.0000.0002.00

Related commands

isis enable

network-entity

IS-IS commands -- isis authentication send-only

Use isis authentication send-only to configure an IS-IS interface not to check the authentication information in the received hello packets.

Use undo isis authentication send-only to remove the configuration.

Syntax

isis authentication send-only [ level-1 | level-2 ]

undo isis authentication send-only [ level-1 | level-2 ]

Default

When interface authentication mode and key are configured, an IS-IS interface checks the authentication information in the received packets.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Configures IS-IS not to check the authentication information in the received Level-1 hello packets.

level-2: Configures IS-IS not to check the authentication information in the received Level-2 hello packets.

Usage guidelines

When peer authentication mode and key are configured, an IS-IS interface adds the key in the specified mode into transmitted hello packets. It also checks the key in the received hello packets.

To prevent packet exchange failure in case of an authentication key change, configure the IS-IS interface not to check the authentication information in the received packets.

Examples

# Configure GigabitEthernet 1/0/1 not to check the authentication information in the received Level-1 hello packets. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis authentication send-only level-1

# Configure VLAN-interface 10 not to check the authentication information in the received Level-1 hello packets. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis authentication send-only level-1

Related commands

area-authentication send-only

domain-authentication send-only

isis authentication-mode

IS-IS commands -- isis authentication-mode

Use isis authentication-mode to specify the neighbor relationship authentication mode and a key.

Use undo isis authentication-mode to remove the configuration.

Syntax

isis authentication-mode { { gca key-id { hmac-sha-1 | hmac-sha-224 | hmac-sha-256 | hmac-sha-384 | hmac-sha-512 } [ nonstandard ] | md5 | simple } { cipher | plain } string | keychain keychain-name } [ level-1 | level-2 ] [ ip | osi ]

undo isis authentication-mode [ level-1 | level-2 ]

Default

No neighbor relationship authentication mode or key is configured.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

gca: Specifies the GCA mode.

key-id: Uniquely identifies an SA in the range of 1 to 65535. The sender inserts the Key ID into the authentication TLV, and the receiver authenticates the packet by using the SA that is selected based on the Key ID.

hmac-sha-1: Specifies the HMAC-SHA-1 algorithm.

hmac-sha-224: Specifies the HMAC-SHA-224 algorithm.

hmac-sha-256: Specifies the HMAC-SHA-256 algorithm.

hmac-sha-384: Specifies the HMAC-SHA-384 algorithm.

hmac-sha-512: Specifies the HMAC-SHA-512 algorithm.

nonstandard: Specifies the nonstandard GCA mode.

md5: Specifies the MD5 authentication mode.

simple: Specifies the simple authentication mode.

cipher: Specifies a key in encrypted form.

plain: Specifies a key in plaintext form. For security purposes, the key specified in plaintext form will be stored in encrypted form.

string: Specifies the key. Its plaintext form is a case-sensitive string of 1 to 16 characters. Its encrypted form is a case-sensitive string of 33 to 53 characters.

keychain: Specifies the keychain authentication mode.

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters.

level-1: Configures the key for Level-1.

level-2: Configures the key for Level-2.

ip: Checks IP-related fields in LSPs and SNPs.

osi: Checks OSI-related fields in LSPs and SNPs.

Usage guidelines

The key in the specified mode is inserted into all outbound hello packets and is used for authenticating inbound hello packets. Only if the authentication succeeds can the neighbor relationship be formed.

IS-IS keychain authentication can operate correctly only when the keys in the keychain use the HMAC-MD5 authentication algorithm.

· Before IS-IS sends a Hello packet, it uses the valid send key obtained from the keychain to authenticate the packet. If no valid send key exists or the valid send key does not use the HMAC-MD5 algorithm, the authentication fails and the packet does not contain the authentication information.

· After IS-IS receives a Hello packet, it uses a valid accept key obtained from the keychain to authenticate the packet. If no valid accept key exists or all valid accept keys fail to authenticate the packet, the authentication fails and the packet is discarded.

The level-1 and level-2 keywords are configurable on an interface that has had IS-IS enabled with the isis enable command.

If you configure a key without specifying a level, the key applies to both Level-1 and Level-2.

For two routers to become neighbors, the authentication mode and key at both ends must be identical.

If neither ip nor osi is specified, the OSI-related fields in LSPs are checked.

When you specify the GCA mode, follow these guidelines:

· If you do not specify the nonstandard keyword, the device can communicate only with devices that use the GCA mode.

· If you specify the nonstandard keyword, the device can communicate only with devices that use the nonstandard GCA mode.

Examples

# On GigabitEthernet 1/0/1, set the authentication mode to simple, and set the plaintext key to 123456. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis authentication-mode simple plain 123456

# On VLAN-interface 10, set the authentication mode to simple, and set the plaintext key to 123456. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis authentication-mode simple plain 123456

Related commands

area-authentication-mode

domain authentication-mode

isis authentication send-only

IS-IS commands -- isis bfd enable

Use isis bfd enable to enable BFD.

Use undo isis bfd enable to disable BFD.

Syntax

isis bfd enable

undo isis bfd enable

Default

IS-IS BFD is disabled.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Examples

# Enable BFD for IS-IS on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable

[Sysname-GigabitEthernet1/0/1] isis bfd enable

# Enable BFD for IS-IS on VLAN-interface 11. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 11

[Sysname-Vlan-interface11] isis enable

[Sysname-Vlan-interface11] isis bfd enable

IS-IS commands -- isis circuit-level

Use isis circuit-level to set the circuit level for the interface.

Use undo isis circuit-level to restore the default.

Syntax

isis circuit-level [ level-1 | level-1-2 | level-2 ]

undo isis circuit-level

Default

An interface can establish either the Level-1 or Level-2 adjacency.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Sets the circuit level to Level-1.

level-1-2: Sets the circuit level to Level-1-2.

level-2: Sets the circuit level to Level-2.

Usage guidelines

For a Level-1 (Level-2) router, the circuit level can only be Level-1 (Level-2). For a Level-1-2 router, you must specify a circuit level for a specific interface to form only the specified level neighbor relationship.

Examples

# GigabitEthernet 1/0/1 is connected to a non-backbone router in the same area. Set the circuit level of Ethernet 1/1 to Level-1 to prevent sending and receiving Level-2 Hello packets. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable

[Sysname-GigabitEthernet1/0/1] isis circuit-level level-1

# VLAN-interface 10 is connected to a non-backbone router in the same area. Set the circuit level of VLAN-interface 10 to Level-1 to prevent sending and receiving Level-2 Hello packets. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis enable

[Sysname-Vlan-interface10] isis circuit-level level-1

Related commands

is-level

IS-IS commands -- isis circuit-type p2p

Use isis circuit-type p2p to set the network type of an interface to P2P.

Use undo isis circuit-type to restore the default.

Syntax

isis circuit-type p2p

undo isis circuit-type

Default

The network type of an interface varies by physical media. (The network type of a VLAN interface is broadcast.)

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Use this command only on a broadcast network with two attached routers.

Interfaces with different network types operate differently. For example, broadcast interfaces must elect a DIS and flood CSNP packets to synchronize the LSDBs. P2P interfaces do not need to elect a DIS, and use a different LSDB synchronization mechanism.

If only two routers exist on a broadcast network, set the network type of attached interfaces to P2P to avoid DIS election and CSNP flooding. This saves network bandwidth and speeds up network convergence.

Examples

# Set the network type of GigabitEthernet 1/0/1 to P2P. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable

[Sysname-GigabitEthernet1/0/1] isis circuit-type p2p

# Set the network type of VLAN-interface 10 to P2P. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis enable

[Sysname-Vlan-interface10] isis circuit-type p2p

IS-IS commands -- isis cost

Use isis cost to set the IS-IS cost for an interface.

Use undo isis cost to remove the configuration.

Syntax

isis cost cost-value [ level-1 | level-2 ]

undo isis cost [ level-1 | level-2 ]

Default

No IS-IS cost is configured for an interface.

Views

Interface view

IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Parameters

cost-value: Specifies an IS-IS cost in the range of 1 to 16777215.

level-1: Applies the cost to Level-1.

level-2: Applies the cost to Level-2.

Usage guidelines

If neither level-1 nor level-2 is included, the cost applies to both Level-1 and Level-2.

Examples

# Set the Level-2 IS-IS cost to 5 for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis cost 5 level-2

# Set the Level-2 IS-IS cost to 5 for VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis cost 5 level-2

Related commands

auto-cost enable

bandwidth-reference

IS-IS commands -- isis dis-name

Use isis dis-name to configure a name for a DIS to represent the pseudo node on a broadcast network.

Use undo isis dis-name to restore the default.

Syntax

isis dis-name symbolic-name

undo isis dis-name

Default

No name is configured for the DIS.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

symbolic-name: Specifies a DIS name, a case-insensitive string of 1 to 64 characters.

Usage guidelines

This command takes effect only on routers that have dynamic system ID to host name mapping enabled. This command does not take effect on Point-to-Point interfaces.

Examples

# Set the DIS name to LOCALAREA. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis dis-name LOCALAREA

# Set the DIS name to LOCALAREA. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis dis-name LOCALAREA

Related commands

display isis name-table

is-name

IS-IS commands -- isis dis-priority

Use isis dis-priority to specify a DIS priority at a specified level for an interface.

Use undo isis dis-priority to remove the configuration.

Syntax

isis dis-priority priority [ level-1 | level-2 ]

undo isis dis-priority [ level-1 | level-2 ]

Default

The priority of Level-1 and Level-2 is 64.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

priority: Specifies a DIS priority in the range of 0 to 127.

level-1: Applies the DIS priority to Level-1.

level-2: Applies the DIS priority to Level-2.

Usage guidelines

On an IS-IS broadcast network, a router must be elected as the DIS at each routing level. Specify a DIS priority at a level for an interface. The greater the interface's priority is, the more likelihood it becomes the DIS. If multiple routers in the broadcast network have the same highest DIS priority, the router with the highest Subnetwork Point of Attachment (SNPA) address becomes the DIS. SNPA addresses are MAC addresses on a broadcast network.

IS-IS has no backup DIS. The router with a priority of 0 can also participate in DIS election.

If neither level-1 nor level-2 is specified, the DIS priority applies to both Level-1 and Level-2.

Examples

# Set the Level-2 DIS priority to 127 for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis dis-priority 127 level-2

# Set the Level-2 DIS priority to 127 for VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis dis-priority 127 level-2

IS-IS commands -- isis enable

Use isis enable to enable an IS-IS process on an interface.

Use undo isis enable to disable IS-IS.

Syntax

isis enable [ process-id ]

undo isis enable

Default

No IS-IS process is enabled on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. The default is 1.

Examples

# Enable IS-IS process 1 globally and enable it on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable 1

# Enable IS-IS process 1 globally and enable it on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis enable 1

Related commands

isis

network-entity

IS-IS commands -- isis fast-reroute lfa-backup exclude

Use isis fast-reroute lfa-backup exclude to disable LFA calculation on an interface.

Use undo isis fast-reroute lfa-backup exclude to restore the default.

Syntax

isis fast-reroute lfa-backup exclude

undo isis fast-reroute lfa-backup exclude

Default

LFA calculation is enabled on an interface, and the interface can be elected as a backup interface.

Views

Interface view

IPv4 unicast topology view of the interface

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When this command is configured, the interface does not participate in the LFA calculation, and cannot be elected as a backup interface.

Examples

# Disable LFA calculation on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable 1

[Sysname-GigabitEthernet1/0/1] isis fast-reroute lfa-backup exclude

# Disable LFA calculation on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis enable 1

[Sysname-Vlan-interface10] isis fast-reroute lfa-backup exclude

Related commands

fast-reroute

IS-IS commands -- isis ipv6 bfd enable

Use isis ipv6 bfd enable to enable BFD for IPv6 IS-IS.

Use undo isis ipv6 bfd enable to disable BFD for IPv6 IS-IS.

Syntax

isis ipv6 bfd enable

undo isis ipv6 bfd enable

Default

BFD for IPv6 IS-IS is disabled.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Examples

# Enable BFD for IPv6 IS-IS on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 bfd enable

# Enable BFD for IPv6 IS-IS on VLAN-interface 11. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 11

[Sysname-Vlan-interface11] isis ipv6 bfd enable

IS-IS commands -- isis ipv6 cost

Use isis ipv6 cost to set the IPv6 IS-IS cost for an interface.

Use undo isis ipv6 cost to remove the configuration.

Syntax

isis ipv6 cost cost-value [ level-1 | level-2 ]

undo isis ipv6 cost [ level-1 | level-2 ]

Default

No IPv6 IS-IS cost is configured for an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

cost-value: Specifies an IPv6 IS-IS cost in the range of 1 to 16777215.

level-1: Applies the cost to Level-1 routes.

level-2: Applies the cost to Level-2 routes.

Usage guidelines

This command applies to interfaces that are enabled with IPv6 IS-IS.

This command takes effect only when the standard MTR mode is enabled.

Examples

# Set the IPv6 IS-IS cost to 10 for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv6 unicast

[Sysname-isis-100-ipv6] quit

[Sysname-isis-100] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 enable 100

[Sysname-GigabitEthernet1/0/1] isis ipv6 cost 10

# Set the IPv6 IS-IS cost to 10 for VLAN-interface 11. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv6 unicast

[Sysname-isis-100-ipv6] quit

[Sysname-isis-100] quit

[Sysname] interface vlan-interface 11

[Sysname-Vlan-interface11] isis ipv6 enable 100

[Sysname-Vlan-interface11] isis ipv6 cost 10

IS-IS commands -- isis ipv6 enable

Use isis ipv6 enable to enable IPv6 for IS-IS on an interface.

Use undo isis ipv6 enable to disable IPv6 for IS-IS on an interface.

Syntax

isis ipv6 enable [ process-id ]

undo isis ipv6 enable

Default

IPv6 is disabled for IS-IS on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. The default is 1.

Examples

# Enable IPv6 for IS-IS on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] address-family ipv6 unicast

[Sysname-isis-1-ipv6] quit

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] ipv6 address 2002::1/64

[Sysname-GigabitEthernet1/0/1] isis ipv6 enable 1

# Enable IPv6 for IS-IS on VLAN-interface 100. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] address-family ipv6 unicast

[Sysname-isis-1-ipv6] quit

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 100

[Sysname-Vlan-interface100] ipv6 address 2002::1/64

[Sysname-Vlan-interface100] isis ipv6 enable 1

IS-IS commands -- isis ipv6 fast-reroute lfa-backup exclude

Use isis ipv6 fast-reroute lfa-backup exclude to disable LFA calculation on an interface.

Use undo isis ipv6 fast-reroute lfa-backup exclude to restore the default.

Syntax

isis ipv6 fast-reroute lfa-backup exclude

undo isis ipv6 fast-reroute lfa-backup exclude

Default

LFA calculation is enabled on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Examples

# Disable LFA calculation on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 enable 1

[Sysname-GigabitEthernet1/0/1] isis ipv6 fast-reroute lfa-backup exclude

# Disable LFA calculation on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis ipv6 enable 1

[Sysname-Vlan-interface10] isis ipv6 fast-reroute lfa-backup exclude

Related commands

fast-reroute

IS-IS commands -- isis ipv6 prefix-suppression

Use isis ipv6 prefix-suppression to enable prefix suppression on an interface.

Use undo isis ipv6 prefix-suppression to disable prefix suppression on an interface.

Syntax

isis ipv6 prefix-suppression

undo isis ipv6 prefix-suppression

Default

Prefix suppression is disabled on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

By default, IS-IS interfaces advertise their IPv6 prefixes in LSPs. Use this command to disable an interface from advertising its IPv6 prefix in LSPs. This enhances network security by preventing IP routing to the internal nodes and speeds up network convergence.

Examples

# Enable prefix suppression on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 prefix-suppression

# Enable prefix suppression on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis ipv6 prefix-suppression

IS-IS commands -- isis ipv6 primary-path-detect bfd

Use isis ipv6 primary-path-detect bfd to enable BFD for IPv6 IS-IS.

Use undo isis ipv6 primary-path-detect bfd to disable BFD for IPv6 IS-IS.

Syntax

isis ipv6 primary-path-detect bfd { ctrl | echo }

undo isis ipv6 primary-path-detect bfd

Default

BFD is disabled for IPv6 IS-IS.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

ctrl: Enables BFD control packet mode.

echo: Enables BFD echo packet mode.

Usage guidelines

This command enables IPv6 IS-IS FRR or IPv6 IS-IS PIC to use BFD to detect primary link failures.

Examples

# Enable BFD control packet mode for IPv6 IS-IS FRR on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv6

[Sysname-isis-1-ipv6] fast-reroute lfa

[Sysname-isis-1-ipv6] quit

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 primary-path-detect bfd ctrl

# Enable BFD echo packet mode for IPv6 IS-IS PIC on GigabitEthernet 1/0/2. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] pic additional-path-always

[Sysname-isis-1] quit

[Sysname] bfd echo-source-ipv6 1::1

[Sysname] interface gigabitethernet 1/0/2

[Sysname-GigabitEthernet1/0/2] isis ipv6 primary-path-detect bfd echo

# Enable BFD control packet mode for IPv6 IS-IS FRR on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv6

[Sysname-isis-1-ipv6] fast-reroute lfa

[Sysname-isis-1-ipv6] quit

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis ipv6 primary-path-detect bfd ctrl

# Enable BFD echo packet mode for IPv6 IS-IS PIC on VLAN-interface 11. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] pic additional-path-always

[Sysname-isis-1] quit

[Sysname] bfd echo-source-ipv6 1::1

[Sysname] interface vlan-interface 11

[Sysname-Vlan-interface11] isis ipv6 primary-path-detect bfd echo

IS-IS commands -- isis ipv6 tag

Use isis ipv6 tag to configure the tag value on an interface.

Use undo isis ipv6 tag to restore the default.

Syntax

isis ipv6 tag tag

undo isis ipv6 tag

Default

No tag value is configured on an interface.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

tag: Specifies a tag value in the range of 1 to 4294967295.

Usage guidelines

When IS-IS advertises an IPv6 prefix with a tag value, it adds the tag to the IPv6 reachability information TLV, regardless of the link cost style.

Examples

# Set the tag value on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis ipv6 tag 4294967295

# Set the tag value on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis ipv6 tag 4294967295

IS-IS commands -- isis mesh-group

Use isis mesh-group to add an interface into a mesh group or block the interface.

Use undo isis mesh-group to restore the default.

Syntax

isis mesh-group { mesh-group-number | mesh-blocked }

undo isis mesh-group

Default

An interface does not belong to any mesh group and is not blocked.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

mesh-group-number: Specifies a mesh group by its number in the range of 1 to 4294967295.

mesh-blocked: Configures the interface to send LSPs only after receiving LSP requests.

Usage guidelines

An interface not in a mesh group floods received LSPs to other interfaces. For an NBMA network with multiple point-to-point links, this mechanism causes repeated LSP flooding and bandwidth waste.

To solve this problem, use this command to add relevant interfaces to a mesh group. An interface in a mesh group only floods a received LSP to interfaces not in the same mesh group.

You can also use this command to block an interface. A blocked interface sends LSPs only after receiving LSP requests.

The mesh-group feature takes effect only on point-to-point links.

Examples

# Add frame relay subinterface Serial2/1/1.1 to mesh group 3.

<Sysname> system-view

[Sysname] interface serial 2/1/1

[Sysname-Serial2/1/1] link-protocol fr

[Sysname-Serial2/1/1] quit

[Sysname] interface serial 2/1/1.1

[Sysname-Serial2/1/1.1] isis mesh-group 3

IS-IS commands -- isis mib-binding

Use isis mib-binding to bind an IS-IS process to MIB.

Use undo isis mib-binding to restore the default.

Syntax

isis mib-binding process-id

undo isis mib-binding

Default

MIB operation is bound to the IS-IS process with the smallest process ID.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535.

Usage guidelines

If the specified the process ID does not exist, the MIB binding configuration fails.

Deleting an IS-IS process bound to MIB operation deletes the MIB binding configuration. MIB operation is bound to the IS-IS process with the smallest process ID.

Examples

# Bind IS-IS process 100 to MIB.

<Sysname> system-view

[Sysname] isis mib-binding 100

IS-IS commands -- isis peer-ip-check

Use isis peer-ip-check to enable source address check for hello packets on an IS-IS PPP interface. An IS-IS PPP interface can establish a neighbor relationship only with a peer on the same network.

Use undo isis peer-ip-check to restore the default.

Syntax

isis peer-ip-check

undo isis peer-ip-check

Default

An IS-IS PPP interface can have a peer on a different network.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Examples

# Enable source address check for hello packets on Serial 2/1/0.

<Sysname> system-view

[Sysname] interface serial 2/1/0

[Sysname-Serial2/1/0] isis peer-ip-check

IS-IS commands -- isis prefix-suppression

Use isis prefix-suppression to enable prefix suppression on an interface.

Use undo isis prefix-suppression to disable prefix suppression on an interface.

Syntax

isis prefix-suppression

undo isis prefix-suppression

Default

Prefix suppression is disabled on an interface.

Views

Interface view

IPv4 unicast topology view of the interface

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Use this command to disable an interface from advertising its prefix in LSPs. This enhances network security by preventing IP routing to the interval nodes and speeds up network convergence.

This command is also applicable to the secondary IP address of the interface.

Examples

# Enable prefix suppression on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis prefix-suppression

# Enable prefix suppression on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis prefix-suppression

IS-IS commands -- isis primary-path-detect bfd

Use isis primary-path-detect bfd to enable BFD for IS-IS FRR or IS-IS PIC.

Use undo isis primary-path-detect bfd to disable BFD for IS-IS FRR or IS-IS PIC.

Syntax

isis primary-path-detect bfd { ctrl | echo }

undo isis primary-path-detect bfd

Default

BFD is disabled for IS-IS FRR or IS-IS PIC.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

ctrl: Specifies the BFD control packet mode.

echo: Specifies the BFD echo packet mode.

Usage guidelines

This command enables IS-IS FRR or IS-IS PIC to use BFD to detect primary link failures.

Examples

# Enable BFD control packet mode for IS-IS FRR on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] fast-reroute lfa

[Sysname-isis-1-ipv4] quit

[Sysname-isis-1] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis primary-path-detect bfd ctrl

# Enable BFD echo packet mode for IS-IS PIC on GigabitEthernet 1/0/2. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] pic additional-path-always

[Sysname-isis-1] quit

[Sysname] bfd echo-source-ip 1.1.1.1

[Sysname] interface gigabitethernet 1/0/2

[Sysname-GigabitEthernet1/0/2] isis primary-path-detect bfd echo

# Enable BFD control packet mode for IS-IS FRR on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] fast-reroute lfa

[Sysname-isis-1-ipv4] quit

[Sysname-isis-1] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis primary-path-detect bfd ctrl

# Enable BFD echo packet mode for IS-IS PIC on VLAN-interface 11. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] pic additional-path-always

[Sysname-isis-1] quit

[Sysname] bfd echo-source-ip 1.1.1.1

[Sysname] interface vlan-interface 11

[Sysname-Vlan-interface11] isis primary-path-detect bfd echo

IS-IS commands -- isis silent

Use isis silent to disable the interface from sending and receiving IS-IS packets.

Use undo isis silent to restore the default.

Syntax

isis silent

undo isis silent

Default

An interface can send and receive IS-IS packets.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command is not available in loopback interface view.

Examples

# Disable GigabitEthernet 1/0/1 from sending and receiving IS-IS packets. (Applicable to routers.)

<<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis silent

# Disable VLAN-interface 10 from sending and receiving IS-IS packets. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis silent

IS-IS commands -- isis small-hello

Use isis small-hello to configure the interface to send small hello packets without CLVs.

Use undo isis small-hello to restore the default.

Syntax

isis small-hello

undo isis small-hello

Default

An interface sends standard hello packets.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command is not available in loopback interface view.

Examples

# Configure GigabitEthernet 1/0/1 to send small Hello packets. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis small-hello

# Configure VLAN-interface 10 to send small Hello packets. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis small-hello

IS-IS commands -- isis tag

Use isis tag to configure the tag value for an interface.

Use undo isis tag to restore the default.

Syntax

isis tag tag

undo isis tag

Default

The interface is not configured with a tag value.

Views

Interface view

IPv4 unicast topology view of the interface

Predefined user roles

network-admin

mdc-admin

Parameters

tag: Specifies the tag value in the range of 1 to 4294967295.

Usage guidelines

When IS-IS advertises an IP prefix with a tag value, it adds the tag to the IP reachability information TLV if the link cost style is wide, wide-compatible, or compatible.

Examples

# Configure the tag value for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis tag 4294967295

# Configure the tag value for VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis tag 4294967295

IS-IS commands -- isis timer csnp

Use isis timer csnp to set on the DIS of a broadcast network the interval for sending CSNP packets.

Use undo isis timer csnp to remove the configuration.

Syntax

isis timer csnp seconds [ level-1 | level-2 ]

undo isis timer csnp [ level-1 | level-2 ]

Default

The default CSNP interval is 10 seconds.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies on the DIS of a broadcast network the interval for sending CSNP packets. The value range is 1 to 600 seconds.

level-1: Applies the interval to Level-1.

level-2: Applies the interval to Level-2.

Usage guidelines

On a broadcast network, this command only applies to the DIS, because the DIS sends CSNP packets periodically for LSDB synchronization.

If no level is specified, the CSNP interval applies to both Level-1 and Level-2.

Examples

# Configure Level-2 CSNP packets to be sent every 15 seconds over GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis timer csnp 15 level-2

# Configure Level-2 CSNP packets to be sent every 15 seconds over VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis timer csnp 15 level-2

IS-IS commands -- isis timer hello

Use isis timer hello to set the interval for sending hello packets.

Use undo isis timer hello to remove the configuration.

Syntax

isis timer hello seconds [ level-1 | level-2 ]

undo isis timer hello [ level-1 | level-2 ]

Default

The hello interval is 10 seconds.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the interval for sending hello packets, in the range of 3 to 255 seconds.

level-1: Specifies the interval for sending Level-1 hello packets.

level-2: Specifies the interval for sending Level-2 hello packets.

Usage guidelines

If a neighbor does not receive any hello packets from the router within the advertised hold time, it considers the router down and recalculates the routes. The hold time is the hello multiplier multiplied by the hello interval.

Level-1 and Level-2 hello packets are sent independently on a broadcast network, so you need to specify an interval for each level. On a P2P link, Level-1 and Level-2 packets are both sent in P2P hello packets, and you need not specify an interval for each level.

You can configure the level-1 and level-2 keywords only on broadcast interfaces. Before you configure the level-1 or level-2 keyword, enable IS-IS on the interface.

The shorter the interval, the more system resources will be occupied.

If no level is specified, the hello interval applies to both Level-1 and Level-2.

Examples

# Configure Level-2 hello packets to be sent every 20 seconds over GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis timer hello 20 level-2

# Configure Level-2 hello packets to be sent every 20 seconds over VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis timer hello 20 level-2

Related commands

isis timer holding-multiplier

IS-IS commands -- isis timer holding-multiplier

Use isis timer holding-multiplier to set the IS-IS hello multiplier.

Use undo isis timer holding-multiplier to remove the configuration.

Syntax

isis timer holding-multiplier value [ level-1 | level-2 ]

undo isis timer holding-multiplier [ level-1 | level-2 ]

Default

The default IS-IS hello multiplier is 3.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

value: Specifies the number of hello intervals, in the range of 3 to 1000.

level-1: Applies the number to the Level-1 IS-IS neighbor.

level-2: Applies the number to the Level-2 IS-IS neighbor.

Usage guidelines

The hello multiplier is the number of hello packets a neighbor must miss before declaring the router is down.

If a neighbor does not receive any hello packets from the router within the advertised hold time, it considers the router down and recalculates the routes. The hold time is the hello multiplier multiplied by the hello interval.

Level-1 and Level-2 hello packets are sent independently on a broadcast network, so you need to specify a hello multiplier for each level. On a P2P link, Level-1 and Level-2 packets are both sent in P2P hello packets, and you need not specify Level-1 or Level-2.

You can configure the level-1 and level-2 keywords only on broadcast interfaces. Before you configure the level-1 or level-2 keyword, enable IS-IS on the interface.

If no level is specified, the hello multiplier applies to both Level-1 and Level-2.

The value of hello multiplier multiplied by hello interval cannot be more than 65535.

Examples

# Set the hello multiplier to 6 for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis timer holding-multiplier 6 level-2

# Set the hello multiplier to 6 for VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis timer holding-multiplier 6

Related commands

isis timer hello

IS-IS commands -- isis timer lsp

Use isis timer lsp to set the minimum interval for sending LSPs on the interface and specify the maximum number of LSPs that can be sent per time.

Use undo isis timer lsp to restore the default.

Syntax

isis timer lsp time [ count count ]

undo isis timer lsp

Default

The minimum interval for sending LSPs on the interface is 33 milliseconds, and the maximum number of LSPs that can be sent at a time is 5.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

time: Specifies the minimum interval for sending link-state packets, in the range of 1 to 1000 milliseconds.

count: Specifies the maximum number of link-state packets to be sent at one time, in the range of 1 to 1000.

Usage guidelines

If a change occurs in the LSDB, IS-IS advertises the changed LSP to neighbors. You can specify the minimum interval for sending these LSPs to control the amount of LSPs on the network.

Examples

# Set the interval to 500 milliseconds for sending LSPs on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis timer lsp 500

# Set the interval to 500 milliseconds for sending LSPs on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis timer lsp 500

Related commands

isis timer retransmit

IS-IS commands -- isis timer retransmit

Use isis timer retransmit to configure the interval for retransmitting LSP packets over a point-to-point link.

Use undo isis timer retransmit to restore the default.

Syntax

isis timer retransmit seconds

undo isis timer retransmit

Default

The retransmission interval on a P2P link is 5 seconds.

Views

Interface view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the interval for retransmitting LSP packets, in the range of 1 to 300 seconds.

Usage guidelines

On a P2P link, IS-IS requires an advertised LSP be acknowledged. If no acknowledgment is received within a configurable interval, IS-IS will retransmit the LSP.

You do not need to use this command over a broadcast link where CSNPs are periodically broadcast to implement LSDB synchronization.

Examples

# Set the LSP retransmission interval on a P2P link to 50 seconds for GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis timer retransmit 50

# Set the LSP retransmission interval on a P2P link to 50 seconds for VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis circuit-type p2p

[Sysname-Vlan-interface10] isis timer retransmit 50

Related commands

isis circuit-type p2p

isis timer lsp

IS-IS commands -- isis topology enable

Use isis topology enable to enable IS-IS for the specified topology.

Use undo isis topology enable to disable IS-IS for the specified topology.

Syntax

isis topology enable

undo isis topology enable

Default

IS-IS is disabled for the topology.

Views

IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

To configure this command, you must complete the following tasks:

· Enable IS-IS on the interface.

· Create an IS-IS IPv4 unicast topology.

Examples

# Enable IS-IS for IPv4 unicast topology voice on GigabitEthernet 1/0/1. (Applicable to routers.)

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv4

[Sysname-isis-100-ipv4] topology voice tid 4000

[Sysname-isis-100-ipv4-topo-voice] quit

[Sysname-isis-100-ipv4] quit

[Sysname-isis-100] quit

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] isis enable 100

[Sysname-GigabitEthernet1/0/1] topology ipv4 voice

[Sysname-GigabitEthernet1/0/1-topo-voice] isis topology enable

# Enable IS-IS for IPv4 unicast topology voice on VLAN-interface 10. (Applicable to switches.)

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv4

[Sysname-isis-100-ipv4] topology voice tid 4000

[Sysname-isis-100-ipv4-topo-voice] quit

[Sysname-isis-100-ipv4] quit

[Sysname-isis-100] quit

[Sysname] interface vlan-interface 10

[Sysname-Vlan-interface10] isis enable 100

[Sysname-Vlan-interface10] topology ipv4 voice

[Sysname-Vlan-interface10-topo-voice] isis topology enable

IS-IS commands -- is-level

Use is-level to specify the IS level.

Use undo is-level to restore the default.

Syntax

is-level { level-1 | level-1-2 | level-2 }

undo is-level

Default

The IS level is level-1-2.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Specifies Level-1, which means IS-IS only calculates intra-area routes and maintains the Level-1 LSDB.

level-1-2: Specifies Level-1-2, which means IS-IS calculates routes and maintains the LSDBs for both Level-1 and Level-2.

level-2: Specifies Level-2, which means IS-IS calculates routes and maintains the LSDB for Level-2 only.

Usage guidelines

If only one area exists, configure all the routers as either Level-1 or Level-2, because the routers do not need to maintain two identical LSDBs at the same time.

If the only area is an IP network, configure all the routers as Level-2 for scalability.

Examples

# Set the IS level to Level-1 for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] is-level level-1

IS-IS commands -- is-name

Use is-name to specify a host name for the IS and enable dynamic system ID to hostname mapping.

Use undo is-name to disable dynamic system ID to hostname mapping.

Syntax

is-name sys-name

undo is-name

Default

Dynamic system ID to hostname mapping is disabled, and no host name is configured for the IS.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

sys-name: Specifies a host name for the local IS, a case-insensitive string of 1 to 64 characters.

Usage guidelines

To display the host name rather than the system ID of an IS by using the display isis lsdb command, first enable dynamic system ID to hostname mapping.

Examples

# Configure a host name for the local IS.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] is-name RUTA

Related commands

display isis name-table

IS-IS commands -- is-name map

Use is-name map to configure a system ID to host name mapping for a remote IS.

Use undo is-name map to remove the mapping.

Syntax

is-name map sys-id map-sys-name

undo is-name map sys-id

Default

No system ID to host name mapping is configured for a remote IS.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

sys-id: Specifies the system ID or pseudonode ID of a remote IS.

map-sys-name: Specifies a host name for the remote IS, a case-insensitive string of 1 to 64 characters.

Usage guidelines

Each remote IS system ID corresponds to only one name.

Examples

# Map the host name RUTB to the system ID 0000.0000.0041 of the remote IS.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] is-name map 0000.0000.0041 RUTB

Related commands

display isis name-table

IS-IS commands -- ispf enable

Use ispf enable to enable incremental SPF (ISPF).

Use undo ispf enable to disable ISPF.

Syntax

ispf enable

undo ispf enable

Default

IS-IS ISPF is enabled.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When a network topology is changed, ISPF recomputes only the affected part of the SPT, instead of the entire SPT.

Examples

# Enable ISPF.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] ispf enable

IS-IS commands -- log-peer-change

Use log-peer-change to enable the logging of neighbor state changes.

Use undo log-peer-change to disable the logging.

Syntax

log-peer-change

undo log-peer-change

Default

The logging of IS-IS neighbor state changes is enabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command enables sending logs about IS-IS neighbor state changes to the information center. For IS-IS neighbor state change logs to be sent correctly, you must also configure the information center parameters on the device. For more information about information center, see the network management and monitoring configuration guide for the device.

Examples

# Disable the logging of IS-IS neighbor state changes.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] undo log-peer-change

IS-IS commands -- lsp-fragments-extend

Use lsp-fragments–extend to enable LSP fragment extension for a level.

Use undo lsp-fragments–extend to restore the default.

Syntax

lsp-fragments-extend [ level-1 | level-1-2 | level-2 ]

undo lsp-fragments-extend

Default

LSP fragment extension is disabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Applies the fragment extension to Level-1 LSPs.

level-1-2: Applies the fragment extension to both Level-1 and Level-2 LSPs.

level-2: Applies the fragment extension to Level-2 LSPs.

Usage guidelines

If no level is specified, the command enables LSP fragment extension for both Level-1 and Level-2.

Examples

# Enable LSP fragment extension for Level-2.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] lsp-fragments-extend level-2

IS-IS commands -- lsp-length originate

Use lsp-length originate to configure the maximum size of generated Level-1 or Level-2 LSPs.

Use undo lsp-length originate to remove the configuration.

Syntax

lsp-length originate size [ level-1 | level-2 ]

undo lsp-length originate [ level-1 | level-2 ]

Default

The maximum size of generated Level-1 and Level-2 LSPs is 1497 bytes.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

size: Specifies the maximum size of LSP packets, in the range of 512 to 16384 bytes.

level-1: Applies the size to Level-1 LSP packets.

level-2: Applies the size to Level-2 LSP packets.

Usage guidelines

If neither Level-1 nor Level-2 is specified in the command, the configured maximum size applies to the current IS-IS level.

Examples

# Set the maximum size of the generated Level-2 LSPs to 1024 bytes.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] lsp-length originate 1024 level-2

IS-IS commands -- lsp-length receive

Use lsp-length receive to configure the maximum size of received LSPs.

Use undo lsp-length receive to restore the default.

Syntax

lsp-length receive size

undo lsp-length receive

Default

The maximum size of received LSPs is 1497 bytes.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

size: Specifies the maximum size of received LSPs, in the range of 512 to 16384 bytes.

Examples

# Configure the maximum size of received LSPs to 1024 bytes.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] lsp-length receive 1024

IS-IS commands -- maximum load-balancing

Use maximum load-balancing to configure the maximum number of ECMP routes for load balancing.

Use undo maximum load-balancing to restore the default.

Syntax

maximum load-balancing number

undo maximum load-balancing

Default

The maximum number of IS-IS ECMP routes equals the maximum number of ECMP routes supported by the system.

Views

IS-IS IPv4 unicast address family vie w

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

number: Specifies the maximum number of ECMP routes. The value of 1 indicates that IS-IS does not perform load balancing. The range and default number vary by device model.

Usage guidelines

If you use the max-ecmp-num command to configure the maximum number of ECMP routes supported by the system as m:

· The default setting for the maximum load-balancing command is m.

· The value range for the number argument of the maximum load-balancing command is 1 to m.

Examples

# Set the maximum number of ECMP routes to 2.

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv4

[Sysname-isis-100-ipv4] maximum load-balancing 2

Related commands

max-ecmp-num

IS-IS commands -- multi-topology

Use multi-topology to enable IPv6 IS-IS MTR.

Use undo multiple-topology to disable IPv6 IS-IS MTR.

Syntax

multi-topology [ compatible ]

undo multi-topology

Default

IPv6 IS-IS MTR is disabled.

Views

IS-IS IPv6 address family view

Predefined user roles

network-admin

mdc-admin

Parameters

compatible: Specifies the compatible mode to advertise IPv6 prefixes to both IPv4 and IPv6 topologies. If you do not specify this keyword, the command advertises IPv6 prefixes only to the IPv6 topology.

Usage guidelines

This command enables separate route calculation in IPv4 and IPv6 topologies.

This command is available when the link cost style is wide, compatible, or wide-compatible.

Examples

# Enable IPv6 IS-IS MTR.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv6

[Sysname-isis-1-ipv6] multi-topology

Related commands

cost-style

IS-IS commands -- network-entity

Use network-entity to configure the Network Entity Title (NET) for an IS-IS process.

Use undo network-entity to delete a NET.

Syntax

network-entity net

undo network-entity net

Default

No NET is configured.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

net: Specifies a NET as a dotted hexadecimal string in the X…X.XXXX....XXXX.00 format. The X…X segment represents the area address, the XXXX....XXXX segment represents the system ID, and the 00 segment is the SEL.

Usage guidelines

A NET is a special NSAP address with the SEL being 0. The length of the NET is in the range of 8 to 20 bytes.

A NET comprises the following parts:

· Area ID—With a length of 1 to 13 bytes.

· System ID—A system ID uniquely identifies a host or router in the area and has a fixed 6-byte length.

· SEL—It has a value of 0 and a fixed 1-byte length.

For example, a NET of ab.cdef.1234.5678.9abc.00 specifies the area ID ab.cdef, the system ID 1234.5678.9abc, and the SEL 00.

Examples

# Set the NET to 10.0001.1010.1020.1030.00, of which 10.0001 is the area ID and 1010.1020.1030 is the system ID.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] network-entity 10.0001.1010.1020.1030.00

Related commands

isis

isis enable

IS-IS commands -- non-stop-routing

Use non-stop-routing to enable IS-IS NSR.

Use undo non-stop-routing to disable IS-IS NSR.

Syntax

non-stop-routing

undo non-stop-routing

Default

IS-IS NSR is disabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

IS-IS NSR takes effect on a per-process basis. As a best practice, enable NSR for each IS-IS process.

IS-IS NSR and IS-IS GR are mutually exclusive. Therefore, do not configure the non-stop-routing command and the graceful-restart command at the same time.

Examples

# Enable NSR for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] non-stop-routing

IS-IS commands -- pic

Use pic to enable IS-IS PIC.

Use undo pic to disable IS-IS PIC.

Syntax

pic [ additional-path-always ]

undo pic

Default

IS-IS PIC is enabled.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

additional-path-always: Allows the indirect suboptimal route as the backup route.

Usage guidelines

Prefix Independent Convergence (PIC) enables the device to speed up network convergence by ignoring the number of prefixes. PIC applies only to indirect routes.

When both IS-IS PIC and IS-IS FRR are configured, only IS-IS FRR takes effect.

Examples

# Configure IS-IS PIC to support the indirect suboptimal route as the backup route.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] pic additional-path-always

IS-IS commands -- preference

Use preference to configure the preference for IS-IS.

Use undo preference to restore the default.

Syntax

preference { preference | route-policy route-policy-name } *

undo preference

Default

IS-IS preference is 15.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

preference: Specifies an IS-IS protocol preference in the range of 1 to 255.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters, to assign a priority to the matching routes.

Usage guidelines

If multiple routing protocols find routes to the same destination, the route found by the routing protocol with the highest preference is selected as the optimal route.

If a routing policy is specified in this command, the preference set by the routing policy applies to the matching routes. Other routes use the preference set by the preference command.

Examples

# Set the preference for IS-IS to 25.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] preference 25

IS-IS commands -- prefix-priority

Use prefix-priority to assign convergence priorities to specific IS-IS routes.

Use undo prefix-priority to remove the configuration.

Syntax

prefix-priority { critical | high | medium } { prefix-list prefix-list-name | tag tag-value }

prefix-priority route-policy route-policy-name

undo prefix-priority { critical | high | medium } [ prefix-list | tag ]

undo prefix-priority route-policy

Default

IS-IS routes have the lowest convergence priority.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

critical: Specifies the highest convergence priority.

high: Specifies the high convergence priority.

medium: Specifies the medium convergence priority.

prefix-list prefix-list-name: Specifies a prefix list by its name, a case-sensitive string of 1 to 63 characters.

tag tag-value: Specifies a tag value in the range of 1 to 4294967295.

route-policy route-policy-name: Specifies a routing policy by its name, a case-sensitive string of 1 to 63 characters.

Usage guidelines

The higher the convergence priority, the faster the convergence speed.

IS-IS host routes have a medium convergence priority.

Examples

# Assign the high convergence priority to IS-IS routes permitted by IP prefix list standtest.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] prefix-priority high prefix-list standtest

IS-IS commands -- reset isis all

Use reset isis all to clear all IS-IS data structure information.

Syntax

reset isis all [ process-id ] [ graceful-restart ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535 to clear the data structure information for an IS-IS process.

graceful-restart: Recovers the data through graceful restart after the data is cleared.

Usage guidelines

If no IS-IS process is specified, the command clears data structure information for all IS-IS processes.

Use this command when LSPs must be updated immediately.

Examples

# Clear all IS-IS data structure information.

<Sysname> reset isis all

IS-IS commands -- reset isis event-log graceful-restart

Use reset isis event-log graceful-restart to clear IS-IS GR log information.

Syntax

Centralized devices:

reset isis event-log graceful-restart

Distributed devices in standalone mode:Centralized IRF devices:

reset isis event-log graceful-restart slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset isis event-log graceful-restart chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# (Centralized devices.) Clear IS-IS GR log information.

<Sysname> reset isis event-log graceful-restart

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Clear IS-IS GR log information for the specified slot.

<Sysname> reset isis event-log graceful-restart slot 1

IS-IS commands -- reset isis event-log lsp

Use reset isis event-log lsp to clear IS-IS LSP log information.

Syntax

reset isis event-log lsp [ process-id ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command clears LSP log information for all IS-IS processes.

Examples

# Clear LSP log information for IS-IS process 1.

<Sysname> reset isis event-log lsp 1

Related commands

display isis event-log lsp

IS-IS commands -- reset isis event-log non-stop-routing

Use reset isis event-log non-stop-routing to clear IS-IS NSR log information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

reset isis event-log non-stop-routing slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset isis event-log non-stop-routing chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Usage guidelines

This command is applicable only to distributed devices and IRF-capable devices.

Examples

# (Distributed devices in standalone mode.) (Centralized IRF devices.) Clear IS-IS NSR log information for the specified slot.

<Sysname> reset isis event-log non-stop-routing slot 1

IS-IS commands -- reset isis event-log spf

Use reset isis event-log spf to clear IS-IS route calculation log information.

Syntax

reset isis event-log spf [ process-id ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command clears route calculation log information for all IS-IS processes.

Examples

# Clear route calculation log information for IS-IS process 1.

<Sysname> reset isis event-log spf 1

Related commands

display isis event-log spf

IS-IS commands -- reset isis packet

Use reset isis packet to clear IS-IS packet statistics.

Syntax

reset isis packet [ csnp | hello | lsp | psnp ] [ interface-type interface-number ] [ process-id ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

csnp: Clears CSNP packet statistics.

hello: Clears hello packet statistics.

lsp: Clears LSP packet statistics.

psnp: Clears PSNP packet statistics.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this option, the command clears IS-IS packet statistics for all interfaces.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command clears IS-IS packet statistics for all IS-IS processes.

Examples

# Clear IS-IS packet statistics for all IS-IS processes.

<Sysname> reset isis packet

Related commands

display isis packet

IS-IS commands -- reset isis peer

Use reset isis peer to clear data structure information for a specified IS-IS neighbor.

Syntax

reset isis peer system-id [ process-id ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

system-id: Specifies an IS-IS neighbor by its system ID.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535 to clear data structure information for the neighbor in the specified IS-IS process.

Usage guidelines

Use this command when you re-establish an IS-IS neighbor relationship.

Examples

# Clear the data structure information of the neighbor with the system ID 0000.0c11.1111.

<Sysname> reset isis peer 0000.0c11.1111

IS-IS commands -- reset osi statistics

Use reset osi statistics to clear OSI packet statistics.

Syntax

reset osi statistics

Views

User view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

To obtain OSI packet statistics from the specified time point, first clear the existing statistics.

Examples

# Clear OSI packet statistics.

<Sysname> reset osi statistics

Related commands

display osi statistics

IS-IS commands -- set-att

Use set-att to set the ATT bit of Level-1 LSPs.

Use undo set-att to restore the default.

Syntax

set-att { always | never }

undo set-att

Default

The ATT bit is not set for Level-1 LSPs.

Views

IS-IS view

IS-IS IPv4 unicast topology view

Predefined user roles

network-admin

mdc-admin

Parameters

always: Sets the ATT bit of Level-1 LSPs.

never: Keeps the ATT bit of Level-1 LSPs not set.

Examples

# Set the ATT bit of Level-1 LSPs.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] set-att always

IS-IS commands -- set-overload

Use set-overload to set the overload bit.

Use undo set-overload to restore the default.

Syntax

In IS-IS view/IS-IS IPv4 unicast topology view:

set-overload [ on-startup [ [ start-from-nbr system-id [ timeout1 [ nbr-timeout ] ] ] | timeout2 | wait-for-bgp [ timeout3 ] ] ] [ allow { external | interlevel } * ]

undo set-overload

In IS-IS IPv6 unicast address family view:

set-overload [ on-startup [ [ start-from-nbr system-id [ timeout1 [ nbr-timeout ] ] ] | timeout2 | wait-for-bgp+ [ timeout3 ] ] ] [ allow { external | interlevel } * ]

undo set-overload

Default

The overload bit is not set.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

on-startup: Sets the overload bit upon system startup.

start-from-nbr system-id [ timeout1 [ nbr-timeout ] ]: Starts the nbr-timeout timer when the router begins to establish the neighbor relationship with the neighbor after system startup. If the neighbor relationship is formed within the nbr-timeout interval, IS-IS keeps the overload bit set. If not, the bit is cleared. IS-IS keeps the overload bit set within the timeout1 interval after the neighbor relationship is formed within the nbr-timeout interval.

· system-id—Specifies the neighbor.

· timeout1—The timeout1 interval is in the range of 5 to 86400 seconds, and the default is 600 seconds.

· nbr-timeout—The timer has an interval from 5 to 86400 seconds. The default is 1200 seconds.

timeout2: Sets the overload bit within the timeout2 interval after system startup. The interval is in the range of 5 to 86400 seconds, and the default is 600 seconds.

wait-for-bgp [ timeout3 ]: Starts the timeout3 timer for BGP convergence after system startup. If BGP is not converged within the timeout3 interval, IS-IS clears the overload bit. The value range for the timeout3 argument is 5 to 86400 seconds, and the default is 600 seconds.

wait-for-bgp4+ [ timeout3 ]: Starts the timeout3 timer for IPv6 BGP convergence after system startup. If IPv6 BGP is not converged within the timeout3 interval, IPv6 IS-IS clears the overload bit. The value range for the timeout3 argument is 5 to 86400 seconds, and the default is 600 seconds.

allow: Allows advertising address prefixes. By default, no address prefixes are allowed to be advertised when the overload bit is set.

external: Allows advertising IP address prefixes redistributed from other routing protocols with the allow keyword specified.

interlevel: Allows advertising IP address prefixes learned from different IS-IS levels with the allow keyword specified.

Usage guidelines

If the on-startup keyword is not specified, the command sets the overload bit immediately until the undo set-overload command is executed.

If the on-startup keyword is specified, IS-IS sets the overload bit upon system startup and keeps it set within the timeout2 interval.

Examples

# Set overload flag on the current router.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] set-overload

IS-IS commands -- snmp context-name

Use snmp context-name to set the context name for the SNMP object for managing IS-IS.

Use undo snmp context-name to restore the default.

Syntax

snmp context-name context-name

undo snmp context-name

Default

No context name is set for the SNMP object for managing IS-IS.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

context-name: Specifies a context name, a case-sensitive string of 1 to 32 characters.

Usage guidelines

TRILL shares the standard IS-IS MIB with IS-IS. The standard IS-IS MIB provides only single-instance MIB objects. For SNMP to correctly identify TRILL's management information in the standard IS-IS MIB, you must configure a unique context for TRILL.

Context is a method introduced to SNMPv3 for multiple-instance management. For SNMPv1/v2c, you must specify a community name as a context name for protocol identification.

Examples

# Configure the context name as isis for the SNMP object for managing IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] snmp context-name isis

IS-IS commands -- snmp-agent trap enable isis

Use snmp-agent trap enable isis to enable IS-IS SNMP notifications.

Use undo snmp-agent trap enable isis to disable IS-IS SNMP notifications.

Syntax

snmp-agent trap enable isis [ adjacency-state-change | area-mismatch | authentication | authentication-type | buffsize-mismatch | id-length-mismatch | lsdboverload-state-change | lsp-corrupt | lsp-parse-error | lsp-size-exceeded | manual-address-drop | max-seq-exceeded | maxarea-mismatch | own-lsp-purge | protocol-support | rejected-adjacency | skip-sequence-number | version-skew ] *

undo snmp-agent trap enable isis [ adjacency-state-change | area-mismatch | authentication | authentication-type | buffsize-mismatch | id-length-mismatch | lsdboverload-state-change | lsp-corrupt | lsp-parse-error | lsp-size-exceeded | manual-address-drop | max-seq-exceeded | maxarea-mismatch | own-lsp-purge | protocol-support | rejected-adjacency | skip-sequence-number | version-skew ] *

Default

IS-IS SNMP notifications are enabled.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

adjacency-state-change: Specifies notifications about IS-IS adjacency status changes.

area-mismatch: Specifies notifications about area address mismatches between hello packets.

authentication: Specifies notifications about authentication failures of IS-IS packets.

authentication-type: Specifies notifications about authentication type errors of IS-IS packets.

buffsize-mismatch: Specifies notifications about buffer size mismatches for LSPs.

id-length-mismatch: Specifies notifications about system ID length mismatches of IS-IS packets.

lsdboverload-state-change: Specifies notifications about LSDB overload state changes.

lsp-corrupt: Specifies notifications about LSP checksum errors in the LSDB.

lsp-parse-error: Specifies notifications about LSP packet parse failures.

lsp-size-exceeded: Specifies notifications about propagation failures caused by oversized LSPs.

manual-address-drop: Specifies notifications about manually configured area addresses that have been dropped.

max-seq-exceeded: Specifies notifications about attempts to exceed the maximum LSP sequence number.

maxarea-mismatch: Specifies notifications about maximum area address mismatches of hello packets.

own-lsp-purge: Specifies notifications about attempts to remove the local LSP.

protocol-support: Specifies notifications about supported-protocol mismatches.

rejected-adjacency: Specifies notifications about adjacency creation failures.

skip-sequence-number: Specifies notifications about LSP sequence number duplications.

version-skew: Specifies notifications about hello packet version mismatches.

Usage guidelines

If you do not specify a notification, this command enables all IS-IS SNMP notifications.

If no IS-IS process exists, the configuration is not allowed.

This function does not take effect if all configured IS-IS processes are deleted.

Examples

# Disable IS-IS SNMP notifications.

<Sysname> system-view

[Sysname] undo snmp-agent trap enable isis

IS-IS commands -- summary

Use summary to configure a summary route.

Use undo summary to remove a summary route.

Syntax

In IS-IS IPv4 unicast address family view/IS-IS IPv4 unicast topology view:

summary ip-address { mask-length | mask } [ avoid-feedback | generate_null0_route | [ level-1 | level-1-2 | level-2 ] | tag tag ] *

undo summary ip-address { mask-length | mask } [ level-1 | level-1-2 | level-2 ]

In IS-IS IPv6 unicast address family view:

summary ipv6-prefix prefix-length [ avoid-feedback | generate_null0_route | [ level-1 | level-1-2 | level-2 ] | tag tag ] *

undo summary ipv6-prefix prefix-length [ level-1 | level-1-2 | level-2 ]

Default

No summary route is configured.

Views

IS-IS IPv4 unicast address family view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Specifies the destination IP address of the summary route.

mask-length: Specifies the mask length of the summary route, in the range of 0 to 32.

mask: Specifies the mask of the destination IP address, in dotted decimal notation.

ipv6-prefix: Specifies an IPv6 prefix for the summary route.

prefix-length: Specifies the length of the IPv6 prefix, in the range of 0 to 128.

avoid-feedback: Avoids learning summary routes by route calculation.

generate_null0_route: Generates the Null 0 route to avoid routing loops.

level-1: Summarizes only the routes redistributed to Level-1.

level-1-2: Summarizes the routes redistributed to both Level-1 and Level-2.

level-2: Summarizes only the routes redistributed to Level-2.

tag tag: Specifies a management tag in the range of 1 to 4294967295.

Usage guidelines

To reduce the size of the routing table, as well as the size of LSP and LSDB generated by the router, summarize multiple contiguous networks into a single network. You can summarize native IS-IS routes and redistributed routes. After summarization, the cost of the summary route is the smallest cost of the summarized routes.

If no level is specified, only level-2 routes are summarized.

The router summarizes only routes generated from local LSPs.

Examples

# Configure a summary route of 202.0.0.0/8.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] address-family ipv4

[Sysname-isis-1-ipv4] summary 202.0.0.0 255.0.0.0

IS-IS commands -- timer lsp-generation

Use timer lsp-generation to set the LSP generation interval.

Use undo timer lsp-generation to remove the configuration.

Syntax

timer lsp-generation maximum-interval [ minimum-interval [ incremental-interval ] ] [ level-1 | level-2 ]

undo timer lsp-generation [ level-1 | level-2 ]

Default

The maximum interval is 5 seconds, the minimum interval is 50 milliseconds, and the incremental interval is 200 milliseconds.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

maximum-interval: Specifies the maximum interval in the range of 1 to 120 seconds.

minimum-interval: Specifies the minimum interval in the range of 10 to 60000 milliseconds.

incremental-interval: Specifies the incremental interval in the range of 10 to 60000 milliseconds.

level-1: Applies the intervals to Level-1.

level-2: Applies the intervals to Level-2. If no level is specified, the specified intervals apply to both Level-1 and Level-2.

Usage guidelines

By adjusting the LSP generation interval, you can prevent bandwidth and router resources from being over consumed due to frequent topology changes.

When network changes are not frequent, the minimum-interval is adopted. If network changes become frequent, the LSP generation interval increases by the incremental-interval each time a generation occurs until the maximum-interval is reached.

The minimum interval and the incremental interval cannot be greater than the maximum interval.

Examples

# Set the maximum interval, minimum interval, and incremental interval to 10 seconds, 100 milliseconds, and 200 milliseconds, respectively.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1]timer lsp-generation 10 100 200

IS-IS commands -- timer lsp-max-age

Use timer lsp-max-age to set the LSP maximum age in the LSDB.

Use undo timer lsp-max-age to restore the default.

Syntax

timer lsp-max-age second s

undo timer lsp-max-age

Default

The LSP maximum age is 1200 seconds.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

seconds: Specifies the LSP maximum aging time in the range of 1 to 65535 seconds.

Usage guidelines

Each LSP has an age that decreases in the LSDB. Any LSP with an age of 0 is deleted from the LSDB. You can adjust the age value based on the scale of a network.

Examples

# Set the maximum LSP age to 1500 seconds.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] timer lsp-max-age 1500

Related commands

timer lsp-refresh

IS-IS commands -- timer lsp-refresh

Use timer lsp-refresh to set the LSP refresh interval.

Use undo timer lsp-refresh to restore the default.

Syntax

timer lsp-refresh second s

undo timer lsp-refresh

Default

The default LSP refresh interval is 900 seconds.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

second s: Specifies the LSP refresh interval in the range of 1 to 65534 seconds.

Usage guidelines

Each router refreshes its LSPs at a configurable interval and sends them to other routers to achieve the following purposes:

· Prevent valid routes from aging out.

· Synchronize LSPs in the network.

A smaller refresh interval speeds up network convergence but consumes more bandwidth.

To refresh LSPs before they are aged out, the interval configured by the timer lsp-refresh command must be smaller than that configured by the timer lsp-max-age command.

Examples

# Set the LSP refresh interval to 1500 seconds.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] timer lsp-refresh 1500

Related commands

timer lsp-max-age

IS-IS commands -- timer spf

Use timer spf to set the SPF calculation interval.

Use undo timer spf to restore the default.

Syntax

timer spf maximum-interval [ minimum-interval [ incremental-interval ] ]

undo timer spf

Default

The maximum interval is 5 seconds, the minimum interval is 50 milliseconds, and the incremental interval is 200 milliseconds.

Views

IS-IS view

IS-IS IPv4 unicast topology view

IS-IS IPv6 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

maximum-interval: Specifies the maximum SPF calculation interval in the range of 1 to 120 seconds.

minimum-interval: Specifies the minimum SPF calculation interval in the range of 10 to 60000 milliseconds.

incremental-interval: Specifies the incremental SPF calculation interval in the range of 10 to 60000 milliseconds.

Usage guidelines

Based on the LSDB, an IS-IS router uses the SPF algorithm to calculate a shortest path tree with itself being the root, and uses the shortest path tree to determine the next hop to a destination network. By adjusting the SPF calculation interval, you can prevent bandwidth and router resources from being overused due to frequent topology changes.

When network changes are not frequent, the minimum-interval is adopted. If network changes become frequent, the SPF calculation interval increases by the incremental-interval each time a generation happens until the maximum-interval is reached.

The minimum interval and the incremental interval cannot be greater than the maximum interval.

Examples

# Set the maximum interval to 10 seconds, the minimum interval to 100 milliseconds, and the incremental interval to 300 milliseconds, respectively.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] timer spf 10 100 300

IS-IS commands -- topology

Use topology to create an IS-IS IPv4 unicast topology and enter its view.

Use undo topology to remove the IS-IS IPv4 unicast topology and all configurations in the view.

Syntax

topology topo-name [ tid tid ]

undo topology topo-name

Default

No IS-IS IPv4 unicast topologies exist.

Views

IS-IS IPv4 unicast address family view

Predefined user roles

network-admin

mdc-admin

Parameters

topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters.

tid: Specifies the topology number in the range of 6 to 4095.

Usage guidelines

The name base is reserved for the base topology.

This command takes effect after the related IPv4 subtopology is configured.

This command can be configured only when the link cost style is wide, compatible, or wide-compatible.

Examples

# Create IS-IS IPv4 unicast topology voice (4000) and enter its view.

<Sysname> system-view

[Sysname] isis 100

[Sysname-isis-100] address-family ipv4

[Sysname-isis-100-ipv4] topology voice tid 4000

[Sysname-isis-100-ipv4-topo-voice]

Related commands

cost-style

IS-IS commands -- virtual-system

Use virtual-system to configure a virtual system ID for the IS-IS process.

Use undo virtual-system to remove a virtual system ID.

Syntax

virtual-system virtual-system-id

undo virtual-system virtual-system-id

Default

No virtual system ID is configured.

Views

IS-IS view

Predefined user roles

network-admin

mdc-admin

Parameters

virtual-system-id: Specifies a virtual system ID for the IS-IS process.

Examples

# Set a virtual system ID of 2222.2222.2222 for IS-IS process 1.

<Sysname> system-view

[Sysname] isis 1

[Sysname-isis-1] virtual-system 2222.2222.2222