Basic MPLS probe commands -- debugging system internal mpls lfib

Use debugging system internal mpls lfib to enable MPLS LFIB debugging.

Use undo debugging system internal mpls lfib to disable MPLS LFIB debugging.

Syntax

Centralized devices:

debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync }

undo debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync }

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync } slot slot-number [ cpu cpu-number ]

undo debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync } chassis chassis-number slot slot-number [ cpu cpu-number ]

undo debugging system internal mpls lfib { all | config | ilm | message | nhlfe | sync } chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

MPLS LFIB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all types of MPLS LFIB debugging.

config: Specifies MPLS LFIB configuration debugging.

ilm: Specifies MPLS LFIB ILM debugging.

message: Specifies MPLS LFIB message debugging.

nhlfe: Specifies MPLS LFIB NHLFE debugging.

sync: Specifies MPLS LFIB synchronization debugging.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls forwarding temporary-ilm

Use display system internal mpls forwarding temporary-ilm to display temporary ILM entries.

Syntax

Centralized devices:

display system internal mpls forwarding temporary-ilm [ label ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls forwarding temporary-ilm [ label ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls forwarding temporary-ilm [ label ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

label: Specifies an incoming label. The value range varies by device model. If you do not specify this argument, the command displays all temporary ILM entries.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls lfib ilm

Use display system internal mpls lfib ilm to display detailed MPLS ILM information.

Syntax

Centralized devices:

display system internal mpls lfib ilm label

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls lfib ilm label slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls lfib ilm label chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

label: Specifies an incoming label. The value range varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls lfib nhlfe

Use display system internal mpls lfib nhlfe to display detailed MPLS NHLFE information.

Syntax

Centralized devices:

display system internal mpls lfib nhlfe nid

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls lfib nhlfe nid slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls lfib nhlfe nid chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nid: Specifies an NHLFE entry index. The value range varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls lfib nhlfe reflist

Use display system internal mpls lfib nhlfe reflist to display MPLS NHLFE reverse mapping information.

Syntax

Centralized devices:

display system internal mpls lfib nhlfe nid reflist

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls lfib nhlfe nid reflist slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls lfib nhlfe nid reflist chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nid: Specifies an NHLFE entry index. The value range varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls lfib record

Use display system internal mpls lfib record to display information recorded by the MPLS LFIB module, including information received by MPLS LFIB, information LFIB set to the driver, and information returned from the driver.

Syntax

Centralized devices:

display system internal mpls lfib record [ start start-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls lfib record [ start start-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls lfib record [ start start-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

start start-number: Specifies the number of a record. This command displays the specified record and all records that follow. If you do not specify this keyword, the command displays all records. The value range for the start-number argument varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Related commands

reset system internal mpls lfib record

Basic MPLS probe commands -- display system internal mpls lfib statistics

Use display system internal mpls lfib statistics to display MPLS LFIB statistics.

Syntax

Centralized devices:

display system internal mpls lfib statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls lfib statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls lfib statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- display system internal mpls lsp-pending

Use display system internal mpls lsp-pending to display information about LSPs not deployed to the forwarding plane during the GR process of LDP, BGP, or RSVP.

Syntax

display system internal mpls lsp-pending

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic MPLS probe commands -- display system internal mpls statistics

Use display system internal mpls statistics to display internal statistics for MPLS.

Syntax

display system internal mpls statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Basic MPLS probe commands -- mpls lfib record size

Use mpls lfib record size to set the maximum number of entries that the MPLS LFIB module records.

Syntax

Centralized devices:

mpls lfib record size size

Distributed devices in standalone mode:Centralized IRF devices:

mpls lfib record size size slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

mpls lfib record size size chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

The MPLS LFIB module can record a maximum of 4096 entries.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

size: Specifies the maximum number of entries. The value range varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Basic MPLS probe commands -- reset system internal mpls lfib record

Use reset system internal mpls lfib record to clear information recorded by the MPLS LFIB module.

Syntax

Centralized devices:

reset system internal mpls lfib record

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal mpls lfib record slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal mpls lfib record chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Related commands

display system internal mpls lfib record