MAC address table probe commands -- debugging system internal drmac

| NOTE: Support for this command depends on the device model.

Use debugging system internal drmac to enable debugging for the MAC address synchronization module.

Use undo debugging system internal drmac to disable debugging for the MAC address synchronization module.

Syntax

debugging system internal drmac { all | error | event | message [ receive | send ] }

undo debugging system internal drmac { all | error | event | message [ receive | send ] }

Default

Debugging is disabled for the MAC address synchronization module.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies all debugging functions.

error: Specifies error debugging.

event: Specifies event debugging.

message [ receive | send ] : Specifies message debugging. If you use the message keyword without the receive or send keyword, this command enables both received and sent message debugging for the MAC address synchronization module.

· receive: Specifies received message debugging.

· send: Specifies sent message debugging.

MAC address table probe commands -- display system internal drmac mac-address

| NOTE: Support for this command depends on the device model.

Use display system internal drmac mac-address to display MAC address entries for the MAC address synchronization module.

Syntax

display system internal drmac mac-address [ mac-address [ vlan vlan-id ] | [ local | remote ] [ interface interface-type interface-number ] [ vlan vlan-id ] [ count ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mac-address: Specifies a MAC address in the format of H-H-H. When entering a MAC address, you can omit the leading zeros in each H section. For example, enter f-e2-1 for 000f-00e2-0001.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

local: Specifies MAC address entries that are synchronized from the local device to a remote device.

remote: Specifies MAC address entries that are synchronized from a remote device to the local device.

interface interface-type interface-number: Specifies an interface by its type and number. The interface can only be a DR interface or an IPP. If you do not specify this option, the command displays MAC address entries on all DR interfaces and the IPP.

count: Displays only the number of MAC address entries that match all entry attributes you specify in the command. Detailed information about MAC address entries is not displayed. If you do not specify this keyword, the command displays detailed information about the specified MAC address entries

MAC address table probe commands -- display system internal drmac statistics

| NOTE: Support for this command depends on the device model.

Use display system internal drmac statistics to display packet statistics on DR interfaces and the IPP.

Syntax

display system internal drmac statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

MAC address table probe commands -- display system internal mac-address configuration

Use display system internal mac-address configuration to display MAC address table configuration information.

Syntax

Centralized devices:

display system internal mac-address configuration { blackhole | multiport | multicast | static } [ count ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-address configuration { blackhole | multiport | multicast | static } [ count ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mac-address configuration { blackhole | multiport | multicast | static } [ count ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

blackhole: Displays blackhole MAC address entries.

multiport: Displays multiport unicast MAC address entries. Support for this keyword depends on the device model.

multicast: Displays multicast MAC address entries. Support for this keyword depends on the device model.

static: Displays static MAC address entries.

count: Displays the total number of MAC address entries that match all entry attributes you specify in the command. If you do not specify an entry attribute, the command displays the total number of entries in the MAC address table. If you do not specify this keyword, the command displays detailed information about specified MAC address entries.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MAC address table probe commands -- display system internal mac-address learned

| NOTE: Support for this command depends on the device model.

Use display system internal mac-address learned to display dynamic MAC address entries.

Syntax

Centralized devices:

display system internal mac-address learned [ mac-address [ vlan vlan-id ] | [ interface interface-type interface-number ] [ vlan vlan-id ] [ count ] ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-address learned [ mac-address [ vlan vlan-id ] | [ interface interface-type interface-number ] [ vlan vlan-id ] [ count ] ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mac-address learned [ mac-address [ vlan vlan-id ] | [ interface interface-type interface-number ] [ vlan vlan-id ] [ count ] ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mac-address: Specifies a MAC address in the format of H-H-H. When entering a MAC address, you can omit the leading zeros in each H section. For example, enter f-e2-1 for 000f-00e2-0001.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

interface interface-type interface-number: Specifies an interface by its type and number.

count: Displays only the number of dynamic MAC address entries that match all entry attributes you specify in the command. Detailed information about dynamic MAC address entries is not displayed. If you do not specify this keyword, the command displays detailed information about the specified dynamic MAC address entries.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MAC address table probe commands -- display system internal mac-address protocol

Use display system internal mac-address protocol to display feature-specific MAC address entries or VLAN interface-based MAC address entries.

Syntax

Centralized devices:

display system internal mac-address protocol [ auth | client | dot1x | ead | evb | openflow | security | vlan-interface | voice-vlan ] [ count ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-address protocol [ auth | client | dot1x | ead | evb | openflow | security | vlan-interface | voice-vlan ] [ count ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mac-address protocol [ auth | client | dot1x | ead | evb | openflow | security | vlan-interface | voice-vlan ] [ count ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

auth: Displays MAC address entries for MAC authentication.

client: Displays MAC address entries for online wireless clients.

dot1x: Displays MAC address entries for 802.1X.

ead: Displays MAC address entries for EAD.

evb: Displays MAC address entries for EVB.

openflow: Displays MAC address entries for OpenFlow.

security: Displays secure MAC address entries for port security.

vlan-interface: Displays MAC address entries on VLAN interfaces.

voice-vlan: Displays MAC address entries for voice VLANs.

count: Displays only the number of MAC address entries that match all entry attributes you specify in the command. Detailed information about MAC address entries is not displayed. If you do not specify this keyword, the command displays detailed information about the specified MAC address entries.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MAC address table probe commands -- display system internal mac-address statistics

Use display system internal mac-address statistics to display MAC address table statistics.

Syntax

Centralized devices:

display system internal mac-address statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-address statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mac-address statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MAC address table probe commands -- reset system internal drmac statistics

| NOTE: Support for this command depends on the device model.

Use reset system internal drmac statistics to clear packet statistics on DR interfaces and the IPP.

Syntax

reset system internal drmac statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

MAC address table probe commands -- reset system internal mac-address statistics

Use reset system internal mac-address statistics to clear MAC address table statistics.

Syntax

Centralized devices:

reset system internal mac-address statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal mac-address statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal mac-address statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.