IP multicast probe commands -- debugging system internal igmp-snooping fsm tracing

Use debugging system internal igmp-snooping fsm tracing to enable trace log debugging for the IGMP snooping state machine.

Use undo debugging system internal igmp-snooping fsm tracing to disable trace log debugging for the IGMP snooping state machine.

Syntax

Centralized devices:

debugging system internal igmp-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ] [ group-address source-address ] ] undo debugging system internal igmp-snooping fsm tracing

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal igmp-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ] [ group-address source-address ] ] [ slot slot-number [ cpu cpu-number ] ]

undo debugging system internal igmp-snooping fsm tracing

Distributed devices in IRF mode:

debugging system internal igmp-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ][ group-address source-address ] ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

undo debugging system internal igmp-snooping fsm tracing

Default

Trace log debugging is disabled for the IGMP snooping state machine.

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command outputs trace logs for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command outputs trace logs for all VSIs.

group-address: Specifies a multicast group address. If you do not specify a multicast group, this command outputs trace logs for all multicast groups.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command outputs trace logs for all multicast sources.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command outputs trace logs for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command outputs trace logs for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command outputs trace logs for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command outputs trace logs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command outputs trace logs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- debugging system internal mld-snooping fsm tracing

Use debugging system internal mld-snooping fsm tracing to enable trace log debugging for the MLD snooping state machine.

Use undo debugging system internal mld-snooping fsm tracing to disable trace log debugging for the MLD snooping state machine.

Syntax

Centralized devices:

debugging system internal mld-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ] [ ipv6-group-address ipv6-source-address ] ]

undo debugging system internal mld-snooping fsm tracing

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal mld-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ] [ ipv6-group-address ipv6-source-address ] ] [ slot slot-number [ cpu cpu-number ] ]

undo debugging system internal mld-snooping fsm tracing

Distributed devices in IRF mode:

debugging system internal mld-snooping fsm tracing [ [ vlan vlan-id | vsi vsi-name ] [ ipv6-group-address ipv6-source-address ] ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

undo debugging system internal mld-snooping fsm tracing

Default

Trace log debugging is disabled for the MLD snooping state machine.

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command outputs trace logs for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command outputs trace logs for all VSIs.

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command outputs trace logs for all IPv6 multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source address by its IPv6 address. If you do not specify an IPv6 multicast source, this command outputs trace logs for all IPv6 multicast sources.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command outputs trace logs for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command outputs trace logs for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command outputs trace logs for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command outputs trace logs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command outputs trace logs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal igmp group standby

Use display system internal igmp group standby to display IGMP multicast group information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal igmp [ vpn-instance vpn-instance-name ] group [ group-address | interface interface-type interface-number ] [ static | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal igmp [ vpn-instance vpn-instance-name ] group [ group-address | interface interface-type interface-number ] [ static | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

group-address: Specifies an IGMP multicast group by its IP address in the range of 224.0.1.0 to 239.255.255.255. If you do not specify an IGMP multicast group, this command displays backup information about all IGMP multicast groups.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup information about IGMP multicast groups for all interfaces.

static: Specifies IGMP multicast groups that hosts have joined statically. If you do not specify this keyword, the command displays backup information about IGMP multicast groups that hosts have joined dynamically.

verbose: Displays detailed backup information about IGMP multicast groups.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal igmp host group standby

| NOTE: Support for this command depends on the device model.

Use display system internal igmp host group standby to display information about IGMP host groups (multicast groups that contain IGMP host-enabled interfaces) for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal igmp [ vpn-instance vpn-instance-name ] host group [ group-address | interface interface-type interface-number ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal igmp [ vpn-instance vpn-instance-name ] host group [ group-address | interface interface-type interface-number ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

group-address: Specifies a multicast group by its IP address in the range of 224.0.1.0 to 239.255.255.255. If you do not specify a multicast group, this command displays backup information for all IGMP host groups.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup information about IGMP host groups for all interfaces.

verbose: Displays detailed backup information about IGMP host groups.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal igmp interface standby

Use display system internal igmp interface standby to display IGMP interface information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal igmp [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number ] [ host ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal igmp [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number ] [ host ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup IGMP information for all interfaces.

host: Specifies interfaces enabled with the IGMP host feature. If you do not specify this keyword, the command displays backup IGMP information for interfaces enabled with IGMP and those enabled with the IGMP host feature. For more information about the IGMP host feature, see VXLAN Configuration Guide. Support for this keyword depends on the device model.

verbose: Displays detailed backup IGMP information for interfaces.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal igmp user-authorization record

| NOTE: Support for this command depends on the device model.

Use display system internal igmp user-authorization record to display per-user statistics for messages that the authentication module sends to the IGMP process.

Syntax

display system internal igmp user-authorization record

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- display system internal igmp user-authorization statistics

| NOTE: Support for this command depends on the device model.

Use display system internal igmp user-authorization statistics to display per-access-type statistics for messages that the authentication module sends to the IGMP process.

Syntax

display system internal igmp user-authorization statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- display system internal ipv6 l2-multicast ip forwarding verbose

Use display system internal ipv6 l2-multicast ip forwarding verbose to display detailed information about IPv6 forwarding entries for Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast ip forwarding verbose [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast ip forwarding verbose [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast ip forwarding verbose [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command displays detailed information about IPv6 forwarding entries for all IPv6 multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays detailed information about IPv6 forwarding entries for all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about IPv6 forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about IPv6 forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IPv6 forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IPv6 forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 l2-multicast ip verbose

Use display system internal ipv6 l2-multicast ip verbose to display detailed information about IPv6 multicast groups for Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast ip verbose [ group ipv6-group-address | source ipv6-source-address] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast ip verbose [ group ipv6-group-address | source ipv6-source-address] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast ip verbose [ group ipv6-group-address | source ipv6-source-address] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command displays detailed information about all IPv6 multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays detailed information about IPv6 multicast groups with all IPv6 multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about IPv6 multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about IPv6 multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IPv6 multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IPv6 multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 l2-multicast ipc statistics

Use display system internal ipv6 l2-multicast ipc statistics to display inter-process communication (IPC) statistics for Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast ipc statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast ipc statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast ipc statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPC statistics for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPC statistics for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPC statistics for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 l2-multicast mac forwarding verbose

Use display system internal ipv6 l2-multicast mac forwarding verbose to display detailed information about MAC forwarding entries for Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

mac-address: Specifies a MAC multicast group. If you do not specify a MAC multicast group, this command displays detailed information about MAC forwarding entries for all MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about MAC forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about MAC forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about MAC forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 l2-multicast mac verbose

Use display system internal ipv6 l2-multicast mac verbose to display detailed information about MAC multicast groups for Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

mac-address: Specifies an IPv6 multicast MAC address. If you do not specify an IPv6 MAC multicast group, this command displays detailed information about all IPv6 MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about MAC multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about MAC multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about MAC multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 l2-multicast trill-offload-table

Use display system internal ipv6 l2-multicast trill-offload-table to display TRILL entries maintained by Layer 2 IPv6 multicast.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ] [ slot slot-number ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ] [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

local: Specifies ingress entries.

remote: Specifies egress entries.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for all VLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays TRILL entries maintained by Layer 2 IPv6 multicast for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

IP multicast probe commands -- display system internal ipv6 l2-multicast fast-forwarding cache verbose

Use display system internal ipv6 l2-multicast fast-forwarding cache verbose to display detailed information about Layer 2 IPv6 multicast fast forwarding entries.

Syntax

Centralized devices:

display system internal ipv6 l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ ipv6-source-address | ipv6-group-address ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ ipv6-source-address | ipv6-group-address ] * [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ ipv6-source-address | ipv6-group-address ] * [chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for all VLANs.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address.

ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers from 0 to F.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about Layer 2 IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 mrib interface statistics

Use display system internal ipv6 mrib interface statistics to display statistics for the interfaces that are maintained by the IPv6 MRIB.

Syntax

display system internal ipv6 mrib [ vpn-instance vpn-instance-name ] interface statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays statistics for the interfaces maintained by the IPv6 MRIB on the public network.

IP multicast probe commands -- display system internal ipv6 mrib mbr

Use display system internal ipv6 mrib mbr interface to display join/prune information maintained by the multicast border router (MBR) in the IPv6 MRIB process.

Syntax

display system internal ipv6 mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number [ source ipv6-source-address group ipv6-group-address ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays join/prune information on the public network.

interface interface-type interface-number: Specifies an interface by its type and number.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command does not display IPv6 MBR entries.

group ipv6-group-address: Specifies an IPv6 multicast group address by its IPv6 address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command does not display IPv6 MBR entries.

IP multicast probe commands -- display system internal ipv6 mrib mbr interface standby

Use display system internal ipv6 mrib mbr interface standby to display information about interfaces maintained by IPv6 PIM MRIB for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 multicast boundary standby

Use display system internal ipv6 multicast boundary standby to display IPv6 multicast boundary information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] boundary { group [ ipv6-group-address [ prefix-length ] ] | scope [ scope-id ] } [ interface interface-type interface-number ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] boundary { group [ ipv6-group-address [ prefix-length ] ] | scope [ scope-id ] } [ interface interface-type interface-number ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

group: Displays backup IPv6 multicast boundary information for the specified IPv6 multicast groups.

ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command displays backup IPv6 multicast boundary information for all IPv6 multicast groups.

prefix-length: Specifies an address prefix length in the range of 8 to 128. The default is 128.

scope: Displays backup IPv6 multicast boundary information for the specified the admin-scoped zone.

scope-id: Specifies an admin-scope zone by its ID in the range of 3 to 15, which is identified by the scope field in the IPv6 multicast group address. If you do not specify an admin-scoped zone, this command displays backup IPv6 multicast boundary information for all IPv6 admin-scoped zones.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup IPv6 multicast boundary information for all interfaces.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 multicast forwarding vlan reference

Use display system internal ipv6 multicast forwarding vlan reference to display mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries.

Syntax

Centralized devices:

display system internal ipv6 multicast forwarding vlan reference [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast forwarding vlan reference [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 multicast forwarding vlan reference [ group ipv6-group-address | source ipv6-source-address ] * [ vlan vlan-id ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. If you do not specify an IPv6 multicast group, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for all multicast groups.

source ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for all multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for all VLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays mappings between outgoing VLAN interfaces and Layer 2 IPv6 multicast entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 multicast forwarding-table dummy

Use display system internal ipv6 multicast forwarding-table dummy to display temporary IPv6 multicast forwarding entries.

Syntax

Centralized devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | statistics ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | statistics | slot slot-number [ cpu cpu-number ] ] *

Distributed devices in IRF mode:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | statistics ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays temporary IPv6 multicast forwarding entries on the public network.

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command displays temporary IPv6 multicast forwarding entries for all IPv6 multicast sources.

ipv6-group-address: Specifies an IPv6 multicast group address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command displays temporary IPv6 multicast forwarding entries for all IPv6 multicast groups.

prefix-length: Specifies an address prefix length. The default value is 128. For an IPv6 multicast group address, the value range for this argument is 8 to 128. For an IPv6 multicast source address, the value range for this argument is 0 to 128.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays temporary IPv6 multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays temporary IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays temporary IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays temporary IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays temporary IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

statistics: Displays statistics.

IP multicast probe commands -- display system internal ipv6 multicast forwarding-table verbose

Use display system internal ipv6 multicast forwarding-table verbose to display detailed information about IPv6 multicast forwarding entries.

Syntax

Centralized devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number | slot slot-number [ cpu cpu-number ] ] *

Distributed devices in IRF mode:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays detailed information about IPv6 multicast forwarding entries on the public network.

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command displays detailed information about IPv6 multicast forwarding entries for all IPv6 multicast sources.

ipv6-group-address: Specifies an IPv6 multicast group address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command displays detailed information about IPv6 multicast forwarding entries for all IPv6 multicast groups.

prefix-length: Specifies an address prefix length. The default value is 128. For an IPv6 multicast group address, the value range for this argument is 8 to 128. For an IPv6 multicast source address, the value range for this argument is 0 to 128.

incoming-interface: Specifies the IPv6 multicast forwarding entries that include the specified incoming interface. If you do not specify the keyword, this command displays detailed information about IPv6 multicast forwarding entries for all incoming interfaces.

interface-type interface-number: Specifies an incoming interface by its type and number.

outgoing-interface: Specifies the IPv6 multicast forwarding entries that include the specified outgoing interface. If you do not specify the keyword, this command displays detailed information about IPv6 multicast forwarding entries for all outgoing interfaces.

exclude: Specifies the IPv6 multicast forwarding entries that do not include the specified interface in the outgoing interface list.

include: Specifies the IPv6 multicast forwarding entries that include the specified interface in the outgoing interface list.

match: Specifies the IPv6 multicast forwarding entries that include only the specified interface in the outgoing interface list.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 multicast-vlan forwarding-table verbose

Use display system internal ipv6 multicast-vlan forwarding-table verbose to display detailed information about IPv6 multicast VLAN forwarding entries.

Syntax

Centralized devices:

display system internal ipv6 multicast-vlan forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast-vlan forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in IRF mode:

display system internal ipv6 multicast-vlan forwarding-table verbose [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command displays detailed information about IPv6 multicast VLAN forwarding entries for all IPv6 multicast sources.

ipv6-group-address: Specifies an IPv6 multicast group address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command displays detailed information about IPv6 multicast VLAN forwarding entries for all IPv6 multicast groups.

prefix-length: Specifies an address prefix length. The default value is 128. For an IPv6 multicast group address, the value range for this argument is 8 to 128. For an IPv6 multicast source address, the value range for this argument is 0 to 128.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 multicast VLAN forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IPv6 multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IPv6 multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

subvlan vlan-id: Specifies a sub-VLAN by its ID. If you do not specify a sub-VLAN, this command displays detailed information about IPv6 multicast VLAN forwarding entries for all sub-VLANs.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about IPv6 multicast VLAN forwarding entries for all VLANs.

IP multicast probe commands -- display system internal ipv6 multicast fast-forwarding cache verbose

Use display system internal ipv6 multicast fast-forwarding cache verbose to display detailed information about IPv6 multicast fast forwarding entries.

Syntax

Centralized devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ ipv6-source-address | ipv6-group-address ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ ipv6-source-address | ipv6-group-address ] * [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ ipv6-source-address | ipv6-group-address ] * [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays detailed information about IPv6 multicast fast forwarding entries on the public network.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address.

ipv6-group-address: Specifies an IPv6 multicast group by its IPv6 address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers from 0 to F.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IPv6 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IPv6 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim bsr-info standby

Use display system internal ipv6 pim bsr-info standby to display IPv6 PIM BSR information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] bsr-info standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] bsr-info standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim c-rp standby

Use display system internal ipv6 pim c-rp standby to display IPv6 PIM C-RP information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] c-rp standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] c-rp standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim interface

Use display system internal ipv6 pim interface to display interface information maintained by the label information base (LIB) in the IPv6 PIM process.

Syntax

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number [ address | gateway | prefix] ] | ipv6-address prefix-length ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number.

address: Specifies an IPv6 address.

gateway: Specifies an IPv6 gateway address.

prefix: Specifies an IPv6 address prefix.

ipv6-address: Specifies an IPv6 address except ::. If you do not specify an IPv6 address, this command displays interface information for all IPv6 addresses.

prefix-length: Specifies an address prefix length in the range of 0 to 128.

IP multicast probe commands -- display system internal ipv6 pim neighbor standby

Use display system internal ipv6 pim neighbor standby to display IPv6 PIM neighbor information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] neighbor [ interface interface-type interface-number [ ipv6-neighbor-address ] ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] neighbor [ interface interface-type interface-number [ ipv6-neighbor-address ] ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup IPv6 PIM neighbor information for all interfaces.

ipv6-neighbor-address: Specifies an IPv6 PIM neighbor by its IP address. If you do not specify an IPv6 PIM neighbor, this command displays backup information for all IPv6 PIM neighbors.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim routing-table standby

Use display system internal ipv6 pim routing-table standby to display IPv6 PIM routing entries for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] routing-table [ipv6-group-address | ipv6-source-address ] * standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] routing-table [ipv6-group-address | ipv6-source-address ] * standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays entries on the public network.

ipv6-group-address: Specifies an IPv6 multicast group address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command displays backup IPv6 PIM routing entries for all IPv6 multicast groups.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays backup IPv6 PIM routing entries for all IPv6 multicast sources.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim rp

Use display system internal ipv6 pim rp to display IPv6 PIM RP statistics.

Syntax

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] rp

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays IPv6 PIM RP statistics on the public network.

IP multicast probe commands -- display system internal ipv6 pim rp-info standby

Use display system internal ipv6 pim rp-info standby to display IPv6 PIM RP information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] rp-info standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim [ vpn-instance vpn-instance-name ] rp-info standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal ipv6 pim thread

Use display system internal ipv6 pim thread to display statistics for an IPv6 PIM thread.

Syntax

display system internal ipv6 pim thread { event | main | route }

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

event: Specifies the IPv6 PIM event thread.

main: Specifies the IPv6 PIM main thread.

route: Specifies the IPv6 PIM routing thread.

IP multicast probe commands -- display system internal ipv6 pim thread main standby

Use display system internal ipv6 pim thread main standby to display IPv6 PIM main thread statistics for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 pim thread main standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal ipv6 pim thread main standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast ip forwarding verbose

Use display system internal l2-multicast ip forwarding verbose to display detailed information about IP forwarding entries for Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast ip forwarding verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast ip forwarding verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number ] [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal l2-multicast ip forwarding verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number ] [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group group-address: Specifies a multicast group by its IP address. If you do not specify a multicast group, this command displays detailed information about IP multicast forwarding entries for all multicast groups.

source source-address: Specifies a multicast source address by its IP address. If you do not specify a multicast source, this command displays detailed information about IP multicast forwarding entries for all multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about IP multicast forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about IP multicast forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IP multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IP multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about IP multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IP multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about IP multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast ip verbose

Use display system internal l2-multicast ip verbose to display detailed information about IP multicast groups for Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast ip verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast ip verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal l2-multicast ip verbose [ group group-address | source source-address ] * [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group group-address: Specifies a multicast group by its IP address. If you do not specify a multicast group, this command displays detailed information about all multicast groups.

source source-address: Specifies a multicast source by its IP address. If you do not specify a multicast source, this command displays detailed information about multicast groups with all multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast ipc statistics

Use display system internal l2-multicast ipc statistics to display IPC statistics for Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast ipc statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast ipc statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal l2-multicast ipc statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPC statistics for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPC statistics for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPC statistics for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast mac forwarding verbose

Use display system internal l2-multicast mac forwarding verbose to display detailed information about MAC forwarding entries for Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal l2-multicast mac forwarding verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

mac-address: Specifies a multicast MAC address. If you do not specify a MAC multicast group, this command displays detailed information about MAC forwarding entries for all MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about MAC forwarding entries for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about MAC forwarding entries for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about MAC forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about MAC forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about MAC forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast mac verbose

Use display system internal l2-multicast mac verbose to display detailed information about MAC multicast groups for Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal l2-multicast mac verbose [ mac-address ] [ vlan vlan-id | vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

mac-address: Specifies a multicast MAC address. If you do not specify a MAC multicast group, this command displays detailed information about all MAC multicast groups.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about MAC multicast groups for all VLANs.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSI, this command displays detailed information about MAC multicast groups for all VSIs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about the MAC multicast groups for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about MAC multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about MAC multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast trill-offload-table

Use display system internal l2-multicast trill-offload-table to display TRILL entries maintained by Layer 2 multicast.

Syntax

Centralized devices:

display system internal l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ] [ slot slot-number ]

Distributed devices in IRF mode:

display system internal l2-multicast trill-offload-table [ local | remote ] [ vlan vlan-id ] [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

local: Specifies ingress entries.

remote: Specifies egress entries.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays TRILL entries maintained by Layer 2 multicast for all VLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays TRILL entries maintained by Layer 2 multicast for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays TRILL entries maintained by Layer 2 multicast for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays TRILL entries maintained by Layer 2 multicast for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays TRILL entries maintained by Layer 2 multicast for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays TRILL entries maintained by Layer 2 multicast for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

IP multicast probe commands -- display system internal mld group standby

Use display system internal mld group standby to display MLD multicast group information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mld [ vpn-instance vpn-instance-name ] group [ ipv6-group-address | interface interface-type interface-number ] [ static | verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mld [ vpn-instance vpn-instance-name ] group [ ipv6-group-address | interface interface-type interface-number ] [ static | verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

ipv6-group-address: Specifies an MLD multicast group by its IPv6 address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an MLD multicast group, this command displays backup information about all MLD multicast groups.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup information about MLD multicast groups for all interfaces.

static: Specifies MLD multicast groups that hosts have joined statically. If you do not specify the keyword, this command displays backup information about MLD multicast groups that hosts have joined dynamically.

verbose: Displays detailed backup information about MLD multicast groups.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal mld interface standby

Use display system internal mld interface standby to display MLD interface information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mld [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mld [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup MLD information for all interfaces.

verbose: Displays detailed backup MLD information for interfaces.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal l2-multicast fast-forwarding cache verbose

Use display system internal l2-multicast fast-forwarding cache verbose to display detailed information about Layer 2 multicast fast forwarding entries.

Syntax

Centralized devices:

display system internal l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ source-address | group-address ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ source-address | group-address ] * [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal l2-multicast fast-forwarding cache verbose [ vlan vlan_id ] [ source-address | group-address ] * [chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about Layer 2 multicast fast forwarding entries for all VLANs.

source-address: Specifies a multicast source by its IP address.

group-address: Specifies an multicast group by its IP address in the range of 224.0.1.0 to 239.255.255.255.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about Layer 2 multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about Layer 2 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about Layer 2 multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about Layer 2 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about Layer 2 multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal mld user-authorization record

| NOTE: Support for this command depends on the device model.

Use display system internal mld user-authorization record to display per-user statistics for messages that the authentication module sends to the MLD process.

Syntax

display system internal mld user-authorization record

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- display system internal mld user-authorization statistics

| NOTE: Support for this command depends on the device model.

Use display system internal mld user-authorization statistics to display per-access-type statistics for messages that the authentication module sends to the MLD process.

Syntax

display system internal mld user-authorization statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- display system internal mrib interface statistics

Use display system internal mrib interface statistics to display statistics for the interfaces that are maintained by the MRIB.

Syntax

display system internal mrib [ vpn-instance vpn-instance-name ] interface statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays statistics for the interfaces that are maintained by MRIB on the public network.

IP multicast probe commands -- display system internal mrib mbr

Use display system internal mrib mbr to display join/prune information maintained by the MBR in the MRIB process.

Syntax

display system internal mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number [ source source-address group group-address ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays join/prune information that is maintained by the MBR in the MRIB process on the public network.

interface interface-type interface-number: Specifies an interface by its type and number.

source source-address: Specifies a multicast source by its IP address. If you do not specify a multicast source, this command does not display MBR entries.

group group-address: Specifies a multicast group by its IP address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command does not display MBR entries.

IP multicast probe commands -- display system internal mrib mbr interface standby

Use display system internal mrib mbr interface standby to display information about interfaces maintained by PIM MRIB for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mrib [ vpn-instance vpn-instance-name ] mbr interface interface-type interface-number standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp brief standby

Use display system internal msdp brief standby to display brief information about MSDP peers for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] brief [ state { connect | disabled | established | listen | shutdown } ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] brief [ state { connect | disabled | established | listen | shutdown } ] standby chassis chassis-numbe r slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

state: Specifies MSDP peers in a state. If you do not specify this keyword, the command displays information for MSDP peers in all states.

connect: Specifies MSDP peers in connecting state.

disabled: Specifies MSDP peers in connection failure state.

established: Specifies MSDP peers in session state.

listen: Specifies MSDP peers in listening state.

shutdown: Specifies MSDP peers in shutdown state.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp global-configuration

Use display system internal msdp global-configuration to display global MSDP configuration information.

Syntax

Centralized devices:

display system internal msdp [ vpn-instance vpn-instance-name ] global-configuration

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] global-configuration [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] global-configuration [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays global MSDP configuration information on the public network.

standby slot slot-number: Specifies the slot number of the card where a standby process resides. If you do not specify a member device, this command displays global MSDP configuration information for the MPU. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. If you do not specify a member device, this command displays global MSDP configuration information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

standby slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. If you do not specify a member device or PEX, this command displays global MSDP configuration information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays global MSDP configuration information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays global MSDP configuration information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp local-source

Use display system internal msdp local-source to display local multicast source information.

Syntax

Centralized devices:

display system internal msdp [ vpn-instance vpn-instance-name ] local-source rp rp-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] local-source rp rp-address [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] local-source rp rp-address [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays local multicast source information on the public network.

rp rp-address: Specifies an RP by its IP address.

standby slot slot-number: Specifies the slot number of the card where a standby process resides. If you do not specify a card, this command displays local multicast source information for the MPU. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies the slot number of the card where a standby process resides. If you do not specify a member device, this command displays local multicast source information for the MPU. (Centralized IRF devices.) (IRF 3 incapable.)

standby slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. If you do not specify a member device or PEX, this command displays local multicast source information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays local multicast source information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays local multicast source information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp peer-configuration

Use display system internal msdp peer-configuration to display configuration information about MSDP peers.

Syntax

Centralized devices:

display system internal msdp [ vpn-instance vpn-instance-name ] peer-configuration [ peer-address ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] peer-configuration [ peer-address ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] peer-configuration [ peer-address ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays configuration information about MSDP peers on the public network.

peer-address: Specifies a state. If you do not specify this keyword, the command displays configuration information about all MSDP peers.

standby slot slot-number: Specifies the slot number of the card where a standby process resides. If you do not specify a card, this command displays configuration information about MSDP peers for the MPU. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. If you do not specify a member device, this command displays configuration information about MSDP peers for the MPU. (Centralized IRF devices.) (IRF 3 incapable.)

standby slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. If you do not specify a member device or PEX, this command displays configuration information about MSDP peers for the master device. (Centralized IRF devices.) (IRF 3 capable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays configuration information about MSDP peers for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

standby chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays configuration information about MSDP peers for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp peer-status standby

Use display system internal msdp peer-status standby to display status information about MSDP peers for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] peer-status [ peer-address ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] peer-status [ peer-address ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

peer-address: Specifies an MSDP peer by its IP address. If you do not specify an MSDP peer, this command displays backup status information for all MSDP peers.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp sa-cache standby

Use display system internal msdp sa-cache standby to display (S, G) entries in the backup SA cache for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] sa-cache [ group-address | source-address | as-number ] * standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] sa-cache [ group-address | source-address | as-number ] * standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the entries on the public network.

group-address: Specifies a multicast group address in the range of 224.0.1.0 to 239.255.255.255. If you do not specify a multicast group, this command displays (S, G) entries in the backup SA cache for all multicast groups.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command displays (S, G) entries in the backup SA cache for all multicast sources.

as-number: Specifies an AS by its number in the range of 1 to 4294967295. If you do not specify an AS, this command displays (S, G) entries in the backup SA cache for all ASs.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp sa-count standby

Use display system internal msdp sa-count standby to display the number of (S, G) entries in the SA cache for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal msdp [ vpn-instance vpn-instance-name ] sa-count [ as-number ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal msdp [ vpn-instance vpn-instance-name ] sa-count [ as-number ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the number on the public network.

as-number: Specifies an AS by its number in the range of 1 to 4294967295.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal msdp statistics

Use display system internal msdp statistics to display MSDP statistics.

Syntax

display system internal msdp statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- display system internal multicast boundary standby

Use display system internal multicast boundary standby to display multicast boundary information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast [ vpn-instance vpn-instance-name ] boundary [ group-address [ mask-length | mask ] ] [ interface interface-type interface-number ] standby slot slot-number [ cpu cpu-numbe r ]

Distributed devices in IRF mode:

display system internal multicast [ vpn-instance vpn-instance-name ] boundary [ group-address [ mask-length | mask ] ] [ interface interface-type interface-number ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

group-address: Specifies a multicast group by its IP address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command displays backup multicast boundary information for all multicast groups.

mask-length: Specifies an address mask length in the range of 4 to 32. The default is 32.

mask: Specifies an address mask. The default is 255.255.255.255.

interface interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup multicast boundary information for all interfaces.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal multicast capability

Use display system internal multicast capability to display multicast capability.

Syntax

Centralized devices:

display system internal multicast capability

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast capability [ slot slot-number ]

Distributed devices in IRF mode:

display system internal multicast capability [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays multicast capability for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays multicast capability for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays multicast capability for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays multicast capability for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays multicast capability for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

IP multicast probe commands -- display system internal multicast forwarding vlan reference

Use display system internal multicast forwarding vlan reference to display mappings between outgoing VLAN interfaces and Layer 2 multicast entries.

Syntax

Centralized devices:

display system internal multicast forwarding vlan reference [ group group-address | source source-address ] * [ vlan vlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast forwarding vlan reference [ group group-address | source source-address ] * [ vlan vlan-id ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal multicast forwarding vlan reference [ group group-address | source source-address ] * [ vlan vlan-id ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group group-address: Specifies a multicast group by its IP address. If you do not specify a multicast group, this command displays mappings between outgoing VLAN interfaces and Layer 2 multicast entries for all multicast groups.

source source-address: Specifies a multicast source by its IP address. If you do not specify a multicast source, this command displays mappings between outgoing VLAN interfaces and Layer 2 multicast entries for all multicast sources.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays mappings between outgoing VLAN interfaces and all multicast groups for all VLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays mappings between outgoing VLAN interfaces and Layer 2 multicast entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays mappings between outgoing VLAN interfaces and all multicast groups for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays mappings between outgoing VLAN interfaces and all multicast groups for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays mappings between outgoing VLAN interfaces and all multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays mappings between outgoing VLAN interfaces and all multicast groups for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal multicast forwarding-table dummy

Use display system internal multicast forwarding-table dummy to display temporary multicast forwarding entries.

Syntax

Centralized devices:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | statistics ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | statistics | slot slot-number [ cpu cpu-number ] ] *

Distributed devices in IRF mode:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | statistics ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays temporary multicast forwarding entries on the public network.

group-address: Specifies a multicast group address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command displays temporary multicast forwarding entries for all multicast groups.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command displays temporary multicast forwarding entries for all multicast sources.

mask-length: Specifies an address mask length. The default value is 32. For a multicast group address, the value range for this argument is 4 to 32. For a multicast source address, the value range for this argument is 0 to 32.

mask: Specifies an address mask. The default value is 255.255.255.255.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays temporary multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays temporary multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays temporary multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays temporary multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays temporary multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

statistics: Displays statistics.

IP multicast probe commands -- display system internal multicast forwarding-table verbose

Use display system internal multicast forwarding-table verbose to display detailed information about multicast forwarding entries.

Syntax

Centralized devices:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number | slot slot-number [ cpu cpu-number ] ] *

Distributed devices in IRF mode:

display system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | incoming-interface interface-type interface-number | outgoing-interface { exclude | include | match } interface-type interface-number ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays detailed information about multicast forwarding entries on the public network.

group-address: Specifies a multicast group address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command displays detailed information about multicast forwarding entries for all multicast groups.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command displays detailed information about multicast forwarding entries for all multicast sources.

mask-length: Specifies an address mask length. The default value is 32. For a multicast group address, the value range for this argument is 4 to 32. For a multicast source address, the value range for this argument is 0 to 32.

mask: Specifies an address mask. The default value is 255.255.255.255.

incoming-interface: Specifies the multicast forwarding entries that include the specified incoming interface. If you do not specify the keyword, this command displays detailed information about multicast forwarding entries for all incoming interfaces.

interface-type interface-number: Specifies an incoming interface by its type and number.

outgoing-interface: Specifies the multicast forwarding entries that include the specified outgoing interface. If you do not specify the keyword, this command displays detailed information about multicast forwarding entries for all outgoing interfaces.

exclude: Specifies the multicast forwarding entries that do not include the specified interface in the outgoing interface list.

include: Specifies the multicast forwarding entries that include the specified interface in the outgoing interface list.

match: Specifies the multicast forwarding entries that include only the specified interface in the outgoing interface list.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about the multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal multicast record

Use display system internal multicast record to display operation records about multicast entries.

Syntax

Centralized devices:

display system internal multicast record { statistics | { { all | fail } [ { group [ group-address | ipv6-group-address ] | source [ source-address | ipv6-source-address ] } * | item item-list | filter { exclude | include } { { add-l2-ip | add-l2-ip-port | add-l2-ip-slot | add-l2-mac | add-l2-mac-port | add-l2-mac-slot | add-l3-ipm | add-l3-oif | add-l3-port | add-l3-slot | del-l2-ip | del-l2-ip-port | del-l2-ip-slot | del-l2-mac | del-l2-mac-port | del-l2-mac-slot | del-l3-ipm | del-l3-oif | del-l3-port | del-l3-slot | set-l3-iif } * | ipmc-type-all } ] [ verbose ] } }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast record { statistics | { { all | fail } [ { group [ group-address | ipv6-group-address ] | source [ source-address | ipv6-source-address ] } * | item item-list | filter { exclude | include } { { add-l2-ip | add-l2-ip-port | add-l2-ip-slot | add-l2-mac | add-l2-mac-port | add-l2-mac-slot | add-l3-ipm | add-l3-oif | add-l3-port | add-l3-slot | del-l2-ip | del-l2-ip-port | del-l2-ip-slot | del-l2-mac | del-l2-mac-port | del-l2-mac-slot | del-l3-ipm | del-l3-oif | del-l3-port | del-l3-slot | set-l3-iif } * | ipmc-type-all } ] [ verbose ] } } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal multicast record { statistics | { { all | fail } [ { group [ group-address | ipv6-group-address ] | source [ source-address | ipv6-source-address ] } * | item item-list | filter { exclude | include } { { add-l2-ip | add-l2-ip-port | add-l2-ip-slot | add-l2-mac | add-l2-mac-port | add-l2-mac-slot | add-l3-ipm | add-l3-oif | add-l3-port | add-l3-slot | del-l2-ip | del-l2-ip-port | del-l2-ip-slot | del-l2-mac | del-l2-mac-port | del-l2-mac-slot | del-l3-ipm | del-l3-oif | del-l3-port | del-l3-slot | set-l3-iif } * | ipmc-type-all } ] [ verbose ] } } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

statistics: Displays statistics for operation records.

all: Specifies all operation records.

fail: Specifies failed operation records.

group-address: Specifies a multicast group address.

ipv6-group-address: Specifies an IPv6 multicast group address.

source-address: Specifies a multicast source address.

ipv6-source-address: Specifies an IPv6 multicast source address.

item item-list: Specifies one or more records. To display one record, set the value of the item-list argument to 1. To display more records, use the form start-item [ to end-item ]. The value ranges for the start-item argument and the end-item argument are 1 to 500000.

filter: Specifies the operation records in the specified filtering mode.

exclude: Specifies the operation records that do not meet the specified criteria.

include: Specifies the operation records that meet the specified criteria.

add-l2-ip: Specifies the operation records of adding Layer 2 IP multicast entries.

add-l2-ip-port: Specifies the operation records of adding ports to Layer 2 IP multicast entries.

add-l2-ip-slot: Specifies the operation records of adding cards to Layer 2 IP multicast entries.

add-l2-mac: Specifies the operation records of adding Layer 2 MAC multicast entries.

add-l2-mac-port: Specifies the operation records of adding ports to Layer 2 MAC multicast entries.

add-l2-mac-slot: Specifies the operation records of adding cards to Layer 2 MAC multicast entries.

add-l3-ipm: Specifies the operation records of adding Layer 3 multicast entries.

add-l3-oif: Specifies the operation records of adding outgoing interfaces to Layer 3 multicast entries.

add-l3-port: Specifies the operation records of adding outgoing ports to Layer 3 multicast entries.

add-l3-slot: Specifies the operation records of adding distributed forwarding cards where outgoing interfaces reside to Layer 3 multicast entries.

del-l2-ip: Specifies the operation records of deleting Layer 2 IP multicast entries.

del-l2-ip-port: Specifies the operation records of deleting ports from Layer 2 IP multicast entries.

del-l2-ip-slot: Specifies the operation records of deleting cards from Layer 2 IP entries.

del-l2-mac: Specifies the operation records of deleting Layer 2 MAC multicast entries.

del-l2-mac-port: Specifies the operation records of deleting ports from Layer 2 MAC multicast entries.

del-l2-mac-slot: Specifies the operation records of deleting cards from Layer 2 MAC entries.

del-l3-ipm: Specifies the operation records of deleting Layer 3 IP multicast entries.

del-l3-oif: Specifies the operation records of deleting outgoing interfaces from Layer 3 multicast entries.

del-l3-port: Specifies the operation records of deleting outgoing ports from Layer 3 multicast entries.

del-l3-slot: Specifies the operation records of removing distributed forwarding cards where outgoing interfaces reside from Layer 3 multicast entries.

set-l3-iif: Specifies the operation records of setting incoming interfaces for Layer 3 multicast entries.

ipmc-type-all: Specifies all types of operation records.

verbose: Displays detailed information. If the outgoing interface and outgoing port in the record are not complete, you need to specify this keyword.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays operation records about multicast entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays operation records about multicast entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays operation records about multicast entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays operation records about multicast entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays operation records about multicast entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal multicast-vlan forwarding-table verbose

Use display system internal multicast-vlan forwarding-table verbose to display detailed information about the multicast VLAN forwarding table.

Syntax

Centralized devices:

display system internal multicast-vlan forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast-vlan forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in IRF mode:

display system internal multicast-vlan forwarding-table verbose [ group-address [ mask { mask-length | mask } ] | source-address [ mask { mask-length | mask } ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

group-address: Specifies a multicast group address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command displays detailed information about multicast VLAN forwarding entries for all multicast groups.

mask { mask-length | mask }: Specifies a mask length or mask for the multicast group address. The value range for the mask-length argument is 4 to 32 and the default is 32. The default value for the mask argument is 255.255.255.255.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command displays detailed information about multicast VLAN forwarding entries for all multicast sources.

mask { mask-length | mask }: Specifies a mask length or mask for the multicast source address. The value range for the mask-length argument is 0 to 32 and the default is 32. The default value for the mask argument is 255.255.255.255.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about multicast VLAN forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

subvlan vlan-id: Specifies a sub-VLAN by its VLAN ID. If you do not specify a sub-VLAN, this command displays detailed information about multicast VLAN forwarding entries for all sub-VLANs.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify a VLAN, this command displays detailed information about multicast VLAN forwarding entries for all VLANs.

IP multicast probe commands -- display system internal multicast fast-forwarding cache verbose

Use display system internal multicast fast-forwarding cache verbose to display detailed information about multicast fast forwarding entries.

Syntax

Centralized devices:

display system internal multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ source address | group address ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ source address | group address ] * [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal multicast [ vpn-instance vpn-instance-name ] fast-forwarding cache verbose [ source address | group address ] * [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays detailed information about multicast fast forwarding entries on the public network.

source-address: Specifies a multicast source address.

group-address: Specifies a multicast group address in the range of 224.0.1.0 to 239.255.255.255.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about multicast fast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about multicast fast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about multicast fast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim bsr-info standby

Use display system internal pim bsr-info standby to display PIM BSR information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim [ vpn-instance vpn-instance-name ] bsr-info standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim [ vpn-instance vpn-instance-name ] bsr-info standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim c-rp standby

Use display system internal pim c-rp standby to display PIM C-RP information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim [ vpn-instance vpn-instance-name ] c-rp standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim [ vpn-instance vpn-instance-name ] c-rp standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays -RP information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim interface

Use display system internal pim interface to display interface information maintained by LIB in the PIM process.

Syntax

display system internal pim [ vpn-instance vpn-instance-name ] interface [ interface-type interface-number | ip-address { mask-length | mask } ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays interface information maintained by LIB on the public network.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays information about all interfaces.

ip-address: Specifies an IP address except 0.0.0.0. If you do not specify an IP address, this command displays interface information for all IP addresses.

mask-length: Specifies a mask length in the range of 0 to 32.

mask: Specifies a mask.

IP multicast probe commands -- display system internal pim neighbor standby

Use display system internal pim neighbor standby to display PIM neighbor information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim [ vpn-instance vpn-instance-name ] neighbor [ interface interface-type interface-number [ neighbor-address ] ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim [ vpn-instance vpn-instance-name ] neighbor [ interface interface-type interface-number [ neighbor-address ] ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

interface-type interface-number: Specifies an interface by its type and number. If you do not specify an interface, this command displays backup PIM neighbor information for all interfaces.

neighbor-address: Specifies a PIM neighbor by its IP address. If you do not specify a PIM neighbor, this command displays backup information for all PIM neighbors.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim routing-table standby

Use display system internal pim routing-table standby to display PIM routing entries for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim [ vpn-instance vpn-instance-name ] routing-table [ group-address | source-address ] * standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim [ vpn-instance vpn-instance-name ] routing-table [ group-address | source-address ] * standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays entries on the public network.

group-address: Specifies a multicast group by its IP address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command displays backup PIM routing entries for all multicast groups.

source-address: Specifies a multicast source by its IP address. If you do not specify a multicast source, this command displays backup PIM routing entries for all multicast sources.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim rp

Use display system internal pim rp to display PIM RP statistics.

Syntax

display system internal pim [ vpn-instance vpn-instance-name ] rp

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays PIM RP statistics on the public network.

IP multicast probe commands -- display system internal pim rp-info standby

Use display system internal pim rp-info standby to display PIM RP information for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim [ vpn-instance vpn-instance-name ] rp-info standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim [ vpn-instance vpn-instance-name ] rp-info standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays information on the public network.

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- display system internal pim thread

Use display system internal pim thread to display statistics for a PIM thread.

Syntax

display system internal pim thread { event | main | route }

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

event: Specifies the PIM event thread.

main: Specifies the PIM main thread.

route: Specifies the PIM routing thread.

IP multicast probe commands -- display system internal pim thread main standby

Use display system internal pim thread main standby to display PIM main thread statistics for a standby process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pim thread main standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal pim thread main standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

slot slot-number: Specifies the slot number of the card where a standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where a standby process resides. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the IRF member device or the PEX where a standby process resides. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the card on the IRF member device where a standby process resides or specifies the PEX where a standby process resides. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- igmp user-authorization record limit

| NOTE: Support for this command depends on the device model.

Use igmp user-authorization record limit to set the maximum number of users for whom the IGMP process collects authorization message statistics.

Syntax

igmp user-authorization record limit limit-value

Default

The default setting is 512.

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

limit-value: Specifies a maximum number in the range of 0 to 524288.

IP multicast probe commands -- mld user-authorization record limit

| NOTE: Support for this command depends on the device model.

Use mld user-authorization record limit to set the maximum number users for whom the MLD process collects authorization message statistics.

Syntax

mld user-authorization record limit limit-value

Default

The default setting is 512.

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

limit-value: Specifies a maximum number in the range of 0 to 524288.

IP multicast probe commands -- multicast record limit

Use multicast record limit to set the maximum number of operation records for multicast entries.

Use undo multicast record limit to restore the default.

Syntax

multicast record [ fail ] limit limit-value

undo multicast record [ fail ] limit

Default

The maximum number is 0. The device does not keep operation records for multicast entries.

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

fail: Specifies records of failed operations on multicast entries.

limit-value: Specifies the maximum number of operation records for multicast entries, in the range of 0 to 500000.

IP multicast probe commands -- reset system internal igmp user-authorization record

| NOTE: Support for this command depends on the device model.

Use reset system internal igmp user-authorization record to clear per-access-type statistics for messages that the authentication module sends to the IGMP process.

Syntax

reset system internal igmp user-authorization record

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- reset system internal igmp user-authorization statistics

| NOTE: Support for this command depends on the device model.

Use reset system internal igmp user-authorization statistics to clear per-user statistics for messages that the authentication module sends to the IGMP process.

Syntax

reset system internal igmp user-authorization statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- reset system internal ipv6 multicast forwarding-table dummy

Use reset system internal ipv6 multicast forwarding-table dummy to clear temporary IPv6 multicast forwarding entries.

Syntax

Centralized devices:

reset system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { ipv6-group-address [ prefix-length ] | ipv6-source-address [ prefix-length ] } * | all }

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { ipv6-group-address [ prefix-length ] | ipv6-source-address [ prefix-length ] } * | all } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ipv6 multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { ipv6-group-address [ prefix-length ] | ipv6-source-address [ prefix-length ] } * | all } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command clears temporary IPv6 multicast forwarding entries on the public network.

ipv6-group-address: Specifies an IPv6 multicast group address in the range of FFxy::/16, where "x" and "y" represent any hexadecimal numbers from 0 to F. If you do not specify an IPv6 multicast group, this command clears temporary IPv6 multicast forwarding entries for all IPv6 multicast groups.

ipv6-source-address: Specifies an IPv6 multicast source address. If you do not specify an IPv6 multicast source, this command clears temporary IPv6 multicast forwarding entries for all IPv6 multicast sources.

prefix-length: Specifies an address prefix length. The default value is 128. For an IPv6 multicast group address, the value range for this argument is 8 to 128. For an IPv6 multicast source address, the value range for this argument is 0 to 128.

all: Specifies all entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears temporary IPv6 multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command clears temporary IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command clears temporary IPv6 multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears temporary IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command clears temporary IPv6 multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- reset system internal mld user-authorization record

| NOTE: Support for this command depends on the device model.

Use reset system internal mld user-authorization record to clear per-access-type statistics for messages that the authentication module sends to the MLD process.

Syntax

reset system internal mld user-authorization record

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- reset system internal mld user-authorization statistics

| NOTE: Support for this command depends on the device model.

Use reset system internal mld user-authorization statistics to clear per-user statistics for messages that the authentication module sends to the MLD process.

Syntax

reset system internal mld user-authorization statistics

Views

Probe view

Predefined user role

network-admin

mdc-admin

IP multicast probe commands -- reset system internal multicast forwarding-table dummy

Use reset system internal multicast forwarding-table dummy to clear temporary multicast forwarding entries.

Syntax

Centralized devices:

reset system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] } * | all }

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] } * | all } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal multicast [ vpn-instance vpn-instance-name ] forwarding-table dummy { { source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] } * | all } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user role

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command clears temporary multicast forwarding entries on the public network.

source-address: Specifies a multicast source address. If you do not specify a multicast source, this command clears temporary multicast forwarding entries for all multicast sources.

group-address: Specifies a multicast group address in the range of 224.0.0.0 to 239.255.255.255. If you do not specify a multicast group, this command clears temporary multicast forwarding entries for all multicast groups.

mask-length: Specifies an address mask length. The default value is 32. For a multicast group address, the value range for this argument is 4 to 32. For a multicast source address, the value range for this argument is 0 to 32.

mask: Specifies the address mask. The default is 255.255.255.255.

all: Specifies all routing entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears temporary multicast forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command clears temporary multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command clears temporary multicast forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears temporary multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command clears temporary multicast forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IP multicast probe commands -- reset system internal multicast record

Use reset system internal multicast record to clear operation records for multicast entries.

Syntax

reset system internal multicast record

Views

Probe view

Predefined user role

network-admin

mdc-admin