Layer 2 forwarding probe commands -- Normal Layer 2 forwarding probe commands -- display system internal mac-forwarding controlblock

| NOTE: Support for this command depends on the device model.

Use display system internal mac-forwarding controlblock to display the interface control information of Layer 2 forwarding.

Syntax

Centralized devices:

display system internal mac-forwarding controlblock interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-forwarding controlblock interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mac-forwarding controlblock interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Layer 2 forwarding probe commands -- Fast Layer 2 forwarding probe commands -- display system internal mac-forwarding cache ip verbose

| NOTE: Support for this command depends on the device model.

Use display system internal mac-forwarding cache ip verbose to display detailed information about IPv4 fast forwarding entries.

Syntax

Centralized devices:

display system internal mac-forwarding cache ip [ ip-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-forwarding cache ip [ ip-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal mac-forwarding cache ip [ ip-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Specifies an IPv4 address. If you do not specify an IPv4 address, this command displays detailed information about all IPv4 fast forwarding entries.

slot slot-numbe: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv4 fast forwarding entries for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv4 fast forwarding entries for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays detailed information about IPv4 fast forwarding entries for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information about IPv4 fast forwarding entries for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv4 fast forwarding entries for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays detailed information about IPv4 fast forwarding entries for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information about IPv4 fast forwarding entries for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Layer 2 forwarding probe commands -- Fast Layer 2 forwarding probe commands -- display system internal mac-forwarding cache ipv6 verbose

| NOTE: Support for this command depends on the device model.

Use display system internal mac-forwarding cache ipv6 verbose to display detailed information about IPv6 fast forwarding entries.

Syntax

Centralized devices:

display system internal mac-forwarding cache ipv6 [ ipv6-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mac-forwarding cache ipv6 [ ipv6-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal mac-forwarding cache ipv6 [ ipv6-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-address: Specifies an IPv6 address. If you do not specify an IPv6 address, this command displays detailed information about all IPv6 fast forwarding entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 fast forwarding entries for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 fast forwarding entries for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays detailed information about IPv6 fast forwarding entries for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information about IPv6 fast forwarding entries for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 fast forwarding entries for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays detailed information about IPv6 fast forwarding entries for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information about IPv6 fast forwarding entries for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Layer 2 forwarding probe commands -- Fast bridge forwarding probe commands -- display system internal bridge cache ip verbose

| NOTE: Support for this command depends on the device model.

Use display system internal bridge cache ip verbose to display detailed information about IPv4 fast bridge forwarding entries.

Syntax

Centralized devices:

display system internal bridge cache ip { inline | inter-vlan } [ ip-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bridge cache ip { inline | inter-vlan } [ ip-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bridge cache ip { inline | inter-vlan } [ ip-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

inline: Specifies inline forwarding entries.

inter-vlan: Specifies inter-VLAN forwarding entries.

ip-address: Specifies an IPv4 address. If you do not specify an IPv4 address, this command displays detailed information about all IPv4 fast bridge forwarding entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv4 fast bridge forwarding entries for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv4 fast bridge forwarding entries for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays detailed information about IPv4 fast bridge forwarding entries for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information about IPv4 fast bridge forwarding entries for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv4 fast bridge forwarding entries for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays detailed information about IPv4 fast bridge forwarding entries for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information about IPv4 fast bridge forwarding entries for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Layer 2 forwarding probe commands -- Fast bridge forwarding probe commands -- display system internal bridge cache ipv6 verbose

| NOTE: Support for this command depends on the device model.

Use display system internal bridge cache ipv6 verbose to display detailed information about IPv6 fast bridge forwarding entries.

Syntax

Centralized devices:

display system internal bridge cache ipv6 { inline | inter-vlan } [ ipv6-address ] verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal bridge cache ipv6 { inline | inter-vlan } [ ipv6-address ] verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal bridge cache ipv6 { inline | inter-vlan } [ ipv6-address ] verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

inline: Specifies inline forwarding entries.

inter-vlan: Specifies inter-VLAN forwarding entries.

ipv6-address: Specifies an IPv6 address. If you do not specify an IPv6 address, this command displays detailed information about all IPv6 fast bridge forwarding entries.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about IPv6 fast bridge forwarding entries for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about IPv6 fast bridge forwarding entries for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays detailed information about IPv6 fast bridge forwarding entries for all member devices if you do not specify a member device. On an IRF 3 system, this command displays detailed information about IPv6 fast bridge forwarding entries for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about IPv6 fast bridge forwarding entries for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays detailed information about IPv6 fast bridge forwarding entries for all cards if you do not specify a card. On an IRF 3 system, this command displays detailed information about IPv6 fast bridge forwarding entries for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.