IP address management probe commands -- display system internal ip address

Use display system internal ip address to display detailed IP address information.

Syntax

Centralized devices:

display system internal ip address [ vpn-instance vpn-instance-name ] [ ip-address | interface interface-type interface-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip address [ vpn-instance vpn-instance-name ] [ ip-address | interface interface-type interface-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip address [ vpn-instance vpn-instance-name ] [ ip-address | interface interface-type interface-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance to which an IP address belongs.

ip-address: Specifies an IP address.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed IP address information on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed IP address information on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed IP address information on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed IP address information on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed IP address information on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

If you do not specify any parameters, this command displays detailed information about all IPv4 addresses for the public network.