VXLAN probe commands -- Basic VXLAN probe commands -- debugging system internal overlay mac-address

Use debugging system internal overlay mac-address to enable MAC address debugging for the Overlay module.

Use undo debugging system internal overlay mac-address to disable MAC address debugging for the Overlay module.

Syntax

debugging system internal overlay mac-address { all | event | hardware | isis }

undo debugging system internal overlay mac-address { all | event | hardware | isis }

Default

Overlay MAC address debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of MAC address debugging.

event: Enables MAC event debugging.

hardware: Enables MAC hardware debugging.

isis: Enables MAC IS-IS debugging.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal multicast tunnel nexthop

Use display system internal multicast tunnel nexthop to display next hop entries for VXLAN multicast tunnels.

Syntax

Centralized devices:

display system internal multicast tunnel nexthop [ source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] | mtunnel tunnel-number | outgoing-interface interface-type interface-number ] *

Distributed devices in standalone mode:Centralized IRF devices:

display system internal multicast tunnel nexthop [ source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] | mtunnel tunnel-number | outgoing-interface interface-type interface-number | slot slot-number [ cpu cpu-number ] ] *

Distributed devices in IRF mode:

display system internal multicast tunnel nexthop [ source-address [ mask { mask-length | mask } ] | group-address [ mask { mask-length | mask } ] | mtunnel tunnel-number | outgoing-interface interface-type interface-number | chassis chassis-number slot slot-number [ cpu cpu-number ] ] *

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

source-address: Specifies an outgoing interface by its IP address.

group-address: Specifies a multicast group address in the range of 224.0.0.0 to 239.255.255.255.

mask-length: Specifies a subnet mask length. The value range for this argument is 4 to 32 for a multicast group address and 0 to 32 for an outgoing interface address. The default is 32.

mask: Specifies a subnet mask. The default is 255.255.255.255.

mtunnel tunnel-number: Specifies a VXLAN multicast tunnel by its number. The value range for the tunnel-number argument varies by device model.

outgoing-interface interface-type interface-number: Specifies an outgoing interface by its type and number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the next hop entries on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the next hop entries on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the next hop entries on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the next hop entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays the next hop entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal overlay arp suppression

Use display system internal overlay arp suppression to display ARP flood suppression information.

Syntax

Centralized devices:

display system internal overlay arp suppression vsi vsi-name

Distributed devices in standalone mode:Centralized IRF devices:

display system internal overlay arp suppression vsi vsi-name [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal overlay arp suppression vsi vsi-name [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays ARP flood suppression information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays ARP flood suppression information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays ARP flood suppression information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays ARP flood suppression information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays ARP flood suppression information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal overlay flooding

Use display system internal overlay flooding to display flooding information.

Syntax

Centralized devices:

display system internal overlay flooding vsi vsi-name

Distributed devices in standalone mode:Centralized IRF devices:

display system internal overlay flooding vsi vsi-name [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal overlay flooding vsi vsi-name [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays flooding information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays flooding information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays flooding information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays flooding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays flooding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal overlay mac-address

Use display system internal overlay mac-address to display remote-MAC address entries.

Syntax

Centralized devices:

display system internal overlay mac-address [ dynamic | evpn | isis-learned | openflow | ovsdb | static ] [ interface tunnel tunnel-number ] [ vsi vsi-name ] [ count ]

display system internal overlay mac-address mac-address [ vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal overlay mac-address [ dynamic | evpn | isis-learned | openflow | ovsdb | static ] [ vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ] [ count ]

display system internal overlay mac-address mac-address [ vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal overlay mac-address [ dynamic | evpn | isis-learned | openflow | ovsdb | static ] [ vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] [ count ]

display system internal overlay mac-address mac-address [ vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

dynamic: Specifies dynamic remote-MAC entries.

evpn: Specifies remote-MAC entries learned through EVPN.

isis-learned: Specifies remote-MAC entries advertised through VXLAN IS-IS.

openflow: Specifies remote-MAC entries set by OpenFlow.

ovsdb: Specifies remote-MAC entries set by OVSDB.

static: Specifies static remote-MAC entries.

interface tunnel tunnel-number: Specifies a VXLAN tunnel interface by its number. The value range for the tunnel-number argument varies by device model.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

count: Displays the number of matching remote-MAC entries. If you do not specify this keyword, the command displays detailed information about matching remote-MAC entries.

mac-address: Specifies a MAC address in H-H-H format. You can omit the consecutive 0s at the beginning of each segment. For example, you can enter f-e2-1 for 000f-00e2-0001.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays remote-MAC entries on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays remote-MAC entries on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays remote-MAC entries on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays remote-MAC entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays remote-MAC entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal overlay selective-flooding mac-address

Use display system internal overlay selective-flooding mac-address to display selective flood MAC entries.

Syntax

Centralized devices:

display system internal overlay selective-flooding mac-address [ mac-address ] [ vsi vsi-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal overlay selective-flooding mac-address [ mac-address ] [ vsi vsi-name ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal overlay selective-flooding mac-address [ mac-address ] [ vsi vsi-name ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

mac-address: Specifies a MAC address in H-H-H format. You can omit the consecutive 0s at the beginning of each segment. For example, you can enter f-e2-1 for 000f-00e2-0001.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays selective flood MAC entries on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays selective flood MAC entries on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays selective flood MAC entries on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays selective flood MAC entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays selective flood MAC entries on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal overlaymac statistics

Use display system internal overlaymac statistics to display MAC statistics for the Overlay module.

Syntax

Centralized devices:

display system internal overlaymac statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal overlaymac statistics [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal overlaymac statistics [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays Overlay MAC statistics for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays Overlay MAC statistics for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays Overlay MAC statistics for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays Overlay MAC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays Overlay MAC statistics for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal vxlan forwarding tunnel

Use display system internal vxlan forwarding tunnel to display VXLAN tunnel forwarding information.

Syntax

Centralized devices:

display system internal vxlan forwarding tunnel [ vxlan-id vxlan-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal vxlan forwarding tunnel [ vxlan-id vxlan-id ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal vxlan forwarding tunnel [ vxlan-id vxlan-id ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vxlan-id vxlan-id: Specifies a VXLAN by its ID in the range of 0 to 16777215. If you do not specify a VXLAN, this command displays tunnel forwarding information for all VXLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays VXLAN tunnel forwarding information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays VXLAN tunnel forwarding information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays VXLAN tunnel forwarding information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays VXLAN tunnel forwarding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays VXLAN tunnel forwarding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VXLAN probe commands -- Basic VXLAN probe commands -- display system internal vxlan isis status

Use display system internal vxlan isis status to display the status of the VXLAN IS-IS process.

Syntax

display system internal vxlan isis status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

VXLAN probe commands -- Basic VXLAN probe commands -- reset system internal overlaymac statistics

Use reset system internal overlaymac statistics to clear MAC statistics for the Overlay module.

Syntax

reset system internal overlaymac statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

VXLAN probe commands -- OVSDB VTEP probe commands -- display system internal ovsdb server dump

Use display system internal ovsdb server dump to display the OVSDB database.

Syntax

display system internal ovsdb server dump

Views

Probe view

Predefined user roles

network-admin

mdc-admin

VXLAN probe commands -- OVSDB VTEP probe commands -- vtep-ctl

Use vtep-ctl to configure and display the OVSDB database.

Syntax

vtep-ctl options

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

options: Specifies options. The options are the same as the options of the vtep-ctl command at the Linux Bash CLI. To view available options, execute vtep-ctl –help.