EVI probe commands -- display system internal evi flooding

Use display system internal evi flooding to display EVI flooding information.

Syntax

Centralized devices:

display system internal evi flooding interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi flooding interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal evi flooding interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.

EVI probe commands -- display system internal evi selective-flooding

Use display system internal evi selective-flooding to display driver information for a MAC address that is enabled with selective flood in a VLAN on an EVI tunnel interface.

Syntax

Centralized devices:

display system internal evi selective-flooding interface tunnel interface-number mac-address mac-address vlan vlan-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi selective-flooding interface tunnel interface-number mac-address mac-address vlan vlan-id slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal evi selective-flooding interface tunnel interface-number mac-address mac-address vlan vlan-id chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface tunnel interface-number: Specifies an EVI tunnel interface by its number.

mac-address mac-address: Specifies a selective-flood-enabled MAC address.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.

EVI probe commands -- display system internal evi statistics

Use display system internal evi statistics to display EVI statistics.

Syntax

Centralized devices:

display system internal evi statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal evi statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.

EVI probe commands -- display system internal evi vlan-mapping

Use display system internal evi vlan-mapping to display remote VLAN mapping information for a local VLAN.

Syntax

Centralized devices:

display system internal evi vlan-mapping vlan vlan-id interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi vlan-mapping vlan vlan-id interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal evi vlan-mapping vlan vlan-id interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a local VLAN by its ID in the range of 1 to 4094.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.

EVI probe commands -- display system internal evi vlan-status

Use display system internal evi vlan-status to display driver information for a VLAN on an EVI tunnel interface.

Syntax

Centralized devices:

display system internal evi vlan-status interface tunnel interface-number vlan vlan-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi vlan-status interface tunnel interface-number vlan vlan-id slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal evi vlan-status interface tunnel interface-number vlan vlan-id chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface tunnel interface-number: Specifies an EVI tunnel interface by its number.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.

EVI probe commands -- display system internal eviisis status

Use display system internal eviisis status to display EVI IS-IS process state information.

Syntax

display system internal eviisis status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

EVI probe commands -- display system internal evi-link data

Use display system internal evi-link data to display kernel data for an EVI-Link interface.

Syntax

Centralized devices:

display system internal evi-link data interface evi-link number [ cpu cpu-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evi-link data interface evi-link number [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal evi-link data interface evi-link number [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface evi-link number: Specifies an existing EVI-Link interface by its interface number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays kernel data for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays kernel data for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays kernel data for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option varies by device model.