EVB probe commands -- display system internal evb global-info

Use display system internal evb global-info to display information about multiple EVB threads.

Syntax

display system internal evb global-info

Views

Probe view

Predefined user roles

network-admin

mdc-admin

EVB probe commands -- display system internal evb kernel

Use display system internal evb kernel to display EVB kernel information.

Syntax

Centralized devices:

display system internal evb kernel interface s-channel { interface-number:channel-id | interface-number:channel-id.vsi-

local-id } [ section section-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal evb kernel slot slot-number interface s-channel { interface-number:channel-id | interface-number:channel-id.vsi-

local-id } [ section section-number ]

Distributed devices in IRF mode:

display system internal evb kernel chassis chassis-number slot slot-number interface s-channel { interface-number:channel-id | interface-number:channel-id.vsi-local-id } [ section section-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the IRF member device by its ID. The slot-number argument specifies the slot where the card resides. (Distributed devices in IRF mode.)

interface s-channel { interface-number:channel-id | interface-number:channel-id.vsi-local-id }: Specifies an S-channel interface or a VSI. The interface-number argument specifies the physical port where the S-channel resides. The channel-id argument specifies the ID of the S-channel. This S-channel ID must exist. The vsi-local-id argument specifies the local ID of the VSI. This VSI local ID must exist.

section section-number: Displays filtering information for the specified section on the VSI interface (each section contains 60 filtering records). The section-number argument specifies the section number in the range of 1 to 65535. If you do not specify this argument, the command only displays the filtering information for the first section.