Process monitoring and maintenance probe commands -- process

Use process to start, stop, or restart a process.

Syntax

Centralized devices:

process { restart | shutdown | start } { job job-id | name process-name }

Distributed devices in standalone mode:Centralized IRF devices:

process { restart | shutdown | start } { job job-id [ slot slot-number [ cpu cpu-number ] ] | name process-name [ all | slot slot-number [ cpu cpu-number ] ] }

Distributed devices in IRF mode:

process { restart | shutdown | start } { job job-id [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | name process-name [ all | chassis chassis-number slot slot-number [ cpu cpu-number ] ] }

Default

The start and restart of a process are controlled by the device as needed.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

restart: Restarts a process.

shutdown: Stops a process. A stopped process does not restart automatically.

start: Starts a process.

job job-id: Specifies a job by its ID in the range of 1 to 2147483647. A job ID uniquely identifies a process.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command applies to the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command applies to the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command applies to the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command applies to the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command applies to the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number.

name process-name: Specifies a process by its name, a case-sensitive string of 1 to 31 characters. The process name cannot contain question marks (?) or spaces.

all: Specifies all processes.