Preprovisioning commands -- chassis slot

Use chassis slot to select a slot to provision and enter slot view.

Syntax

chassis chassis-number slot slot-number

Views

System view

Predefined user roles

network-admin

Parameters

chassis chassis-number slot slot-number: Specifies an interface card slot on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the interface card to be preprovisioned. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies an interface card slot on an IRF member device or specifies a PEX slot. The chassis-number argument represents the member ID of the IRF member device or the virtual PEX chassis number. The slot-number argument represents the slot number for the interface card or PEX to be preprovisioned. (Distributed devices in IRF mode.) (IRF 3 capable.)

Examples

# Enter the slot view of slot 1 in chassis 1.

<Sysname> system-view

[Sysname] chassis 1 slot 1

[Sysname-chassis-1-slot-1]

Related commands

provision

Preprovisioning commands -- display provision failed-config

Use display provision failed-config to display preprovisioned-commands application failure records.

Syntax

display provision failed-config

Views

Any view

Predefined user roles

network-admin

network-operator

Usage guidelines

A preprovisioned command cannot be applied if it conflicts with the running configuration.

Use this command to verify the application result of preprovisioned commands except for the following commands:

· duplex

· location

· oc-3

· speed

· sflow

· threshold

· using oc-3c

To verify the application result of the listed commands, use the display current-configuration command. The display provision failed-config command might display incorrect application results for the listed commands.

Examples

# Display preprovisioned-commands application failure records.

<Sysname> display provision failed-config

Configuration applied at: Sat Jun 14 06:06:00 2014

Slot information: slot 1

Commands that failed to be applied:

#

interface FortyGigE1/1/0/1

speed 40000

#

Related commands

provision

reset provision failed-config

Preprovisioning commands -- provision

Use provision to enable preprovisioning.

Use undo provision to disable preprovisioning.

Syntax

provision [ subslot subslot-number ] model model

undo provision [ subslot subslot-number ] model

Default

Preprovisioning is disabled.

Views

Slot view

Predefined user roles

network-admin

Parameters

subslot subslot-number: Specifies a subslot by its subslot number. If you do not specify a subslot, preprovisioning is enabled on the slot. To specify a subslot, you must first enable provisioning on the slot and make sure the provisioned slot has subslots.

model model: Specifies the card, IRF member device, PEX, or subcard model to be preprovisioned. To obtain available models, enter a question mark (?) for the model argument.

Usage guidelines

This command allows you to enable preprovisioning on offline modules, including interface cards, subcards, IRF member devices, and PEXs.

The device automatically creates interfaces when preprovisioning is enabled for a module. The display interface command will not display these interfaces until the module comes online.

When you disable preprovisioning on a slot, the device removes all preconfigured settings for the slot, including the preconfigured settings for the subslots.

When you disable preprovisioning on a subslot, the device removes preconfigured settings for the subslot.

Examples

# Enable preprovisioning for the SIM3110 module on a slot.

<Sysname> system-view

[Sysname] slot 2

[Sysname-slot-2] provision model SIM3110

Related commands

chassis slot

display provision failed-config

reset provision failed-config

slot

Preprovisioning commands -- reset provision failed-config

Use reset provision failed-config to clear preprovisioned-commands application failure records.

Syntax

reset provision failed-config

Views

User view

Predefined user roles

network-admin

Usage guidelines

Preprovisioned modules that repeatedly come online and go offline (or join and leave the IRF fabric) might leave a number of commands that were not applied in memory. To release the occupied memory space, execute the reset provision failed-config command.

Examples

# Clear preprovisioned-commands application failure records.

<Sysname> reset provision failed-config

Related commands

display provision failed-config

provision

Preprovisioning commands -- slot

Use slot to select a slot to provision and enter slot view.

Syntax

slot slot-number

Views

System view

Predefined user roles

network-admin

Parameters

slot-number: Specifies a slot number. (Centralized devices.)

slot-number: Specifies a slot number. (Distributed devices in standalone mode.) (Distributed devices in IRF mode.)

slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

Examples

# Enter the view of a slot.

<Sysname> system-view

[Sysname] slot 2

[Sysname-slot-2]

Related commands

provision