MVRP probe commands -- display system internal mvrp interface

Use display system internal mvrp interface to display MVRP operation information of an interface in a VLAN.

Syntax

display system internal mvrp interface interface-type interface-number vlan vlan-id

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

MVRP probe commands -- display system internal mvrp map-count

Use display system internal mvrp map-count to display the propagation count of a VLAN.

Syntax

display system internal mvrp map-count vlan vlan-id

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its ID in the range of 1 to 4094.

Usage guidelines

This command displays the total number of interfaces in STP forwarding state that have registered the specified VLAN through MVRP.