MPLS protection switching probe commands -- debugging system internal mpls forwarding protection

Use debugging system internal mpls forwarding protection to enable debugging for MPLS forwarding plane protection switching.

Use undo debugging system internal mpls forwarding protection to disable debugging for MPLS forwarding plane protection switching.

Syntax

Centralized devices:

debugging system internal mpls forwarding protection { all | error | process }

undo debugging system internal mpls forwarding protection { all | error | process }

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal mpls forwarding protection { all | error | process } slot slot-number [ cpu cpu-number ]

undo debugging system internal mpls forwarding protection { all | error | process } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal mpls forwarding protection { all | error | process } chassis chassis-number slot slot-number [ cpu cpu-number ]

undo debugging system internal mpls forwarding protection { all | error | process } chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

Debugging for MPLS forwarding plane protection switching is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for MPLS forwarding plane protection switching.

error: Enables error debugging for MPLS forwarding plane protection switching.

process: Enables process debugging for MPLS forwarding plane protection switching.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

MPLS protection switching probe commands -- display system internal mpls protection statistics

Use debugging system internal mpls protection statistics to display MPLS protection switching statistics, including the following information:

· Information received by MPLS protection switching.

· PSC information.

· Error processing information.

Syntax

Centralized devices:

display system internal mpls protection statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal mpls protection statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal mpls protection statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.