Interface management probe commands -- display system internal ifmgr brief

Use display system internal ifmgr brief to display brief information about an interface.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr brief { para slot slot-number [ cpu cpu-number ] | help }

Distributed devices in IRF mode:

display system internal ifmgr brief { para chassis chassis-number slot slot-number [ cpu cpu-number ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an interface index.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr down

Use display system internal ifmgr down to display the down types that have been registered.

Syntax

Centralized devices:

display system internal ifmgr down

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr down [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ifmgr down [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the registered down types for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the registered down types for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the registered down types for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the registered down types for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays the registered down types for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Interface management probe commands -- display system internal ifmgr entry

Use display system internal ifmgr entry to display data structure information for an interface.

Syntax

Centralized devices:

display system internal ifmgr entry { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr entry { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr entry { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an interface name or index in the format of 1*Interface index or 2*Interface name.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays data structure information for interfaces on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays data structure information for interfaces on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays data structure information for interfaces on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays data structure information for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays data structure information for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr event

Use display system internal ifmgr event to display register information for an interface event.

Syntax

Centralized devices:

display system internal ifmgr event { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr event { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr event { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an event type or interface type. If you specify both an event type and an interface type, connect them by using an asterisk (*) in the form of event*type.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays interface event register information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays interface event register information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays interface event register information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays interface event register information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays interface event register information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr hotplug

Use display system internal ifmgr hotplug to display hotplug information for a card or subcard.

Syntax

Centralized devices:

display system internal ifmgr hotplug [ para | help ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr hotplug [ [ para ] [ slot slot-number [ cpu cpu-number ] ] | help ]

Distributed devices in IRF mode:

display system internal ifmgr hotplug [ [ para ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies a slot number or both a slot number and subslot number in the form of slot-number*subslot-number. If you do not specify this argument and the help keyword, the command displays hotplug information for all cards.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays card or subcard hotplug information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays card or subcard hotplug information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays card or subcard hotplug information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays card or subcard hotplug information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays card or subcard hotplug information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr index

Use display system internal ifmgr index to display interface index information.

Syntax

Centralized devices:

display system internal ifmgr index { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr index { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr index { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an interface index in decimal format.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays interface index information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays interface index information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays interface index information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays interface index information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays interface index information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr list

Use display system internal ifmgr list to display a tree structure for interfaces. The tree structure displays interfaces and subinterfaces as tree nodes, and displays the name and index of each node.

Syntax

Centralized devices:

display system internal ifmgr list [ para | help ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr list [ [ para ] [ slot slot-number [ cpu cpu-number ] ] | help ]

Distributed devices in IRF mode:

display system internal ifmgr list [ [ para ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an interface type. To view valid interface type values, specify the help keyword. If you do not specify this argument and the help keyword, the command displays a tree structure for all interface types.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays a tree structure of interfaces for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays a tree structure of interfaces for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays a tree structure of interfaces for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays a tree structure of interfaces for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays a tree structure of interfaces for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr mdc

Use display system internal ifmgr mdc to display information about the interfaces assigned to MDCs.

Syntax

Centralized devices:

display system internal ifmgr mdc { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr mdc { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr mdc { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies a parameter for the command. Valid formats for this argument include:

· 1*ID of the group to which the interface belongs.

· 2*Interface name.

· 3*MDC ID.

· 4*Slot number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays the interfaces assigned to MDCs for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays the interfaces assigned to MDCs for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays the interfaces assigned to MDCs for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays the interfaces assigned to MDCs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays the interfaces assigned to MDCs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr name

Use display system internal ifmgr name to display a tree structure for parsing an interface name and obtaining help information. Tree structures include information such as interface indexes, interface numbers, and help information.

Syntax

Centralized devices:

display system internal ifmgr name { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr name { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr name { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies the full name or abbreviated name of an interface.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays tree structures for interfaces on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays tree structures for interfaces on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays tree structures for interfaces on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays tree structures for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays tree structures for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.

Interface management probe commands -- display system internal ifmgr type

Use display system internal ifmgr type to display interface type information.

Syntax

Centralized devices:

display system internal ifmgr type { para | help }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ifmgr type { para [ slot slot-number [ cpu cpu-number ] ] | help }

Distributed devices in IRF mode:

display system internal ifmgr type { para [ chassis chassis-number slot slot-number [ cpu cpu-number ] ] | help }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

para: Specifies an interface type, a string of 1 to 127 characters.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays interface type information for interfaces on the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays interface type information for interfaces on the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF 2 member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays interface type information for interfaces on the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays interface type information for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF 2 member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF 2 member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. The slot number is fixed at 0 for the PEX. If you do not specify a card or PEX, this command displays interface type information for interfaces on the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

help: Displays help information for valid parameters that you can specify.