PPP probe commands -- display system internal ppp statistics

Use display system internal ppp statistics to display PPP statistics.

Syntax

Centralized devices:

display system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

aaa-event: Specifies PPP AAA events.

aggregation: Specifies PPP users that log in through aggregate interfaces.

all: Specifies all PPP statistics.

cp-event: Specifies PPP control protocol events.

external-event: Specifies PPP external events.

interface-event: Specifies PPP interface events.

offline-reason: Specifies PPP offline reasons.

vsrp [ vsrp-instance vsrp-instance-name ]: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSRP instance, this command displays PPP statistics for all VSRP instances. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays PPP statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. If you do not specify a member device, this command displays PPP statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays PPP statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays PPP statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays PPP statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays PPP statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays PPP statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

You can use this command on both the master and the backup devices for VSRP networks.

PPP probe commands -- display system internal pppoe-server statistics

Use display system internal pppoe-server statistics to display PPPoE server statistics.

Syntax

Centralized devices:

display system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

aggregation: Specifies PPPoE users that log in through aggregate interfaces.

all: Specifies all PPPoE server statistics. Support for this keyword depends on the device model.

vsrp [ vsrp-instance vsrp-instance-name ]: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSRP instance, this command displays PPPoE server statistics for all VSRP instances. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays PPPoE server statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. If you do not specify a member device, this command displays PPPoE server statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command displays PPPoE server statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command displays PPPoE server statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays PPPoE server statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command displays PPPoE server statistics for all cards if you do not specify a card. On an IRF 3 system, this command displays PPPoE server statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

You can use this command on both the master and the backup devices.

PPP probe commands -- reset system internal ppp statistics

Use reset system internal ppp statistics to clear PPP statistics.

Syntax

Centralized devices:

reset system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] }

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal ppp statistics { aaa-event | aggregation | all | cp-event | external-event | interface-event | offline-reason | vsrp [ vsrp-instance vsrp-instance-name ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

aaa-event: Specifies PPP AAA events.

aggregation: Specifies PPP users that log in through aggregate interfaces.

all: Specifies all PPP statistics.

cp-event: Specifies PPP control protocol events.

external-event: Specifies PPP external events.

interface-event: Specifies PPP interface events.

offline-reason: Specifies PPP offline reasons.

vsrp [ vsrp-instance vsrp-instance-name ]: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSRP instance, this command clears PPP statistics for all VSRP instances. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears PPP statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. If you do not specify a member device, this command clears PPP statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command clears PPP statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command clears PPP statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears PPP statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command clears PPP statistics for all cards if you do not specify a card. On an IRF 3 system, this command clears PPP statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

You can use this command on both the master and backup devices for VSRP networks.

PPP probe commands -- reset system internal pppoe-server statistics

Use reset system internal pppoe-server statistics to clear PPPoE server statistics.

Syntax

Centralized devices:

reset system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] }

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] } [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

reset system internal pppoe-server statistics { aggregation | all | vsrp [ vsrp-instance vsrp-instance-name ] } [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

aggregation: Specifies PPPoE users that log in through aggregate interfaces.

all: Specifies all PPPoE server statistics. Support for this keyword depends on the device model.

vsrp [ vsrp-instance vsrp-instance-name ]: Specifies a VSRP instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VSRP instance, this command clears PPPoE server statistics for all VSRP instances. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command clears PPPoE server statistics for all cards. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its ID. If you do not specify a member device, this command clears PPPoE server statistics for all member devices. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. On an IRF fabric, this command clears PPPoE server statistics for all member devices if you do not specify a member device. On an IRF 3 system, this command clears PPPoE server statistics for all IRF member devices and PEXs if you do not specify an IRF member device or PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command clears PPPoE server statistics for all cards. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. On an IRF fabric, this command clears PPPoE server statistics for all cards if you do not specify a card. On an IRF 3 system, this command clears PPPoE server statistics for all cards and PEXs if you do not specify a card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Usage guidelines

You can use this command on both the master and the backup devices.