ARP probe commands -- debugging system internal arp event

Use debugging system internal arp event to enable ARP event debugging.

Use undo debugging system internal arp event to disable ARP event debugging.

Syntax

debugging system internal arp event

undo debugging system internal arp event

Default

ARP event debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

ARP probe commands -- debugging system internal arp features

Use debugging system internal arp features to enable ARP features debugging.

Use undo debugging system internal arp features to disable ARP features debugging.

Syntax

debugging system internal arp features { notify | packet }

undo debugging system internal arp features { notify | packet }

Default

ARP features debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

notify: Enables notification debugging for ARP features.

packet: Enables packet debugging for ARP features.

ARP probe commands -- debugging system internal arp mac-forced-forwarding

Use debugging system internal arp mac-forced-forwarding to enable MAC-forced forwarding (MFF) debugging.

Use undo debugging system internal arp mac-forced-forwarding to disable MFF debugging.

Syntax

debugging system internal arp mac-forced-forwarding { event | notify | hardware }

undo debugging system internal arp mac-forced-forwarding { event | notify | hardware }

Default

MFF debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

event: Enables MFF event debugging.

notify: Enables MFF notification debugging.

hardware: Enables MFF hardware debugging.

ARP probe commands -- debugging system internal arp notify

Use debugging system internal arp notify to enable ARP notification debugging.

Use undo debugging system internal arp notify to disable ARP notification debugging.

Syntax

debugging system internal arp notify

undo debugging system internal arp notify

Default

ARP notification debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

ARP probe commands -- debugging system internal arp sync

Use debugging system internal arp sync to enable ARP synchronization debugging.

Use undo debugging system internal arp sync to disable ARP synchronization debugging.

Syntax

debugging system internal arp sync

undo debugging system internal arp sync

Default

ARP synchronization debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

ARP probe commands -- display system internal arp

Use display system internal arp to display ARP entries that are not synchronized from other cards or devices.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp { all | static | dynamic | multiport } slot slot-number [ cpu cpu-number ] [ count ]

Distributed devices in IRF mode:

display system internal arp { all | static | dynamic | multiport } chassis chassis-number slot slot-number [ cpu cpu-number ] [ count ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Displays all ARP entries that are not synchronized from other cards or devices.

static: Displays static ARP entries that are not synchronized from other cards or devices.

dynamic: Displays dynamic ARP entries that are not synchronized from other cards or devices.

multiport: Displays multiport ARP entries that are not synchronized from other cards or devices.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

count: Displays the total number of ARP entries that are not synchronized from other cards or devices.

ARP probe commands -- display system internal arp ifcb

Use display system internal arp ifcb to display ARP control block information for a Layer 2 or Layer 3 interface.

Syntax

Centralized devices:

display system internal arp ifcb interface interface-type interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp ifcb interface interface-type interface-number slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp ifcb interface interface-type interface-number chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp ip-address

Use display system internal arp ip-address to display the ARP entry for a specific IP address.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp ip-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp ip-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip-address: Displays the ARP entry for the specified IP address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp mac-forced-forwarding

Use display system internal arp mac-forced-forwarding to display MFF configuration.

Syntax

Centralized devices:

display system internal arp mac-forced-forwarding vlan vlan-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp mac-forced-forwarding vlan vlan-id slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp mac-forced-forwarding vlan vlan-id chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Displays MFF configuration for the specified VLAN.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp machash

Use display system internal arp machash to display machash entries.

Syntax

Centralized devices:

display system internal arp machash { vlan vlan-id | vsi vsi-name } ip ip-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp machash { vlan vlan-id | vsi vsi-name } ip ip-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp machash { vlan vlan-id | vsi vsi-name } ip ip-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its ID.

vsi vsi-name: Specifies a VSI by its name, a case-sensitive string of 1 to 31 characters.

ip ip-address: Specifies an IP address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp probe

Use display system internal arp probe to display ARP probe link entries.

Syntax

Centralized devices:

display system internal arp probe

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp probe slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp probe chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp rbhash

Use display system internal arp rbhash to display rbhash entries.

Syntax

Centralized devices:

display system internal arp rbhash vlan vlan-id ip ip-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp rbhash vlan vlan-id ip ip-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp rbhash vlan vlan-id ip ip-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Displays ARP rbhash entries for the specified VLAN.

ip ip-address: Displays ARP rbhash entries for the specified IP address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp reload

Use display system internal arp reload to display ARP reload link entries.

Syntax

Centralized devices:

display system internal arp reload

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp reload slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp reload chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp rule

Use display system internal arp rule to display ARP rules.

Syntax

Centralized devices:

display system internal arp rule { all | interface interface-type interface-number [ ip-address ] }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp rule { all | interface interface-type interface-number [ ip-address ] } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp rule { all | interface interface-type interface-number [ ip-address ] } chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Displays all ARP rules.

interface interface-type interface-number: Specifies an interface by its type and number.

ip ip-address: Displays the ARP rule for the specified IP address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp snooping

Use display system internal arp snooping to display ARP snooping entries.

Syntax

Centralized devices:

display system internal arp snooping [ vlan vlan-id ] [ count ]

display system internal arp snooping ip ip-address

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp snooping [ vlan vlan-id ] slot slot-number [ cpu cpu-number ] [ count ]

display system internal arp snooping ip ip-address slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp snooping [ vlan vlan-id ] chassis chassis-number slot slot-number [ cpu cpu-number ] [ count ]

display system internal arp snooping ip ip-address chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Specifies a VLAN by its ID. The value range is 1 to 4094.

count: Displays the total number of ARP snooping entries.

ip ip-address: Specifies an IP address.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp source-suppression cache

Use display system internal arp source-suppression cache to display ARP source suppression entries.

Syntax

Centralized devices:

display system internal arp source-suppression cache

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp source-suppression cache slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp source-suppression cache chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp statistics

Use display system internal arp statistics to display ARP statistics.

Syntax

Centralized devices:

display system internal arp statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal arp statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp suppression xconnect-group verbose

| NOTE: Support for this command depends on the device model.

Use display system internal arp suppression xconnect-group verbose to display detailed information about ARP suppression entries.

Syntax

Centralized devices:

display system internal arp suppression xconnect-group verbose

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp suppression xconnect-group verbose [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal arp suppression xconnect-group verbose [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays detailed information about ARP suppression entries for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays detailed information about ARP suppression entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays detailed information about ARP suppression entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays detailed information about ARP suppression entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays detailed information about ARP suppression entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

ARP probe commands -- display system internal arp vlan

Use display system internal arp vlan to display ARP entries for a specific VLAN.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal arp vlan vlan-id slot slot-number [ cpu cpu-number ] [ count ]

Distributed devices in IRF mode:

display system internal arp vlan vlan-id chassis chassis-number slot slot-number [ cpu cpu-number ] [ count ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan vlan-id: Displays ARP entries for the specified VLAN.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

count: Displays the total number of ARP entries.

ARP probe commands -- reset system internal arp statistics

Use reset system internal arp statistics to clear ARP statistics.

Syntax

Centralized devices:

reset system internal arp statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal arp statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal arp statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.