NVGRE probe commands -- display system internal nvgre forwarding tunnel

Use display system internal nvgre forwarding tunnel to display NVGRE tunnel forwarding information.

Syntax

Centralized devices:

display system internal nvgre forwarding tunnel [ vsid vsid ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal nvgre forwarding tunnel [ vsid vsid ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal nvgre forwarding tunnel [ vsid vsid ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsid vsid: Specifies an NVGRE network by its VSID in the range of 4096 to 16777214. If you do not specify an NVGRE network, this command displays NVGRE tunnel forwarding information for all NVGRE networks.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays NVGRE tunnel forwarding information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays NVGRE tunnel forwarding information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays NVGRE tunnel forwarding information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays NVGRE tunnel forwarding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays NVGRE tunnel forwarding information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.