IPv6 multicast VLAN commands -- display ipv6 multicast-vlan

Use display ipv6 multicast-vlan to display information about IPv6 multicast VLANs.

Syntax

display ipv6 multicast-vlan [ vlan-id ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

vlan-id: Specifies an IPv6 multicast VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify an IPv6 multicast VLAN, this command displays information about all IPv6 multicast VLANs.

Examples

# Display information about all IPv6 multicast VLANs.

<Sysname> display ipv6 multicast-vlan

Total 2 IPv6 multicast VLANs.

IPv6 multicast VLAN 100:

Sub-VLAN list(3 in total):

2-3, 6

Port list(3 in total):

GE1/0/1

GE1/0/2

GE1/0/3

IPv6 multicast VLAN 200:

Sub-VLAN list(0 in total):

Port list(0 in total):

Table 1 Command output

Field | Description
Total 2 IPv6 multicast VLANs | Total number of IPv6 multicast VLANs.
Sub-VLAN list(3 in total) | Sub-VLAN list of the IPv6 multicast VLAN, and the total number of the sub-VLANs.
Port list(3 in total) | Port list of the IPv6 multicast VLAN, and the total number of the ports.

IPv6 multicast VLAN commands -- display ipv6 multicast-vlan forwarding-table

Use display ipv6 multicast-vlan forwarding-table to display IPv6 multicast VLAN forwarding entries.

Syntax

Centralized devices:

display ipv6 multicast-vlan forwarding-table [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 multicast-vlan forwarding-table [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Distributed devices in IRF mode:

display ipv6 multicast-vlan forwarding-table [ ipv6-source-address [ prefix-length ] | ipv6-group-address [ prefix-length ] | chassis chassis-number slot slot-number [ cpu cpu-number ] | subvlan vlan-id | vlan vlan-id ] *

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays IPv6 multicast VLAN forwarding entries for all IPv6 multicast sources.

prefix-length: Specifies a prefix length of the IPv6 multicast source address. The value range is 0 to 128 and the default value is 128.

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16, where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command displays IPv6 multicast VLAN forwarding entries for all IPv6 multicast groups.

prefix-length: Specifies a prefix length of the IPv6 multicast group address. The value range is 8 to 128 and the default value is 128.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6 multicast VLAN forwarding entries for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6 multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPv6 multicast VLAN forwarding entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6 multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPv6 multicast VLAN forwarding entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

subvlan vlan-id: Specifies a sub-VLAN by its VLAN ID. If you do not specify a sub-VLAN, this command displays IPv6 multicast VLAN forwarding entries for all sub-VLANs.

vlan vlan-id: Specifies an IPv6 multicast VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify an IPv6 multicast VLAN, this command displays IPv6 multicast VLAN forwarding entries for all VLANs.

Examples

# Display all IPv6 multicast VLAN forwarding entries.

<Sysname> display ipv6 multicast-vlan forwarding-table

IPv6 multicast VLAN 100 Forwarding Table

Total 1 entries, 1 matched

00001. (1::1, FF0E::1)

Flags: 0x10000

IPv6 multicast VLAN: 100

List of sub-VLANs (3 in total):

1: VLAN 10

2: VLAN 20

3: VLAN 30

Table 2 Command output

Field | Description
IPv6 multicast VLAN 100 Forwarding Table | The multicast forwarding table for IPv6 multicast VLAN 100.
Total 1 entries, 1 matched | Total number of (S, G) entries, and the number of matching entries.
00001 | Sequence number of the (S, G) entry.
(1::1, FF0E::1) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Flags | Entry flag. This field displays one flag or the sum of multiple flags. In this example, the value 0x10000 means that the entry has only one flag 0x10000. The following flags are available for an entry: · 0x1—The entry is in inactive state. · 0x4—The entry fails to update. · 0x8—The sub-VLAN information fails to update for the entry. · 0x200—The entry is in GR state. · 0x10000—The entry is an IPv6 multicast VLAN forwarding entry.
List of sub-VLANs (3 in total) | Sub-VLAN list of the IPv6 multicast VLAN, and the total number of the sub-VLANs.

IPv6 multicast VLAN commands -- display ipv6 multicast-vlan group

Use display ipv6 multicast-vlan group to display information about IPv6 multicast groups in IPv6 multicast VLANs.

Syntax

Centralized devices:

display ipv6 multicast-vlan group [ ipv6-source-address | ipv6-group-address | verbose | vlan vlan-id ] *

Distributed devices in standalone mode:Centralized IRF devices:

display ipv6 multicast-vlan group [ ipv6-source-address | ipv6-group-address | slot slot-number [ cpu cpu-number ] | verbose | vlan vlan-id ] *

Distributed devices in IRF mode:

display ipv6 multicast-vlan group [ ipv6-source-address | ipv6-group-address | chassis chassis-number slot slot-number [ cpu cpu-number ] | verbose | vlan vlan-id ] *

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command displays information about IPv6 multicast groups for all IPv6 multicast sources in IPv6 multicast VLANs.

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command displays information about all IPv6 multicast groups in IPv6 multicast VLANs.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about IPv6 multicast groups in IPv6 multicast VLANs for the MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about IPv6 multicast groups in IPv6 multicast VLANs for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about IPv6 multicast groups in IPv6 multicast VLANs for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about IPv6 multicast groups in IPv6 multicast VLANs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about IPv6 multicast groups in IPv6 multicast VLANs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

verbose: Displays detailed information. If you do not specify the keyword, this command displays brief information.

vlan vlan-id: Specifies an IPv6 multicast VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify an IPv6 multicast VLAN, this command displays information about IPv6 multicast groups for all IPv6 multicast VLANs.

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot.

Examples

# Display detailed information about all IPv6 multicast groups in IPv6 multicast VLANs.

<Sysname> display ipv6 multicast-vlan group verbose

Total 6 entries.

IPv6 multicast VLAN 10: Total 3 entries.

(2::2, FF0E::2)

Flags: 0x70000020

Sub-VLANs (1 in total):

VLAN 40

(22::22, FF0E::4)

Flags: 0x70000030

Sub-VLANs (1 in total):

VLAN 40

(::, FF0E::10)

Flags: 0x10000030

Sub-VLANs (1 in total):

VLAN 40

IPv6 multicast VLAN 20: Total 3 entries.

(2::2, FF0E::2)

Flags: 0x70000010

Sub-VLANs (0 in total):

(22::22, FF0E::4)

Flags: 0x70000010

Sub-VLANs (0 in total):

(::, FF0E::10)

Flags: 0x50000010

Sub-VLANs (0 in total):

Table 3 Command output

Field | Description
Total 6 entries | Total number of (S, G) entries.
IPv6 multicast VLAN 10: Total 3 entries | Total number of (S, G) entries in IPv6 multicast VLAN 10.
(::, FF0E::10) | (S, G) entry, where a double colon (::) in the S position means all IPv6 multicast sources.
Flags | Entry flag. This field displays one flag or the sum of multiple flags. For example, the value 0x70000020 means that the entry has flags 0x20, 0x10000000, 0x20000000, and 0x40000000. The following flags are available for an entry: · 0x10—The entry is created by the IPv6 multicast VLAN. · 0x20—The entry is created by the sub-VLAN of the IPv6 multicast VLAN. · 0x40—The entry is to be deleted. · 0x10000000—This value represents one of the following situations: ?span style='font:7.0pt "Times New Roman"'> The entry is newly created. ?span style='font:7.0pt "Times New Roman"'> The device receives an MLD query within an MLD general query interval. · 0x20000000—The device does not receive MLDv1 or MLDv2 reports that match the entry within an MLD general query interval. · 0x40000000—The device does not receive MLDv2 IS_EX (NULL) reports that match the entry within an MLD general query interval.
Sub-VLANs (1 in total) | Sub-VLAN list of the IPv6 multicast VLAN, and the total number of the sub-VLANs.

Related commands

reset ipv6 multicast-vlan group

IPv6 multicast VLAN commands -- ipv6 multicast-vlan

Use ipv6 multicast-vlan to configure an IPv6 multicast VLAN and enter its view, or enter the view of an existing IPv6 multicast VLAN.

Use undo ipv6 multicast-vlan to remove the configuration of IPv6 multicast VLANs.

Syntax

ipv6 multicast-vlan vlan-id

undo ipv6 multicast-vlan { all | vlan-id }

Default

No IPv6 multicast VLANs exist.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan-id: Specifies an existing VLAN ID in the range of 1 to 4094.

all: Specifies all IPv6 multicast VLANs.

Usage guidelines

The total number of IPv6 multicast VLANs on a device cannot exceed the system upper limit, which varies by the device model.

You must enable MLD snooping for the VLAN to be configured as an IPv6 multicast VLAN.

As a best practice, do not configure an IPv6 multicast VLAN on a device that is enabled with IPv6 multicast routing.

Examples

# Enable MLD snooping for VLAN 100. Configure VLAN 100 as an IPv6 multicast VLAN and enter its view.

<Sysname> system-view

[Sysname] mld-snooping

[Sysname-mld-snooping] quit

[Sysname] vlan 100

[Sysname-vlan100] mld-snooping enable

[Sysname-vlan100] quit

[Sysname] ipv6 multicast-vlan 100

[Sysname-ipv6-mvlan-100]

Related commands

ipv6 multicast routing

mld-snooping enable

IPv6 multicast VLAN commands -- ipv6 multicast-vlan entry-limit

Use ipv6 multicast-vlan entry-limit to set the maximum number of IPv6 multicast VLAN forwarding entries.

Use undo ipv6 multicast-vlan entry-limit to restore the default.

Syntax

ipv6 multicast-vlan entry-limit limit

undo ipv6 multicast-vlan entry-limit

Default

The maximum number of IPv6 multicast VLAN forwarding entries varies by device model.

Views

System view

Predefined user roles

network-admin

mdc-admin

Parameters

limit: Specifies the maximum number of IPv6 multicast VLAN forwarding entries. The value range varies by device model.

Examples

# Set the maximum number of IPv6 multicast VLAN forwarding entries to 120.

<Sysname> system-view

[Sysname] ipv6 multicast-vlan entry-limit 120

Related commands

entry-limit (MLD-snooping view)

IPv6 multicast VLAN commands -- ipv6 port multicast-vlan

Use ipv6 port multicast-vlan to assign a user port to an IPv6 multicast VLAN.

Use undo ipv6 port multicast-vlan to restore the default.

Syntax

ipv6 port multicast-vlan vlan-id

undo ipv6 port multicast-vlan

Default

A port does not belong to an IPv6 multicast VLAN.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Layer 2 RPR logical interface view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan-id: Specifies an IPv6 multicast VLAN by its VLAN ID in the range of 1 to 4094.

Usage guidelines

You can assign a port to only one IPv6 multicast VLAN.

For the port to be assigned to an IPv6 multicast VLAN, you must enable MLD snooping for the VLAN to which the port belongs.

Examples

# Assign GigabitEthernet 1/0/1 to IPv6 multicast VLAN 100.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] ipv6 port multicast-vlan 100

IPv6 multicast VLAN commands -- port (IPv6 multicast VLAN view)

Use port to assign user ports to an IPv6 multicast VLAN.

Use undo port to delete user ports from an IPv6 multicast VLAN.

Syntax

port interface-list

undo port { all | interface-list }

Default

An IPv6 multicast VLAN does not have user ports.

Views

IPv6 multicast VLAN view

Predefined user roles

network-admin

mdc-admin

Parameters

interface-list: Specifies a port in the form of interface-type interface-number, or a port range in the form of interface-type interface-number to interface-type interface-number.

all: Specifies all user ports in the current IPv6 multicast VLAN.

Usage guidelines

You can assign only Layer 2 Ethernet interfaces, Layer 2 RPR logical interfaces, or Layer 2 aggregate interfaces as user ports to an IPv6 multicast VLAN. Additionally, you can assign a port to only one IPv6 multicast VLAN.

For ports to be assigned to an IPv6 multicast VLAN, you must enable MLD snooping for the VLANs to which the ports belong.

Examples

# Assign GigabitEthernet 1/0/1 through GigabitEthernet 1/0/5 as user ports to IPv6 multicast VLAN 100.

<Sysname> system-view

[Sysname] ipv6 multicast-vlan 100

[Sysname-ipv6-mvlan-100] port gigabitethernet 1/0/1 to gigabitethernet 1/0/5

IPv6 multicast VLAN commands -- reset ipv6 multicast-vlan group

Use reset ipv6 multicast-vlan group to clear IPv6 multicast group entries in IPv6 multicast VLANs.

Syntax

reset ipv6 multicast-vlan group [ ipv6-group-address [ prefix-length ] | ipv6-source-address [ prefix-length ] | vlan vlan-id ] *

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv6-group-address: Specifies an IPv6 multicast group address. The value range for this argument is FFxy::/16 (excluding FFx1::/16 and FFx2::/16), where "x" and "y" represent any hexadecimal numbers in the range of 0 to F. If you do not specify an IPv6 multicast group, this command clears all IPv6 multicast group entries in IPv6 multicast VLANs.

prefix-length: Specifies a prefix length of the IPv6 multicast group address. The value range is 8 to 128 and the default value is 128.

ipv6-source-address: Specifies an IPv6 multicast source by its IPv6 address. If you do not specify an IPv6 multicast source, this command clears IPv6 multicast group entries for all IPv6 multicast sources in IPv6 multicast VLANs.

prefix-length: Specifies a prefix length of the IPv6 multicast source address. The value range is 0 to 128 and the default value is 128.

vlan vlan-id: Specifies an IPv6 multicast VLAN by its VLAN ID in the range of 1 to 4094. If you do not specify an IPv6 multicast VLAN, this command clears IPv6 multicast group entries for all IPv6 multicast VLANs.

Examples

# Clear all IPv6 multicast group entries for all IPv6 multicast VLANs.

<Sysname> reset ipv6 multicast-vlan group

Related commands

display ipv6 multicast-vlan group

IPv6 multicast VLAN commands -- subvlan (IPv6 multicast VLAN view)

Use subvlan to assign VLANs as sub-VLANs to an IPv6 multicast VLAN.

Use undo subvlan to delete sub-VLANs from an IPv6 multicast VLAN.

Syntax

subvlan vlan-list

undo subvlan { all | vlan-list }

Default

An IPv6 multicast VLAN does not have sub-VLANs.

Views

IPv6 multicast VLAN view

Predefined user roles

network-admin

mdc-admin

Parameters

vlan-list: Specifies a space-separated list of up to 10 VLAN items. Each item specifies a VLAN by its ID or a range of VLANs in the form of start-vlan-id to end-vlan-id. The value range for the VLAN ID is 1 to 4094. The specified VLANs must exist and cannot be multicast VLANs or sub-VLANs of other IPv6 multicast VLANs.

all: Specifies all sub-VLANs of the current IPv6 multicast VLAN.

Usage guidelines

You must enable MLD snooping for VLANs to be configured as sub-VLANs of an IPv6 multicast VLAN.

Examples

# Assign VLAN 10 through VLAN 15 as sub-VLANs to multicast VLAN 100.

<Sysname> system-view

[Sysname] ipv6 multicast-vlan 100

[Sysname-ipv6-mvlan-100] subvlan 10 to 15