Wireless location commands -- display wlan rfid-tracking radio

Use display wlan rfid-tracking radio to display radio information for AeroScout location.

Syntax

display wlan rfid-tracking radio [ ap ap-name ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

ap ap-name: Specifies an AP by its name, a case-insensitive string of 1 to 64 characters. The name can include letters, numbers, underscores (_), left brackets ([), right brackets (]), slashes (/), and minus signs (-). If you do not specify this option, the command displays radio information for all APs.

Examples

# Display radio information for AeroScout location.

<Sysname> display wlan rfid-tracking radio

Wireless Locating

--------------------------------------------------------------------------------

AP name Radio ID Type

--------------------------------------------------------------------------------

ap1 1 MU/Tag

ap2 1 MU

ap3 2 Tag

ap4 1 N/A

--------------------------------------------------------------------------------

Table 1 Command output

Field | Description
Type | Type of devices to locate: · MU/Tag—Both MU and Tag devices. · MU. · Tag. · N/A—The AP does not locate any devices.

Wireless location commands -- rfid-tracking aeroscout

Use rfid-tracking aeroscout enable to enable AeroScout location.

Use rfid-tracking aeroscout disable to disable AeroScout location.

Use undo rfid-tracking aeroscout to restore the default.

Syntax

rfid-tracking aeroscout { disable | enable }

undo rfid-tracking aeroscout

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, AeroScout location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

For an AP to send location packets to the location server, you must enable both AeroScout location and radio-based location for the AP.

Examples

# Enable AeroScout location for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking aeroscout enable

# Enable AeroScout location for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking aeroscout enable

# Enable AeroScout location globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking aeroscout enable

Related commands

rfid-tracking radio

Wireless location commands -- rfid-tracking aeroscout vendor-port

Use rfid-tracking aeroscout vendor-port to specify the port for an AP to listen to.

Use undo rfid-tracking aeroscout vendor-port to restore the default.

Syntax

rfid-tracking aeroscout vendor-port vendor-port-number

undo rfid-tracking aeroscout vendor-port

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, an AP listens to port 1144.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

vendor-port-number: Specifies a port number in the range of 1 to 65535.

Usage guidelines

The location server and an AP communicate with each other over UDP. This command enables an AP to get query and configuration messages from the location server.

Examples

# Specify the port for AP ap1 to listen to as port 3000.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking aeroscout vendor-port 3000

# Specify the port for APs in AP group 10 to listen to as port 3000.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking aeroscout vendor-port 3000

# Specify the port to listen to as port 3000 globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking aeroscout vendor-port 3000

Related commands

rfid-tracking aeroscout enable

Wireless location commands -- rfid-tracking ble

Use rfid-tracking ble enable to enable Bluetooth Low Energy (BLE) location.

Use rfid-tracking ble disable to disable BLE location.

Use undo rfid-tracking ble to restore the default.

Syntax

rfid-tracking ble { disable | enable }

undo rfid-tracking ble

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, BLE location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Examples

# Enable BLE location for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-wlan-ap-ap1] rfid-tracking ble enable

# Enable BLE location for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking ble enable

# Enable BLE location globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble enable

Wireless location commands -- rfid-tracking ble aging-time

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble aging-time to set the aging time for BLE neighbors.

Use undo rfid-tracking ble aging-time to restore the default.

Syntax

rfid-tracking ble aging-time aging-time

undo rfid-tracking ble aging-time

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the aging time for BLE neighbors is 180 seconds.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configure this command to help an AP discover BLE devices that are powered off or moved.

If the AP does not receive any packets from a BLE neighbor within the aging time, the AP performs the following actions:

· Removes the neighbor from the BLE neighbor list.

· Notifies the location server of the BLE neighbor removal event.

Parameters

aging-time: Specifies the aging time for BLE neighbors, in the range of 60 to 3600 seconds.

Examples

# Set the aging time for BLE neighbors to 60 seconds for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-wlan-ap-ap1] rfid-tracking ble aging-time 60

# Set the aging time for BLE neighbors to 60 seconds for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking ble aging-time 60

# Set the aging time for BLE neighbors to 60 seconds globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble aging-time 60

Wireless location commands -- rfid-tracking ble engine-address

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble engine-address to specify an IPv4 address and a port number for the location server.

Use undo rfid-tracking ble engine-address to restore the default.

Syntax

rfid-tracking ble engine-address engine-address engine-port engine-port

undo rfid-tracking ble engine-address

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the IPv4 address and port number for the location server are not specified.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

engine-address engine-address: Specifies the IPv4 address for the location server.

engine-port engine-port: Specifies the port number for the location server, in the range of 1 to 65535.

Usage guidelines

APs use the IPv4 address and port number to communicate with the location server.

Examples

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking ble engine-address 192.168.10.10 engine-port 1145

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking ble engine-address 192.168.10.10 engine-port 1145

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble engine-address 192.168.10.10 engine-port 1145

Wireless location commands -- rfid-tracking ble report

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble report enable to enable BLE neighbor list reporting.

Use rfid-tracking ble report disable to disable BLE neighbor list reporting.

Use undo rfid-tracking ble report to restore the default.

Syntax

rfid-tracking ble report { disable | enable }

undo rfid-tracking ble report

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, BLE neighbor list reporting is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configure this command to enable APs to send BLE neighbor list reports to the location server at the specified interval. The BLE neighbor list uses MAC addresses as indexes and records the UUID, major ID, minor ID, and the most recently collected transmit power and RSSI of BLE neighbors.

This command takes effect only when you enable BLE location.

Examples

# Enable BLE neighbor list reporting for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking ble report enable

# Enable BLE neighbor list reporting for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking ble report enable

# Enable BLE neighbor list reporting globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble report enable

Related commands

rfid-tracking ble enable

rfid-tracking ble report interval

Wireless location commands -- rfid-tracking ble report interval

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble report interval to set the interval for sending BLE neighbor list reports.

Use undo rfid-tracking ble report interval to restore the default.

Syntax

rfid-tracking ble report interval interval

undo rfid-tracking ble report interval

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the interval for sending BLE neighbor list reports is 900 seconds.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies the interval for sending BLE neighbor list reports, in the range of 1 to 86400 seconds.

Usage guidelines

This command takes effect only when you enable both BLE location and BLE neighbor list reporting.

Examples

# Set the interval for sending BLE neighbor list reports to 5 seconds for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking ble report interval 5

# Set the interval for sending BLE neighbor list reports to 5 seconds for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking ble report interval 5

# Set the interval for sending BLE neighbor list reports to 5 seconds globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble report interval 5

Related commands

rfid-tracking ble enable

rfid-tracking ble report enable

Wireless location commands -- rfid-tracking ble rssi

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble rssi enable to enable RSSI-based packet filtering for BLE location.

Use rfid-tracking ble rssi disable to disable RSSI-based packet filtering for BLE location.

Use undo rfid-tracking ble rssi to restore the default.

Syntax

rfid-tracking ble rssi { disable | enable }

undo rfid-tracking ble rssi

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, RSSI-based packet filtering for BLE location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This command disables an AP from sending packets with an RSSI lower than the RSSI threshold to the location server.

Examples

# Enable RSSI-based packet filtering for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking ble rssi enable

# Enable RSSI-based packet filtering for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking ble rssi enable

# Enable RSSI-based packet filtering globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble rssi enable

Related commands

rfid-tracking ble rssi threshold

Wireless location commands -- rfid-tracking ble rssi threshold

| NOTE: Support for this command depends on the AP model.

Use rfid-tracking ble rssi threshold to set the RSSI threshold for packet filtering of BLE location.

Use undo rfid-tracking ble rssi threshold to restore the default.

Syntax

rfid-tracking ble rssi threshold rssi-threshold

undo rfid-tracking ble rssi threshold

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the RSSI threshold for packet filtering of BLE location is 5.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

rssi-threshold: Specifies the RSSI threshold for packet filtering of BLE location, in the range of 5 to 255.

Usage guidelines

This command takes effect only when you enable both BLE location and RSSI-based packet filtering for BLE location.

Examples

# Set the RSSI threshold for packet filtering of BLE location to 10 for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking ble rssi threshold 10

# Set the RSSI threshold for packet filtering of BLE location to 10 for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking ble rssi threshold 10

# Set the RSSI threshold for packet filtering of BLE location to 10 globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ble rssi threshold 10

Wireless location commands -- rfid-tracking client rate-limit

Use rfid-tracking client rate-limit enable to enable client packet rate limiting for an AP.

Use rfid-tracking client rate-limit disable to disable client packet rate limiting for an AP.

Use undo rfid-tracking client rate-limit to restore the default.

Syntax

rfid-tracking client rate-limit { disable | enable }

undo rfid-tracking client rate-limit

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, client packet rate limiting is disabled for an AP.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configure this command to enable the AP to discard excessive wireless packets when both the CIR and the CBS are exceeded. This feature ensures that the location information for each client can be sent to the location server and prevents client packets from flooding the AP.

Examples

# Enable client packet rate limiting for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking client rate-limit enable

# Enable client packet rate limiting for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking client rate-limit enable

# Enable client packet rate limiting globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking client rate-limit enable

Related commands

rfid-tracking client rate-limit cir

Wireless location commands -- rfid-tracking client rate-limit cir

Use rfid-tracking client rate-limit cir to set the rate limits for client packets.

Use undo rfid-tracking client rate-limit cir to restore the default.

Syntax

rfid-tracking client rate-limit cir cir [ cbs cbs ]

undo rfid-tracking client rate-limit cir

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, both the CIR and the CBS are 0. An AP does not limit the rate for incoming wireless packets.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

cir cir: Specifies the CIR for client packets, in the range of 1 to 1300000 kbps.

cbs cbs: Specifies the CBS for client packets, in the range of 80 to 130000000 bytes. The default CBS is the CIR ?700 bytes.

Usage guidelines

The CIR and CBS configuration takes effect only when you enable client packet rate limiting.

Examples

# Set the CIR and CBS to 200000 kbps and 50000 bytes, respectively for client packets for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking client rate-limit cir 200000 cbs 50000

# Set the CIR and CBS to 200000 kbps and 50000 bytes, respectively for client packets for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking client rate-limit cir 200000 cbs 50000

# Set the CIR to 200000 kbps and the CBS to 50000 bytes for client packets globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking client rate-limit cir 200000 cbs 50000

Related commands

rfid-tracking client rate-limit enable

Wireless location commands -- rfid-tracking cupid

Use rfid-tracking cupid enable to enable CUPID location.

Use rfid-tracking cupid disable to disable CUPID location.

Use undo rfid-tracking cupid to restore the default.

Syntax

rfid-tracking cupid { disable | enable }

undo rfid-tracking cupid

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, CUPID location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Examples

# Enable CUPID location for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking cupid enable

# Enable CUPID location for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking cupid enable

# Enable CUPID location globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking cupid enable

Wireless location commands -- rfid-tracking cupid engine-address

Use rfid-tracking cupid engine-address to specify an IPv4 address and a port number for the location server.

Use undo rfid-tracking cupid engine-address to restore the default.

Syntax

rfid-tracking cupid engine-address engine-address engine-port engine-port

undo rfid-tracking cupid engine-address

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the IPv4 address and port number for the location server are not configured.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

engine-address engine-address: Specifies an IPv4 address for the CUPID location server.

engine-port engine-port: Specifies a port number for the CUPID location server, in the range of 1 to 65535.

Usage guidelines

APs send location packets to the specified IPv4 address and port number for communicating with the location server.

Examples

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320-ACN-B

[Sysname-ap-ap1] rfid-tracking cupid engine-address 192.168.10.10 engine-port 1145

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking cupid engine-address 192.168.10.10 engine-port 1145

# Set the IPv4 address and port number for the location server to 192.168.10.10 and 1145 globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking cupid engine-address 192.168.10.10 engine-port 1145

Wireless location commands -- rfid-tracking cupid report

Use rfid-tracking cupid report enable to enable client list reporting.

Use rfid-tracking cupid report disable to disable client list reporting.

Use undo rfid-tracking cupid report to restore the default.

Syntax

rfid-tracking cupid report { disable | enable }

undo rfid-tracking cupid report

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, client list reporting is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

A client can be located only when its associated AP is enabled with both CUPID location and client list reporting.

After you enable client list reporting for an AP, the AP sends client list reports to the location server at the specified interval. The location server selects a group of location APs for each client based on the client list reports.

This command takes effect only when you enable CUPID location.

Examples

# Enable client list reporting for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking cupid report enable

# Enable client list reporting for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking cupid report enable

# Enable client list reporting globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking cupid report enable

Wireless location commands -- rfid-tracking cupid report interval

Use rfid-tracking cupid report interval to set the interval for sending client list reports.

Use undo rfid-tracking location-aware report interval to restore the default.

Syntax

rfid-tracking cupid report interval interval

undo rfid-tracking cupid report interval

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the interval for sending client list reports is 1 second.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

interval: Specifies the interval for sending client list reports, in the range of 1 to 10 seconds.

Usage guidelines

This command takes effect only when you enable client list reporting.

Examples

# Set the interval for sending client list reports to 9 seconds for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking cupid report interval 9

# Set the interval for sending client list reports to 9 seconds for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking cupid report interval 9

# Set the interval for sending client list reports to 9 seconds globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking cupid report interval 9

Wireless location commands -- rfid-tracking cupid unassociated-measurement

Use rfid-tracking cupid unassociated-measurement enable to enable unassociated client location.

Use rfid-tracking cupid unassociated-measurement disable to disable unassociated client location.

Use undo rfid-tracking cupid unassociated-measurement to restore the default.

Syntax

rfid-tracking cupid unassociated-measurement { disable | enable }

undo rfid-tracking cupid unassociated-measurement

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, unassociated client location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

After you enable unassociated client location for an AP, the AP performs a location measurement for an unassociated client upon receiving a probe request from the client.

In a WLAN that has a large amount of unassociated clients, configure packet dilution to prevent frequent location measurements.

Examples

# Enable unassociated client location for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking cupid unassociated-measurement enable

# Enable unassociated client location for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group10] rfid-tracking cupid unassociated-measurement enable

# Enable unassociated client location globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking cupid unassociated-measurement

Wireless location commands -- rfid-tracking dilution

Use rfid-tracking dilution enable to enable packet dilution.

Use rfid-tracking dilution disable to disable packet dilution.

Use undo rfid-tracking dilution to restore the default.

Syntax

rfid-tracking dilution { disable | enable }

undo rfid-tracking dilution

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, packet dilution is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

This feature takes effect only on MU clients for AeroScout location and unassociated clients for CUPID location.

For AeroScout location, this feature controls the number of location packets from an AP to the location server. For CUPID location, this feature controls the frequency of location measurements for an unassociated client.

Examples

# Enable packet dilution for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking dilution enable

# Enable packet dilution for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking dilution enable

# Enable packet dilution globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking dilution enable

Related commands

rfid-tracking dilution factor

Wireless location commands -- rfid-tracking dilution factor

Use rfid-tracking dilution factor to set the packet dilution factor and the dilution timeout timer.

Use undo rfid-tracking dilution factor to restore the default.

Syntax

rfid-tracking dilution factor factor timeout timeout

undo rfid-tracking dilution factor

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the packet dilution factor and the dilution timeout timer are not set.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

factor factor: Specifies the dilution factor in the range of 1 to 10000.

timeout timeout: Specifies the dilution timeout timer in the range of 1 to 60 seconds.

Usage guidelines

Packet dilution takes effect only on MU clients for AeroScout location and unassociated clients for CUPID location.

If the dilution factor is 10 and the timeout timer is 5 seconds, packet dilution operates as follows:

· If AeroScout location is enabled, the AP sends a location packet every time it receives 10 wireless packets from an MU client (excluding management and broadcast packets). If the AP fails to receive 10 packets from an MU client within the timeout timer, it sends the most recent wireless packet to the location server.

· If CUPID location is enabled, the AP performs a location measurement every time it receives 10 probe requests from an unassociated client. If the AP fails to receive 10 probe requests from an unassociated client within the timeout timer, it performs a location measurement when the timer expires.

The dilution factor and dilution timeout timer take effect only when you enable packet dilution.

Examples

# Set the dilution factor to 10 and the dilution timeout timer to 10 seconds for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking dilution factor 10 timeout 10

# Set the dilution factor to 10 and the dilution timeout timer to 10 seconds for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking dilution factor 10 timeout 10

# Set the dilution factor to 10 and the dilution timeout timer to 10 seconds globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking dilution factor 10 timeout 10

Related commands

rfid-tracking dilution enable

Wireless location commands -- rfid-tracking ignore beacon

Use rfid-tracking ignore beacon enable to enable ignoring beacon frames.

Use rfid-tracking ignore beacon disable to disable ignoring beacon frames.

Use undo rfid-tracking ignore beacon to restore the default.

Syntax

rfid-tracking ignore beacon { disable | enable }

undo rfid-tracking ignore beacon

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, ignoring beacon frames is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Ignoring beacon frames disables an AP from sending the received beacon frames to the location server to ensure performance of the location server.

Examples

# Configure AP ap1 to not send beacon frames to the location server.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking ignore beacon enable

# Configure APs in AP group 10 to not send beacon frames to the location server.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking ignore beacon enable

# Configure APs to not send beacon frames to the location server globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking ignore beacon enable

Wireless location commands -- rfid-tracking mode

Use rfid-tracking mode to specify the type of devices to locate.

Use undo rfid-tracking mode to restore the default.

Syntax

rfid-tracking mode { mu | tag }

undo rfid-tracking mode mu { mu | tag }

Default

In radio view, the configuration in AP group view is used.

In AP group radio view, the type of wireless devices to locate is not specified.

Views

Radio view

AP group radio view

Predefined user roles

network-admin

mdc-admin

Parameters

mu: Specifies the type of devices to locate as MU.

tag: Specifies the type of devices to locate as Tag.

Usage guidelines

An AP sends location packets from devices to the location server only when you execute the rfid-tracking mode command.

You can configure an AP to locate both MUs and Tags.

This command takes effect only when you enable both AeroScout location and radio-based location.

Examples

# Specify the type of wireless devices to locate as MU for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] rfid-tracking mode mu

# Specify the type of wireless devices to locate as MU for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-wlan-ap-group-10] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-10-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-10-ap-model-WA4320i-ACN-radio-1] rfid-tracking mode mu

Wireless location commands -- rfid-tracking radio

Use rfid-tracking radio enable to enable radio-based location.

Use rfid-tracking radio disable to disable radio-based location.

Use undo rfid-tracking radio to restore the default.

Syntax

rfid-tracking radio { disable | enable }

undo rfid-tracking radio

Default

In radio view, the configuration in AP group view is used.

In AP group radio view, radio-based location is disabled.

Views

Radio view

AP group view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

An AP encapsulates and sends received wireless packets to the location server only when you enable both AeroScout and radio-based location.

This command is applicable only to AeroScout location.

Examples

# Enable radio-based location for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] radio 1

[Sysname-wlan-ap-ap1-radio-1] rfid-tracking radio enable

# Enable radio-based location for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-wlan-ap-group-10] ap-model WA4320i-ACN

[Sysname-wlan-ap-group-10-ap-model-WA4320i-ACN] radio 1

[Sysname-wlan-ap-group-10-ap-model-WA4320i-ACN-radio-1] rfid-tracking radio enable

Wireless location commands -- rfid-tracking rate-limit

Use rfid-tracking rate-limit enable to enable location packet rate limiting for an AP.

Use rfid-tracking rate-limit disable to disable location packet rate limiting for an AP.

Use undo rfid-tracking rate-limit to restore the default.

Syntax

rfid-tracking rate-limit { disable | enable }

undo rfid-tracking rate-limit

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, location packet rate limiting is disabled for an AP.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

Configure this command to enable an AP to discard excessive location packets when both the CIR and the CBS are exceeded.

Examples

# Enable location packet rate limiting for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking rate-limit enable

# Enable location packet rate limiting for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking rate-limit enable

# Enable location packet rate limiting globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking rate-limit enable

Related commands

rfid-tracking rate-limit cir

Wireless location commands -- rfid-tracking rate-limit cir

Use rfid-tracking rate-limit cir to set the rate limits for location packets for an AP.

Use undo rfid-tracking rate-limit cir to restore the default.

Syntax

rfid-tracking rate-limit cir cir [ cbs cbs ]

undo rfid-tracking rate-limit cir

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, both the CIR and the CBS are 0. An AP does not limit the rate for outgoing location packets.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

cir cir: Specifies the CIR for location packets, in the range of 8 to 1300000 kbps.

cbs cbs: Specifies the CBS for location packets, in the range of 500 to 130000000 bytes. The default CBS is the CIR ?700 bytes.

Usage guidelines

The CIR and CBS configuration takes effect only when you enable location packet rate limiting.

Examples

# Set the CIR and CBS to 800000 kbps and 50000 bytes, respectively for location packets for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking rate-limit cir 800000 cbs 50000

# Set the CIR and CBS to 800000 kbps and 50000 bytes, respectively for location packets for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking rate-limit cir 800000 cbs 50000

# Set the CIR to 800000 kbps and the CBS to 50000 bytes for location packets globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking rate-limit cir 800000 cbs 50000

Related commands

rfid-tracking rate-limit enable

Wireless location commands -- rfid-tracking rssi

Use rfid-tracking rssi enable to enable RSSI-based packet filtering for AeroScout location.

Use rfid-tracking rssi disable to disable RSSI-based packet filtering for AeroScout location.

Use undo rfid-tracking rssi to restore the default.

Syntax

rfid-tracking rssi { disable | enable }

undo rfid-tracking rssi

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, RSSI-based packet filtering for AeroScout location is disabled.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

After you enable RSSI filtering for AeroScout location, an AP discards packets with an RSSI lower than the specified RSSI threshold.

Examples

# Enable RSSI-based packet filtering for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking rssi enable

# Enable RSSI-based packet filtering for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking rssi enable

# Enable RSSI-based packet filtering globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking rssi enable

Related commands

rfid-tracking rssi threshold

Wireless location commands -- rfid-tracking rssi threshold

Use rfid-tracking rssi threshold to set the RSSI threshold for packet filtering of AeroScout location.

Use undo rfid-tracking rssi threshold to restore the default.

Syntax

rfid-tracking rssi threshold rssi-threshold

undo rfid-tracking rssi threshold

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the RSSI threshold for packet filtering of AeroScout location is 5.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

threshold rssi-threshold: Specifies the RSSI threshold for packet filtering of AeroScout location, in the range of 5 to 100. A packet is discarded if its RSSI is lower than the specified RSSI threshold.

Usage guidelines

This command takes effect only when you enable both AeroScout location and RSSI-based packet filtering for AeroScout location.

Examples

# Set the RSSI threshold for packet filtering of AeroScout location to 50 for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking rssi threshold 50

# Set the RSSI threshold for packet filtering of AeroScout location to 50 for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking rssi threshold 50

# Set the RSSI threshold for packet filtering of AeroScout location to 50 globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking rssi threshold 50

Related commands

rfid-tracking rssi enable

Wireless location commands -- rfid-tracking timestamp

Use rfid-tracking timestamp to specify the type of timestamps to be encapsulated in MU packets.

Use undo rfid-tracking timestamp to restore the default.

Syntax

rfid-tracking timestamp { absolute | relative }

undo rfid-tracking timestamp

Default

In AP view, the configuration in AP group view is used. If no configuration exists in AP group view, the configuration in global configuration view is used.

In AP group view, the configuration in global configuration view is used.

In global configuration view, the timestamp type is relative.

Views

AP view

AP group view

Global configuration view

Predefined user roles

network-admin

mdc-admin

Parameters

absolute: Specifies the absolute timestamp. An absolute timestamp represents the time elapsed since 1970, in milliseconds.

relative: Specifies the relative timestamp. A relative time represents the time elapsed since the AP started, in milliseconds.

Usage guidelines

Tag packets can be encapsulated only with the relative time. Whether MU packets are encapsulated with the relative time or absolute time depends on the configuration on the location server.

Examples

# Set the timestamp type to absolute for AP ap1.

<Sysname> system-view

[Sysname] wlan ap ap1 model WA4320i-ACN

[Sysname-wlan-ap-ap1] rfid-tracking timestamp absolute

# Set the timestamp type to absolute for APs in AP group 10.

<Sysname> system-view

[Sysname] wlan ap-group 10

[Sysname-ap-group-10] rfid-tracking timestamp absolute

# Set the timestamp type to absolute globally.

<Sysname> system-view

[Sysname] wlan global-configuration

[Sysname-wlan-global-configuration] rfid-tracking timestamp absolute