Keychain probe commands -- display system internal keychain kernel

| NOTE: Support for this command depends on the device model.

Use display system internal keychain kernel to display internal keychain information.

Syntax

Centralized devices:

display system internal keychain kernel name keychain-name [ key key-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal keychain kernel name keychain-name [ key key-id ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal keychain kernel name keychain-name [ key key-id ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters.

key-id: Specifies a key by its ID in the range of 0 to 281474976710655. If you do not specify a key ID, this command displays internal keychain information for all keys in a keychain.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. Support for this option depends on the device model.