WIPS probe commands -- display system internal wips statistics

Use display system internal wips statistics to display WIPS statistics.

Syntax

display system internal wips statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

WIPS probe commands -- wips fix-channel-scan

Use wips fix-channel-scan to enable WIPS to scan the specified channel.

Use undo wips fix-channel-scan to disable WIPS from scanning the specified channel.

Syntax

wips fix-channel-scan ap id apid radio radioid channel number

undo wips fix-channel-scan ap id apid radio radioid

Default

WIPS is disabled from scanning the specified channel.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

apid: Specifies an AP by its ID in the range of 1 to 65535.

radioid: Specifies a radio by its ID in the range of 1 to 4.

number: Specifies a channel by its number in the range of 1 to 255.

Usage guidelines

This command enables WIPS to scan only the specified channel. However, devices on adjacent channels might be detected because of channel overlapping.