VLAN probe commands -- debugging system internal vlan

Use debugging system internal vlan to enable debugging for VLANs.

Use undo debugging system internal vlan to disable debugging for VLANs.

Syntax

debugging system internal vlan { all | error | event | execution | hardware }

undo debugging system internal vlan { all | error | event | execution | hardware }

Default

Debugging for VLANs is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Enables all types of debugging for VLANs.

error: Enables error debugging for VLANs.

event: Enables event debugging for VLANs.

execution: Enables execution debugging for VLANs.

hardware: Enables hardware debugging for VLANs.

VLAN probe commands -- display system internal vlan

Use display system internal vlan to display the internal information of the VLAN module.

Syntax

Centralized devices:

display system internal vlan { instance vlan-id | interface interface-type interface-number | summary }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal vlan { instance vlan-id | interface interface-type interface-number | summary } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal vlan { instance vlan-id | interface interface-type interface-number | summary } chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance vlan-id: Displays the VLAN module information of the VLAN specified by its VLAN ID in the range of 1 to 4094.

interface interface-type interface-number: Displays the VLAN module information of an interface specified by its type and number.

summary: Displays the summary VLAN module information.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its CPU number. If you do not specify this option, the command displays the VLAN module information of the default CPU. Support for this option depends on the device model.