Service loopback group probe commands -- display system internal service-loopback running

Use display system internal service-loopback running to display running data and driver information for a service loopback group.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal service-loopback running group group-id slot slot-number

Distributed devices in IRF mode:

display system internal service-loopback running group group-id chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

group group-id: Specifies a service loopback group by its group ID, in the range of 1 to 1024.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

Usage guidelines

(Distributed devices.) Use this command to obtain status and driver information for the specified service loopback group on each card. You can use this information to troubleshoot driver problems and verify data consistency across cards.

(Centralized IRF devices.) Use this command to obtain status and driver information for the specified service loopback group on each member device. You can use this information to troubleshoot driver problems and verify data consistency across member devices.

Service loopback group probe commands -- display system internal service-loopback interface-list

Use display system internal service-loopback interface-list to display node information for the interface event queue.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal service-loopback interface-list slot slot-number

Distributed devices in IRF mode:

display system internal service-loopback interface-list chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

Usage guidelines

This command helps you locate out-of-order problems for interface events.