IPCIM probe commands -- display system internal ip source binding

Use display system internal ip source binding to display detailed information about IPv4SG bindings.

Syntax

Centralized devices:

display system internal ip source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcp-relay | dhcp-server | dhcp-snooping | dot1x | wlan-snooping ] ] [ ip-address ip-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ip source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcp-relay | dhcp-server | dhcp-snooping | dot1x | wlan-snooping ] ] [ ip-address ip-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ip source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcp-relay | dhcp-server | dhcp-snooping | dot1x | wlan-snooping ] ] [ ip-address ip-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

static: Specifies static IPv4SG bindings.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays dynamic IPv4SG bindings for the public network.

dhcp-relay: Displays dynamic IPv4SG bindings that are generated based on DHCP relay.

dhcp-server: Displays dynamic IPv4SG bindings that are generated based on DHCP server.

dhcp-snooping: Displays dynamic IPv4SG bindings that are generated based on DHCP snooping.

dot1x: Displays dynamic IPv4SG bindings that are generated based on 802.1X.

wlan-snooping: Displays dynamic IPv4SG bindings that are generated based on WLAN snooping.

ip-address ip-address: Specifies an IPv4 address.

mac-address mac-address: Specifies a MAC address in H-H-H format.

vlan vlan-id: Specifies a VLAN ID in the range of 1 to 4094.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv4SG bindings for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv4SG bindings for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPv4SG bindings for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv4SG bindings for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPv4SG bindings for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IPCIM probe commands -- display system internal ipv6 source binding

Use display system internal ipv6 source binding to display detailed information about IPv6SG bindings.

Syntax

Centralized devices:

display system internal ipv6 source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcpv6-relay | dhcpv6-snooping | nd-snooping | wlan-snooping ] ] [ ip-address ipv6-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal ipv6 source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcpv6-relay | dhcpv6-snooping | nd-snooping | wlan-snooping ] ] [ ip-address ipv6-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ] [ slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal ipv6 source binding [ static | [ vpn-instance vpn-instance-name ] [ dhcpv6-relay | dhcpv6-snooping | nd-snooping | wlan-snooping ] ] [ ip-address ipv6-address ] [ mac-address mac-address ] [ vlan vlan-id ] [ interface interface-type interface-number ] [ chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

static: Specifies static IPv6SG bindings.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays dynamic IPv6SG bindings for the public network.

dhcpv6-relay: Displays dynamic IPv6SG bindings that are generated based on DHCPv6 relay agent.

dhcpv6-snooping: Displays dynamic IPv6SG bindings that are generated based on DHCPv6 snooping.

nd-snooping: Displays dynamic IPv6SG bindings that are generated based on ND snooping.

wlan-snooping: Displays dynamic IPv6SG bindings that are generated based on WLAN snooping.

ip-address ipv6-address: Specifies an IPv6 address.

mac-address mac-address: Specifies a MAC address in H-H-H format.

vlan vlan-id: Specifies a VLAN ID in the range of 1 to 4094.

interface interface-type interface-number: Specifies an interface by its type and number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays IPv6SG bindings for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays IPv6SG bindings for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays IPv6SG bindings for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays IPv6SG bindings for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays IPv6SG bindings for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.