QoS probe commands -- display system internal control-plane management statistics

| NOTE: Support for this command depends on the device model.

Use display system internal control-plane management statistics to display statistics for the management interface control plane.

Syntax

display system internal control-plane management statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

QoS probe commands -- display system internal control-plane statistics

| NOTE: Support for this command depends on the device model.

Use display system internal control-plane statistics to display statistics for a control plane.

Syntax

Centralized devices:

display system internal control-plane statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal control-plane statistics slot slot-number

Distributed devices in IRF mode:

display system internal control-plane statistics chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies the control plane of a card. The slot-number argument represents the slot number of the card. (Distributed devices in standalone mode.)

slot slot-number: Specifies the control plane of an IRF member device. The slot-number argument represents the member ID of the IRF member device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the control plane of an IRF member device or a PEX. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the control plane of a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the control plane of a card on an IRF member device or of a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

QoS probe commands -- reset system internal control-plane management statistics

| NOTE: Support for this command depends on the device model.

Use reset system internal control-plane management statistics to clear statistics for the management interface control plane.

Syntax

reset system internal control-plane management statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

QoS probe commands -- reset system internal control-plane statistics

| NOTE: Support for this command depends on the device model.

Use reset system internal control-plane statistics to clear statistics for a control plane.

Syntax

Centralized devices:

reset system internal control-plane statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal control-plane statistics slot slot-number

Distributed devices in IRF mode:

reset system internal control-plane statistics chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies the control plane of a card. The slot-number argument represents the slot number of the card. (Distributed devices in standalone mode.)

slot slot-number: Specifies the control plane of an IRF member device. The slot-number argument represents the member ID of the IRF member device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies the control plane of an IRF member device or a PEX. The slot-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies the control plane of a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies the control plane of a card on an IRF member device or of a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)