LISP probe commands -- debugging system internal lisp database

Use debugging system internal lisp database to enable LISP database debugging.

Use undo debugging system internal lisp database to disable LISP database debugging.

Syntax

debugging system internal lisp database [ hardware | message ]

undo debugging system internal lisp database [ hardware | message ]

Default

LISP database debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

hardward: Enables hardware debugging.

message: Enables database message debugging.

LISP probe commands -- debugging system internal lisp forward

Use debugging system internal lisp forward to enable LISP forwarding debugging.

Use undo debugging system internal lisp forward to disable LISP forwarding debugging.

Syntax

debugging system internal lisp forward [ decap [ fs ] [ eid-addr prefix-len ] | encap [ fs ] [ eid-addr prefix-len ] | statistics upcall { kernel | user } [ eid-addr prefix-len ] | tracert ]

undo debugging system internal lisp forward [ decap [ fs ] | encap [ fs ] | statistics upcall { kernel | user } | tracert ]

Default

LISP forwarding debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

decap: Enables slow forwarding decapsulation debugging.

encap: Enables slow forwarding encapsulation debugging.

fs: Enables fast forwarding encapsulation and decapsulation debugging.

statistics: Enables forwarding statistics debugging.

upcall: Enables statistics upcall debugging

kernel: Enables statistics debugging.

user: Enables debugging for statistics upcall to users.

tracert: Enables tracert debugging.

LISP probe commands -- debugging system internal lisp map-cache

Use debugging system internal lisp map-cache to enable LISP mapping cache debugging.

Use undodebugging system internal lisp map-cache to disable LISP mapping cache debugging.

Syntax

debugging system internal lisp map-cache [ hardware | message ]

undo debugging system internal lisp map-cache [ hardware | message ]

Default

LISP mapping cache debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

hardward: Enables hardware debugging.

message: Enables mapping cache message debugging.

LISP probe commands -- debugging system internal lisp mobility

Use debugging system internal lisp mobility to enable LISP VM mobility debugging.

Use undo debugging system internal lisp mobility to disable LISP VM mobility debugging.

Syntax

debugging system internal lisp mobility [ dynamic-eid | mobility-interface | roaming-host }

undo debugging system internal lisp mobility [ dynamic-eid | mobility-interface | roaming-host }

Default

LISP VM mobility debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

dynamic-eid: Enables dynamic EID debugging.

mobility-interface: Enables roaming interface debugging.

roaming-host: Enables roaming host route debugging.

LISP probe commands -- debugging system internal lisp tunnel

Use debugging system internal lisp tunnel to enable LISP tunnel debugging.

Use undo debugging system internal lisp tunnel to disable LISP tunnel debugging.

Syntax

debugging system internal lisp tunnel [ bind | hardware [ eid-addr prefix-len ] | message ]

undo debugging system internal lisp tunnel [ bind | hardware | message ]

Default

LISP tunnel debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

bind: Enables tunnel binding debugging.

hardware: Enables tunnel hardware debugging.

message: Enables tunnel message debugging.

LISP probe commands -- debugging system internal lisp upcall

Use debugging system internal lisp upcall to enable LISP upcall debugging.

Use undo debugging system internal lisp upcall to disable LISP upcall debugging.

Syntax

debugging system internal lisp upcall [ host-mobility | lsb-bits | no-cache | smr ]

undo debugging system internal lisp upcall [ host-mobility | lsb-bits | no-cache | smr ]

Default

LISP upcall debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

host-mobility: Enables VM mobility upcall debugging.

lsb-bits: Enables LSB change upcall debugging.

no-cache: Enables no-cache message upcall debugging.

smr: Enables SMR message upcall debugging.

LISP probe commands -- display system internal lisp forwarding ipv4 database

Use display system internal lisp forwarding ipv4 database to display the local EID-to-RLOC mapping database.

Syntax

Centralized devices:

display system internal lisp forwarding ipv4 database [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding ipv4 database [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding ipv4 database [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays the local EID-to-RLOC mapping database for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding ipv4 dynamic-eid

Use display system internal lisp forwarding ipv4 dynamic-eid to display dynamic EIDs.

Syntax

Centralized devices:

display system internal lisp forwarding ipv4 dynamic-eid [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding ipv4 dynamic-eid [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding ipv4 dynamic-eid [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays the dynamic EIDs for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding ipv4 map-cache

Use display system internal lisp forwarding ipv4 map-cache to display the EID-to-RLOC mapping cache entries.

Syntax

Centralized devices:

display system internal lisp forwarding ipv4 map-cache [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding ipv4 map-cache [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding ipv4 map-cache [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays the EID-to-RLOC mapping cache entries for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding ipv4 roaming-host

Use display system internal lisp forwarding ipv4 roaming-host to display dynamic EID routing information.

Syntax

Centralized devices:

display system internal lisp forwarding ipv4 roaming-host [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding ipv4 roaming-host [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding ipv4 roaming-host [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays dynamic EID routing information for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding mobile-interface

Use display system internal lisp forwarding mobile-interface to display mobile interface information.

Syntax

Centralized devices:

display system internal lisp forwarding mobile-interface [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding mobile-interface [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding mobile-interface [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays mobile interface information for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding running-status

Use display system internal lisp forwarding running-status to display the running status of the LISP forwarding thread.

Syntax

Centralized devices:

display system internal lisp forwarding running-status [ default | vrf vrf-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding running-status [ default | vrf vrf-name ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding running-status [ default | vrf vrf-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

default: Displays the running status of the LISP forwarding thread for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding statistics

Use display system internal lisp forwarding statistics to display statistics of the LISP forwarding thread.

Syntax

Centralized devices:

display system internal lisp forwarding statistics { count | error }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding statistics { count | error } slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding statistics { count | error } chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

count: Displays packet statistics.

error: Displays error statistics.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding tunnel

Use display system internal lisp forwarding tunnel to display tunnel entry information.

Syntax

Centralized devices:

display system internal lisp forwarding tunnel

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding tunnel slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding tunnel chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp forwarding vrf-mapping

Use display system internal lisp forwarding vrf-mapping to display the instance ID-to-VRF mapping table.

Syntax

Centralized devices:

display system internal lisp forwarding vrf-mapping [ instance-id instance-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp forwarding vrf-mapping [ instance-id instance-id ] slot slot-number

Distributed devices in IRF mode:

display system internal lisp forwarding vrf-mapping [ instance-id instance-id ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

instance-id instance-id: Specifies a LISP instance by its ID in the range of 1 to 16777215. A LISP instance is an instance to which the LISP tunnel belongs. Each LISP instance is mapped to a VRF instance. If you do not specify a LISP instance, this command displays the instance ID-to-VRF mapping table for all LISP instances. Support for this option depends on the device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp nib

Use display system internal lisp nib to display the LISP RIB next hop information.

Syntax

display system internal lisp nib [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

nib-id: Specifies a next hop by its ID in the range of 1 to FFFFFFFF.

verbose: Displays detailed information about the LISP RIB next hop. If you do not specify the keyword, this command displays brief information about the LISP RIB next hop.

LISP probe commands -- display system internal lisp nib log

Use display system internal lisp nib log to display logs about the LISP RIB next hop.

Syntax

display system internal lisb nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

LISP probe commands -- display system internal lisp nsr no-cache

Use display system internal lisp nsr no-cache to display the tentative entries created during the NSR active/standby switchover.

Syntax

display system internal lisp nsr no-cache [ eid-prefix [ prefix-length ] ] [default | vrf vrf-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

eid-prefix: Specifies an EID prefix. If you do not specify an EID prefix, this command displays all tentative entries created during the NSR active/standby switchover.

prefix-length: Specifies the prefix length in the range of 0 to 32.

default: Displays the tentative entries for the public VRF instance.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the tentative entries for all VRF instances. Support for this option depends on the device model.

LISP probe commands -- display system internal lisp nsr status

Use display system internal lisp nsr status to display LISP NSR state.

Syntax

display system internal lisp nsr status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

LISP probe commands -- display system internal lisp nsr tunnel-mapping

Use display system internal lisp nsr backup-tunnel-mapping to display the backup tunnel mapping table information when the NSR state is smooth.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal lisp nsr backup-tunnel-mapping [ rloc-address ] [ default | vrf vrf-name ] standby slot slot-number

Distributed devices in IRF mode:

display system internal lisp nsr backup-tunnel-mapping [ rloc-address ] [ default | vrf vrf-name ] chassis chassis-number standby slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

rloc-address: Specifies an RLOC address.

default: Displays the backup tunnel mapping table information for the public network.

vrf vrf-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify a VPN instance, this command displays the backup tunnel mapping table information for all instances. Support for this option depends on the device model.

standby slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

standby slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- display system internal lisp routing-table

Use display system internal lisp routing-table to display the LISP routing table information.

Syntax

display system internal lisp routing-table ipv4 [ eid-prefix [ prefix-length ] ] [ default | vrf vrf-name ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

eid-prefix [ prefix-length ]: Specifies an EID prefix and its length. The value range for the prefix-length argument is 0 to 32. If you do not specify an EID prefix, this command displays LISP routing table information for all EID prefixes. If you do not specify the prefix length, this command displays the LISP routing table information for the optimal route.

default | vrf vrf-name: Displays the LISP routing table information for the public network or for an MPLS L3VPN instance. The MPLS L3VPN instance name is a case-sensitive string of 1 to 31 characters. If you do not specify the default keyword or a VPN instance, this command displays the LISP routing table information for all VPN instances and the public network. Support for this option depends on the device model.

LISP probe commands -- display system internal lisp statistics

Use display system internal lisp statistics to display statistics about the communication between the LISP user mode and kernel mode, and between the LISP user mode and RIB.

Syntax

display system internal lisp statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin

LISP probe commands -- reset system internal lisp forwarding statistics

Use reset system internal lisp forwarding statistics to clear LISP thread statistics.

Syntax

Centralized devices:

reset system internal lisp forwarding statistics

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal lisp forwarding statistics slot slot-number

Distributed devices in IRF mode:

reset system internal lisp forwarding statistics chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument specifies the member ID of the IRF member device. The slot-number argument specifies the slot number of the card. (Distributed devices in IRF mode.)

LISP probe commands -- reset system internal lisp statistics

Use reset system internal lisp statistics to clear LISP statistics.

Syntax

reset system internal lisp statistics

Views

Probe view

Predefined user roles

network-admin

mdc-admin