IS-IS probe commands -- display system internal isis import-route

Use display system internal isis import-route to display routes redistributed by IS-IS.

Syntax

Centralized devices:

display system internal isis import-route [ ipv4 [ topology topo-name ] ] [ process-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis import-route [ ipv4 [ topology topo-name ] ] [ process-id ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal isis import-route [ ipv4 [ topology topo-name ] ] [ process-id ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4: Displays routes redistributed by IS-IS.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays redistributed routes for the public network. Support for this option depends on the device model.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays routes redistributed by all IS-IS processes.

standby slot slot-number: Displays backup routes redistributed by IS-IS for an IRF member device. If you do not specify this option, the command displays routes redistributed by IS-IS. (Centralized IRF devices.)

standby slot slot-number: Displays backup routes redistributed by IS-IS for a card. If you do not specify this option, the command displays routes redistributed by IS-IS. (Distributed devices in standalone mode.)

standby chassis chassis-number slot slot-number: Displays backup routes redistributed by IS-IS for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays routes redistributed by IS-IS. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis interface

Use display system internal isis interface to display IS-IS interface information.

Syntax

display system internal isis interface [ ipv4 ] [ vpn-instance vpn-instance-name ] [ interface-type interface-number | ip-address { mask | mask-length } ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4: Displays information about IS-IS interfaces.

vpn-instance vpn-instance-name: Specifies an MPLS L3VPN instance by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays interface information for the public network. Support for this option depends on the device model.

interface-type interface-number: Specifies an interface by its type and number.

ip-address: Specifies an IP address in dotted decimal notation.

mask: Specifies the IP address mask in dotted decimal notation.

mask-length: Specifies the mask length, an integer in the range of 0 to 32.

IS-IS probe commands -- display system internal isis interface standby

Use display system internal isis interface standby to display backup IS-IS interface information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis interface [ interface-type interface-number ] [ verbose ] [ process-id ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal isis interface [ interface-type interface-number ] [ verbose ] [ process-id ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface-type interface-number: Specifies an interface by its type and number. If you do not specify this argument, the command displays information about all interfaces.

verbose: Displays detailed IS-IS interface information. If you do not specify this keyword, the command displays brief IS-IS interface information.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays interface information for all IS-IS processes.

standby slot slot-number: Displays backup IS-IS interface information for a card. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IS-IS interface information. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IS-IS interface information for an IRF member device. The slot-number argument represents the member ID of the IRF member device. If you do not specify this option, the command displays IS-IS interface information. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IS-IS interface information for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IS-IS interface information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis keychain

Use display system internal isis keychain to display IS-IS keychain information.

Syntax

display system internal isis keychain [ name keychain-name [ key key-id ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

keychain-name: Specifies a keychain by its name, a case-sensitive string of 1 to 63 characters. If you do not specify this argument, the command displays information for all keychains.

key-id: Specifies a key by its ID in the range of 0 to 281474976710655. If you do not specify this argument, the command displays information for all keys in the specified keychain.

IS-IS probe commands -- display system internal isis link-state

Use display system internal isis link-state to display IS-IS link state information.

Syntax

display system internal isis link-state [ link | log { control | data } | node | prefix | statistics ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

link: Displays IS-IS link state link information.

log: Displays IS-IS link state change log information.

control: Displays IS-IS link state control log information.

data: Displays IS-IS link state data log information.

node: Displays IS-IS link state node information.

prefix: Displays IS-IS link state prefix information.

statistics: Displays IS-IS link state change statistics.

Usage guidelines

If you do not specify any keyword, the command displays link state information for all IS-IS processes.

IS-IS probe commands -- display system internal isis lsdb standby

Use display system internal isis lsdb standby to display backup IS-IS LSDB information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis lsdb [ [ level-1 | level-2 ] | local | [ lsp-id lspid | lsp-name lspname ] | verbose ] * [ process-id ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal isis lsdb [ [ level-1 | level-2 ] | local | [ lsp-id lspid | lsp-name lspname ] | verbose ] * [ process-id ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

level-1: Displays the level-1 LSDB.

level-2: Displays the level-2 LSDB.

local: Displays LSP information generated locally.

lsp-id lspid: Specifies an LSP ID, in the form of SYSID.Pseudonode ID-fragment num, where SYSID specifies the system ID of the originating node or pseudo node, Pseudonode ID specifies the pseudo node ID, and fragment num specifies the fragment number of the LSP.

lsp-name lspname: Specifies the LSP name, in the form of Symbolic name.[Pseudo ID]-fragment num.

verbose: Displays detailed LSDB information. If you do not specify this keyword, the command displays brief information about LSDB.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays LSDBs for all IS-IS processes.

standby slot slot-number: Displays backup IS-IS LSDB information for a card. The slot-number argument represents the slot number of the card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IS-IS LSDB information for an IRF member device. The slot-number argument represents the member ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IS-IS LSDB information for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis nib

Use display system internal isis nib to display IS-IS next hop information.

Syntax

display system internal isis nib [ ipv4 ] [ nib-id ] [ verbose ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4: Displays IS-IS next hop information.

nib-id: Specifies a next hop by its ID, a hexadecimal number in the range of 1 to ffffffff. If you do not specify this argument, the command displays information about all next hops.

verbose: Displays detailed IS-IS next hop information. If you do not specify this keyword, the command displays brief IS-IS next hop information.

IS-IS probe commands -- display system internal isis nib log

Use display system internal isis nib log to display IS-IS next hop log information.

Syntax

display system internal isis nib log

Views

Probe view

Predefined user roles

network-admin

mdc-admin

IS-IS probe commands -- display system internal isis peer standby

Use display system internal isis peer standby to display backup IS-IS neighbor information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis peer [ statistics | verbose ] [ process-id ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal isis peer [ statistics | verbose ] [ process-id ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

statistics: Displays IS-IS neighbor statistics.

verbose: Displays detailed IS-IS neighbor information. If you do not specify this keyword, the command displays brief IS-IS neighbor information.

process-id: Displays IS-IS neighbor information for an IS-IS process specified by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays neighbor information for all IS-IS processes.

standby slot slot-number: Displays backup IS-IS neighbor information for a card. The slot-number argument represents the slot number of the card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IS-IS neighbor information for an IRF member device. The slot-number argument represents the member ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IS-IS neighbor information for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis prefix

Use display system internal isis prefix to display IS-IS prefix information.

Syntax

Centralized devices:

display system internal isis prefix [ ipv4 [ topology topo-name ] ] [ [ level-1 | level-2 ] | [ prefix mask-length ] ] * [ process-id ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis prefix [ ipv4 [ topology toponame ] ] [ [ level-1 | level-2 ] | [ prefix mask-length ] ] * [ process-id ] [ standby slot slot-number [ cpu cpu-number ] ]

Distributed devices in IRF mode:

display system internal isis prefix [ ipv4 [ topology toponame ] ] [ [ level-1 | level-2 ] | [ prefix mask-length ] ] * [ process-id ] [ standby chassis chassis-number slot slot-number [ cpu cpu-number ] ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ipv4: Displays IS-IS prefix information.

topology topo-name: Specifies a topology by its name, a case-sensitive string of 1 to 31 characters. If you do not specify this option, the command displays IS-IS prefix information for the public network. Support for this option depends on the device model.

level-1: Displays IS-IS Level-1 prefix information. If you do not specify a level, the command displays both Level-1 and Level-2 prefix information.

level-2: Displays IS-IS Level-2 prefix information. If you do not specify a level, the command displays both Level-1 and Level-2 prefix information.

prefix mask-length: Specifies a prefix and the mask length.

process-id: Specifies an IS-IS process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays prefix information for all IS-IS processes.

standby slot slot-number: Displays backup IS-IS prefix information for an IRF member device. If you do not specify this option, the command displays IS-IS prefix information. (Centralized IRF devices.)

standby slot slot-number: Displays backup IS-IS prefix information for a card. If you do not specify this option, the command displays IS-IS prefix information. (Distributed devices in standalone mode.)

standby chassis chassis-number slot slot-number: Displays IS-IS prefix information for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays IS-IS prefix information. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis standby

Use display system internal isis standby to display backup IS-IS process information.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal isis [ process-id ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal isis [ process-id ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

process-id: Specifies a process by its ID in the range of 1 to 65535. If you do not specify this argument, the command displays information about all IS-IS processes.

standby slot slot-number: Displays backup IS-IS process information for a card. The slot-number argument represents the slot number of the card. (Distributed devices in standalone mode.)

standby slot slot-number: Displays backup IS-IS process information for an IRF member device. The slot-number argument represents the member ID of the IRF member device. (Centralized IRF devices.)

standby chassis chassis-number slot slot-number: Displays backup IS-IS process information for a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

IS-IS probe commands -- display system internal isis status

Use display system internal isis status to display global IS-IS status information.

Syntax

display system internal isis status

Views

Probe view

Predefined user roles

network-admin

mdc-admin

IS-IS probe commands -- reset system internal isis link-state

Use reset system internal isis link-state to clear IS-IS link state statistics and log information.

Syntax

reset system internal isis link-state { log { control | data } | statistics }

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

log: Clears IS-IS link state change log information.

control: Clears IS-IS link state control log information.

data: Clears IS-IS link state data log information.

statistics: Clears IS-IS link state change statistics