FCoE probe commands -- display system internal fc fib

Use display system internal fc fib to display information about FC FIB entries of a VSAN.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal fc fib [ fcid [ mask-length ] ] vsan vsan-id [ slot slot-number ]

Distributed devices in IRF mode:

display system internal fc fib [ fcid [ mask-length ] ] vsan vsan-id [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

fcid: Specifies an FC FIB entry by an FC address in the range of 0 to ffffff (hexadecimal).

mask-length: Specifies the mask length for the FC address, in the range of 0 to 24.

vsan vsan-id: Specifies a VSAN by its ID in the range of 1 to 3839.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, the command displays the FC FIB entries for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, the command displays the FC FIB entries for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, the command displays the FC FIB entries for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays the FC FIB entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, the command displays the FC FIB entries for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

FCoE probe commands -- display system internal fcoe vfcinfo

Use display system internal fcoe vfcinfo to display the internal information of a VFC interface.

Syntax

Centralized devices:

display system internal fcoe vfcinfo interface vfc interface-number

Distributed devices in standalone mode:Centralized IRF devices:

display system internal fcoe vfcinfo vfc interface-number [ slot slot-number ]

Distributed devices in IRF mode:

display system internal fcoe vfcinfo vfc interface-number [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface vfc interface-number: Specifies a VFC interface by its number.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, the command displays the internal information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, the command displays the internal information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, the command displays the internal information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays the internal information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, the command displays the internal information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

FCoE probe commands -- display system internal fcoe vsaninfo

Use display system internal fcoe vsaninfo to display the internal information of a VSAN.

Syntax

Centralized devices:

display system internal fcoe vsaninfo interface vfc interface-number vsan vsan-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal fcoe vsaninfo interface vfc interface-number vsan vsan-id [ slot slot-number ]

Distributed devices in IRF mode:

display system internal fcoe vsaninfo interface vfc interface-number vsan vsan-id [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

interface vfc interface-number: Specifies a VFC interface by its number.

vsan vsan-id: Specifies a VSAN by its ID in the range of 1 to 3839.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, the command displays the internal information for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, the command displays the internal information for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, the command displays the internal information for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays the internal information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, the command displays the internal information for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

FCoE probe commands -- display system internal zone acl

Use display system internal zone acl to display information about issued zone ACLs in a VSAN.

Syntax

Centralized devices:

display system internal zone acl vsan vsan-id

Distributed devices in standalone mode:Centralized IRF devices:

display system internal zone acl vsan vsan-id [ slot slot-number ]

Distributed devices in IRF mode:

display system internal zone acl vsan vsan-id [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

vsan vsan-id: Specifies a VSAN by its ID in the range of 1 to 3839.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, the command displays information about issued zone ACLs for the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, the command displays information about issued zone ACLs for the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, the command displays information about issued zone ACLs for the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. If you do not specify this option, the command displays information about issued zone ACLs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, the command displays information about issued zone ACLs for the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)