MVRP commands -- display mvrp running-status

Use display mvrp running-status to display MVRP running status.

Syntax

display mvrp running-status [ interface interface-list ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

interface interface-list: Specifies a range of Ethernet interfaces in the form of interface-type interface-number1 [ to interface-type interface-number2 ]. The interface-type interface-number argument represents the interface type and interface number. The value for the interface-number2 argument must be greater than or equal to the value for the interface-number1 argument. If the specified interfaces are not enabled with MVRP, this command displays global MVRP information. If you do not specify this option, the command displays global MVRP information and MVRP running status for all MVRP-enabled ports.

Examples

# Display global MVRP information and MVRP running status for all MVRP-enabled ports.

<Sysname> display mvrp running-status

-------[MVRP Global Info]-------

Global Status : Enabled

Compliance-GVRP : False

----[GigabitEthernet1/0/1]----

Config Status : Enabled

Running Status : Enabled

Join Timer : 20 (centiseconds)

Leave Timer : 60 (centiseconds)

Periodic Timer : 100 (centiseconds)

LeaveAll Timer : 1000 (centiseconds)

Registration Type : Normal

Registered VLANs :

1(default), 2-10

Declared VLANs :

1(default), 2-10

Propagated VLANs :

1(default), 2-10

----[GigabitEthernet1/0/2]----

Config Status : Enabled

Running Status : Disabled

Join Timer : 20 (centiseconds)

Leave Timer : 60 (centiseconds)

Periodic Timer : 100 (centiseconds)

LeaveAll Timer : 1000 (centiseconds)

Registration Type : Normal

Registered VLANs :

None

Declared VLANs :

None

Propagated VLANs :

None

Table 1 Command output

Field | Description
MVRP Global Info | Global MVRP information.
Global Status | Global MVRP status: · Enabled. · Disabled.
Compliance-GVRP | GVRP compatibility status: · True—Compatible. · False—Incompatible.
Config Status | Whether MVRP is enabled on the port: · Enabled. · Disabled.
Running Status | Whether MVRP takes effect on the port: · Enabled—MVRP takes effect on the port. · Disabled—MVRP does not take effect on the port. Whether MVRP takes effect on a port is determined by the following items: · Global and port-specific MVRP enabling status. · Physical link state of the port. · Port link type. · Whether the port is a member of an aggregation group.
Registration Type | MVRP registration mode: · Normal. · Fixed. · Forbidden.
Registered VLANs | VLANs that the port has registered.
Declared VLANs | VLANs that the port has declared to its peer participant.
Propagated VLANs | VLANs that the port has learned and notified other participants on the same device to declare to their respective peer participants.

‌

MVRP commands -- display mvrp state

Use display mvrp state to display the MVRP state of a port in a VLAN.

Syntax

display mvrp state interface interface-type interface-number vlan vlan-id

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

interface interface-type interface-number: Specifies a port by its type and number.

vlan vlan-id: Specifies a VLAN by its VLAN ID in the range of 1 to 4094.

Examples

# Display the MVRP state of GigabitEthernet 1/0/1 in VLAN 2.

<Sysname> display mvrp state interface gigabitethernet 1/0/1 vlan 2

MVRP state of VLAN 2 on port GE1/0/1:

Port VLAN App-state Reg-state

------------------------ ------ ----------- -----------

GE1/0/1 2 VP IN

Table 2 Command output

Field | Description
MVRP state of VLAN 2 on port GE1/0/1 | MVRP state of GigabitEthernet 1/0/1 in VLAN 2.
App-state | State of the attribute that the local participant declares to its peer participant: · VO—Very anxious observer. · VP—Very anxious passive. · VN—Very anxious new. · AN—Anxious new. · AA—Anxious active. · QA—Quiet active. · LA—Leaving active. · AO—Anxious observer. · QO—Quiet observer. · AP—Anxious passive. · QP—Quiet passive. · LO—Leaving observer.
Reg-state | Registration state of the attribute declared by the peer participant on the local participant: · IN—The attribute is registered. · LV—The attribute is previously registered, but now it is being deregistered. · MT—The attribute is not registered.

‌

MVRP commands -- display mvrp statistics

Use display mvrp statistics to display MVRP statistics.

Syntax

display mvrp statistics [ interface interface-list ]

Views

Any view

Predefined user roles

network-admin

network-operator

mdc-admin

mdc-operator

Parameters

interface interface-list: Specifies a range of Ethernet interfaces in the form of interface-type interface-number1 [ to interface-type interface-number2 ]. The interface-type interface-number argument represents the interface type and interface number. The value for the interface-number2 argument must be greater than or equal to the value for the interface-number1 argument. If you do not specify this option, the command displays MVRP statistics of all MVRP-enabled ports.

Usage guidelines

If MVRP is disabled on the specified ports, this command does not provide any output.

Examples

# Display MVRP statistics of all ports.

<Sysname> display mvrp statistics

----[GigabitEthernet1/0/1]----

Failed Registrations : 1

Last PDU Origin : 000f-e200-0010

Frames Received : 201

New Event Received : 0

JoinIn Event Received : 1167

In Event Received : 0

JoinMt Event Received : 22387

Mt Event Received : 31

Leave Event Received : 210

LeaveAll Event Received : 63

Frames Transmitted : 120

New Event Transmitted : 0

JoinIn Event Transmitted : 311

In Event Transmitted : 0

JoinMt Event Transmitted : 873

Mt Event Transmitted : 11065

Leave Event Transmitted : 167

LeaveAll Event Transmitted : 4

Frames Discarded : 0

----[GigabitEthernet1/0/2]----

Failed Registrations : 0

Last PDU Origin : 0000-0000-0000

Frames Received : 0

New Event Received : 0

JoinIn Event Received : 0

In Event Received : 0

JoinMt Event Received : 0

Mt Event Received : 0

Leave Event Received : 0

LeaveAll Event Received : 0

Frames Transmitted : 0

New Event Transmitted : 0

JoinIn Event Transmitted : 0

In Event Transmitted : 0

JoinMt Event Transmitted : 0

Mt Event Transmitted : 0

Leave Event Transmitted : 0

LeaveAll Event Transmitted : 0

Frames Discarded : 0

Table 3 Command output

Field | Description
Failed Registrations | Number of VLAN registration failures through MVRP on the local participant.
Last PDU Origin | Source MAC address of the last MVRPDU.
Frames Received | Number of MVRP frames received.
New Event Received | Number of New events received.
JoinIn Event Received | Number of JoinIn events received.
In Event Received | Number of In events received.
JoinMt Event Received | Number of JoinMt events received.
Mt Event Received | Number of Mt events received.
Leave Event Received | Number of Leave events received.
LeaveAll Event Received | Number of LeaveAll events received.
Frames Transmitted | Number of MVRP frames sent.
New Event Transmitted | Number of New events sent.
JoinIn Event Transmitted | Number of JoinIn events sent.
In Event Transmitted | Number of In events sent.
JoinMt Event Transmitted | Number of JoinMt events sent.
Mt Event Transmitted | Number of Mt events sent.
Leave Event Transmitted | Number of Leave events sent.
LeaveAll Event Transmitted | Number of LeaveAll events sent.
Frames Discarded | Number of MVRP frames dropped.

‌

MVRP commands -- mrp timer join

Use mrp timer join to set the Join timer.

Use undo mrp timer join to restore the default.

Syntax

mrp timer join timer-value

undo mrp timer join

Default

The Join timer is 20 centiseconds.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Parameters

timer-value: Specifies the Join timer value (in centiseconds). The Join timer must meet the following requirements:

· Not less than 20 centiseconds.

· Less than half the Leave timer.

· Divisible by 20 centiseconds.

Examples

# Set the Join timer to 40 centiseconds. (In this example, the Leave timer is 100 centiseconds.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mrp timer join 40

Related commands

display mvrp running-status

mrp timer leave

MVRP commands -- mrp timer leave

Use mrp timer leave to set the Leave timer.

Use undo mrp timer leave to restore the default.

Syntax

mrp timer leave timer-value

undo mrp timer leave

Default

The Leave timer is 60 centiseconds.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Parameters

timer-value: Specifies the Leave timer value (in centiseconds). The Leave timer must meet the following requirements:

· Greater than two times the Join timer.

· Less than the LeaveAll timer.

· Divisible by 20 centiseconds.

Examples

# Set the Leave timer to 100 centiseconds. (In this example, the Join timer and LeaveAll timer use their default settings.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mrp timer leave 100

Related commands

display mvrp running-status

mrp timer join

mrp timer leaveall

MVRP commands -- mrp timer leaveall

Use mrp timer leaveall to set the LeaveAll timer.

Use undo mrp timer leaveall to restore the default.

Syntax

mrp timer leaveall timer-value

undo mrp timer leaveall

Default

The LeaveAll timer is 1000 centiseconds.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Parameter

timer-value: Specifies the LeaveAll timer value (in centiseconds). The LeaveAll timer must meet the following requirements:

· Greater than any Leave timer on each port.

· Not greater than 32760 centiseconds.

· Divisible by 20 centiseconds.

Usage guidelines

Each time the LeaveAll timer of a port expires, all attributes of the MSTIs on the port are deregistered throughout the network. To prevent this type of deregistration from affecting the network, do not set the LeaveAll timer to less than its default value.

To keep the dynamic VLANs learned through MVRP stable, do not set the LeaveAll timer less than its default value.

The device randomly changes the LeaveAll timer within a certain range when an MRP participant restarts its LeaveAll timer. This prevents the LeaveAll timer of a particular participant from always expiring first.

Examples

# Set the LeaveAll timer to 1500 centiseconds. (In this example, the Leave timer on each port uses the default setting.)

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mrp timer leaveall 1500

Related commands

display mvrp running-status

mrp timer leave

MVRP commands -- mrp timer periodic

Use mrp timer periodic to set the Periodic timer.

Use undo mrp timer periodic to restore the default.

Syntax

mrp timer periodic timer-value

undo mrp timer periodic

Default

The Periodic timer is 100 centiseconds.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Parameters

timer-value: Specifies the Periodic timer, which can be 0 or 100 centiseconds.

Usage guidelines

Setting the Periodic timer to 0 disables the Periodic timer.

Setting the Periodic timer to 100 enables the Periodic timer. The participant then sends MRP frames at an interval of 100 centiseconds.

Examples

# Disable the Periodic timer.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mrp timer periodic 0

Related commands

display mvrp running-status

MVRP commands -- mvrp enable

Use mvrp enable to enable MVRP on a port.

Use undo mvrp enable to disable MVRP on a port.

Syntax

mvrp enable

undo mvrp enable

Default

MVRP is disabled on a port.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

For MVRP to take effect on a port, make sure the following requirements are met:

· MVRP is enabled both globally and on the port.

· The port is physically up.

· The port link type is trunk.

· The port is not a member of an aggregation group.

Examples

# Enable MVRP on GigabitEthernet 1/0/1.

<Sysname> system-view

[Sysname] mvrp global enable

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] port link-type trunk

[Sysname-GigabitEthernet1/0/1] mvrp enable

Related commands

display mvrp running-status

MVRP commands -- mvrp global enable

Use mvrp global enable to enable MVRP globally.

Use undo mvrp global enable to disable MVRP globally.

Syntax

mvrp global enable

undo mvrp global enable

Default

MVRP is disabled globally.

Views

System view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

For MVRP to take effect on a port, enable MVRP both on the port and globally.

Disabling MVRP globally also disables MVRP on all ports.

Examples

# Enable MVRP globally.

<Sysname> system-view

[Sysname] mvrp global enable

Related commands

display mvrp running-status

MVRP commands -- mvrp gvrp-compliance enable

Use mvrp gvrp-compliance enable to enable GVRP compatibility for MVRP.

Use undo mvrp gvrp-compliance enable to restore the default.

Syntax

mvrp gvrp-compliance enable

undo mvrp gvrp-compliance enable

Default

MVRP is incompatible with GVRP.

Views

System view

Predefined user roles

network-admin

mdc-admin

Usage guidelines

When you enable GVRP compatibility for MVRP, the device can receive and send both MVRP and GVRP frames.

Examples

# Enable GVRP compatibility for MVRP.

<Sysname> system-view

[Sysname] mvrp gvrp-compliance enable

Related commands

display mvrp running-status

MVRP commands -- mvrp registration

Use mvrp registration to set the MVRP registration mode on a port.

Use undo mvrp registration to restore the default.

Syntax

mvrp registration { fixed | forbidden | normal }

undo mvrp registration

Default

The MVRP registration mode is normal.

Views

Layer 2 Ethernet interface view

Layer 2 aggregate interface view

Predefined user roles

network-admin

mdc-admin

Parameters

fixed: Specifies the fixed registration mode.

forbidden: Specifies the forbidden registration mode.

normal: Specifies the normal registration mode.

Examples

# Set the MVRP registration mode to fixed on GigabitEthernet 1/0/1.

<Sysname> system-view

[Sysname] interface gigabitethernet 1/0/1

[Sysname-GigabitEthernet1/0/1] mvrp registration fixed

Related commands

display mvrp running-status

MVRP commands -- reset mvrp statistics

Use reset mvrp statistics to clear MVRP statistics for ports.

Syntax

reset mvrp statistics [ interface interface-list ]

Views

User view

Predefined user roles

network-admin

mdc-admin

Parameters

interface interface-list: Specifies a range of Ethernet interfaces in the form of interface-type interface-number1 [ to interface-type interface-number2 ]. The interface-type interface-number argument represents the interface type and interface number. The value for the interface-number2 argument must be greater than or equal to the value for the interface-number1 argument. If you do not specify this option, the command clears MVRP statistics of all ports.

Examples

# Clear MVRP statistics for all ports.

<Sysname> reset mvrp statistics

Related commands

display mvrp statistics