VPLS probe commands -- debugging system internal l2vpn l2vfib

Use debugging system internal l2vpn l2vfib to enable L2VPN L2VFIB debugging.

Use undo debugging system internal l2vpn l2vfib to disable L2VPN L2VFIB debugging.

Syntax

Centralized devices:

debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync }

undo debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync }

Distributed devices in standalone mode:Centralized IRF devices:

debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync } slot slot-number [ cpu cpu-number ]

undo debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync } slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync } chassis chassis-number slot slot-number [ cpu cpu-number ]

undo debugging system internal l2vpn l2vfib { ac | all | config | lpw | sync } chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

L2VPN L2VFIB debugging is disabled.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ac: Specifies L2VPN L2VFIB AC debugging.

all: Specifies all L2VPN L2VFIB debugging functions.

config: Specifies L2VPN L2VFIB configuration debugging.

lpw: Specifies L2VPN L2VFIB LPW debugging.

sync: Specifies L2VPN L2VFIB synchronization debugging.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VPLS probe commands -- display system internal l2vpn l2vfib record

Use display system internal l2vpn l2vfib record to display information recorded by the L2VPN L2VFIB module.

Syntax

Centralized devices:

display system internal l2vpn l2vfib record [ start start-number ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2vpn l2vfib record [ start start-number ] slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal l2vpn l2vfib record [ start start-number ] chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

start start-number: Specifies the number of a record. This command displays the specified record and all records that follow. The value range for the start-number argument varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Related commands

reset system internal l2vpn l2vfib record

VPLS probe commands -- display system internal l2vpn l2vfib statistics

Use display system internal l2vpn l2vfib statistics to display L2VPN L2VFIB statistics.

Syntax

Centralized devices:

display system internal l2vpn l2vfib statistics

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2vpn l2vfib statistics slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal l2vpn l2vfib statistics chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VPLS probe commands -- display system internal l2vpn ldp

Use display system internal l2vpn ldp to display LDP PW label information for a standby LDP process.

Syntax

Distributed devices in standalone mode:Centralized IRF devices:

display system internal l2vpn ldp [ peer ip-address [ pw-id pw-id | vpls-id vpls-id ] ] [ verbose ] standby slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

display system internal l2vpn ldp [ peer ip-address [ pw-id pw-id | vpls-id vpls-id ] ] [ verbose ] standby chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Any view

Predefined user roles

network-admin

mdc-admin

Parameters

peer ip-address: Displays LDP PW label information advertised by the specified peer PE. The ip-address argument specifies the LSR ID of the peer PE. If you do not specify a peer PE, this command displays LDP PW label information advertised by all peer PEs.

pw-id pw-id: Displays FEC 128 LDP PW label information for the PW specified by its PW ID in the range of 1 to 4294967295. If you specify the peer ip-address option without the pw-id pw-id option, this command displays all LDP PW label information advertised by the specified peer PE.

vpls-id vpls-id: Displays FEC 129 LDP PW label information for the VPLS instance specified by its ID, which is a string of 3 to 21 characters. You can specify a VPLS ID in one of the following formats:

· 16-bit AS number:32-bit user-defined number. For example, 101:3.

· 32-bit IP address:16-bit user-defined number. For example, 192.168.122.15:1.

· 32-bit AS number:16-bit user-defined number, where the AS number must be equal to or greater than 65536. For example, 65536:1.

verbose: Displays detailed information. If you do not specify this keyword, the command displays brief information.

standby: Displays LDP PW label information for a standby LDP process.

slot slot-number: Specifies the slot number of the card where the standby process resides. (Distributed devices in standalone mode.)

slot slot-number: Specifies the member ID of the IRF member device where the standby process resides. (Centralized IRF devices.)

chassis chassis-number slot slot-number: Specifies the card where the standby process resides. The chassis-number argument represents the IRF member ID of the device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.)

cpu cpu-number: Specifies the CPU where the standby process resides. Support for this option depends on the device model.

Usage guidelines

LDP advertises PW label-PW bindings in the following ways:

· After you specify a remote PE with the peer command, LDP advertises a FEC 128-to-PW label binding to the remote PE.

· After BGP discovers a remote PE, LDP advertises a FEC 129-to-PW label binding to the remote PE.

This command can display the PW labels in the following ways:

· If you specify the pw-id pw-id option, this command displays PW labels for FEC 128.

· If you specify the vpls-id vpls-id option, this command displays PW labels for FEC 129.

· If you do not specify pw-id pw-id or vpls-id vpls-id, this command displays PW labels for both FEC 128 and FEC 129.

This command displays all the LDP PW labels received by the local device, and the PW labels successfully advertised by the local device to the peer PEs.

VPLS probe commands -- l2vpn l2vfib record size

Use l2vpn l2vfib record size to set the maximum number of entries that the L2VPN L2VFIB module can record.

Syntax

Centralized devices:

l2vpn l2vfib record size size

Distributed devices in standalone mode:Centralized IRF devices:

l2vpn l2vfib record size size slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

l2vpn l2vfib record size size chassis chassis-number slot slot-number [ cpu cpu-number ]

Default

The L2VPN L2VFIB module can record a maximum of 4096 entries.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

size: Specifies the maximum number of entries. The value range varies by device model.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. The slot-number argument represents the ID of the IRF member device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

VPLS probe commands -- reset system internal l2vpn l2vfib record

Use reset system internal l2vpn l2vfib record to clear information recorded by the L2VPN L2VFIB module.

Syntax

Centralized devices:

reset system internal l2vpn l2vfib record

Distributed devices in standalone mode:Centralized IRF devices:

reset system internal l2vpn l2vfib record slot slot-number [ cpu cpu-number ]

Distributed devices in IRF mode:

reset system internal l2vpn l2vfib record chassis chassis-number slot slot-number [ cpu cpu-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID of the IRF member device. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)

cpu cpu-number: Specifies a CPU by its number. This option is available only if multiple CPUs are available on the specified slot. Support for this option depends on the device model.

Related commands

display system internal l2vpn l2vfib record