Object group probe commands -- display system internal object-group

Use display system internal object-group to display configuration and reference information about object groups.

Syntax

Centralized devices:

display system internal object-group [ { { ip | ipv6 } address | port | service } [ default ] [ name object-group-name ] | name object-group-name ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal object-group [ { { ip | ipv6 } address | port | service } [ default ] [ name object-group-name ] | name object-group-name ] slot slot-number

Distributed devices in IRF mode:

display system internal object-group [ { { ip | ipv6 } address | port | service } [ default ] [ name object-group-name ] | name object-group-name ] chassis chassis-number slot slot-number

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

ip address: Specifies IPv4 address object groups.

ipv6 address: Specifies IPv6 address object groups.

port: Specifies port object groups.

service: Specifies service object groups.

default: Specifies the default object groups.

name object-group-name: Specifies an object group by its name, a case-insensitive string of 1 to 31 characters.

slot slot-number: Specifies a card by its slot number. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the member ID. The slot-number argument represents the slot number of the card. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. (Distributed devices in IRF mode.) (IRF 3 capable.)