DRNI probe commands -- debugging system internal distributed-relay rlink packet

Use debugging system internal distributed-relay rlink packet to enable RLINK packet debugging for DRNI.

Use undo debugging system internal distributed-relay rlink packet to disable RLINK packet debugging for DRNI.

Syntax

debugging system internal distributed-relay rlink packet { all | receive | send } [ interface interface-list ]

undo debugging system internal distributed-relay rlink packet { all | receive | send }

Default

RLINK packet debugging is disabled for DRNI.

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

all: Specifies debugging for received and sent RLINK packets.

receive: Specifies debugging for received RLINK packets.

send: Specifies debugging for sent RLINK packets.

interface interface-list: Specifies a list of Layer 2 aggregate interfaces, in the format of interface-type interface-number1 [ to interface-type interface-number2 ]. You can specify only Layer 2 aggregate interfaces. If you do not specify any interfaces, this command applies to all Layer 2 aggregate interfaces on which RLINK runs.

DRNI probe commands -- display system internal distributed-relay global

Use display system internal distributed-relay global to display global DRNI information.

Syntax

Centralized devices:

display system internal distributed-relay global [ drcp | keepalive | kernel | rlink ]

Distributed devices in standalone mode:Centralized IRF devices:

display system internal distributed-relay global [ drcp | keepalive | kernel | rlink ] [ slot slot-number ]

Distributed devices in IRF mode:

display system internal distributed-relay global [ drcp | keepalive | kernel | rlink ] [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

drcp: Displays DRCPDU information.

keepalive: Displays keepalive packet information.

kernel: Displays kernel information.

rlink: Display RLINK packet information.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)

DRNI probe commands -- display system internal distributed-relay interface

Use display system internal distributed-relay interface to display information about an IPP or a DR interface.

Syntax

Centralized devices:

display system internal distributed-relay interface bridge-aggregation interface-number { local | peer | drcp-local | drcp-peer | drcpdu | fsm | kernel }

Distributed devices in standalone mode:Centralized IRF devices:

display system internal distributed-relay interface bridge-aggregation interface-number { local | peer | drcp-local | drcp-peer | drcpdu | fsm | kernel } [ slot slot-number ]

Distributed devices in IRF mode:

display system internal distributed-relay interface bridge-aggregation interface-number { local | peer | drcp-local | drcp-peer | drcpdu | fsm | kernel } [ chassis chassis-number slot slot-number ]

Views

Probe view

Predefined user roles

network-admin

mdc-admin

Parameters

bridge-aggregation interface-number: Specifies an IPP or a DR interface.

local: Displays local information.

peer: Displays remote information.

drcp-local: Displays local DRCPDU information.

drcp-peer: Displays remote DRCPDU information.

drcpdu: Displays DRCPDU statistics.

fsm: Displays FSM information.

kernel: Displays kernel information.

slot slot-number: Specifies a card by its slot number. If you do not specify a card, this command displays information about the active MPU. (Distributed devices in standalone mode.)

slot slot-number: Specifies an IRF member device by its member ID. If you do not specify a member device, this command displays information about the master device. (Centralized IRF devices.) (IRF 3 incapable.)

slot slot-number: Specifies an IRF member device by its member ID or specifies a PEX by its virtual slot number. If you do not specify a member device or PEX, this command displays information about the master device. (Centralized IRF devices.) (IRF 3 capable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device. The chassis-number argument represents the IRF member ID. The slot-number argument represents the slot number of the card. If you do not specify a card, this command displays information about the global active MPU. (Distributed devices in IRF mode.) (IRF 3 incapable.)

chassis chassis-number slot slot-number: Specifies a card on an IRF member device or specifies a PEX. The chassis-number argument represents the member ID of the IRF member device or the virtual chassis number of the PEX. The slot-number argument represents the slot number of the card or PEX. If you do not specify a card or PEX, this command displays information about the global active MPU. (Distributed devices in IRF mode.) (IRF 3 capable.)